(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "RF_WIFI_BT")
	(net 3 "VDD_NRF")
	(net 4 "Net-(IC1-VDD)")
	(net 5 "Net-(U1-VIN)")
	(net 6 "Net-(U1-VBST)")
	(net 7 "Net-(U1-SW)")
	(net 8 "Bat Shunt 1")
	(net 9 "+5V")
	(net 10 "Net-(C20-Pad2)")
	(net 11 "Net-(IC2-VG)")
	(net 12 "Net-(IC2-VCC)")
	(net 13 "USE_ANT_2")
	(net 14 "+4V")
	(net 15 "Net-(S1-RFC)")
	(net 16 "RF_LORA")
	(net 17 "unconnected-(C37-Pad1)")
	(net 18 "unconnected-(C40-Pad1)")
	(net 19 "Net-(S1-RF2)")
	(net 20 "Net-(S2-RFC)")
	(net 21 "Net-(J7-In)")
	(net 22 "Net-(S1-RF1)")
	(net 23 "Net-(S2-RF1)")
	(net 24 "Net-(IC3-TX)")
	(net 25 "Net-(S2-RF2)")
	(net 26 "Net-(IC3-RX3)")
	(net 27 "Net-(IC3-ANT)")
	(net 28 "Net-(J3-In)")
	(net 29 "Net-(D1-K)")
	(net 30 "Net-(D1-A)")
	(net 31 "Net-(D2-A)")
	(net 32 "Net-(D3-K)")
	(net 33 "Net-(D3-A)")
	(net 34 "Net-(D5-K)")
	(net 35 "Net-(D6-K)")
	(net 36 "Sys Load")
	(net 37 "D+")
	(net 38 "CC1")
	(net 39 "unconnected-(IC1-CFG3-Pad3)")
	(net 40 "unconnected-(IC1-CFG2-Pad2)")
	(net 41 "Net-(IC1-VBUS)")
	(net 42 "Net-(IC1-CFG1)")
	(net 43 "D-")
	(net 44 "CC2")
	(net 45 "Net-(IC2-MPPT)")
	(net 46 "Net-(IC2-COM)")
	(net 47 "Net-(IC2-CSP)")
	(net 48 "Net-(IC2-DRV)")
	(net 49 "RADIO C1")
	(net 50 "RADIO TX")
	(net 51 "Net-(IC3-RX1)")
	(net 52 "RADIO C2")
	(net 53 "unconnected-(IC4-DIO3-Pad22)")
	(net 54 "unconnected-(IC4-DCC_SW-Pad14)")
	(net 55 "unconnected-(IC4-DIO2-Pad23)")
	(net 56 "unconnected-(IC4-VREG-Pad12)")
	(net 57 "unconnected-(IC4-VBAT_RF-Pad2)")
	(net 58 "unconnected-(IC4-DNC_2-Pad17)")
	(net 59 "unconnected-(IC4-GND_1-Pad13)")
	(net 60 "unconnected-(IC4-DIO9-Pad9)")
	(net 61 "unconnected-(IC4-DIO4-Pad21)")
	(net 62 "unconnected-(IC4-RFI_N_LF1-Pad27)")
	(net 63 "unconnected-(IC4-DIO6-Pad19)")
	(net 64 "unconnected-(IC4-DIO1-Pad24)")
	(net 65 "unconnected-(IC4-DIO0{slash}BUSY-Pad25)")
	(net 66 "unconnected-(IC4-32K_N{slash}_DIO10-Pad8)")
	(net 67 "unconnected-(IC4-VTCXO-Pad3)")
	(net 68 "unconnected-(IC4-VR_PA-Pad1)")
	(net 69 "unconnected-(IC4-RFIO_HF-Pad26)")
	(net 70 "unconnected-(IC4-RFO_HP_LF-Pad32)")
	(net 71 "unconnected-(IC4-RFO_LP_LF-Pad31)")
	(net 72 "unconnected-(IC4-XTA-Pad4)")
	(net 73 "unconnected-(IC4-DNC_3-Pad18)")
	(net 74 "unconnected-(IC4-GND_2-Pad33)")
	(net 75 "unconnected-(IC4-RFI_N_LF0-Pad29)")
	(net 76 "unconnected-(IC4-XTB-Pad5)")
	(net 77 "unconnected-(IC4-DIO5-Pad20)")
	(net 78 "unconnected-(IC4-32K_P{slash}_DIO11-Pad7)")
	(net 79 "unconnected-(IC4-VBAT-Pad15)")
	(net 80 "unconnected-(IC4-DIO7-Pad11)")
	(net 81 "unconnected-(IC4-DNC_1-Pad16)")
	(net 82 "unconnected-(IC4-DIO8-Pad10)")
	(net 83 "unconnected-(IC4-RFI_P_LF0-Pad30)")
	(net 84 "unconnected-(IC4-NRESET-Pad6)")
	(net 85 "unconnected-(IC4-RFI_P_LF1-Pad28)")
	(net 86 "Net-(J1-D--PadA7)")
	(net 87 "VBUS")
	(net 88 "unconnected-(J1-SBU1-PadA8)")
	(net 89 "Net-(J1-D+-PadA6)")
	(net 90 "unconnected-(J1-SBU2-PadB8)")
	(net 91 "GPS_RX")
	(net 92 "GPS_TX")
	(net 93 "GPS_EN")
	(net 94 "Sol Shunt 1")
	(net 95 "unconnected-(J6-NC{slash}TDI-Pad8)")
	(net 96 "RST")
	(net 97 "unconnected-(J6-KEY-Pad7)")
	(net 98 "SWDIO")
	(net 99 "unconnected-(J6-SWO{slash}TDO-Pad6)")
	(net 100 "SWDCLK")
	(net 101 "Net-(U2-L)")
	(net 102 "Net-(U3-L)")
	(net 103 "Charger Load")
	(net 104 "Net-(U1-EN)")
	(net 105 "Net-(U1-VFB)")
	(net 106 "unconnected-(R13-Pad1)")
	(net 107 "unconnected-(R14-Pad2)")
	(net 108 "I2C SDA")
	(net 109 "I2C SCL")
	(net 110 "Net-(U3-FB)")
	(net 111 "USE_ANT_1")
	(net 112 "unconnected-(R23-Pad1)")
	(net 113 "USR_BUTTON")
	(net 114 "Net-(R25-Pad1)")
	(net 115 "Net-(R27-Pad2)")
	(net 116 "Net-(R28-Pad2)")
	(net 117 "Net-(R30-Pad2)")
	(net 118 "RADIO RX")
	(net 119 "unconnected-(U5-CRITICAL-Pad9)")
	(net 120 "unconnected-(U5-PV-Pad10)")
	(net 121 "unconnected-(U5-WARNING-Pad8)")
	(net 122 "unconnected-(U5-EP-Pad17)")
	(net 123 "unconnected-(U5-TC-Pad13)")
	(net 124 "unconnected-(U5-A0-Pad5)")
	(net 125 "unconnected-(U7-TRACEDATA1{slash}P0.12-PadU1)")
	(net 126 "unconnected-(U7-SWDCLK-PadAA24)")
	(net 127 "unconnected-(U7-ANT-PadH23)")
	(net 128 "unconnected-(U7-P1.13-PadA16)")
	(net 129 "Net-(U7-VSS-PadB7)")
	(net 130 "unconnected-(U7-AIN1{slash}P0.03-PadB13)")
	(net 131 "unconnected-(U7-XC2-PadA23)")
	(net 132 "unconnected-(U7-P1.05-PadT23)")
	(net 133 "unconnected-(U7-P0.20-PadAD16)")
	(net 134 "unconnected-(U7-P0.13-PadAD8)")
	(net 135 "unconnected-(U7-AIN3{slash}P0.05-PadK2)")
	(net 136 "unconnected-(U7-XC1-PadB24)")
	(net 137 "Net-(U7-VDD-PadA22)")
	(net 138 "unconnected-(U7-P1.11-PadB19)")
	(net 139 "unconnected-(U7-D+-PadAD6)")
	(net 140 "unconnected-(U7-DEC1-PadC1)")
	(net 141 "unconnected-(U7-DEC3-PadD23)")
	(net 142 "unconnected-(U7-XL2{slash}P0.01-PadF2)")
	(net 143 "unconnected-(U7-D--PadAD4)")
	(net 144 "unconnected-(U7-AIN2{slash}P0.04-PadJ1)")
	(net 145 "unconnected-(U7-P1.10-PadA20)")
	(net 146 "unconnected-(U7-AIN0{slash}P0.02-PadA12)")
	(net 147 "unconnected-(U7-TRACEDATA0{slash}P1.00-PadAD22)")
	(net 148 "unconnected-(U7-P1.03-PadV23)")
	(net 149 "unconnected-(U7-NFC1{slash}P0.09-PadL24)")
	(net 150 "unconnected-(U7-DEC5-PadN24)")
	(net 151 "unconnected-(U7-P1.12-PadB17)")
	(net 152 "unconnected-(U7-NFC2{slash}P0.10-PadJ24)")
	(net 153 "unconnected-(U7-P0.21-PadAC17)")
	(net 154 "unconnected-(U7-P1.02-PadW24)")
	(net 155 "unconnected-(U7-AIN4{slash}P0.28-PadB11)")
	(net 156 "unconnected-(U7-P0.15-PadAD10)")
	(net 157 "unconnected-(U7-VBUS-PadAD2)")
	(net 158 "unconnected-(U7-VSS_PA-PadF23)")
	(net 159 "unconnected-(U7-P1.08-PadP2)")
	(net 160 "unconnected-(U7-P0.06-PadL1)")
	(net 161 "unconnected-(U7-TRACEDATA2{slash}P0.11-PadT2)")
	(net 162 "unconnected-(U7-P0.18{slash}~{RESET}-PadAC13)")
	(net 163 "unconnected-(U7-P0.24-PadAD20)")
	(net 164 "unconnected-(U7-P0.08-PadN1)")
	(net 165 "unconnected-(U7-P1.14-PadB15)")
	(net 166 "unconnected-(U7-P0.14-PadAC9)")
	(net 167 "unconnected-(U7-P0.23-PadAC19)")
	(net 168 "unconnected-(U7-XL1{slash}P0.00-PadD2)")
	(net 169 "unconnected-(U7-DEC4-PadB5)")
	(net 170 "unconnected-(U7-AIN7{slash}P0.31-PadA8)")
	(net 171 "unconnected-(U7-DCCH-PadAB2)")
	(net 172 "unconnected-(U7-P0.25-PadAC21)")
	(net 173 "unconnected-(U7-AIN5{slash}P0.29-PadA10)")
	(net 174 "unconnected-(U7-P1.07-PadP23)")
	(net 175 "unconnected-(U7-DECUSB-PadAC5)")
	(net 176 "unconnected-(U7-P0.26-PadG1)")
	(net 177 "unconnected-(U7-DEC2-PadA18)")
	(net 178 "unconnected-(U7-P1.15-PadA14)")
	(net 179 "unconnected-(U7-DEC6-PadE24)")
	(net 180 "unconnected-(U7-SWDIO-PadAC24)")
	(net 181 "unconnected-(U7-P0.27-PadH2)")
	(net 182 "unconnected-(U7-P0.19-PadAC15)")
	(net 183 "unconnected-(U7-P1.04-PadU24)")
	(net 184 "unconnected-(U7-P1.06-PadR24)")
	(net 185 "unconnected-(U7-P1.01-PadY23)")
	(net 186 "unconnected-(U7-P0.17-PadAD12)")
	(net 187 "unconnected-(U7-TRACECLK{slash}P0.07-PadM2)")
	(net 188 "unconnected-(U7-DCC-PadB3)")
	(net 189 "unconnected-(U7-P0.16-PadAC11)")
	(net 190 "unconnected-(U7-TRACEDATA3{slash}P1.09-PadR1)")
	(net 191 "unconnected-(U7-VDDH-PadY2)")
	(net 192 "unconnected-(U7-P0.22-PadAD18)")
	(net 193 "unconnected-(U7-AIN6{slash}P0.30-PadB9)")
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "034ede17-6c51-4211-812b-5e254b8955c6")
		(at 163.235 69.605)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D3"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "9ff76902-0a2c-46c9-b2f2-819711798cd2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "442f676c-f295-48d4-8b13-393f35d0c23c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d33a38f0-8195-48d7-966d-54724786ed66")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "fe877985-78e3-4f72-b285-49efc9a72250")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/a43975a2-00d5-4ed2-9ce3-de26a28fb474")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84c0c6a0-65d4-4e86-a2ea-5dab40e7db51")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "64abb8cf-573c-45da-bdb9-f31a4dff18e9")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f14f7e2e-0dac-4dca-af0c-9766c82695b2")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a5bdc5ba-4970-458d-805d-286947fdc686")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3a3b8c8f-bc5a-4306-9a51-966c5b76478d")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fc6d058e-5983-4b4a-8aca-4dc36a7b5e9c")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3bd1df56-42c2-4c72-8e5a-b3d7bb7ccc63")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "91fbaf5d-db30-4a88-a8b2-b8806927817b")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "67fb19ce-db53-4fc3-871c-fb80b2779ea5")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8d7fe56-1c4a-4fea-bc94-e3e844f7916c")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80fa3248-4b57-4d07-8b54-ddcae7d60b82")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "03ab5c7e-e833-497f-88f2-a16d9af7a5ff")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e3b8948e-2f7d-4f85-add1-662e7d32e55f")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 32 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "508337bd-298d-460c-a0c8-37f570fa6a54")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 33 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "8a615705-c252-4d58-9ab7-527439850497")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "0565dc1b-f17a-4436-bf11-8d5d7f8cee40")
		(at 147.15 105.09)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C44"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "ce529ef0-35e6-483d-b7db-933e7b40976b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "afa703aa-4a67-40ae-bea2-1198e297b962")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bf222390-4310-4b89-a15e-196c06a66f49")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "69d4f2f5-dbb7-4d5b-8ffd-e4676cac7ed6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/005bfe92-e5dc-412e-822d-0a1e1b4040f7")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f305fc75-1c37-4ba4-9a90-414aff33a545")
		)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4926ace7-9eaf-4625-b022-2ce4011ba708")
		)
		(fp_line
			(start -1.65 -0.73)
			(end 1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b039e69c-3759-40c4-8b79-ba7ed486d6f5")
		)
		(fp_line
			(start -1.65 0.73)
			(end -1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0aa61600-d392-4f50-8ff3-c33c2bda6687")
		)
		(fp_line
			(start 1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c6225412-ce3e-4627-b51e-327606deb824")
		)
		(fp_line
			(start 1.65 0.73)
			(end -1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3a6d0409-4928-4d33-ad12-a7491f8baf75")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fdc4d020-c740-45d7-9905-c79b007d17fc")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1f9a94e2-9349-46b6-a412-d347f27e0fba")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c6a93e6-42a0-4959-a515-00302c031a87")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32a9dc5c-c92c-4395-a755-4484aa6d6882")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "841b4263-65a4-496c-b763-36435659e794")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(S2-RF2)")
			(pintype "passive")
			(uuid "af0b03a6-8fa3-4256-98d0-ce4ca48db664")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(IC3-RX3)")
			(pintype "passive")
			(uuid "fa38c103-6499-49c0-a5e5-94b2c0e80eb2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "0633c1b3-10b3-49af-8fc5-c8e48a112146")
		(at 163.235 66.565)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "8a39229e-a8f3-4748-a15e-19e6489fdfbf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "400eeb5d-2c09-4c2a-910f-22c4da039ad2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6f98d1d7-c6de-487a-ad63-bbb6e15783fa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5c6b324f-3248-45b2-a0db-7877714eb883")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/38d60f25-e00c-4565-b040-4604500ef45c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9b26881a-c41f-4c71-9571-35b8672b2ced")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f68867b6-cab6-4ce2-96e0-eeb03c79d33e")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c4aefbba-a910-4ee4-bdd2-f17b7040288e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "efe4a207-aa7e-4693-9d02-7b5aa0c0b2e4")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "48c56547-a02c-4b2c-8eb1-8e2b01d98a1d")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eefcb70a-15c9-4bbb-a790-b5604bb4a817")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "874eaaf0-fc74-4340-a6ad-fbd8ce9c9fde")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c1453f9-5121-4b96-9c3f-f8e0861c889e")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3fa1de63-b2c4-4124-9926-22c1d923a5fb")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e06275a8-1780-4229-b804-169c1d583076")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc54ffed-276b-41b1-8b11-55b7883a4d60")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7fe8b8fc-e5b8-48aa-9f8b-4005b1346623")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e74f13ec-40aa-43b2-9f4c-c4769d0878fe")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "cdb91647-816e-40ce-8805-b05c047b7690")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 31 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "dcf7f01b-2c9e-4c6a-bc96-4efad80bbd3e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "083f134e-ecbe-4983-a03b-96c409c61f83")
		(at 115.35 63.48)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "a60804d8-a191-459a-aa2b-ed41d3f527f7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "33.2k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "7b437262-582d-465c-b448-71808b0f2e42")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "af2181fb-2655-4a5f-93fd-56f55bef50c7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b3b60719-bc6b-4d38-a96a-6c9f0f4704ad")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/ae453145-5347-4639-bc75-c1f10260037b")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "04110862-d68e-4373-94b0-3447467ba498")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "224cee07-5389-4b3c-a966-588052148a6e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12db28de-d4da-40cc-b780-066f38365623")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "148885b9-c0b1-427f-9556-0785aa700413")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "20483304-dfed-43e3-82bb-c0518871e6ab")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "579e3b37-ff73-4efd-b183-80132119c637")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0f995ad3-c7cb-46fc-a523-a4cb563f8d79")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8bc9fcc7-e48f-4462-9d18-87b987d19326")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c293f7b-b8f3-4170-96a7-8609d90155a8")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f2d4e48-1057-4198-9d3a-d9cac2ad0fa7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c77f549b-4d4b-4767-8b70-1ea0b4eaef28")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "68cc6827-f780-4092-b14c-348f1e1d8dc7")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 105 "Net-(U1-VFB)")
			(pintype "passive")
			(uuid "43fa61b6-ceb4-4175-94f5-809bcd8fcad0")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "09c5de8d-0d04-4117-b2c7-8d6b2cf983e4")
		(at 139.25 81.57)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C34"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "7b926f4d-0dfb-40e6-8e59-c13ee539a834")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "8909db2b-0cdc-4d5e-9bdb-b2d060460f7c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "83689b0a-b221-4134-8cd5-bf48c02d03f8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "65aa971a-41fd-453d-b0c4-114358badd1d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/45a12d5e-c3b2-4a0f-8c5c-df015225923d")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d27b9bdb-dbf8-49e1-8899-f65b20362dc0")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bfa30fbf-45d7-40cd-bc8d-c7d0e2493fe5")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "46436e74-56ab-43be-beb0-1e8b4a54353d")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f9d3ad80-b731-4825-a134-f426bd33bb2a")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc66d79d-b596-4ba3-8071-06679a1b8a51")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2750694a-6b17-48d0-9f70-46d66541899d")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ad3a2f7f-71b8-4749-830d-cab3c2d15155")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "09b87744-2bfb-43d3-b1e3-abafe5f27677")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3866e16d-923e-4d2e-bdde-f5af1c416d72")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de9573e8-41ee-4204-ba51-b4ccd3b39a49")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d871d2e8-1697-454d-9d70-56e5305b1f5b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "cfe723dd-7c0d-4548-8540-60e7514e7ee9")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "b4bd90e7-f3e2-421a-9575-e6b060eef869")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "0b0afdb3-afdb-4039-a5e9-107caa06c8fe")
		(at 134.44 78.56)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C13"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "fec01155-db18-46e3-b4fe-aea89589ac42")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "728cf8f8-8eff-4240-9f48-50b37176a1f2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "65074f51-47fc-4468-b099-c2dcb5440aa6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cae0273a-8e73-4fe4-8da1-9b534b809d3a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5386a405-ca64-4db7-9b58-2b01b62dfa51")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "09ab2f7e-6d66-48cd-a320-59cd3fff5dfb")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "60f2282c-2801-4a4c-be96-d0da4d21a5ae")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "04c17203-2acd-4568-ad3a-55c22fe598ee")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ae307076-6a50-4507-b0e8-c70b2dc63706")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0bd0a947-77e8-4a14-81df-627a0cd6ba25")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "22f48a7d-bdab-4c76-b9af-d8a4f1de946c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c4f95516-8b25-45b7-98e1-a28f3e684780")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5f5fb32c-6020-4635-a903-191388e68886")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c120ef2c-adc8-4f34-8f3c-9cabe5a5f41f")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b7568c3-d431-4a96-bcb0-ef0fd15e896a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8228e0cd-f4c8-473f-a319-f82cac3c5a2c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "fe82993d-510b-4334-8466-6aa5efa87563")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "23e4ad8c-83d2-4865-bad6-9e2dcf4931e8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
		(layer "F.Cu")
		(uuid "0ef7b568-9417-4c55-84d5-033e622242a2")
		(at 168.17 96.61)
		(descr "Texas RGV0016A VQFN, 16 Pin (http://www.ti.com/lit/ds/symlink/ina3221.pdf#page=44), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "Texas VQFN NoLead")
		(property "Reference" "U5"
			(at 0 -3.33 0)
			(layer "F.SilkS")
			(uuid "f0dd34fe-07ab-4e29-a884-f7c28a18144b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "INA3221"
			(at 0 3.33 0)
			(layer "F.Fab")
			(uuid "e5118e75-3676-491b-881f-0638944746ce")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina3221.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ecb29bd1-cbfb-47d2-9c98-a17e1b7a22ea")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Triple-Channel High-Side Shunt and Bus Voltage Monitor with I2C and SMBUS Compatible Interface, QFN-16"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a8fb6c79-2167-4719-a5fe-aca35f7894c9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C181255"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9ce3f7fc-92ad-42ba-a5d1-c35103adc61a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field6" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "810aa144-9b20-490c-9309-22faf6add0cc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ac8ef210-cb18-4f96-9da9-b7bbad113a97")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "08f64ed8-26d4-4aca-944f-b858d61d79d4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Texas*RGV0016A*")
		(path "/baa3bafb-eaa8-4edd-b990-34769c6f289b")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.11 -1.41)
			(end -2.11 -1.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "df4dbfbe-3d00-4e3e-acba-08e0304305f4")
		)
		(fp_line
			(start -2.11 2.11)
			(end -2.11 1.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8bff2116-3595-4c42-bf94-f8481f7086da")
		)
		(fp_line
			(start -1.41 -2.11)
			(end -1.81 -2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9c707c15-9f7e-47f9-9878-b1be4c98dbd8")
		)
		(fp_line
			(start -1.41 2.11)
			(end -2.11 2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "08167561-ff84-4fd8-9f1e-ad3866db0c6a")
		)
		(fp_line
			(start 1.41 -2.11)
			(end 2.11 -2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9b57e04d-a991-4c91-895d-8e9bf91e8161")
		)
		(fp_line
			(start 1.41 2.11)
			(end 2.11 2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e787510e-99e0-406e-b006-b3b43923cf3c")
		)
		(fp_line
			(start 2.11 -2.11)
			(end 2.11 -1.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d713c75c-3d8c-4f20-91dd-607de05c126f")
		)
		(fp_line
			(start 2.11 2.11)
			(end 2.11 1.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4c5013be-9276-412e-8a06-98f55bd3bf37")
		)
		(fp_poly
			(pts
				(xy -2.11 -2.11) (xy -2.35 -2.44) (xy -1.87 -2.44)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "983c8469-1b2a-4826-a6ee-3e5191b64306")
		)
		(fp_rect
			(start -2.63 -2.63)
			(end 2.63 2.63)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "d8609823-fd9d-4060-976a-f81ae18f705d")
		)
		(fp_poly
			(pts
				(xy -2 -1) (xy -2 2) (xy 2 2) (xy 2 -2) (xy -1 -2)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "e0c99129-c9ad-4e3b-bc20-07c4cdd48523")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "91ab14dc-504a-42fd-a079-b991d6b43226")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" smd roundrect
			(at -0.525 -0.525)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "6147390a-562f-4e03-84dc-0c307535d33d")
		)
		(pad "" smd roundrect
			(at -0.525 0.525)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "4b6c8014-f805-4ab4-9c22-5e095f81f578")
		)
		(pad "" smd roundrect
			(at 0.525 -0.525)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "34c360e5-8081-431f-b54d-aa3f26357a62")
		)
		(pad "" smd roundrect
			(at 0.525 0.525)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "691f17c8-ab58-4854-bc7e-9c600bf1fdee")
		)
		(pad "1" smd roundrect
			(at -1.8625 -0.975)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "Sys Load")
			(pinfunction "IN-3")
			(pintype "input")
			(uuid "8a5a61a8-1688-49c7-9e06-7f3c53761857")
		)
		(pad "2" smd roundrect
			(at -1.8625 -0.325)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "Sys Load")
			(pinfunction "IN+3")
			(pintype "input")
			(uuid "8bb4928f-94b6-4c8e-935f-33c4077c8aae")
		)
		(pad "3" smd roundrect
			(at -1.8625 0.325)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "41481be4-fa07-4363-880d-30f4688a9414")
		)
		(pad "4" smd roundrect
			(at -1.8625 0.975)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VDD_NRF")
			(pinfunction "VS")
			(pintype "power_in")
			(uuid "02bfd45b-c654-475e-b188-076cd1294fbd")
		)
		(pad "5" smd roundrect
			(at -0.975 1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 124 "unconnected-(U5-A0-Pad5)")
			(pinfunction "A0")
			(pintype "input+no_connect")
			(uuid "b955cec5-f571-4789-a7c7-7feab3547b6d")
		)
		(pad "6" smd roundrect
			(at -0.325 1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "I2C SCL")
			(pinfunction "SCL")
			(pintype "input")
			(uuid "f36aa8b4-ed2a-4f7f-8cab-3e05bb4aad7d")
		)
		(pad "7" smd roundrect
			(at 0.325 1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "I2C SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
			(uuid "c95e8ed3-57e3-4df5-843b-c30b61ad128c")
		)
		(pad "8" smd roundrect
			(at 0.975 1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "unconnected-(U5-WARNING-Pad8)")
			(pinfunction "WARNING")
			(pintype "open_collector+no_connect")
			(uuid "4bf3e226-eb42-4c0c-ab2e-1d3a2b1b9be9")
		)
		(pad "9" smd roundrect
			(at 1.8625 0.975)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "unconnected-(U5-CRITICAL-Pad9)")
			(pinfunction "CRITICAL")
			(pintype "open_collector+no_connect")
			(uuid "26ef4179-522d-4dd7-bf30-ea077a01e5be")
		)
		(pad "10" smd roundrect
			(at 1.8625 0.325)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 120 "unconnected-(U5-PV-Pad10)")
			(pinfunction "PV")
			(pintype "open_collector+no_connect")
			(uuid "3c2d3ec9-7747-4c7d-afad-72ecc8844853")
		)
		(pad "11" smd roundrect
			(at 1.8625 -0.325)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Bat Shunt 1")
			(pinfunction "IN-1")
			(pintype "input")
			(uuid "eca2e373-6ee4-4d0c-ac89-a975d5240a67")
		)
		(pad "12" smd roundrect
			(at 1.8625 -0.975)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Bat Shunt 1")
			(pinfunction "IN+1")
			(pintype "input")
			(uuid "1b065647-8e0d-45ca-af7c-d16e56997ad8")
		)
		(pad "13" smd roundrect
			(at 0.975 -1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 123 "unconnected-(U5-TC-Pad13)")
			(pinfunction "TC")
			(pintype "open_collector+no_connect")
			(uuid "a6a67329-d7ad-4659-90bd-f47ee51a793f")
		)
		(pad "14" smd roundrect
			(at 0.325 -1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "Sol Shunt 1")
			(pinfunction "IN-2")
			(pintype "input")
			(uuid "7a6844ce-97ff-40e0-af9a-d3cf4adef232")
		)
		(pad "15" smd roundrect
			(at -0.325 -1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "Sol Shunt 1")
			(pinfunction "IN+2")
			(pintype "input")
			(uuid "082ff267-2270-41d3-9d36-74784b9816d5")
		)
		(pad "16" smd roundrect
			(at -0.975 -1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VDD_NRF")
			(pinfunction "VPU")
			(pintype "power_in")
			(uuid "81a1310c-b7bc-4b92-a808-4b03ec750c4a")
		)
		(pad "17" smd rect
			(at 0 0)
			(size 2.1 2.1)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 122 "unconnected-(U5-EP-Pad17)")
			(pinfunction "EP")
			(pintype "passive+no_connect")
			(zone_connect 2)
			(uuid "7ccf1e36-e51d-46f4-83c2-d78721209a54")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic:SS3235SL3"
		(layer "F.Cu")
		(uuid "1287a9ce-7415-472c-9896-b7677a6a881e")
		(at 155.425 109.235)
		(descr "SS-3235S-L3")
		(tags "Switch")
		(property "Reference" "SW3"
			(at 0 0 0)
			(layer "F.SilkS")
			(uuid "199d5daa-e09e-486b-a352-dced87e6d9bf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "SW_DPDT_x2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "a93a9964-346d-45a2-9169-40713c447e6d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e3c6826b-c3a7-45c4-b016-5e7a5dd67e59")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Switch, dual pole double throw, separate symbols"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3ec2464d-043f-4133-9308-23f4f776d960")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C381098"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7a57b058-e5eb-4201-ac74-ba2c040b994f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field6" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "44a7f92c-ac64-4b64-817a-1a3450274549")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cbd61bf3-c2de-4ea8-a637-d65895873eab")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "adce4046-6b78-4ef4-8239-4ff77f8a4b8e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SW*DPDT*")
		(path "/25f5c15c-0d18-4403-8564-3038978e4c9d")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.6 -3.25)
			(end -4.6 -3.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d6814946-7ab0-4e9a-b9a7-832ae2873781")
		)
		(fp_line
			(start -4.6 -3.25)
			(end -4.6 -3.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb87a50e-e942-43e2-9641-83a18b233529")
		)
		(fp_line
			(start -4.55 -1.775)
			(end -4.55 1.775)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2fca6c57-66c6-45a0-8106-1da42593fe99")
		)
		(fp_line
			(start -4.55 1.775)
			(end 4.55 1.775)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6e42fe27-4f1f-447a-9071-5761fc8cd479")
		)
		(fp_line
			(start -4.5 -3.25)
			(end -4.5 -3.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "619d9e32-ebf9-46ea-88bd-529e85e49dae")
		)
		(fp_line
			(start 4.55 -1.775)
			(end -4.55 -1.775)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2464f64e-f37e-4bc2-a9d9-d9e1ca861e2c")
		)
		(fp_line
			(start 4.55 1.775)
			(end 4.55 -1.775)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "25f6ca7a-1d3e-4e15-9d99-138274be30ea")
		)
		(fp_arc
			(start -4.6 -3.25)
			(mid -4.55 -3.3)
			(end -4.5 -3.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc6dc217-e7d8-4a44-9bcb-0dc031dfc902")
		)
		(fp_arc
			(start -4.5 -3.25)
			(mid -4.55 -3.2)
			(end -4.6 -3.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1b554403-b160-4acc-be06-4503cc306bfe")
		)
		(fp_arc
			(start -4.5 -3.25)
			(mid -4.55 -3.2)
			(end -4.6 -3.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5ba523da-1732-486a-8d24-9c425288a9b5")
		)
		(fp_line
			(start -5.55 -4.85)
			(end 5.55 -4.85)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ef160112-a0a5-425a-9c18-62154df3062b")
		)
		(fp_line
			(start -5.55 4.85)
			(end -5.55 -4.85)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "056775de-9e14-40cd-a776-1cd5c1e940b0")
		)
		(fp_line
			(start 5.55 -4.85)
			(end 5.55 4.85)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8808c220-d2aa-4d46-a584-d1970e8e49d6")
		)
		(fp_line
			(start 5.55 4.85)
			(end -5.55 4.85)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "baa3fde1-1297-494d-8ec2-a5bdc41082d7")
		)
		(fp_line
			(start -4.55 -1.775)
			(end -4.55 1.775)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f5db5dd1-6fe8-4e68-bb9d-b407da17c59f")
		)
		(fp_line
			(start -4.55 1.775)
			(end 4.55 1.775)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9bca0900-9ab3-42f7-a4ca-a18b1ad51d13")
		)
		(fp_line
			(start 4.55 -1.775)
			(end -4.55 -1.775)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d7cf65d7-1bba-49f0-9920-8d53b8f3dbf7")
		)
		(fp_line
			(start 4.55 1.775)
			(end 4.55 -1.775)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "61209912-8a5d-435a-a4b9-32181f1669db")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e90f120d-8c17-4eff-aad6-70e09b62fba5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -2.5 -3.25)
			(size 0.7 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 111 "USE_ANT_1")
			(pinfunction "A")
			(pintype "passive")
			(uuid "b28d5262-a102-45b5-8e0b-88fbef4186be")
		)
		(pad "2" smd rect
			(at 0 -3.25)
			(size 0.7 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "+4V")
			(pinfunction "B")
			(pintype "passive")
			(uuid "93f7e0ca-bb68-4626-ab0f-313df9f53bda")
		)
		(pad "3" smd rect
			(at 2.5 -3.25)
			(size 0.7 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "USE_ANT_2")
			(pinfunction "C")
			(pintype "passive")
			(uuid "411f0e00-e725-4701-afa3-a889fb8256fc")
		)
		(pad "4" smd rect
			(at -2.5 3.25)
			(size 0.7 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(uuid "56151dff-0dfb-4b61-bb7b-13e55d1e6437")
		)
		(pad "5" smd rect
			(at 0 3.25)
			(size 0.7 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(uuid "e67daa3e-69c0-41e8-9a4e-c349d68fe2d9")
		)
		(pad "6" smd rect
			(at 2.5 3.25)
			(size 0.7 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(uuid "116c93eb-3dae-475b-83ec-2320da9e3a79")
		)
		(embedded_fonts no)
		(model "SS-3235S-L3.stp"
			(offset
				(xyz 0 0 0.3499999888)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(uuid "12a2eedb-28b7-4a65-97a6-fb695149cb45")
		(at 146.4 118.41)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 -1.998 0)
			(layer "F.SilkS")
			(uuid "a3dd330c-479b-4c17-a76e-c3dd1c7cf87e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.Fab")
			(uuid "ee9ff089-6924-494d-8479-3fb55b98299f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0df99b67-4aa3-43b9-aa45-911a239b45ba")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c814a6df-6df2-45af-91fe-431b2bf56cbb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/5c91fc53-c07f-4cfc-a479-3e45d9a2734b")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_circle
			(center 0 0)
			(end 0 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "a0212afb-825f-4abf-b962-33c487d837c6")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "3961f1d0-2675-41e5-87f2-8d10d9fa2964")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "29ebfc32-c673-474e-a664-8f0bd780dbb0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 36 "Sys Load")
			(pinfunction "1")
			(pintype "passive")
			(uuid "672ffaee-320b-4c3d-b5f5-a4a9f3627265")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
		(layer "F.Cu")
		(uuid "14831507-addb-44ea-a725-1909421671e0")
		(at 131.75 100.79)
		(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R36"
			(at 0 -2.62 0)
			(layer "F.SilkS")
			(uuid "8a02abdd-fc14-473b-bcae-a725f8da0bd2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1"
			(at 0 2.62 0)
			(layer "F.Fab")
			(uuid "c73f1a8f-aba3-4c1c-9309-97a67617fdb3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "549c6dd1-529a-4ad4-97d2-e547c1c54280")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c3dd5163-56c9-4411-8a68-4c45c1fca086")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/728def05-04b3-4581-8e79-23d03058df83")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.177064 -1.71)
			(end 2.177064 -1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c905ff4c-bcc7-4ddf-a423-fb70bdba443f")
		)
		(fp_line
			(start -2.177064 1.71)
			(end 2.177064 1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5dd98a28-cf27-4812-b726-9a12006362d1")
		)
		(fp_line
			(start -4 -1.92)
			(end 4 -1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "56d1263d-c97a-43d6-ac00-7a7690dac49a")
		)
		(fp_line
			(start -4 1.92)
			(end -4 -1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e2f99bec-37cc-435f-ba84-da1be2b1613a")
		)
		(fp_line
			(start 4 -1.92)
			(end 4 1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ae1ced0d-b195-4445-8e55-b5f69737d533")
		)
		(fp_line
			(start 4 1.92)
			(end -4 1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb013987-5b53-43aa-8c04-25283f2dd6bd")
		)
		(fp_line
			(start -3.15 -1.6)
			(end 3.15 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "05230c46-d18d-4166-b661-532bddfb3707")
		)
		(fp_line
			(start -3.15 1.6)
			(end -3.15 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "56754a1e-c01c-4714-8df7-cabd49d0e624")
		)
		(fp_line
			(start 3.15 -1.6)
			(end 3.15 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0daf1794-3198-44c5-a138-554acc42e5a0")
		)
		(fp_line
			(start 3.15 1.6)
			(end -3.15 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f955bd6a-710a-4c04-9c6b-950583365bf0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2c36a483-0df3-49ce-8728-fab522e593ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -3.05 0)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 47 "Net-(IC2-CSP)")
			(pintype "passive")
			(uuid "102e6750-48f0-4c8c-a54c-4d404c46e016")
		)
		(pad "2" smd roundrect
			(at 3.05 0)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 8 "Bat Shunt 1")
			(pintype "passive")
			(uuid "b091c6c7-9207-4b9f-9528-980dda201656")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_LGA:Bosch_LGA-8_2.5x2.5mm_P0.65mm_ClockwisePinNumbering"
		(layer "F.Cu")
		(uuid "15d8d2f4-cfe9-4030-b6c1-b01996d2b290")
		(at 157.185 78.215)
		(descr "LGA-8")
		(tags "lga land grid array")
		(property "Reference" "U4"
			(at 0.015 -2.465 0)
			(layer "F.SilkS")
			(uuid "423a86d3-179e-424f-8d9e-c6a585b020e6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BME280"
			(at 0.015 2.535 0)
			(layer "F.Fab")
			(uuid "0435e0d8-50d8-4f69-ab89-88b606b88aee")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.bosch-sensortec.com/media/boschsensortec/downloads/datasheets/bst-bme280-ds002.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "412a6401-f304-4039-8538-b2400ce51d1a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "3-in-1 sensor, humidity, pressure, temperature, I2C and SPI interface, 1.71-3.6V, LGA-8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2a72eb81-595d-4828-9bf7-ae27052e7d18")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C92489"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4248ed8f-a7ac-411b-bba2-8c4c3b0b209b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0aa7f7ec-f3ba-4464-b2e5-c3fe3b33b34f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "702eacf4-d65c-4100-a445-076d0dfaac70")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*LGA*2.5x2.5mm*P0.65mm*Clockwise*")
		(path "/4e4c8d6c-4ffb-4887-974e-d494aba72112")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.35 1.35)
			(end -1.35 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a94ce5be-1e89-43d1-9d50-341b202041b7")
		)
		(fp_line
			(start -1.35 1.36)
			(end -1.2 1.36)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fcda0f99-ee63-499d-b24f-f180931999eb")
		)
		(fp_line
			(start 1.2 -1.35)
			(end 1.35 -1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3541ccf2-a2e1-41ea-bf3c-d98676ffee71")
		)
		(fp_line
			(start 1.35 -1.35)
			(end 1.35 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3f773327-3f8c-411b-abaf-0a286423bb97")
		)
		(fp_line
			(start 1.35 1.35)
			(end 1.2 1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8c9fbc2f-0cb4-435a-b8d5-5bde908e8752")
		)
		(fp_line
			(start 1.35 1.35)
			(end 1.35 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eb38779a-ebd9-4335-a53f-1bab4b6b57e7")
		)
		(fp_poly
			(pts
				(xy -1.35 -1.35) (xy -1.71 -1.35) (xy -1.35 -1.71) (xy -1.35 -1.35)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "b492bbc4-0456-458b-8d09-356e7b5f4467")
		)
		(fp_line
			(start -1.41 -1.54)
			(end 1.41 -1.54)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c0dd8e69-b891-4dc0-9985-580626ad8920")
		)
		(fp_line
			(start -1.41 1.54)
			(end -1.41 -1.54)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6fc2a7c2-a148-4be0-97a8-34a3c418437f")
		)
		(fp_line
			(start 1.41 -1.54)
			(end 1.41 1.54)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3fb57323-727f-4203-b068-4488592db861")
		)
		(fp_line
			(start 1.41 1.54)
			(end -1.41 1.54)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "760bf66b-f75f-48be-997e-d3ea1d16198b")
		)
		(fp_line
			(start -1.25 -0.5)
			(end -0.5 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b12247b5-2b2a-4253-a982-d080df877f84")
		)
		(fp_line
			(start -1.25 1.25)
			(end -1.25 -0.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "47a297d7-b886-40e0-a172-c69cd4572249")
		)
		(fp_line
			(start -0.5 -1.25)
			(end 1.25 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "490f7fb4-e42d-4adb-b955-6bc387318b13")
		)
		(fp_line
			(start 1.25 -1.25)
			(end 1.25 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3cbee40c-2e7d-4b69-a5be-c2728740c9c0")
		)
		(fp_line
			(start 1.25 1.25)
			(end -1.25 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "78b18fec-19b0-4cef-9ed3-2523791427d4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "7b1726b9-5ea6-4c1a-8a39-d67757c7f3b2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.075)
				)
			)
		)
		(pad "1" smd rect
			(at -0.975 -1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "b0098858-8fbb-4812-8a52-8bd7d452031b")
		)
		(pad "2" smd rect
			(at -0.325 -1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "CSB")
			(pintype "input")
			(uuid "6b9f5482-749c-4ec9-9ed1-003b591b66df")
		)
		(pad "3" smd rect
			(at 0.325 -1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 108 "I2C SDA")
			(pinfunction "SDI")
			(pintype "bidirectional")
			(uuid "bda7c365-23d4-4575-8e05-977248d419c2")
		)
		(pad "4" smd rect
			(at 0.975 -1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "I2C SCL")
			(pinfunction "SCK")
			(pintype "input")
			(uuid "56da6b1b-a35e-4b7f-a251-cac992609429")
		)
		(pad "5" smd rect
			(at 0.975 1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "SDO")
			(pintype "bidirectional")
			(uuid "d686c6d3-23b9-4229-88bf-7ac3d4c6d115")
		)
		(pad "6" smd rect
			(at 0.325 1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "VDDIO")
			(pintype "power_in")
			(uuid "b371387a-07d7-43bb-8747-596cd9b54d1c")
		)
		(pad "7" smd rect
			(at -0.325 1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "a28e0397-6228-4799-b1ae-093df43dfd5f")
		)
		(pad "8" smd rect
			(at -0.975 1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "fae81625-b51b-4a1f-8a2c-db4208b7972d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_LGA.3dshapes/Bosch_LGA-8_2.5x2.5mm_P0.65mm_ClockwisePinNumbering.wrl"
			(offset
				(xyz 0.01500000025 -0.03500000059 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "1668e996-cd9e-437b-a739-75798157d9e4")
		(at 110.6 66.43)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "inductor handsolder")
		(property "Reference" "L5"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "7fab1507-6e7a-418a-b0cc-97278edc9afa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7uH"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "e6fb7ae7-7806-4ad5-ac42-e7a49301b081")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "03eb0973-12e0-4be8-a280-41869f11a024")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e5374fc4-85f9-4040-91c5-034cf765120c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/6a374a2d-4d1e-4970-bd77-c0c3a850d984")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.71)
			(end 0.261252 -0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c0e84caa-fe75-466e-8a8f-d9da632f91d2")
		)
		(fp_line
			(start -0.261252 0.71)
			(end 0.261252 0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0c605250-001d-43e9-afb6-a9fa58db381e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "94aba5da-8815-41e6-ae62-39f343cbd92b")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f3c0f84b-3374-42db-bc74-cd7d6c1c823c")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4c5d8812-5c6c-496b-bf27-5a37b992a908")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1f2490e4-a440-4e8a-8ffa-8efea0a19f7b")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9e413b6d-5c5e-4c5f-aa8e-e366d233bc3a")
		)
		(fp_line
			(start -1 0.6)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83413287-9572-4322-b803-1fdcdafefc58")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5811671a-7259-4a64-986f-f6d20204f4f9")
		)
		(fp_line
			(start 1 0.6)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7aca024e-174f-44ae-afe3-3d690a9ec852")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "530baa25-e8c1-4dc8-803f-a3f25e26dcfb")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 3 "VDD_NRF")
			(pinfunction "1")
			(pintype "passive")
			(uuid "68e78a1a-0299-4ed5-b7fc-659e7cabe63e")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 101 "Net-(U2-L)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "cc4fe631-90bd-4cf6-9443-d24a00bcb080")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "16cdeb3d-f8c8-4108-b512-6d2978938cc2")
		(at 134.44 66.52)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "48537c86-a2ea-41dc-8161-ffa9d02e0175")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "af835c19-ecf7-41cd-9268-0d6721c27c69")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "35b5bc6a-c8da-40e6-8a00-1007275188d4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d865df16-c0fd-47fb-af89-0e5ebaf99a9e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/b50c11c9-1724-4da1-8c0e-a2025eb4ca55")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "18263f28-3067-43f1-9e0d-528ca9786ce6")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f99a38eb-8454-4c1f-822d-f7d26f359bf4")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "043bbd8e-649a-4732-995c-75374a58f675")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb083ea1-04cb-4804-ab3f-97973e91297b")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "01a85736-3ec5-4e0c-b866-fbfb1b828a91")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a1699f89-5dfc-48c7-8d4e-5c6fcc8b3b69")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "627355bf-3258-4323-90ef-aa22d119d03c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "96d24fd6-a95e-4d66-b2d4-7aad0ada1d74")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "26d332eb-32f0-4472-8702-1d78850785d0")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17737579-579c-43f5-a719-3a418676a18e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d385177c-9922-467f-b924-230975ae0d88")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "Net-(IC1-VDD)")
			(pintype "passive")
			(uuid "fd2b2796-a43a-44f4-b49a-fb2e8c848a18")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "3d66708c-017c-4683-85c6-12336dab15d0")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "18a82b6a-b9b5-43e4-973f-4f7333f62f12")
		(at 144.06 69.53)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C38"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "014a45b4-1e78-47b8-8f75-c468c5af048c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "cfbf34c5-a47f-4de8-ae83-aedf0fe9c072")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "22aa5734-0310-46ff-ac16-39989fcbb5e0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ea174e88-e191-48f3-84be-2c9b7811264f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/fd7dc787-8086-4619-91fb-46344c752fb7")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d937b838-1bac-4800-959d-06bbf36fcd63")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "12fc7fa7-0c6d-4d18-962a-85aea84e4aab")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4e677d15-7426-4b2c-83bf-183f0e972736")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "70c62f24-01c6-4c5a-a31f-e18330c54d9f")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6cc3cfe-b661-4b87-af40-603ea970d78f")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "26292d92-ad3e-442b-87b5-379b17f19119")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b614f241-efac-4423-a81a-8afb39d2a318")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a43177e5-97e0-40eb-9000-8b426be620d3")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fd62e202-0fe8-4dcd-8649-77e35a9afaeb")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cdf13818-0d0c-4e3a-9197-b3ecf9f02b2e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "eba24c80-d0d3-4558-abf7-4ba0cfe98ccf")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 9 "+5V")
			(pintype "passive")
			(uuid "db298d2a-e5f6-497b-bf5f-69a8350668d1")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "462f8e4d-4b4e-41c7-a5e5-0029ac01bd11")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "19a808dc-abde-44e5-80f2-08ff30fb3f7f")
		(at 138.45 112.62)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C28"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "08150342-d646-4d19-8d35-4a3cc5a5086e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.047uF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "1be1dd5c-1201-44a3-8a96-e524264a55a1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "57827a61-34df-4bc4-9a95-f7a3c94164fa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "233dc48e-a57e-4020-8e3e-1eead9fb2f76")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/ff9598cd-0bb9-4b77-921e-804b10875021")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cf71b634-4826-49cf-a1e6-bec8d753d970")
		)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97b1b320-2ba8-4732-81d1-a88112109275")
		)
		(fp_line
			(start -1.65 -0.73)
			(end 1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "771560e2-f421-4505-a414-0ff79ee1f7bf")
		)
		(fp_line
			(start -1.65 0.73)
			(end -1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7853fa9a-97c8-46e9-bf4f-c7338e6e04bf")
		)
		(fp_line
			(start 1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2f637007-436a-4c6e-ae1a-c05e577e891c")
		)
		(fp_line
			(start 1.65 0.73)
			(end -1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9cc224aa-3cf5-4248-a02b-3a0cbe2efef0")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fc707044-52e4-4416-bcb0-9baefe4c79a4")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4fb73dc6-6fe3-4761-96f6-cc2e1ee9205e")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37089a51-00b2-47f1-8ab3-8a5b88972b7b")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de2dfbda-155c-45f8-9ddf-9bd6f8157001")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "eeb7fe32-bc1a-4fe4-a7ab-c113ddae765a")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "USE_ANT_2")
			(pintype "passive")
			(uuid "910474cd-3321-48ca-8611-618fa8d0478f")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "f3c38bd3-95e5-45a8-aa26-3b065ff1a931")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
		(layer "F.Cu")
		(uuid "19e66143-a116-4d36-ba2d-5b5fa796cfa3")
		(at 131.75 95.9)
		(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 -2.62 0)
			(layer "F.SilkS")
			(uuid "acc9efb1-f8df-4bfb-8920-f594e0b13ed4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1"
			(at 0 2.62 0)
			(layer "F.Fab")
			(uuid "7325f329-70ea-4abc-a607-0258ee056808")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "912f2f20-4bf9-4bb6-8bc4-ea5eb083d235")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bf226024-ddb0-42eb-be53-7b0fb13d61be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/348368da-ad5e-4fbe-ac3c-75c0da2d5fb5")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.177064 -1.71)
			(end 2.177064 -1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "111a2b68-c2f5-491e-a41e-bab6637a9d16")
		)
		(fp_line
			(start -2.177064 1.71)
			(end 2.177064 1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "21112f8c-5b03-42cf-8be3-7769ad04c427")
		)
		(fp_line
			(start -4 -1.92)
			(end 4 -1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "68b631d0-d100-40fc-bb7a-5dd332eac909")
		)
		(fp_line
			(start -4 1.92)
			(end -4 -1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6222b326-ca77-47e3-b0d9-f1c6ac9dfa17")
		)
		(fp_line
			(start 4 -1.92)
			(end 4 1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2a45f747-b7e0-4d10-ae3a-b10e5485938c")
		)
		(fp_line
			(start 4 1.92)
			(end -4 1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d3ac1f4c-15fa-44b0-b14e-bc70b7165532")
		)
		(fp_line
			(start -3.15 -1.6)
			(end 3.15 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6bde318d-c669-44c1-896e-c1dd3d4d5544")
		)
		(fp_line
			(start -3.15 1.6)
			(end -3.15 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6c15fc88-79e5-428c-829c-56e5e307ad7f")
		)
		(fp_line
			(start 3.15 -1.6)
			(end 3.15 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9a227a53-de32-4550-a45e-0b320e31f838")
		)
		(fp_line
			(start 3.15 1.6)
			(end -3.15 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c0299d5a-0251-48ab-8e1e-7378fc3d141b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "41c37e56-491a-4fac-b13c-ca8b2c6e9339")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -3.05 0)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 8 "Bat Shunt 1")
			(pintype "passive")
			(uuid "4a686da5-b9b0-4437-addd-4834cc3e941c")
		)
		(pad "2" smd roundrect
			(at 3.05 0)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 8 "Bat Shunt 1")
			(pintype "passive")
			(uuid "1ed74ec0-78b5-4007-bbbb-2fa2bc548595")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic:SOT65P210X110-6N"
		(layer "F.Cu")
		(uuid "1a683054-e00c-4beb-b3d0-ce72d4ef4c0d")
		(at 167.955 63.88)
		(descr "SC - 70")
		(tags "Switch")
		(property "Reference" "S1"
			(at 0 0 0)
			(layer "F.SilkS")
			(uuid "7cdd3381-ca8d-4861-b4e1-1d09e139c001")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "MASWSS0136TR-3000"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "350a7f08-7c12-4b2a-a496-ed97489744d5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" "https://rs.componentsearchengine.com/Datasheets/1/MASWSS0136TR-3000.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1c87dac5-0ec2-481a-b7c1-c674ada501d8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "RF Switch ICs DC-3.0GHz ISO 27dB IL .4dB @2.4GHz"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4cb118b2-9a5c-4742-a31c-6895635383fb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "1.1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1a24710e-ae16-490c-9c03-7050079853ad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "MACOM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e4c4e2fa-c509-4f98-ad83-12333eca17b6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "MASWSS0136TR-3000"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "534d7203-e956-47ad-8792-daa2fcd4b2d4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" "937-MASWSS0136-T"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "124b6415-137d-49c2-97a9-236735c92a17")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/MACOM/MASWSS0136TR-3000?qs=3Wmz%2FrCSAaHZLGvANOUDKw%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "80635812-46a4-417a-921e-f8dd9454c588")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c3723250-a49a-453d-8c6a-0d89a7b0add3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "abbc5918-d239-4794-8eff-ccc4ce167870")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/6f443fd5-4c2d-4743-b6f2-e02bc84173d8")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.575 -1.2)
			(end -0.425 -1.2)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e30afe07-6668-48a4-90b1-db6ab357ba4e")
		)
		(fp_line
			(start -0.075 -1)
			(end 0.075 -1)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22aea0dc-5c18-44c2-a19b-cceaafebb379")
		)
		(fp_line
			(start -0.075 1)
			(end -0.075 -1)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cafaf405-82a3-46c1-9689-6ee5d5daa9ac")
		)
		(fp_line
			(start 0.075 -1)
			(end 0.075 1)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97dd36af-3a2b-4e57-8112-8fc251f39a9d")
		)
		(fp_line
			(start 0.075 1)
			(end -0.075 1)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "66943361-865d-42bd-96d6-f6785c1b006a")
		)
		(fp_line
			(start -1.825 -1.35)
			(end 1.825 -1.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b926ad10-86f5-4da0-b65e-bc9174c2f28b")
		)
		(fp_line
			(start -1.825 1.35)
			(end -1.825 -1.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "56e21ff2-3419-489e-a325-a0f92f11bc03")
		)
		(fp_line
			(start 1.825 -1.35)
			(end 1.825 1.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8bf1c25d-3491-46be-92b6-96b117982b6b")
		)
		(fp_line
			(start 1.825 1.35)
			(end -1.825 1.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5b5001dc-17dd-4552-8f5c-c7afceab87f6")
		)
		(fp_line
			(start -0.625 -1)
			(end 0.625 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a0a3b908-91da-40c9-8cce-297704fa6982")
		)
		(fp_line
			(start -0.625 -0.35)
			(end 0.025 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e63f9cf6-bdc8-460a-9846-3fb6dce40245")
		)
		(fp_line
			(start -0.625 1)
			(end -0.625 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7129c397-8671-4e86-9bdf-081e472eb10d")
		)
		(fp_line
			(start 0.625 -1)
			(end 0.625 1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dd6730e1-7d34-4b8a-8f80-0200769c643f")
		)
		(fp_line
			(start 0.625 1)
			(end -0.625 1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77b916c7-422f-46c0-9a09-02f0c836619e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bb487e85-79da-4d5a-ade9-ed9603f73744")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -1 -0.65 90)
			(size 0.4 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(S1-RF1)")
			(pinfunction "RF1")
			(pintype "bidirectional")
			(uuid "e331bd43-e993-4ff6-9abd-3247d7406743")
		)
		(pad "2" smd rect
			(at -1 0 90)
			(size 0.4 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "d82398b0-cc66-4ec2-8de5-737b1af776c2")
		)
		(pad "3" smd rect
			(at -1 0.65 90)
			(size 0.4 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(S1-RF2)")
			(pinfunction "RF2")
			(pintype "passive")
			(uuid "3b3b6ed5-fe0e-4aae-988a-faa4997094b4")
		)
		(pad "4" smd rect
			(at 1 0.65 90)
			(size 0.4 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "USE_ANT_2")
			(pinfunction "V2")
			(pintype "input")
			(uuid "27feb1b0-1660-4132-bbe9-5e98f136e881")
		)
		(pad "5" smd rect
			(at 1 0 90)
			(size 0.4 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(S1-RFC)")
			(pinfunction "RFC")
			(pintype "bidirectional")
			(uuid "d60d812d-2af4-4d9b-9a63-808da03d1dd0")
		)
		(pad "6" smd rect
			(at 1 -0.65 90)
			(size 0.4 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 111 "USE_ANT_1")
			(pinfunction "V1")
			(pintype "input")
			(uuid "b4a538ad-2b43-4042-b7ea-4147318b788e")
		)
		(embedded_fonts no)
		(model "MASWSS0136TR-3000.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "1b585f76-3bca-4506-bcd4-9288a1c0df5d")
		(at 144.06 75.55)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C40"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "50a9075c-e7db-4c3d-bd42-30ab5b01ab2d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "05095a52-62ea-4cfc-a1a1-0b83f7f3b95c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "21bcf04f-13ec-4273-8d27-027dad591550")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b85f92ff-8320-48eb-be12-b5575d72cbab")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/4e291f0a-24a9-4b0c-abec-2ec656891ecf")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7040ddb8-8f62-4921-beb1-54ebf9038e03")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4cccab22-5969-4522-bae5-64edd93a28d6")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b67498d3-ad87-4ba5-87d5-842e6872c4fa")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "146814eb-1d55-4b4b-97e8-caeb856cc886")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4f09edde-a9ac-4e85-9baa-17b8b11bcd5e")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "81b8a4b5-3a62-43e7-9e7f-2d8abb0b04bd")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7981042e-2d9a-42c8-ae57-4faf7a6427e1")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fcb4c037-2004-4a7a-abbe-06e58ca97e91")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "75cb9e13-cc3e-4238-9e52-956c8c4bfc03")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a116966d-f195-46e8-ad3c-c285b711ae0d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5f7bab3f-25c1-4eae-b902-5b23c07f5c91")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 18 "unconnected-(C40-Pad1)")
			(pintype "passive")
			(uuid "dd6d5c9b-9742-4ff3-a83c-689ae27dfc19")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "b08de1ef-f401-42f9-ab8e-5b0d9ec750d6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "1e98437b-1ed0-4032-9c4d-249e8991e63c")
		(at 110.6 81.18)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "2e0207e5-f98e-4e60-b554-e780b4856d22")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "2c3c58ad-d692-41de-b41e-76a8848c06a4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "221c1736-d62b-4e5b-a537-eeb37614007d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b35b781d-f09a-4913-98e8-b02b4b4415fa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4d9d01dc-76fe-458e-90f2-e0d9973b73cf")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b7618841-5744-4204-8c5d-ad2ec445f4c3")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7e366fd2-82f5-429c-b7fb-f19b8ac828bc")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5e5d71b8-a391-4619-9f37-a6f494a645df")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "27782d84-6e68-4db7-9898-d4dad40cc6f9")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b010f4e4-fafb-4966-96e7-3fe37581b92f")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1095dabc-ff5d-40c0-a741-f911ee3031b9")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4ab21f0-9a5f-4911-be12-eb006324a10c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2a5701ab-0283-4f46-bf46-49c55866e8d7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5248cb3b-ddbb-4241-b7c8-21d2e9d49408")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3ea1f85a-1412-4da6-a818-2117f1f3ebf2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b627f6dc-b848-4c0c-bf33-a1ea1345f538")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "80d1cca9-80ad-4ae6-ad55-155d52241d33")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 41 "Net-(IC1-VBUS)")
			(pintype "passive")
			(uuid "3ea7dba4-fbd7-4888-86ce-884e4bc2bb67")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic:QFN50P500X500X100-33N-D"
		(layer "F.Cu")
		(uuid "203063f4-58f4-4a32-91fb-016d322cb91e")
		(at 111.875 118.665)
		(descr "32-QFN")
		(tags "Integrated Circuit")
		(property "Reference" "IC4"
			(at 0 0 0)
			(layer "F.SilkS")
			(uuid "e9ff501c-0230-46bc-ab74-8fe8a7049cad")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "LR1110IMLTRT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "864fe94a-8a50-4e88-8619-a065761b8ad2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7413449a-7b18-4855-bbae-14650f31d2d0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "RF Transceiver LONG RANGE WI-FI LOC LORA TRANSCEIVER"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bc5bf331-fb63-42b8-9607-d7da40b1b583")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "710d34bc-97a8-45a3-8f63-07b66612e64e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "SEMTECH"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "46e3c5e6-10c0-435b-aed1-27d72cb86107")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "LR1110IMLTRT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "be795232-742f-45a4-9941-1f46d44afd71")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" "947-LR1110IMLTRT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5a68fb69-680e-4a48-9e0c-c090cd483fe6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Semtech/LR1110IMLTRT?qs=GedFDFLaBXFCcMA0cJwOqg%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f9fd89be-c232-45c8-a598-095723d9736b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Part Number" "LR1110IMLTRT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "147d6a64-52dc-4ee1-96a0-5a657c1eea43")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/lr1110imltrt/semtech?region=nac"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4f742cc5-dedd-4245-ae7f-3ccdc53d8751")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/6e4f9d11-fc4c-4864-a475-16b77990aaa8")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_circle
			(center -2.9 -2.5)
			(end -2.9 -2.375)
			(stroke
				(width 0.25)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "a32ab4b4-6d3c-4d90-91fa-dead6cc4a918")
		)
		(fp_line
			(start -3.125 -3.125)
			(end 3.125 -3.125)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "37398c49-f252-43e5-9410-99b01a6f1600")
		)
		(fp_line
			(start -3.125 3.125)
			(end -3.125 -3.125)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "52b128dd-3579-4da1-bfe3-e7f1d117f9b7")
		)
		(fp_line
			(start 3.125 -3.125)
			(end 3.125 3.125)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5bf5f6b7-2859-4f0b-b108-97ba84fc5eac")
		)
		(fp_line
			(start 3.125 3.125)
			(end -3.125 3.125)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b2ea156e-8341-4d24-8f94-42428801bdea")
		)
		(fp_line
			(start -2.5 -2.5)
			(end 2.5 -2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "92c60567-0261-4f29-9fa8-ac1c6d8a4e10")
		)
		(fp_line
			(start -2.5 -2)
			(end -2 -2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "53654fda-412a-4f3d-b9de-26098b6412e2")
		)
		(fp_line
			(start -2.5 2.5)
			(end -2.5 -2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "36bb37d4-c9b8-4221-ae67-308ab7e5532e")
		)
		(fp_line
			(start 2.5 -2.5)
			(end 2.5 2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b028cd40-bd81-49e5-99ea-d3c87b9f2fd0")
		)
		(fp_line
			(start 2.5 2.5)
			(end -2.5 2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "523b219e-118d-4058-abf0-b2dcd5f6d664")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "216ef0d7-3456-4016-8ada-55c0b7f5627c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -2.5 -1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "unconnected-(IC4-VR_PA-Pad1)")
			(pinfunction "VR_PA")
			(pintype "passive")
			(uuid "a0bb2d1b-6e29-47b5-9ec3-33f04b625fcf")
		)
		(pad "2" smd rect
			(at -2.5 -1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "unconnected-(IC4-VBAT_RF-Pad2)")
			(pinfunction "VBAT_RF")
			(pintype "passive")
			(uuid "182c3522-3eac-4273-aa37-b244d03e3ac9")
		)
		(pad "3" smd rect
			(at -2.5 -0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "unconnected-(IC4-VTCXO-Pad3)")
			(pinfunction "VTCXO")
			(pintype "passive")
			(uuid "98a87fac-16da-4af4-81ae-31158a665d33")
		)
		(pad "4" smd rect
			(at -2.5 -0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "unconnected-(IC4-XTA-Pad4)")
			(pinfunction "XTA")
			(pintype "passive")
			(uuid "bd2b1cb0-b0f1-4ced-9f0f-827d9afa2e8a")
		)
		(pad "5" smd rect
			(at -2.5 0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "unconnected-(IC4-XTB-Pad5)")
			(pinfunction "XTB")
			(pintype "passive")
			(uuid "d1e58389-98d4-4b1a-89f1-0d1c1e1dd98d")
		)
		(pad "6" smd rect
			(at -2.5 0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "unconnected-(IC4-NRESET-Pad6)")
			(pinfunction "NRESET")
			(pintype "passive")
			(uuid "fcc7d982-c66e-4340-a197-93245354f3d6")
		)
		(pad "7" smd rect
			(at -2.5 1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "unconnected-(IC4-32K_P{slash}_DIO11-Pad7)")
			(pinfunction "32K_P/_DIO11")
			(pintype "passive")
			(uuid "da0d5911-63ef-43aa-9a97-39c0f8514f05")
		)
		(pad "8" smd rect
			(at -2.5 1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "unconnected-(IC4-32K_N{slash}_DIO10-Pad8)")
			(pinfunction "32K_N/_DIO10")
			(pintype "passive")
			(uuid "749a5f87-683b-400d-b538-e76086a37c05")
		)
		(pad "9" smd rect
			(at -1.75 2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "unconnected-(IC4-DIO9-Pad9)")
			(pinfunction "DIO9")
			(pintype "passive")
			(uuid "2750ebf2-e68b-4d2d-820d-23bc40d40964")
		)
		(pad "10" smd rect
			(at -1.25 2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "unconnected-(IC4-DIO8-Pad10)")
			(pinfunction "DIO8")
			(pintype "passive")
			(uuid "f1766f4a-8632-4165-8cea-b8947d4bf2b3")
		)
		(pad "11" smd rect
			(at -0.75 2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "unconnected-(IC4-DIO7-Pad11)")
			(pinfunction "DIO7")
			(pintype "passive")
			(uuid "db6b89f2-1bf5-441b-88ad-f4707cc83cde")
		)
		(pad "12" smd rect
			(at -0.25 2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "unconnected-(IC4-VREG-Pad12)")
			(pinfunction "VREG")
			(pintype "passive")
			(uuid "147fbb5b-1dfc-4198-b818-30cdf6825f01")
		)
		(pad "13" smd rect
			(at 0.25 2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "unconnected-(IC4-GND_1-Pad13)")
			(pinfunction "GND_1")
			(pintype "passive")
			(uuid "23582434-2037-49f3-8f3e-0a5766dbb97c")
		)
		(pad "14" smd rect
			(at 0.75 2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "unconnected-(IC4-DCC_SW-Pad14)")
			(pinfunction "DCC_SW")
			(pintype "passive")
			(uuid "03d47bba-82fe-4cb8-ac1e-7c2d0adb39ac")
		)
		(pad "15" smd rect
			(at 1.25 2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "unconnected-(IC4-VBAT-Pad15)")
			(pinfunction "VBAT")
			(pintype "passive")
			(uuid "da54d1c5-b7e1-41cb-81c0-5cbb5aec99cd")
		)
		(pad "16" smd rect
			(at 1.75 2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "unconnected-(IC4-DNC_1-Pad16)")
			(pinfunction "DNC_1")
			(pintype "passive")
			(uuid "e97d4384-98a3-4405-910c-bb5579fb380d")
		)
		(pad "17" smd rect
			(at 2.5 1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "unconnected-(IC4-DNC_2-Pad17)")
			(pinfunction "DNC_2")
			(pintype "passive")
			(uuid "1c7e28d0-0daa-4791-92d7-b6e2b82a6b6a")
		)
		(pad "18" smd rect
			(at 2.5 1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "unconnected-(IC4-DNC_3-Pad18)")
			(pinfunction "DNC_3")
			(pintype "passive")
			(uuid "c3ff8976-a510-4232-be7a-35634bf2adad")
		)
		(pad "19" smd rect
			(at 2.5 0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "unconnected-(IC4-DIO6-Pad19)")
			(pinfunction "DIO6")
			(pintype "passive")
			(uuid "6af43831-f976-4db4-b9bf-e0a4d55e8675")
		)
		(pad "20" smd rect
			(at 2.5 0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "unconnected-(IC4-DIO5-Pad20)")
			(pinfunction "DIO5")
			(pintype "passive")
			(uuid "d5ed8b3d-0415-40d4-831a-4c7aedd7b5c8")
		)
		(pad "21" smd rect
			(at 2.5 -0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "unconnected-(IC4-DIO4-Pad21)")
			(pinfunction "DIO4")
			(pintype "passive")
			(uuid "3468c925-6843-40b1-b9b2-cb714445050a")
		)
		(pad "22" smd rect
			(at 2.5 -0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "unconnected-(IC4-DIO3-Pad22)")
			(pinfunction "DIO3")
			(pintype "passive")
			(uuid "00a0abe5-e1b6-4ff9-8216-45c613dbed66")
		)
		(pad "23" smd rect
			(at 2.5 -1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "unconnected-(IC4-DIO2-Pad23)")
			(pinfunction "DIO2")
			(pintype "passive")
			(uuid "106c241c-8b02-44d0-ad06-7990cf4c6051")
		)
		(pad "24" smd rect
			(at 2.5 -1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "unconnected-(IC4-DIO1-Pad24)")
			(pinfunction "DIO1")
			(pintype "passive")
			(uuid "6b4f60b4-1736-4d07-8860-5b8fe5fbbdf2")
		)
		(pad "25" smd rect
			(at 1.75 -2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "unconnected-(IC4-DIO0{slash}BUSY-Pad25)")
			(pinfunction "DIO0/BUSY")
			(pintype "passive")
			(uuid "6db673e0-702e-48b2-ab69-9fe352fe4393")
		)
		(pad "26" smd rect
			(at 1.25 -2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "unconnected-(IC4-RFIO_HF-Pad26)")
			(pinfunction "RFIO_HF")
			(pintype "passive")
			(uuid "a374601f-ed33-4a6e-88ea-1c11fba5dd65")
		)
		(pad "27" smd rect
			(at 0.75 -2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "unconnected-(IC4-RFI_N_LF1-Pad27)")
			(pinfunction "RFI_N_LF1")
			(pintype "passive")
			(uuid "62ef1872-0e12-4997-ad69-848bd9fa909d")
		)
		(pad "28" smd rect
			(at 0.25 -2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "unconnected-(IC4-RFI_P_LF1-Pad28)")
			(pinfunction "RFI_P_LF1")
			(pintype "passive")
			(uuid "fefe7c7d-56a4-49a9-a29d-a657e39a0c49")
		)
		(pad "29" smd rect
			(at -0.25 -2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "unconnected-(IC4-RFI_N_LF0-Pad29)")
			(pinfunction "RFI_N_LF0")
			(pintype "passive")
			(uuid "cc76ae92-b4b8-451c-90b2-0172a07ee6c2")
		)
		(pad "30" smd rect
			(at -0.75 -2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "unconnected-(IC4-RFI_P_LF0-Pad30)")
			(pinfunction "RFI_P_LF0")
			(pintype "passive")
			(uuid "f22a4dde-f0b5-4521-b633-459b0a670a6e")
		)
		(pad "31" smd rect
			(at -1.25 -2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "unconnected-(IC4-RFO_LP_LF-Pad31)")
			(pinfunction "RFO_LP_LF")
			(pintype "passive")
			(uuid "b672529c-cfe8-45fd-bc0b-2c5f37c77545")
		)
		(pad "32" smd rect
			(at -1.75 -2.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "unconnected-(IC4-RFO_HP_LF-Pad32)")
			(pinfunction "RFO_HP_LF")
			(pintype "passive")
			(uuid "a9d7d20f-c080-449c-8580-9b8a28a44c21")
		)
		(pad "33" smd rect
			(at 0 0)
			(size 3.8 3.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "unconnected-(IC4-GND_2-Pad33)")
			(pinfunction "GND_2")
			(pintype "passive")
			(uuid "c46668c8-8d7b-494a-a609-75a9ba987de2")
		)
		(embedded_fonts no)
		(model "LR1110IMLTRT.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "20b74cb9-e470-4306-89bd-46ccb3488a83")
		(at 129.63 66.52)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "c340d989-850b-43c8-b98b-343e01e6542f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "ba288325-1883-49ff-9659-8450368bfd18")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e0271fc2-b7c7-48ec-81b6-eb9a28f8a024")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "405ff8af-8bfc-4c6e-bd95-7b806489fe5c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/66a4540a-823d-4b19-bde4-4ed77ffc0f84")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "993bb2a4-dabb-4815-89a9-73f02c6a56d1")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed571130-a590-44e9-87de-0e26281596d0")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a89de556-357a-4ce2-a5ca-2e5e7c95a992")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c777dbc7-3229-4b80-bad8-991771cc71a2")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "54152e92-6b80-43cf-a51b-82975f471794")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bc169dd8-a225-4250-bc77-e03f961cd939")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d201ed50-e31f-46f9-845f-135cd344ff78")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2673bf0a-9ab1-4852-a8d3-e389ce616494")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e2f5a724-37c9-4437-b90b-48da3ab34afa")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e405ad50-3d88-4334-81b0-b56986d224f4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d713bd66-72a5-4d1a-89d0-c7ebcf543e00")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "e987815a-53e1-4954-836b-dd42b6400b93")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "bf6eaba3-40ab-482a-9706-9d6d12ce2e15")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "219ea8f3-7e4f-40bd-846c-84513d9225e4")
		(at 134.44 69.53)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "1c6d13fd-4179-4cc4-9c8b-f3bce85fa89e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "c1694d70-3126-464c-b371-b3b124571731")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b54e1e67-476b-449f-9ec2-0be37dae43d0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c40915c1-375e-48bb-9258-d8eac5d86f42")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/23dcf4dd-d4ca-4f8a-a243-8a31a23acd6e")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "544a51e8-59f2-40ac-8222-78a6d605d355")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "adcb35d8-b6ec-4c6d-b1a7-f0348ce9fc6b")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "294d25ff-7ef3-49a7-84c0-ffaddaa83b59")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2bd0f5f8-4e8e-48dc-b8eb-dbbf241d8d0d")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d46f8c04-4f34-4b4a-9627-c228f99d9342")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "817c74d7-0567-46fe-a66a-bcdf8ccc929f")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8bc8145-851e-43d7-8ea4-8636af35f235")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "53079bae-d37b-4c56-95dd-49815aba15df")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d2245a0b-eadb-4ee3-81ba-efa93ec10d15")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6b99f5f3-e80b-43cd-be23-61431e78facc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "cb6af457-4127-4b0c-bae3-cb0f5687f63d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "Net-(U1-VIN)")
			(pintype "passive")
			(uuid "4649fe4d-afd6-4a52-9dc9-6c6a7a0f3966")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "d6d0ac47-9839-45f5-bbf5-a587e8d52f2b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "235b8c4d-beb9-45a8-bca9-932144da16c7")
		(at 124.85 69.38)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R29"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "33d09352-f348-4f80-8764-cfdb276cce83")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "753c5be7-6fd3-4706-8007-bb183b3186c6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3ce6e718-f290-4e34-9c25-1c3402b441b7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "91dd67d9-9948-42ee-ab08-dc976d255371")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/71bc0379-5e69-458d-967a-dba477305b50")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b0670e27-4315-4974-8f85-141b164d4d3e")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aa88dd0a-1393-45f1-8c4a-4e3f89977989")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9c75ba68-5545-46f4-8629-4732c56ab600")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b483cf0a-31d9-4952-bb4f-5e1f81553dea")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3208c77d-d871-4c0c-9a8e-6227d5892ffd")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8cf0c447-c94d-4342-b70c-c529b8cb5571")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "09496187-2330-436a-931d-cd65481a9911")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ce03ec5-ca52-419d-b15a-d63c8bbfec1e")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54b94d96-8961-43e9-8a92-a1770ab13d28")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "18709c5b-7ce1-435b-aa17-538011378d03")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e9b86cbe-7fa4-45ed-a572-d983681d2ddc")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 116 "Net-(R28-Pad2)")
			(pintype "passive")
			(uuid "fba4d87e-a771-44ba-a484-a09f48dfda7e")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "b85c9ca7-fa4d-4752-aef8-25e4847b8a12")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "2a3ba4a2-5966-4ce7-aa9f-1d0a9e5f2106")
		(at 120.1 87.08)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R26"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "3fdb81c4-f34d-476b-9903-e901b5543332")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "23.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "0d8a7f65-1568-45d4-b8f6-213c1a2674a1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "af08c9d4-77ab-4fae-9a60-e82afcad3c20")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0930018a-006c-4451-9663-8ce5d9ba6d7d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5bb0c5dc-2ea7-4f9c-83a5-c9b77fb41be9")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "02716d20-ee69-4a52-98f9-5015c01deeb9")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c1a30803-e6d7-4528-82aa-b96b8afdee75")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c97582ef-fd0c-40bc-996c-7723e0bf4d9f")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b56f8a98-025b-4113-9e5d-3546c4f3344c")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "30bbb092-2e2f-41ca-b759-7138dc3d92ac")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fd1bed78-a264-4362-8265-42c3b61007a4")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "18ac13f8-5296-484d-8930-3532d207fa6e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "33c69145-842d-42ae-aca8-7994b585bf4b")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc525596-6f19-4f86-9bb7-a8cbab4b4ece")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "35882e7c-6895-4d47-b618-fcba48d8cdcc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "aa6b8cdf-3207-4a0e-a2c7-9d97904a2e96")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 94 "Sol Shunt 1")
			(pintype "passive")
			(uuid "d06c780d-c83e-4b7d-938c-8492ceceae23")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 114 "Net-(R25-Pad1)")
			(pintype "passive")
			(uuid "33a8a131-2ce6-4097-a3e5-90724b066822")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "2da0fc0d-67b5-4ffd-b3bb-a1dbe5a9000f")
		(at 115.35 78.23)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R13"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "cc24e173-7732-483c-a38a-ffdf4ac66d8b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "51.1k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "f5c88a94-96f0-4734-8440-5088e9c1d4c5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "258a2d51-d2d0-4456-a2f6-747a0c14dd2e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "39b5257c-f9c2-4de1-94ae-64ca3f6542ab")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/bd3a0d81-f29b-42ea-ab95-f86bff260041")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "09ff9d6b-b33e-423b-9c96-c5e8a53845e8")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "62776263-ae2b-4715-b485-fd5c6262997a")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "85b8e3e9-5ea8-4d6b-9510-010c0bec6d77")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e1cb9a73-1339-4bbb-98e4-24a90d44d616")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "21e205bf-4edc-4c3c-87a4-2a4993d0a7dd")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ee7ca719-6649-44e4-bc74-042f51ea089b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5a692ed4-d81d-42c3-b6d5-fbd15ad6b2ec")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa15c131-c0e2-4e7d-9d7d-f95764a5b121")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "74684efc-d39a-4c9e-a488-6854ef928b4b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "36c8002a-a9c8-4ef8-986c-d213348e9cef")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "81d94bfe-206c-4f14-bbbe-8adb6def331d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 106 "unconnected-(R13-Pad1)")
			(pintype "passive")
			(uuid "91e3b576-f7c1-47f8-9584-a67c51f29847")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "d5dbbaca-2b5a-4b54-bdc2-cbcc11951e11")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
		(layer "F.Cu")
		(uuid "32688b8f-21a9-4029-b43b-469484e095e2")
		(at 131.75 110.57)
		(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R38"
			(at 0 -2.62 0)
			(layer "F.SilkS")
			(uuid "170beb6f-5431-4765-9bbd-1f01a8ae09a0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1"
			(at 0 2.62 0)
			(layer "F.Fab")
			(uuid "1fe6e80e-7d24-45a0-a3f4-b0871117ca24")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7681bec1-27cc-4347-a4f9-be80fd2ed3c6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e09288fa-b1a7-44d0-a903-d1b4c3ddc92f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/0499b774-d170-4317-8a35-62c4212ef7ba")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.177064 -1.71)
			(end 2.177064 -1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b182824e-8b6b-498a-b3a7-88ab76cbda78")
		)
		(fp_line
			(start -2.177064 1.71)
			(end 2.177064 1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "52868728-9a3b-4eb6-9967-dff80a5ab4a8")
		)
		(fp_line
			(start -4 -1.92)
			(end 4 -1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e47c2f88-82d7-4313-9756-f6a9dde0fdb9")
		)
		(fp_line
			(start -4 1.92)
			(end -4 -1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e17079d4-5fc9-4929-b461-0de394203a0a")
		)
		(fp_line
			(start 4 -1.92)
			(end 4 1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fd1e5a1b-3e2c-40c1-8b43-bab7962122cb")
		)
		(fp_line
			(start 4 1.92)
			(end -4 1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4afcc716-8037-40c4-b83f-d49f32b71f5b")
		)
		(fp_line
			(start -3.15 -1.6)
			(end 3.15 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "60632f7c-a1ff-4030-9267-d77ecfb0b7bb")
		)
		(fp_line
			(start -3.15 1.6)
			(end -3.15 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "47cc062f-ff05-4c51-8817-93ddbace5080")
		)
		(fp_line
			(start 3.15 -1.6)
			(end 3.15 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b0590263-79f6-4414-ab5e-cf583a5a21bd")
		)
		(fp_line
			(start 3.15 1.6)
			(end -3.15 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f07a2e0-a20e-4275-a608-59789440beb7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "eb0da761-86e8-4582-a5f8-69649f470ed1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -3.05 0)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 36 "Sys Load")
			(pintype "passive")
			(uuid "b8c5115c-ad9c-4837-8e0c-cb1b0b3fe3a2")
		)
		(pad "2" smd roundrect
			(at 3.05 0)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 36 "Sys Load")
			(pintype "passive")
			(uuid "8429eb4b-9d23-449a-9f96-32aca10b9e99")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "3740dad7-e27f-4c0e-b515-7d45445bd66e")
		(at 147.15 107.6)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C45"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "0e155804-5d35-4cab-97c2-df9b87d38eb8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "6063dab7-c55c-4a37-865a-ca1331e65fd5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3fa97b03-7c70-4576-acb9-bb2e87b43f6e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c64ca200-bdd6-4f70-bfee-69539dd8d321")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a40b671c-ed77-49bd-8234-732985a137a9")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "913a893a-9a09-4340-94b9-d001af444c4d")
		)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a61e17e9-e367-40d5-a6b7-dba0a2e68557")
		)
		(fp_line
			(start -1.65 -0.73)
			(end 1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c52bb2e9-2800-4288-8cfd-ba8e714b9e4a")
		)
		(fp_line
			(start -1.65 0.73)
			(end -1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fd458b5e-1113-45d2-9e04-a87ef62f7828")
		)
		(fp_line
			(start 1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f695f35c-9581-48c3-a63b-d8c68072c7df")
		)
		(fp_line
			(start 1.65 0.73)
			(end -1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "09fc1a00-06fd-467d-94fb-1918f8c7cc21")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d9e0f29-c66a-46e0-9296-31c1cd73eed8")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0a163505-cc98-4ff1-a487-1e575cd48a64")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8e266be-47ed-48e3-bd1c-2210ae0460e6")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "50100f61-5395-4b6f-89bc-65c08363c2fd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e311ab7d-a8d1-4904-8176-f60e3aac65ab")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(J3-In)")
			(pintype "passive")
			(uuid "f140fb9a-e076-4add-9add-53c62ef04044")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(IC3-ANT)")
			(pintype "passive")
			(uuid "9f98d563-df53-4139-9308-ec00e4722749")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "37ce9df1-234c-49ba-8505-b9fbf455f062")
		(at 110.6 75.28)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "6d80f929-d871-40b3-9b29-a5c4e692e229")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "c85f40e0-3a18-48e0-9fc7-c94684f49f14")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cf2d7d3a-a9df-40b9-bb17-6b9af968cf71")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9ffd750e-782b-4c5b-8546-5609524efdf2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/c064599d-eb2f-41e7-9521-e7d37647e88f")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d9ebdb7d-5f40-49b3-affd-61c5f4dae414")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b83dd38f-99d0-4c7b-b229-8d1ffbbf1d23")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c4cff48f-c4a5-49fe-b881-d4ca0f46b87e")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "da751214-84fe-4983-9fc2-d8aaed637adc")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6468f6e-9f9a-464b-b2ff-9839f1ab0ccc")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f316c02-684b-428d-879d-8e293db66088")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e6aa4f06-90f7-4e0b-94bc-7ec3de91e42e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e7d631d-dfa3-4eb0-86b3-14019543e52c")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fbfb7abf-9251-4d88-bff0-893262cc2725")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da446c21-e966-4dcb-a02d-411b6ad998cb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d03febb9-ca8d-4a2c-bc76-495a1b42fca6")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 87 "VBUS")
			(pintype "passive")
			(uuid "5d82a0e4-7b63-4ff3-971d-1cdc40aa0047")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 4 "Net-(IC1-VDD)")
			(pintype "passive")
			(uuid "e24da8b0-a9f2-4756-a854-7e4850b20def")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "3a12898e-ef01-4d7e-8308-e037bb8db987")
		(at 134.44 81.57)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C14"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "ad969070-85bd-470b-a282-12bad9d7a975")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "b6865e70-0763-4c99-94d7-47dc6d4dad4c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "63cd8478-70ba-4e3f-863d-26ddd4f64553")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "483ca437-e6d3-40dd-9895-a4c6eeda2174")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/3a72942d-8d10-4780-ba77-05e4c7e0c89f")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eaf26ddf-17d1-401f-8c78-e5ba0b11d878")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "edae0617-ab47-41d7-808a-c7f978a00d5f")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5e2a1f6-f1aa-4f06-866c-5f0ec2358078")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7061fb0c-be58-413f-b627-ea15a237754f")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8fc853c3-5c99-42ad-8af2-35b14cbc1cd6")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "47368945-577d-4586-90f6-edebaac07e39")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "91e46a6e-9205-4865-97e2-367bc3df9d3b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3615490a-ebc0-4318-8aff-f07ebc7ae27a")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ab35a30-195f-40af-ab08-34e852c0a040")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "12247bf5-cd99-44c1-9699-aeeb7bb32ac2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "79c0997c-f54d-443a-805b-834519362bfb")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "84458f9b-51de-4174-b981-8abaded7dcbf")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "a71391d8-2f39-4277-8719-83af88da17fa")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "3bf8a6a0-4a81-4112-9925-f21e66b6d3e0")
		(at 139.25 66.52)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C18"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "bf7302b1-119c-48e0-a374-ea5be8082d02")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "ee8a5141-eb0b-4fc8-a30a-cd0e60fca99f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "58fde703-d8ae-4b8d-a8d1-1bc2b14816a9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "18ef3bf9-6cde-4d85-a1df-8c4bc88c65b6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a93ded5b-6273-4ee1-8bd1-5085b3c0a712")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a9c6f77a-f6aa-4ba7-b30e-6f5efc6d37eb")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a62dfa1f-0138-4445-9783-90edec560db0")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "88455565-e982-47c7-b23e-d11533b9bf74")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "57657ade-7ab3-4f33-a81a-d00219a33952")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cbc41bc4-cb5f-4dd6-b33c-015c72934100")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0baf800d-8514-48df-86b1-58aaf6eda248")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "52cf51fb-03b0-4ccf-bfc4-8ca474d850ec")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9e2231f8-af76-496d-8751-9aff0df07763")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46a4153b-37f7-49ac-88e1-b37def931295")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "43241f53-3eaa-4893-a568-428213ccd1c2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a345a306-e813-455c-be7b-e8e290e563de")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "36af2337-a8e5-4a00-9749-48ee80f94e93")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "ea2608b4-d8c5-461b-ba4d-c4cdde9b783e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "3e8b4ac1-96c7-4b47-a9fc-8cc23660516a")
		(at 115.35 72.33)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "08eb049a-9a5b-4366-b13b-dfb9e2a1ebb3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "fc16be2b-aaf6-4481-8555-9b3800a3a0cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "158f93f4-6f2a-455f-88cd-23314cf3a010")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "640cfdb3-3165-4b7f-bce1-367618ef9a5d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1ded191a-4224-4a14-b3f0-f55062cc2bda")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5a34029c-867a-44cc-b2d3-2fe6cde4a4df")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f3b0a431-f0fc-439d-897b-7f65b3b40d02")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2cbfd95f-f8a0-4fd4-ac09-7a9769c377f4")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e3d8f306-0d6c-4392-baa9-443e56e1f902")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "abc261f1-928e-4824-91ec-fa03dc07cc97")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4e7397c9-0fdb-4c3d-8818-c23b35d69df4")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "47f66704-215c-4593-bb9a-55b694e189bf")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3f742120-1433-45ba-b46f-27c5492a4de5")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b46197ba-3bcb-4729-8b88-ee6467b81b8b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6380e5a1-a9ad-498c-a112-cb690e0bb1f6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3045659e-bc35-4fb6-a398-923b5c212739")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "a70129c8-705d-4e7a-b671-3c164a80feb5")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 45 "Net-(IC2-MPPT)")
			(pintype "passive")
			(uuid "7cb68029-2b10-4177-8781-7f4a923049fd")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(uuid "3e9b0c71-7482-40a8-bfa9-6991d020d7ed")
		(at 168.525 71.18)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D6"
			(at 0 -2 0)
			(layer "F.SilkS")
			(uuid "f13d48b5-68ec-456c-9eec-80c08eebfbb1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "D_Schottky"
			(at 0 2.1 0)
			(layer "F.Fab")
			(uuid "e393d0b1-84b4-4e48-a8a1-d121152cd534")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f099e4eb-ec0a-4bdc-a2c5-1e1e7bb64928")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Schottky diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "60685909-e3ab-40ef-a86c-8cbd21ab2230")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "940c677c-15ca-438e-ac98-b9456397e262")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ab7d188e-5b45-423d-bbe5-0ff30848f397")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/44adfc12-e24b-4e03-b51b-197393e705f6")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.36 -1)
			(end -2.36 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b72f029e-113e-4813-8da7-f432a4a5ad15")
		)
		(fp_line
			(start -2.36 -1)
			(end 1.65 -1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "278149c8-4f54-4253-9c7f-ee6a553e0e68")
		)
		(fp_line
			(start -2.36 1)
			(end 1.65 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0d801d3e-cc7a-427c-9825-18132ce1882a")
		)
		(fp_line
			(start -2.35 -1.15)
			(end -2.35 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f2909a68-2baf-481f-899c-69d08eae7b83")
		)
		(fp_line
			(start -2.35 -1.15)
			(end 2.35 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2aeb8435-aea2-4da2-a7e5-38d127e4fb3f")
		)
		(fp_line
			(start 2.35 -1.15)
			(end 2.35 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0587c95d-2ec7-452b-9ed6-f6e8f7485d7a")
		)
		(fp_line
			(start 2.35 1.15)
			(end -2.35 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "289fd465-ecce-4580-b64e-4ea423c3ad32")
		)
		(fp_line
			(start -1.4 -0.9)
			(end 1.4 -0.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d4bb744-7e48-46f1-aece-e4b62269323c")
		)
		(fp_line
			(start -1.4 0.9)
			(end -1.4 -0.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6167869b-0edb-4717-ac35-d1a717547920")
		)
		(fp_line
			(start -0.75 0)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9c734cf2-2903-4b5a-8aee-e1eefe2b3908")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1a0403d0-5bf9-4702-b865-4696c8066725")
		)
		(fp_line
			(start -0.35 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f2785b3-d2bb-4776-b174-bebe63d2d6ca")
		)
		(fp_line
			(start -0.35 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "02cc7c42-e347-4166-9716-7f8ac60aa98f")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "08378fe0-85bf-4590-a66d-188349dc065f")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "650f8864-477f-4fe8-b15d-a5b18440c22f")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.35 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b21ae46-b873-4608-a1d0-63f411db67d0")
		)
		(fp_line
			(start 1.4 -0.9)
			(end 1.4 0.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a4d56a46-d49c-4160-bf7c-fa04d4a13aa3")
		)
		(fp_line
			(start 1.4 0.9)
			(end -1.4 0.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a028656-4ac2-4663-a01d-eb9fb8bf4084")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "115264bf-e9b7-46e1-abb7-16537506d569")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "Net-(D6-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "f7376897-43a8-4088-a5f4-a665d96433eb")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "74bc63dc-7eb0-4e8b-aa25-55174c4a888f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "41fc113a-a30c-4774-a4f0-636e8c4811f1")
		(at 120.1 69.38)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R20"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "eb39e56f-e063-4176-a1f8-838914e6e59b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "257f8480-2991-4576-bd41-f1b6e4c09f56")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c8942fd1-a781-4a66-958b-907638005938")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3b92e4fa-7edd-4b45-bb5b-a6dd7ee0329f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/9aa206f9-44a1-4d19-bc8c-36f9838954c7")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a0c29f38-d7c6-487e-a358-0658de4665c9")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2aa8b98-cf99-43a9-ba3d-22540466d154")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8b7baf81-f8f1-464c-ac96-54943d1ae76e")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1215e946-7961-4a65-abdd-df04c577a77a")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "25e95934-0333-42d6-bc10-2f603c9855f1")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e05f7ae1-cbe5-47f3-9428-c7fcd82069d4")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6aee8ae4-9069-4b98-accb-8d3197d94d12")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0ed33679-d1a3-4107-8427-60c0cae2645e")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b56c09d9-8258-4d01-82d8-c35dd8bc442b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae2d0b31-ad09-4132-b65c-8a76b8392ce9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "367b5389-59fb-4a88-9c3a-4121b791f548")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 110 "Net-(U3-FB)")
			(pintype "passive")
			(uuid "90ddc211-865e-4414-8ccc-bbd17ef4c4e7")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "7fe2192a-00a0-4422-90fc-4d9405116d31")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "449f5814-47e1-4aec-a3d8-0cef1154147b")
		(at 115.35 69.38)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "bda3d371-005b-4f84-a103-4806835a6ac5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "120"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "1cedbf66-1882-4e74-a712-452586052d25")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "fb6983bc-31c8-44bd-918a-9cf60123c199")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "df30b372-d425-4e60-a3d2-c331afedd5fc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/34f90ef6-cdeb-49a0-b801-1a46978c2982")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "87d7dbc7-8903-41aa-865d-cc855c521216")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e83d92f3-3270-48be-9e6a-7ae17d477c49")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1c49a62f-de4e-4c66-aff4-e0c8d9acdfaf")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3a17e057-caca-407c-b8f0-ba04074d1a00")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4f520b2f-9a7d-4e22-80e1-cce89571ed91")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e37e7ecf-9617-4acb-98df-d0d312265b0e")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1ef09836-4369-4cf5-9926-a68aa6445c32")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "772c84bf-ee1b-46b2-932a-fc1f6d26e815")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b8c0233f-fd79-4277-bda9-5e83c861a019")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "05213533-f986-4166-bfe8-9aaad51eaca0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "14b3a796-43e7-4262-8501-b80158740ffc")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 46 "Net-(IC2-COM)")
			(pintype "passive")
			(uuid "32bf8a34-e6ca-4fe0-b79f-f956cd1debe3")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 10 "Net-(C20-Pad2)")
			(pintype "passive")
			(uuid "bc06e4a3-adaf-4215-a160-f563b3ed982b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "470cb5f9-10ab-42bf-a7a6-209e1e84187b")
		(at 110.6 84.13)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "e9fcbd7c-fdea-4a51-9733-99a5e6b80732")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "215c0983-4c0e-4f5e-8709-d50336614ab6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3b38ad00-2770-475c-a828-276e112aa986")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "dcd19277-ca76-4608-8e12-7587dead65ac")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/3a29d0ac-1a2f-4f2e-aa6a-e2c8eea20ac5")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3507292e-5f7b-4541-97ee-dbc81f1b2282")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "61048d01-a6d8-44d5-82e6-dc696fbe938f")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "68e0a200-8d1f-4fe9-996b-137b415e3c29")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dad94e9a-141a-480a-a62b-b808205f1dad")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "33579755-8852-46d7-a3e0-2498033fbf1c")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8729e0d2-4df3-42f7-a60a-e77dcf6cc872")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4f51a23-2ac5-4bc8-87bc-a9ac86a3b416")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37379ba2-5b4d-49b9-bf25-32cc8b765ca6")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "84cfb21c-2891-4cea-a485-54fe98990cba")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8586b0de-c8cd-4027-be66-218a10e9995d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6bcfae84-7962-4682-83a0-a371b1e6052e")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 104 "Net-(U1-EN)")
			(pintype "passive")
			(uuid "fbc37a44-0c75-4542-8a04-bb54fe1449b2")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 5 "Net-(U1-VIN)")
			(pintype "passive")
			(uuid "11c252f3-546f-44a6-9b13-0d11e607c5a9")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "47e9e51a-3046-4505-837c-443e1a307417")
		(at 129.63 78.56)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "3f4dd027-f5ee-4e65-aa26-0066280d1cd9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "80219737-97a0-4fa9-ad26-b69121bc429a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9906d077-05b6-419b-9cba-4fecd70e0c84")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "573addad-961b-4c71-a789-88fe5b59debc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/2aff84df-f517-4280-a422-3aee2ba91baa")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0218ec0d-6a3b-4449-8a8d-518dc5e7b853")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c2318e95-7192-4508-8c8e-dd85e4ddd9a3")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "791a771e-1cf5-4e52-8bf8-d08741b0e4d9")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9d401abd-8b60-48fc-94f6-bda7769951b8")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f4a94ee-66a0-4691-91ab-e573c26591c6")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1565a3ac-5cb0-4857-b255-94111ce67ade")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7d54f69-722d-44ab-83d7-fa751d05cdad")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5266b61d-1860-420e-b314-9cc8a84fad0a")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ccf6d46e-d2ef-4d7b-a9d6-e24fe3483e67")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0828b011-ad30-4b43-937f-a87c06eead88")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f2a68b60-358a-4f74-a654-d4f2830520ba")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "ebbf5351-13e4-4ffa-a89e-75ba499c0d01")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "0d08bc37-75ea-4ef5-bfd1-94126a1ecbcd")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(uuid "4c0086bd-0a3f-48d1-a66d-6834f81503d8")
		(at 146.4 122.46)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 -1.998 0)
			(layer "F.SilkS")
			(uuid "b335088a-42c4-4726-b3c6-05e83e9455f2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.Fab")
			(uuid "8b2e317a-b3b6-4810-a3d4-e58b8e9c2f97")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6f048327-0fcd-4342-a7db-86df3087d55e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c1305068-6ef9-4f27-a5be-650310b9cbef")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/860b2ab8-d4dd-4880-bdeb-4b0f18cdab93")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_circle
			(center 0 0)
			(end 0 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "d452865f-a721-46a6-b398-bd204879b7e6")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "8ee27a79-8a6c-4ad8-a257-ddcbea2261c4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "5d5aa606-4dbd-4ab0-a1a0-40aa90d35b3c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 50 "RADIO TX")
			(pinfunction "1")
			(pintype "passive")
			(uuid "bbcd1ee1-72b6-422f-ba8e-af52d1e7a324")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "4c9115be-9551-40ee-9454-ba136820cd97")
		(at 139.25 78.56)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C23"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "cee9df16-fd36-46da-903d-b84e18a42844")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "b77126de-3d29-4d69-bcc8-3ce702b5a04a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b9e2be52-4975-43f2-85fa-9ce4bad91e7c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "44a08039-4656-4d2d-8d9e-75a1771da8cb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/dd80ffef-09ba-48db-8d24-fb4fc1723e22")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "628a3e4d-a42b-49ef-96cc-1522e914b53a")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ec1c394a-a713-424f-8b7f-ec601343141c")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "28ab4291-8e2b-4aa8-b633-1eb08ad7aab9")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b6ce26d9-3998-4e64-b0dc-5e2937a4ac33")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eceef646-c3b5-4960-9b3a-7f4f603d0b64")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c0f46710-be14-4ead-86e6-e97bfbc10ec3")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32a91a07-4f01-48b0-9cd8-e0141d7b4968")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f7018dd-db98-4bd0-9233-502cdd1b52cb")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ac8b3332-e874-4dee-bd02-b1b72f8bad33")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e0f00497-d5b3-4fd3-b43c-d651f5c62703")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1f907892-717f-4f64-a628-f99aae3d79ac")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "3ca12c04-9c44-4d89-9b9b-4d5173807876")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "ce89e6e8-966b-4610-9baf-8ae4bf5c1925")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "4df7a585-b8e1-43b8-b7c5-a16b62051a6b")
		(at 124.85 75.28)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R31"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "47d2c033-2082-4f48-8f4a-27dbba139f67")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "1c331c4d-c836-457c-86d2-f6d12af69846")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "82129cbf-1676-4747-b3f1-1cb7cc3d3b5a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "61005a99-e316-429c-97cb-c8d7fb3ebd7a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1a822f60-b17c-4df0-98d1-22ceac6a2d4f")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "65909fbe-7cdd-4476-9aa7-4e10e0cdf86c")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "18311e3f-595e-4e7e-9d0d-e9281b133166")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2c8802c-69a5-4d3b-ba86-7a5739f78b30")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b95ee01f-37e8-4ba1-b043-702209ec96b5")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2864932e-a7b1-4f35-9886-e2a84bdfff71")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5bf98bf1-53e2-409a-b0e6-543db238f221")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17d48bd6-ff03-42a1-b5e8-47bfd7d807c7")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc447658-c6c8-4052-91a4-c477fd554702")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab58cfac-dda4-4795-a775-9972833e59b1")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f534a75a-86d6-4d01-b828-32f3f544d4b6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4a4ef499-7cfd-4b82-830b-f84dd5da2097")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 117 "Net-(R30-Pad2)")
			(pintype "passive")
			(uuid "23741289-8e5c-4271-95df-ff4d29bc07b2")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "08bf66a0-0139-45dc-bfd7-fca23607e17f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_EH_S2B-EH_1x02_P2.50mm_Horizontal"
		(layer "F.Cu")
		(uuid "5171f76c-ba5a-4d67-bd0e-0de74f1db12d")
		(at 130.75 90.8)
		(descr "JST EH series connector, S2B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH horizontal")
		(property "Reference" "J4"
			(at 1.25 -7.9 0)
			(layer "F.SilkS")
			(uuid "9cfd1aba-1105-44d8-8738-384271294559")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.25 2.7 0)
			(layer "F.Fab")
			(uuid "7d79b1d9-2b90-4888-9e53-e0f466670d8d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a7727856-9c95-4f3e-96db-8f70599cccb4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "293a15b3-e1bb-4101-91d7-0d79032eb6c7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/296868c1-3d5c-484c-b414-2dd158a853f3")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.61 -6.81)
			(end 5.11 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f2ccf143-6e27-46c5-af63-3bc4a0573988")
		)
		(fp_line
			(start -2.61 -5.59)
			(end -1.39 -5.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4fd6ba96-5d0d-442d-aa73-fc1226bb3d8f")
		)
		(fp_line
			(start -2.61 1.61)
			(end -2.61 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a7074563-fbbf-4e00-a42f-ebc1cc37e19f")
		)
		(fp_line
			(start -1.39 -5.59)
			(end -1.39 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8b335b44-fe8f-48d5-8880-b028031011c8")
		)
		(fp_line
			(start -1.39 -1.59)
			(end 3.89 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "677eb09b-61aa-4a5f-8285-cca26ae661b4")
		)
		(fp_line
			(start -1.39 -0.59)
			(end -2.61 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4778906f-44f6-4277-a054-719327952239")
		)
		(fp_line
			(start -1.39 -0.59)
			(end -1.39 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3e5a1a7b-9c66-4a6d-8271-c4a3ae56ff69")
		)
		(fp_line
			(start -1.39 1.61)
			(end -2.61 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f8af7c3b-9394-4ca3-92b3-508d31e5116f")
		)
		(fp_line
			(start -0.32 -5.01)
			(end 0 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ce753563-6e82-4c01-b825-9d04b81f514a")
		)
		(fp_line
			(start -0.32 -1.59)
			(end -0.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bb6e3ed8-38fa-43ba-8b43-67667f6d6d29")
		)
		(fp_line
			(start -0.3 2.1)
			(end 0.3 2.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e5f9f289-718d-48e0-a25f-a17795633da2")
		)
		(fp_line
			(start 0 -5.09)
			(end 0.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e245b425-32c1-4a99-863f-1a4e1e5e3668")
		)
		(fp_line
			(start 0 -1.59)
			(end -0.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cbdf17fa-eb51-4945-8da0-23c5b2233ce7")
		)
		(fp_line
			(start 0 1.5)
			(end -0.3 2.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4d4ef0e9-c3ae-4091-8f1c-a55352754600")
		)
		(fp_line
			(start 0.3 2.1)
			(end 0 1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c4c83f12-65de-4ed2-94b8-60b3d713296f")
		)
		(fp_line
			(start 0.32 -5.01)
			(end 0.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "be1ae30f-1524-40e9-ae10-01289f45be4f")
		)
		(fp_line
			(start 0.32 -1.59)
			(end 0 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f5766967-27d9-4f76-929e-c0b1b128a656")
		)
		(fp_line
			(start 1.17 -0.59)
			(end 1.33 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "085a88f1-3c53-413a-a468-63424b0d0c17")
		)
		(fp_line
			(start 2.18 -5.01)
			(end 2.5 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "61bc03e2-f815-4326-9157-5528bb42e2f7")
		)
		(fp_line
			(start 2.18 -1.59)
			(end 2.18 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f2a5c6ee-9c61-438d-9adb-c4a6b2819126")
		)
		(fp_line
			(start 2.5 -5.09)
			(end 2.82 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fbf72953-5d0c-45fa-9448-5ac106dc12d2")
		)
		(fp_line
			(start 2.5 -1.59)
			(end 2.18 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "188123a6-855f-4697-80c6-c0f1e1de3af9")
		)
		(fp_line
			(start 2.82 -5.01)
			(end 2.82 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "62710e81-a250-4016-bf71-912e4a8aac12")
		)
		(fp_line
			(start 2.82 -1.59)
			(end 2.5 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ae97ff9-5a58-4bc8-ba61-2cf9ee6d1cee")
		)
		(fp_line
			(start 3.89 -5.59)
			(end 3.89 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5f21d14b-f748-4e0b-abc6-f963ec265e48")
		)
		(fp_line
			(start 3.89 -0.59)
			(end 5.11 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "58583fc1-67d1-4118-93d8-c40451410a99")
		)
		(fp_line
			(start 3.89 1.61)
			(end 3.89 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "569f10f2-28c6-4eeb-9cb0-a8cfe4630200")
		)
		(fp_line
			(start 5.11 -6.81)
			(end 5.11 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9dcb8771-2cfc-47a8-9133-f4ef8dc69b6e")
		)
		(fp_line
			(start 5.11 -5.59)
			(end 3.89 -5.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "15d3cc1e-2ce8-47d4-8fc1-91286d91b734")
		)
		(fp_line
			(start 5.11 1.61)
			(end 3.89 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "42fa1e63-638c-494b-8e54-68b4b208b8c0")
		)
		(fp_line
			(start -3 -7.2)
			(end -3 2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2ad8e026-780f-4f0e-9ea6-fa63d2d451df")
		)
		(fp_line
			(start -3 2)
			(end 5.5 2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3b9cb4c4-e84e-402a-8613-6877c6be75b1")
		)
		(fp_line
			(start 5.5 -7.2)
			(end -3 -7.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6a7bd28f-0d56-4634-acb4-398992c99e58")
		)
		(fp_line
			(start 5.5 2)
			(end 5.5 -7.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2e0dac9e-4746-4599-a286-46f0a60942b9")
		)
		(fp_line
			(start -2.5 -6.7)
			(end 5 -6.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f0b7ba2c-1a93-4fe8-a271-e655f36fb400")
		)
		(fp_line
			(start -2.5 1.5)
			(end -2.5 -6.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "10bc040f-44e3-4431-b537-9a1c01dfb9f1")
		)
		(fp_line
			(start -1.5 -0.7)
			(end -1.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a73ce3c9-a16a-41f3-95ad-33f73fc29e6e")
		)
		(fp_line
			(start -1.5 1.5)
			(end -2.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "495f74d1-c4aa-48ea-89ee-cb010f6d4155")
		)
		(fp_line
			(start -0.5 -0.7)
			(end 0 -1.407107)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "64c7e46c-f0bb-4777-b0e5-5a5f345a9b9e")
		)
		(fp_line
			(start 0 -1.407107)
			(end 0.5 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b21df848-4ef9-4b2e-b1fc-4ac3ec0a0806")
		)
		(fp_line
			(start 4 -0.7)
			(end -1.5 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "82891067-324e-4a46-b6df-2b787e657256")
		)
		(fp_line
			(start 4 1.5)
			(end 4 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4a3a4b02-c883-446c-8b47-e191aff11044")
		)
		(fp_line
			(start 5 -6.7)
			(end 5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f9f6ebe8-2d35-44cf-99bd-7002a7a38de8")
		)
		(fp_line
			(start 5 1.5)
			(end 4 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ddee336-23bb-4296-ad98-be28452c9b74")
		)
		(fp_text user "${REFERENCE}"
			(at 1.25 -2.6 0)
			(layer "F.Fab")
			(uuid "ad50537b-c507-4801-9de2-b8b5038c2c71")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 8 "Bat Shunt 1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "c818ba84-ba5d-4cda-90e9-05df025d5f74")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "d07d9b6b-a904-4f54-853c-c67ad6811ac1")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_S2B-EH_1x02_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical"
		(layer "F.Cu")
		(uuid "5a7cfaa7-58e8-46e6-ae8f-d26ed9aeb399")
		(at 122.77 116.68)
		(descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
		(tags "Through hole pin header THT 2x05 1.27mm double row")
		(property "Reference" "J6"
			(at 0.635 -1.745 0)
			(layer "F.SilkS")
			(uuid "881814f3-2d98-468e-8172-6b7e7c68cd49")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_ARM_JTAG_SWD_10"
			(at 0.635 6.825 0)
			(layer "F.Fab")
			(uuid "d35d6f8a-4189-45c1-8cfc-8810f5ccdc3f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e263ed18-3d94-49f0-8df1-71e35d938245")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7719c59c-b800-406c-9400-cebaf1429b75")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "PinHeader?2x05?P1.27mm*")
		(path "/8d551d4a-caea-4f37-aa1a-447ca7746a77")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.18 -0.81)
			(end 0 -0.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3439d613-d064-499d-abc1-a6bbd60b8ed7")
		)
		(fp_line
			(start -1.18 0)
			(end -1.18 -0.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c84f0352-b538-48b4-bc57-9ce4858941a7")
		)
		(fp_line
			(start -1.18 0.81)
			(end -1.18 5.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6ccbd058-9027-4dbd-9398-8c6a19308ed1")
		)
		(fp_line
			(start -1.18 0.81)
			(end -0.666708 0.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9bd751e8-82ee-4c66-b234-971010e554e9")
		)
		(fp_line
			(start -1.18 5.825)
			(end -0.317923 5.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "59c4498f-d8c3-4a48-9547-6ff13ad9e502")
		)
		(fp_line
			(start 0.317923 5.825)
			(end 0.952077 5.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "23cc7cc0-baad-48fb-bc93-d56c8286feb0")
		)
		(fp_line
			(start 1.587923 -0.745)
			(end 2.45 -0.745)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0bd7a60a-0d3f-4807-a728-ee88a0690acf")
		)
		(fp_line
			(start 1.587923 5.825)
			(end 2.45 5.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f7714056-8979-40b1-930b-2a290ff2b8b5")
		)
		(fp_line
			(start 2.45 -0.745)
			(end 2.45 5.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "df8045f9-3e92-40f2-813c-c0ef01f52768")
		)
		(fp_line
			(start -1.57 -1.14)
			(end -1.57 6.22)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f4c951a8-f299-4c53-bf1d-e725cfaddbbd")
		)
		(fp_line
			(start -1.57 6.22)
			(end 2.84 6.22)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "26f2fee2-6b35-4a5a-966e-ddf7d6924258")
		)
		(fp_line
			(start 2.84 -1.14)
			(end -1.57 -1.14)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "52ed589a-11aa-44f1-a10d-bde684c9a64e")
		)
		(fp_line
			(start 2.84 6.22)
			(end 2.84 -1.14)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50228a5f-9b62-47a8-9079-d7578465f4a5")
		)
		(fp_line
			(start -1.07 0.2175)
			(end -0.2175 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2b2ddfff-ac4f-4b58-bcac-04eb7c76e45b")
		)
		(fp_line
			(start -1.07 5.715)
			(end -1.07 0.2175)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d81df4e6-bfdd-4ae1-859b-1ac5fa2a2081")
		)
		(fp_line
			(start -0.2175 -0.635)
			(end 2.34 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6d365ce0-e0ab-4445-ac28-a12a7fab16d1")
		)
		(fp_line
			(start 2.34 -0.635)
			(end 2.34 5.715)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "910a4f02-daee-4ab0-bab4-8fe6b4155207")
		)
		(fp_line
			(start 2.34 5.715)
			(end -1.07 5.715)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "60c32efa-dc0f-4760-b214-78795f99b4e6")
		)
		(fp_text user "${REFERENCE}"
			(at 0.635 2.54 90)
			(layer "F.Fab")
			(uuid "12e3eb22-d813-4cb1-a842-999939666959")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VDD_NRF")
			(pinfunction "VTref")
			(pintype "power_in")
			(uuid "66cd5c7b-a285-4774-ae2c-896b4ebe304f")
		)
		(pad "2" thru_hole circle
			(at 1.27 0)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "SWDIO")
			(pinfunction "SWDIO/TMS")
			(pintype "bidirectional")
			(uuid "c2d4db3a-56e7-4e50-a0b7-1cbe094a9a2f")
		)
		(pad "3" thru_hole circle
			(at 0 1.27)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "1b64a31d-bfac-470c-ab70-8887eca99738")
		)
		(pad "4" thru_hole circle
			(at 1.27 1.27)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "SWDCLK")
			(pinfunction "SWCLK/TCK")
			(pintype "output")
			(uuid "f6f990db-4495-47f8-8d13-cffa67052547")
		)
		(pad "5" thru_hole circle
			(at 0 2.54)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "8b8c3399-e938-4bb4-a860-89cc404ead4f")
		)
		(pad "6" thru_hole circle
			(at 1.27 2.54)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "unconnected-(J6-SWO{slash}TDO-Pad6)")
			(pinfunction "SWO/TDO")
			(pintype "input+no_connect")
			(uuid "f42567f2-e0c3-4c56-9b64-d06f76f48e8b")
		)
		(pad "7" thru_hole circle
			(at 0 3.81)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "unconnected-(J6-KEY-Pad7)")
			(pinfunction "KEY")
			(pintype "no_connect")
			(uuid "bce82cd3-4311-4d71-bc7a-f820f6021737")
		)
		(pad "8" thru_hole circle
			(at 1.27 3.81)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "unconnected-(J6-NC{slash}TDI-Pad8)")
			(pinfunction "NC/TDI")
			(pintype "output+no_connect")
			(uuid "59af160e-58fe-4b9b-9133-3b7adde12d17")
		)
		(pad "9" thru_hole circle
			(at 0 5.08)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GNDDetect")
			(pintype "passive")
			(uuid "1f84b551-702d-455b-bca5-25faed611007")
		)
		(pad "10" thru_hole circle
			(at 1.27 5.08)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "RST")
			(pinfunction "~{RESET}")
			(pintype "open_collector")
			(uuid "ad3e7d32-a676-4ef8-8dca-033664df9f90")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "61c5222c-aaa7-4f37-99ce-695821d13d82")
		(at 139.25 63.51)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C16"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "01a9f156-462c-4743-aa4f-8a3ff27da990")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "7505fbfd-5405-498f-ba1d-800b95ab0845")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "63b75953-edec-48e7-b9d1-44b8ac406330")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0f31f2cc-69d6-40ce-8cd0-b8582060a712")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/903308f2-98ff-4200-9c95-f1638ce4c5c8")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b4ad9c0b-a83c-47f5-badc-53f1e28f93c8")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4ca61e7a-bb82-46bc-a284-24ee426652b9")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4f91ce79-9709-4077-b8bb-f88558c53e14")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0f424a00-5570-4a2f-b9ff-ce86a1908347")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9ce0fc25-9edb-4496-a15e-7ecfd99d3ef4")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "21ee34fa-8914-4d69-abae-268a68f8c1d3")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "40b354dd-fc18-4098-aab0-479d0b59b341")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9a857733-c7be-437b-b348-4564003df913")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83278ef8-2dd6-4347-ad47-25584debc854")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dab64f29-03d7-4f47-91e9-7bcd16dbcef0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "dc3a11ed-965d-43ac-aa08-50fd403cc133")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 6 "Net-(U1-VBST)")
			(pintype "passive")
			(uuid "0aa10478-ded3-43bb-afa8-1c3e950e9a45")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 7 "Net-(U1-SW)")
			(pintype "passive")
			(uuid "225b816a-35f8-4dbb-9820-d33cd39698ee")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "638beebd-5edf-4e95-b52d-f10644734f95")
		(at 134.44 63.51)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "04b34522-99ce-4e58-8065-585df56926f2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "130f7226-9bdd-42be-980e-c9135ca26071")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e8048d92-1fa9-4935-bae8-fb9b5b249775")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f9eaddfd-8692-4d1b-b949-2dbbf5b90834")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/965795cb-9784-4a8d-9ea2-e2e6ba1e88d3")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "981babcc-bfdd-4bfe-8dbb-b54e89bfd4da")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "500012d1-120a-4c4b-9a98-8a0e7f09510c")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9e175204-8b79-4e21-b456-a7ced36289da")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "501143c4-bcf9-415f-a3ac-06e43560a36b")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "38869982-300c-469e-a6bc-816145f0426f")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "203072e1-d013-4682-91bf-6f6106b2969f")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a1f6bfa4-8d81-4094-9434-7265bc5fc156")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "afc833dc-d3b2-4cf2-a913-76b507579d8e")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca6a31b9-9818-41f9-ae88-0437fdb4b4ff")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a4909b82-3f07-45db-9af5-13e8f7a718c1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "cee832ed-2796-488c-b18b-0d856a53424e")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "f7b3fd87-20dd-4528-88a2-223dd2a2fbca")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "7a9965d2-7771-4bf0-8eab-15c69d551038")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "63f12496-2ecc-4595-beb1-a47dbb8be796")
		(at 129.63 72.54)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "bb4b7809-f83e-4915-a95b-fc27fbc18afb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "9e66f53c-76c8-4922-a38b-faf0513b4e6e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9236a3ec-de9c-4c39-9cc6-406c28b2eeb4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "eacae553-4572-491f-91a3-e427fb131b49")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/31502cff-abd5-4e7b-94dc-a1acf0f3ad7c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cb01c714-4091-40c2-aa11-6f76aaf9f51e")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f60dad28-aa54-415c-bd77-1d166394cd78")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "66153f74-c2bf-4134-997e-003b3c114f96")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cb760fd5-baa1-4f94-a6a9-7fbf52b06b27")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a5d892ce-0781-4033-bffc-bbf3cd4e7673")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1fc68a30-2a3c-407e-a0fd-7558d8fc1f3e")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6d9b1bab-f58f-4c82-894a-0c7710abf465")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6b13cfaf-708a-43be-8897-31ffbdf25473")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1cc6ad3-9fd1-4e70-8c8b-afd11fc2cce1")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "96d8d10d-1270-4a6a-92b1-5bb62ddc79fa")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0516b70d-779f-4998-ab2f-2ddc0cc8d385")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "2830a636-0664-46ce-8ace-4695a26d06ab")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "fcd2ba2d-9382-4aeb-b257-33ad8304b335")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:Texas_R-PDSO-G6"
		(layer "F.Cu")
		(uuid "651809f7-c2f2-420c-98e5-c1e9d1ef988a")
		(at 168.1 116.635)
		(descr "R-PDSO-G6, http://www.ti.com/lit/ds/slis144b/slis144b.pdf")
		(tags "R-PDSO-G6 SC-70-6")
		(property "Reference" "U2"
			(at 0 -2.25 0)
			(layer "F.SilkS")
			(uuid "5a935a00-9816-43a9-a120-e6cf1e97491c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TPS61222DCK"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "59b3dcfc-0b17-4d89-9c44-dde7358ceba8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61220.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "19f36b6d-91f9-4bfb-acd4-8a3f6555259a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9e8f848f-a80c-4d54-ba13-a8bb52dbe9b7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C116461"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b35ef272-0aa2-4c01-ba7c-54094a1be372")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Texas*R*PDSO*G6*")
		(path "/88898e51-2e9a-44c4-b336-70a2f81aebb1")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.7 -1.16)
			(end 0.7 -1.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f12a1043-dd70-4f59-8b21-d0d23a066fbc")
		)
		(fp_line
			(start -0.7 1.16)
			(end 0.7 1.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "196fdb3f-1304-490e-9983-b291930cea03")
		)
		(fp_poly
			(pts
				(xy -1.12 -1.11) (xy -1.36 -1.44) (xy -0.88 -1.44) (xy -1.12 -1.11)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "f5021587-c16f-4cd2-a405-763b055ff16d")
		)
		(fp_line
			(start -1.6 -1.4)
			(end -1.6 1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "19a19a50-6a78-4517-b774-9f5a616e5e25")
		)
		(fp_line
			(start -1.6 -1.4)
			(end 1.6 -1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1a0b28e5-bd49-4b0b-9003-9c1d7d4971c6")
		)
		(fp_line
			(start -1.6 1.4)
			(end 1.6 1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1239ce68-02d0-4317-a48b-3957f72ba033")
		)
		(fp_line
			(start 1.6 1.4)
			(end 1.6 -1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c7190091-22e9-497e-bee1-417eb75fceb6")
		)
		(fp_line
			(start -0.675 -0.6)
			(end -0.675 1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a8aca1cc-87e7-4739-a5e7-de0178d64687")
		)
		(fp_line
			(start -0.175 -1.1)
			(end -0.675 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5df87130-2c5f-4fa3-944c-2edfe796fa1f")
		)
		(fp_line
			(start 0.675 -1.1)
			(end -0.175 -1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a8f07f90-1375-4dbe-91f3-8d317a51069a")
		)
		(fp_line
			(start 0.675 -1.1)
			(end 0.675 1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c98918f-20b1-41aa-a075-dcd314a006e3")
		)
		(fp_line
			(start 0.675 1.1)
			(end -0.675 1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "01890b3a-55f3-43c5-ac77-5ad7c3266e0b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "a32e17aa-0027-4fa9-ae4e-bcfbf12860c6")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.075)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1 -0.65)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VDD_NRF")
			(pinfunction "VIN")
			(pintype "power_in")
			(uuid "a92e1ff0-1138-414b-b123-0252254f5fe5")
		)
		(pad "2" smd roundrect
			(at -1.1 0)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pinfunction "FB")
			(pintype "input")
			(uuid "dc6cc836-d7c6-4b70-9962-622e807eff31")
		)
		(pad "3" smd roundrect
			(at -1.1 0.65)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "b2d2247b-739b-49ec-83f7-6b7f9d5a5da1")
		)
		(pad "4" smd roundrect
			(at 1.1 0.65)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pinfunction "VOUT")
			(pintype "power_out")
			(uuid "8d8d77de-fa82-4c91-8ce5-b26ff28ff3e9")
		)
		(pad "5" smd roundrect
			(at 1.1 0)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "Net-(U2-L)")
			(pinfunction "L")
			(pintype "power_in")
			(uuid "68427514-bc1c-4acf-b2a7-a811ba206413")
		)
		(pad "6" smd roundrect
			(at 1.1 -0.65)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VDD_NRF")
			(pinfunction "EN")
			(pintype "input")
			(uuid "e3fbdb25-f6f4-4d33-be82-cd4b62e9fc58")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "6e904f9b-2ffb-425a-9f55-6286300b7be5")
		(at 129.63 63.51)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "4b8166e5-4e3c-4958-9e36-a0c99d818dc0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "aae11fb4-fd80-4a8e-a18a-b898a728a8c8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5f71fe5f-5d60-4cb3-a7a0-5a7eab273a52")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "72aef4cb-a636-416e-ab4a-99fddbd45df6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/b5865098-a11e-4708-8e9d-eb317f39a27b")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed2208b5-1679-4655-9d2c-abd8f7369df8")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2e05391-486e-490b-a8e3-621a36ec1c5f")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "88e1c896-0cad-4f3b-af2f-d526a2f0dbc2")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "02b7b64e-8278-4ee2-b7be-e585ac287c11")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "571d697f-4520-4f5d-9a04-5bdde357e6e8")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "37ef13bd-b364-4a45-91f7-40c0b4672308")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a6cc9d4b-7822-4ba5-9bbc-fcc55c468df6")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a8cbb363-ed1e-4b49-b6b3-379bf1396f65")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dcfefa06-78a7-46f2-b811-5ad3339998c6")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d59aaae-cc49-471e-be21-e25ff93318b0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "36ea2a9e-2ab4-4826-86db-c5ccbcb080a4")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "3c2aa67c-5748-42a6-9d28-f4b1bcd3432b")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "fd877c29-a81e-4e43-b7da-91451e29aeaf")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(uuid "6ff32a25-2ff5-4ba9-a7ae-890716e76af6")
		(at 123.04 108.4)
		(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
		(tags "sma edge")
		(property "Reference" "J7"
			(at -1.5 7 0)
			(layer "F.SilkS")
			(uuid "d764d644-27c5-4eca-ab97-01a89f2292df")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_Coaxial_Small"
			(at -1.72 -7.11 0)
			(layer "F.Fab")
			(uuid "ebf2ccd6-841d-463f-96fb-10bd796413d7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b0b825ca-53a8-47bd-a5eb-f93467258b0d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "small coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4e25589f-50c4-4124-a3f7-888a778fc01f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(path "/10f8c319-a38b-466f-8ffe-5ca0745434ab")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start 2 0)
			(end 2.5 -0.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cfb0af38-29a9-468b-80a8-20ebdaf6c766")
		)
		(fp_line
			(start 2.5 -0.25)
			(end 2.5 0.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "48dfdf67-9b25-4a56-a146-8a92c7e09acd")
		)
		(fp_line
			(start 2.5 0.25)
			(end 2 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e16f9e2b-63ec-487e-9f41-7ea92a606b88")
		)
		(fp_line
			(start -14.29 -6.09)
			(end -14.29 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "d68ce519-0d9f-4887-b2c8-fc2ab01de2b0")
		)
		(fp_line
			(start -14.29 -6.09)
			(end 2.71 -6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "f9221fba-acbc-4911-8d50-c82e20a5a9e0")
		)
		(fp_line
			(start -14.29 6.09)
			(end 2.71 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e8e35b54-3cb0-40a5-99a9-20458c0d4931")
		)
		(fp_line
			(start 2.71 -6.09)
			(end 2.71 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "9caa526e-3f7a-48ec-9bdb-c9a32a3cbb43")
		)
		(fp_line
			(start -14.29 -6.09)
			(end -14.29 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9ab8bd99-7096-4d08-bcb5-0811949fc34f")
		)
		(fp_line
			(start -14.29 6.09)
			(end 2.71 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "78457b91-1548-4895-9893-d02184206709")
		)
		(fp_line
			(start 2.71 -6.09)
			(end -14.29 -6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "929b085c-ff65-4b12-b4c7-dcc3236fb8a0")
		)
		(fp_line
			(start 2.71 -6.09)
			(end 2.71 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dcb5dc71-8c30-440c-9c65-cbdfd630ed90")
		)
		(fp_line
			(start -13.79 -2.65)
			(end -13.79 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5ce597e5-62e4-493b-b5aa-c8a5882e8778")
		)
		(fp_line
			(start -13.79 -2.65)
			(end -5.91 -2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87a230b8-0b40-445e-a217-8c884f558114")
		)
		(fp_line
			(start -13.79 2.65)
			(end -5.91 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "766df490-315f-4895-8701-0328ffa517db")
		)
		(fp_line
			(start -5.91 -4.76)
			(end -5.91 4.76)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b5ec9da-e20c-425e-938d-932734ae5467")
		)
		(fp_line
			(start -5.91 4.76)
			(end 0.49 4.76)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f4ccd90e-35ca-49ce-85ba-f6631ace2534")
		)
		(fp_line
			(start -4.76 -3.75)
			(end -4.76 3.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f8d5bab-7c5f-4cf1-93e9-a1211f56a0a4")
		)
		(fp_line
			(start -4.76 -3.75)
			(end 0.49 -3.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a3cdc73b-d00d-44dc-844b-e67903504ce9")
		)
		(fp_line
			(start -4.76 -0.38)
			(end 0.49 -0.38)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa71d43c-b2ab-4028-b36e-96f152d99963")
		)
		(fp_line
			(start -4.76 0.38)
			(end 0.49 0.38)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "95c702bf-4d72-4586-9985-404e3073b834")
		)
		(fp_line
			(start -4.76 3.75)
			(end 0.49 3.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be722118-a3a2-4f07-a83d-febfab950a36")
		)
		(fp_line
			(start 0.49 -4.76)
			(end -5.91 -4.76)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a6e4b79b-1a3d-4068-9874-5763b31f063b")
		)
		(fp_line
			(start 0.49 -4.76)
			(end 0.49 -3.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ac31daf2-b69f-4e85-9d6c-13a54c26c933")
		)
		(fp_line
			(start 0.49 -0.38)
			(end 0.49 0.38)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2212749c-2f72-410d-817f-b5e84149e42f")
		)
		(fp_line
			(start 0.49 3.75)
			(end 0.49 4.76)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "07a85a90-0f34-490f-bd40-8e5645abcfcc")
		)
		(fp_line
			(start 2 0)
			(end 2.5 0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca433c38-2d09-497f-8e40-84fec4ecb2e1")
		)
		(fp_line
			(start 2.5 -0.25)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d149c681-bd28-416b-bc1c-63f47be92a8a")
		)
		(fp_line
			(start 2.5 0.25)
			(end 2.5 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f5ef6f1-4ccb-4d7a-9d9c-b1e8f761b356")
		)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 0)
			(layer "F.Fab")
			(uuid "b8306838-71eb-463d-b2a3-c1cbbc962bf2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -1.72 0)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(J7-In)")
			(pinfunction "In")
			(pintype "passive")
			(uuid "17dd61da-c708-49a2-b3a7-f863ce0a7496")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "f0ae0f0d-9ed8-44c4-abe8-8775014df367")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "d64c8bfc-7966-46bf-9cde-68e732926cb7")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "e10073ff-03ce-4737-9e10-2e231ca6cbcb")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "9ebfd9f5-a1a9-4b8f-9d7d-23dbbe8e7b56")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "efe0c621-b22a-4e82-bdf3-fb2bab375c76")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "1c3e60f4-ad04-4d63-8d2e-d65ae4e23b50")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "f8d90f71-67da-4e48-a718-5cd75147864a")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "0f00e819-7373-4776-bee7-b4d450842cab")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "9bef4518-bab1-4a62-a3ab-f1952bba37ca")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "887488f6-6e5b-4041-8144-5041ec05efa6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "71bb7456-d574-463a-8260-fcbccdb5f8ec")
		(at 138.45 107.6)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C26"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "e0dae020-d79a-4bf5-a38c-4c50b3b29983")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "5e2a1d9a-4e9a-4edb-ba30-ea4a3c9c35a2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4ccaf5d3-2669-4d8d-892a-62f53d732617")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f7848067-54dc-48b2-a209-89b555ad744b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/65b26f36-1540-4bd2-8746-120d2100802c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a8cc79c6-8a97-4ca9-99bc-7c71da5b9c2f")
		)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c934404f-5165-4f95-9c32-2dc9d0874c72")
		)
		(fp_line
			(start -1.65 -0.73)
			(end 1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "890acebd-524c-425c-b421-b0144b53b283")
		)
		(fp_line
			(start -1.65 0.73)
			(end -1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "24cb69b9-25de-46d2-b488-7f62b3c9f595")
		)
		(fp_line
			(start 1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f3fd861-bf87-4939-bec9-69804f8f0a54")
		)
		(fp_line
			(start 1.65 0.73)
			(end -1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c2f4da2-541e-4646-b438-4441256e09a0")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b754268-5179-4969-9949-53405b155211")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "610c9b63-b3ce-48b6-9748-62d71c5247cb")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "510a5231-7e3a-48b7-9d29-5569fc428685")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b7b0a473-344e-4c41-90cd-32a640314deb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9a764bad-dd13-46e6-ac8f-9543dacfc50e")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "USE_ANT_2")
			(pintype "passive")
			(uuid "3b59eb24-22e3-4ba4-a659-9ee3b3264691")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "8543a908-9eea-4dad-981e-f0ae95566632")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "74d9890f-1fd8-44da-92a8-138896c70ffb")
		(at 120.1 84.13)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R25"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "f93a4e81-d7a7-42c8-bcc6-9aa932bd81e4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "83367603-fd8d-4d7d-8ef8-e3f50380554a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ab5aa49d-1882-45c0-ac68-d93b562f318c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "01535c26-73bf-4b33-bd7c-9be942938adf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/c09b3889-cb3c-4877-bf7b-1da6db861c17")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "50ba86c2-5fc2-438d-9f11-dea1787cfa6a")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2ed6f069-5860-486a-bbb5-a92a96c83709")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e84e2f06-37c9-4736-838f-ddcb2ae8b077")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fbe8329d-ac48-4a56-a8bc-28be58b70633")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4b8dd358-1513-420b-9b00-42ce656a4538")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e8991c4c-d294-4eb7-8334-54aa9b8d0f25")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "38537804-49ec-4225-a96a-f1b46c5efc9e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "44fac2a7-57c0-408c-8ec9-8b8eec304bd1")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "437b267a-d568-412b-a6f5-0201c25824b8")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6be75af4-db4d-4977-bbca-e45b65df8057")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bb791ca5-c090-4471-ba91-c71e3cff6fc0")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 114 "Net-(R25-Pad1)")
			(pintype "passive")
			(uuid "b74b6df9-91eb-4695-a8b8-34f29e6d5747")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "8fa47e33-b8f3-4a62-8075-22646067eb13")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_EH_S5B-EH_1x05_P2.50mm_Horizontal"
		(layer "F.Cu")
		(uuid "79bb0fbe-7593-47a1-ae78-4bc9f0636872")
		(at 139.8 101.18)
		(descr "JST EH series connector, S5B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH horizontal")
		(property "Reference" "J2"
			(at 5 -7.9 0)
			(layer "F.SilkS")
			(uuid "1305c516-1b38-4add-b450-ea2118e0df83")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x05_Socket"
			(at 5 2.7 0)
			(layer "F.Fab")
			(uuid "3789fc09-00f0-4299-9dd2-1cd97eafdef2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "af5068e6-8afe-4583-ae74-7cff91c03536")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "77d3f0f6-cf1b-4f71-ba07-4f5f9896cccb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/855dc855-fadd-46fb-a7fe-1cc286f51387")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.61 -6.81)
			(end 12.61 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "850ea1df-6cb5-40d0-92e5-086e45624b6d")
		)
		(fp_line
			(start -2.61 -5.59)
			(end -1.39 -5.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "65e94119-3407-4f58-85db-5b1fed140083")
		)
		(fp_line
			(start -2.61 1.61)
			(end -2.61 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5453562b-e50c-4c75-941c-12c8982dcdbb")
		)
		(fp_line
			(start -1.39 -5.59)
			(end -1.39 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6363bc9d-db83-4260-afa6-dbbecc81e76b")
		)
		(fp_line
			(start -1.39 -1.59)
			(end 11.39 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f84bc8d2-21d0-4059-8f8e-e0c286949b92")
		)
		(fp_line
			(start -1.39 -0.59)
			(end -2.61 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8a0b9b94-fb69-4b92-99ab-f3909758a9fe")
		)
		(fp_line
			(start -1.39 -0.59)
			(end -1.39 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac6af73a-de0a-4511-b84f-bbc0a94d1625")
		)
		(fp_line
			(start -1.39 1.61)
			(end -2.61 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a871683d-2291-430b-97e8-2275c05589a4")
		)
		(fp_line
			(start -0.32 -5.01)
			(end 0 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a40bc84-2d7b-4dd2-88e2-cdaa4529c0af")
		)
		(fp_line
			(start -0.32 -1.59)
			(end -0.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "53e5cb6e-8a50-46b6-9c16-4c0df15f9cba")
		)
		(fp_line
			(start -0.3 2.1)
			(end 0.3 2.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e041a8ed-c4b1-4798-9ede-03dade482f3b")
		)
		(fp_line
			(start 0 -5.09)
			(end 0.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "09ee3dd6-f90b-42c3-bfbf-ea06c1533c01")
		)
		(fp_line
			(start 0 -1.59)
			(end -0.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "76241b45-a664-4c7d-be46-a9d136b86e5d")
		)
		(fp_line
			(start 0 1.5)
			(end -0.3 2.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "87a5dc98-6372-4080-99e5-52f86161a6f9")
		)
		(fp_line
			(start 0.3 2.1)
			(end 0 1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "56f91b53-40a9-453c-912d-1f6009e0ad79")
		)
		(fp_line
			(start 0.32 -5.01)
			(end 0.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "425efe28-ba7f-4fc0-be68-c9fbeacb9f2a")
		)
		(fp_line
			(start 0.32 -1.59)
			(end 0 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "63748049-f883-4cb5-8c2a-346031138904")
		)
		(fp_line
			(start 1.17 -0.59)
			(end 1.33 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "62f4bdb4-574d-46a5-8a6d-16be0d3443ea")
		)
		(fp_line
			(start 2.18 -5.01)
			(end 2.5 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "74fa8d6b-be06-4fd9-ba5b-020d56f848c1")
		)
		(fp_line
			(start 2.18 -1.59)
			(end 2.18 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fe03f6a7-c4f9-4dad-8776-bf3c18f350b7")
		)
		(fp_line
			(start 2.5 -5.09)
			(end 2.82 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5cdc1487-4a56-43fa-8a30-19e0a86e1efe")
		)
		(fp_line
			(start 2.5 -1.59)
			(end 2.18 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "25ee69e2-6335-4449-8b96-4d904f5b3b80")
		)
		(fp_line
			(start 2.82 -5.01)
			(end 2.82 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fc43ce3a-fdcb-4458-8795-c0c58ddeddbe")
		)
		(fp_line
			(start 2.82 -1.59)
			(end 2.5 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3fdd767f-8b21-44f8-b28d-f3de0be9d779")
		)
		(fp_line
			(start 3.67 -0.59)
			(end 3.83 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "109b2cb2-e4a2-4d2a-a807-5fb6015dbaac")
		)
		(fp_line
			(start 4.68 -5.01)
			(end 5 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8ac62d91-2949-4418-a262-131c5bedde70")
		)
		(fp_line
			(start 4.68 -1.59)
			(end 4.68 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "990ac853-68c5-4fba-bb6f-888cf1859fc6")
		)
		(fp_line
			(start 5 -5.09)
			(end 5.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7fdece91-af2e-4b96-a0e1-32b1df6b9708")
		)
		(fp_line
			(start 5 -1.59)
			(end 4.68 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f718c8a3-09ff-4c89-9642-7c7d58dda617")
		)
		(fp_line
			(start 5.32 -5.01)
			(end 5.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6a378f01-8c31-4fcb-b5d5-be72e4a3ee23")
		)
		(fp_line
			(start 5.32 -1.59)
			(end 5 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6801af6a-56d0-456d-864c-11a0d32ee3e6")
		)
		(fp_line
			(start 6.17 -0.59)
			(end 6.33 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0b2fe292-ab91-48fe-9024-4d36314a3e22")
		)
		(fp_line
			(start 7.18 -5.01)
			(end 7.5 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "17b73ed4-3504-4546-83fd-61b848fe59a9")
		)
		(fp_line
			(start 7.18 -1.59)
			(end 7.18 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8e300652-6a71-4801-9b4c-18f231021bfa")
		)
		(fp_line
			(start 7.5 -5.09)
			(end 7.82 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "45aace91-11ea-42c2-bef8-70c6093deaad")
		)
		(fp_line
			(start 7.5 -1.59)
			(end 7.18 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d08d4a16-a05c-4cb9-a56b-23843dc97131")
		)
		(fp_line
			(start 7.82 -5.01)
			(end 7.82 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "649a2bf0-58ae-4b5c-bd6a-44d732e1debf")
		)
		(fp_line
			(start 7.82 -1.59)
			(end 7.5 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3e59f300-ce0d-49f4-b872-95de741953ef")
		)
		(fp_line
			(start 8.67 -0.59)
			(end 8.83 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "198e010d-b95b-451c-8e60-10cf374b5b67")
		)
		(fp_line
			(start 9.68 -5.01)
			(end 10 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "96de9dd7-8477-428c-a6c6-b305bc5955d9")
		)
		(fp_line
			(start 9.68 -1.59)
			(end 9.68 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "969e51ff-d926-463e-9765-5a99663a9971")
		)
		(fp_line
			(start 10 -5.09)
			(end 10.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f275f1f1-abcf-40ab-a675-3fd500d4cfce")
		)
		(fp_line
			(start 10 -1.59)
			(end 9.68 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b6a79c1-5bcb-48ba-8ac5-5c87ea656af9")
		)
		(fp_line
			(start 10.32 -5.01)
			(end 10.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d7edf936-5a12-4438-94ce-202913d36648")
		)
		(fp_line
			(start 10.32 -1.59)
			(end 10 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e5132ef5-c22b-47b1-98a2-7d8d605b1a9c")
		)
		(fp_line
			(start 11.39 -5.59)
			(end 11.39 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f57e3f3a-3200-45b9-a7fa-76567003f2ff")
		)
		(fp_line
			(start 11.39 -0.59)
			(end 12.61 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d02ed01b-54ed-4ef4-a874-484b16492ceb")
		)
		(fp_line
			(start 11.39 1.61)
			(end 11.39 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d25f8ec2-84fa-486a-a635-05e0034c674d")
		)
		(fp_line
			(start 12.61 -6.81)
			(end 12.61 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a5710d1c-10dc-45fe-94c8-fd9e24c56b3c")
		)
		(fp_line
			(start 12.61 -5.59)
			(end 11.39 -5.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "df82710f-c5f6-4a37-ba35-651ea6e8dde8")
		)
		(fp_line
			(start 12.61 1.61)
			(end 11.39 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3d4cbde7-9bf5-4e2e-9091-3f05c6e6e729")
		)
		(fp_line
			(start -3 -7.2)
			(end -3 2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6f5ead64-2a42-4871-a3eb-280c256d749e")
		)
		(fp_line
			(start -3 2)
			(end 13 2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b4067094-23fc-4b25-88e5-c1a1cee79a3a")
		)
		(fp_line
			(start 13 -7.2)
			(end -3 -7.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "21956441-48aa-4b27-9c65-4320108517e1")
		)
		(fp_line
			(start 13 2)
			(end 13 -7.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "255b1f29-2d9b-4a38-824c-aed0bc96fbb0")
		)
		(fp_line
			(start -2.5 -6.7)
			(end 12.5 -6.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b78f20fe-d6f3-4c8e-8dce-d9e35ffc3f9e")
		)
		(fp_line
			(start -2.5 1.5)
			(end -2.5 -6.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "43e157b2-a9cf-492f-8d6b-f3ee4868c0d8")
		)
		(fp_line
			(start -1.5 -0.7)
			(end -1.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8128395e-0447-4949-8cdf-d319239220dd")
		)
		(fp_line
			(start -1.5 1.5)
			(end -2.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37e8e316-37fd-4fa3-bcd5-1e44b91aae1e")
		)
		(fp_line
			(start -0.5 -0.7)
			(end 0 -1.407107)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4055702-053d-4b1c-ab4d-6fd93d1667a0")
		)
		(fp_line
			(start 0 -1.407107)
			(end 0.5 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a1abb6cd-4e15-4e42-b49e-a3fecbd6245d")
		)
		(fp_line
			(start 11.5 -0.7)
			(end -1.5 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b6169dc8-e7d5-42c8-839b-d714379b8d52")
		)
		(fp_line
			(start 11.5 1.5)
			(end 11.5 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c8bed5cb-10dc-4269-96d8-0cad58460c89")
		)
		(fp_line
			(start 12.5 -6.7)
			(end 12.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "920a5b30-687e-433e-a400-36e2c48ffb3f")
		)
		(fp_line
			(start 12.5 1.5)
			(end 11.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a97279a1-a220-4265-b72a-97dc6e6b8802")
		)
		(fp_text user "${REFERENCE}"
			(at 5 -2.6 0)
			(layer "F.Fab")
			(uuid "764dcf05-5834-45ff-a27c-67611d80db14")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 3 "VDD_NRF")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "4aa07337-ac85-4640-83f1-87e639a9e5b2")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "GPS_EN")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "f58ec5eb-66e1-4101-804d-eded8cd1354e")
		)
		(pad "3" thru_hole oval
			(at 5 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "GPS_TX")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "27712907-687a-48d1-a11e-15478e892c6e")
		)
		(pad "4" thru_hole oval
			(at 7.5 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GPS_RX")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "1550d844-0538-46d0-852b-ba5dab61c555")
		)
		(pad "5" thru_hole oval
			(at 10 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "42a52f40-eb4f-4ab5-b2a0-69ac37aee824")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_S5B-EH_1x05_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "7a728be3-a94b-4ea5-bdb1-741be1715db8")
		(at 139.25 75.55)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C22"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "0221e412-bea5-437c-a15c-c611694c95dc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "0e1156d2-3c7d-4464-8961-d2d43360ce16")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0f1c061-f68c-4cb4-a79f-54c3b2d425f7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0242f66f-26a5-452b-baa7-38ccbfe763bc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/36c7bd9c-372a-453e-a6c5-cf249c3874d7")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "78b8cb97-2b33-4f6e-a418-49bf4ac33f87")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91abb8bb-dec9-4205-91ec-e4595dd8394a")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b47c111f-f917-48de-bc67-8f2a17a2bfdc")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6deef16e-c7f2-4f62-8302-0d6f066b5cb4")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "99fbb685-7b71-4093-8607-fb73f01e1a49")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c717c8e9-ac22-4948-8d55-382e2d478dfd")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3ada0645-c1ff-4401-b86c-7871f6d1ea10")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7cb9359a-3795-4d4d-a5e4-ad3880512fd3")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51a8c5d9-2895-4c67-872a-e90d56995068")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c1a53191-5a23-4ce2-929a-541a62b9db12")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "59068d8f-9caa-40d4-97e4-581b95dad546")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "ca9f9f28-ca24-4361-9601-d3c8b25ac35a")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "62d617f4-48cc-4367-8685-b189d8a98479")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "7f6c5526-fd80-425e-bcef-faed62a6a35f")
		(at 139.25 69.53)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C19"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "7dc3a8e4-8e38-49d6-8962-212917af8dfe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "de8367b2-7a53-4c99-923d-767968901e63")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "415345cb-edb4-437e-aca8-fe6fc45f2395")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "de8351b2-5835-49db-b95b-fc87e18e7460")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/7b6c0af1-17dc-471c-9e5e-a88867fa8c1e")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "205c1c42-cbda-4653-9dc1-d54416ecdee6")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7c273b88-9486-4ba5-b0c6-9ab5774d77d3")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2a59c42f-2c5b-4976-8b50-20690dd44441")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "42e89308-0eab-4a05-a516-3cb252b8fc36")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "434edfeb-0c89-41d7-b844-76f6f53aee86")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "18b6a660-dddb-4e59-a421-e35c7a1121ea")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb6b9636-d3a2-4412-8e5f-c538cac84466")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0191d584-d370-4cc7-8e2f-72ac273c6961")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "264769b6-5edb-4790-993e-4f94c962a983")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c1b0251-24c7-4f4a-8929-3749ed709ff0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1669a439-79a1-42bf-8336-652d33b88423")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 9 "+5V")
			(pintype "passive")
			(uuid "be16e300-82b7-4d5f-8b3e-d82054bb439a")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "c43f65b5-fb35-437a-9128-24fd11e571a2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "8397cc4e-8b83-4dd8-be98-22df92ed0c67")
		(at 138.45 110.11)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C27"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "4cfb5f5b-a0dc-46ec-b5ba-6bb60d99bea0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4700pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "3f31c405-7543-4ad6-bfd6-6d04994210bb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "11c36978-4ec0-4ff8-a08f-8c83148c3f2d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "32d59c8e-7441-460a-ae5b-561c8e9deac1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/11f7620f-f2d0-48ca-b25e-5e3aa6e598b8")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c73dd94a-38b7-4838-9b60-05b28b76c745")
		)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4206d3ca-3896-4dcb-96b5-0572e2e543bf")
		)
		(fp_line
			(start -1.65 -0.73)
			(end 1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eeeecb43-d805-4450-a9e6-9dec88c53eea")
		)
		(fp_line
			(start -1.65 0.73)
			(end -1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "25f14a47-12be-4025-b8cf-ced9e9271dee")
		)
		(fp_line
			(start 1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "68ab85c1-85e0-4538-8739-9f1d87aba639")
		)
		(fp_line
			(start 1.65 0.73)
			(end -1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a0cfb826-299c-4946-8616-cfed5e93da20")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f55ef575-e2b0-42e1-b79a-fc491d636fcf")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0e9b1bae-7a43-4ea4-bd87-4e7b683b2fb7")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b7eed14e-de0f-4f4a-8d06-45a830b7da76")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da8ffe63-9402-4537-ba00-7d34ab880b72")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "08bc0c1d-9b30-41f2-bcc9-63ed0a4fd656")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "USE_ANT_2")
			(pintype "passive")
			(uuid "57837564-d159-42e7-a98c-a9057a31a3dd")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "a5d74c51-2f4f-49c2-92d3-1d73618f3751")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:CP_Elec_4x5.4"
		(layer "F.Cu")
		(uuid "84200b2e-4231-4e4c-b713-2d7abd16b42d")
		(at 131.1 115.94)
		(descr "SMD capacitor, aluminum electrolytic, Panasonic A5 / Nichicon, 4.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C17"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(uuid "db176fb9-62c6-4d96-a1f6-55d0a05843bf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 3.2 0)
			(layer "F.Fab")
			(uuid "87137056-99a6-489e-9252-1539b5b17acf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b5123134-7d05-47c6-8ee2-88628509ad94")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "74daf4f6-13f7-4aff-864c-6944cfef86fb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "CP_*")
		(path "/f0e06aae-9fe4-4f0a-a301-b4c7a46c9e6a")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -3 -1.56)
			(end -2.5 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f5e9a1e9-e92a-4195-a8fa-3da6d44460cb")
		)
		(fp_line
			(start -2.75 -1.81)
			(end -2.75 -1.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "13e2c83e-6bfa-4e61-acab-53a49e934e06")
		)
		(fp_line
			(start -2.26 -1.195563)
			(end -2.26 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "90a093cc-5061-4c54-b2aa-3f8b9f5538d1")
		)
		(fp_line
			(start -2.26 -1.195563)
			(end -1.195563 -2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d8171d57-af58-42f7-acdc-7883931bb720")
		)
		(fp_line
			(start -2.26 1.195563)
			(end -2.26 1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "38cb302c-98d7-46c5-82f8-86abe44ca9c5")
		)
		(fp_line
			(start -2.26 1.195563)
			(end -1.195563 2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2000ad4b-aa08-4628-b975-897df59bff0b")
		)
		(fp_line
			(start -1.195563 -2.26)
			(end 2.26 -2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7c4d5e1d-b937-435b-aa04-6e73d9dd331a")
		)
		(fp_line
			(start -1.195563 2.26)
			(end 2.26 2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ba94f6a2-c48c-4630-8daf-97aa4347e7c7")
		)
		(fp_line
			(start 2.26 -2.26)
			(end 2.26 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "77e94d73-1f5c-4740-b7c7-2e8e86673a0c")
		)
		(fp_line
			(start 2.26 2.26)
			(end 2.26 1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c5e0b978-ec60-47cb-9861-a3e6a0f38859")
		)
		(fp_line
			(start -3.35 -1.05)
			(end -3.35 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b33bfca5-c7d8-4e8b-90b9-fb0e6ac55a16")
		)
		(fp_line
			(start -3.35 1.05)
			(end -2.4 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dfb6dbd0-cc84-4b50-922b-02534490179c")
		)
		(fp_line
			(start -2.4 -1.25)
			(end -2.4 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6ddb1c72-9200-4d13-a9b0-af0c4bea3e8c")
		)
		(fp_line
			(start -2.4 -1.25)
			(end -1.25 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "989e31ff-23ef-491e-a92f-3c17b07fe6ca")
		)
		(fp_line
			(start -2.4 -1.05)
			(end -3.35 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "932493ff-37d5-4875-ad7e-04a9ab1275d4")
		)
		(fp_line
			(start -2.4 1.05)
			(end -2.4 1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b2249560-1139-45b0-8f17-7ec881490fd1")
		)
		(fp_line
			(start -2.4 1.25)
			(end -1.25 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9951e614-8085-4942-b68c-2e486d87ff97")
		)
		(fp_line
			(start -1.25 -2.4)
			(end 2.4 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0ba2e7ec-9b35-4033-8086-9b24824c2220")
		)
		(fp_line
			(start -1.25 2.4)
			(end 2.4 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fe14b5b8-1a65-4b9a-a954-baf9074bd8af")
		)
		(fp_line
			(start 2.4 -2.4)
			(end 2.4 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3c76bb87-db74-4364-9144-bd6f346ed5e0")
		)
		(fp_line
			(start 2.4 -1.05)
			(end 3.35 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "03c4dedd-4818-4660-853f-485ac3364fd3")
		)
		(fp_line
			(start 2.4 1.05)
			(end 2.4 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ac7cb0c3-e3e4-45f0-9c31-3960a9c8317e")
		)
		(fp_line
			(start 3.35 -1.05)
			(end 3.35 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "591709e0-1cb5-4fe1-8b4e-2b62d495caf6")
		)
		(fp_line
			(start 3.35 1.05)
			(end 2.4 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0e7045f2-eebe-41f2-a534-2675a909a37a")
		)
		(fp_line
			(start -2.15 -1.15)
			(end -2.15 1.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7897cc80-5b2e-4e85-8b5a-dab35800db4d")
		)
		(fp_line
			(start -2.15 -1.15)
			(end -1.15 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c6af45a6-4091-4392-95b5-1c553364ddc4")
		)
		(fp_line
			(start -2.15 1.15)
			(end -1.15 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "290275c3-b479-4478-a9ee-f679219a85a4")
		)
		(fp_line
			(start -1.574773 -1)
			(end -1.174773 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8db5011c-1996-423b-b65a-242cd71ee9d2")
		)
		(fp_line
			(start -1.374773 -1.2)
			(end -1.374773 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37c5363d-102d-49a5-af5c-3b004750d6f9")
		)
		(fp_line
			(start -1.15 -2.15)
			(end 2.15 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "28d8f2db-2f8e-41a2-9f7c-0af26b495461")
		)
		(fp_line
			(start -1.15 2.15)
			(end 2.15 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81cb037c-d712-40f8-a8fc-fe3a56f05c36")
		)
		(fp_line
			(start 2.15 -2.15)
			(end 2.15 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8b83eed0-7768-4d51-b3c0-515d8fc0a938")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "b6c132c3-bcf3-4028-91c7-7e8249d65fb4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "530ec6f5-a321-43cc-bfb8-8f755adce9b5")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.8 0)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 8 "Bat Shunt 1")
			(pintype "passive")
			(uuid "99157857-5047-4f40-9358-45550a9c6fc6")
		)
		(pad "2" smd roundrect
			(at 1.8 0)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 1 "GND")
			(pintype "passive")
			(uuid "238c4cbd-bc2b-4686-81e0-ab3e932655ce")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_4x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "84423baf-4831-4e0d-b784-e015ff6ec2f5")
		(at 115.35 81.18)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R14"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "fd625e0e-d99b-4546-8059-d91fa7cf21fb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "c4770398-2282-4df6-83cf-ff593a7b586d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a8ba2227-fdf8-4d51-8918-51b692bd9157")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5a1b631d-b0fc-4bf1-acf3-d3140d5cb192")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/577adf80-b429-4250-a9e3-dfe0ab9169cc")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "26425bdc-3d14-49ac-bf4c-3c171ed92585")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d60c9538-9f6a-41a8-bd80-ca360471136b")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b11f122e-1d04-4cc1-b40a-4b243313a716")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "77069bd8-7d26-4831-95a4-2546784d23cc")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "de39f80e-3101-4509-b66b-75da5e6c48e8")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "11c51575-a6c7-495a-b3ce-af9a40ca6c20")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "289c66ea-7347-4d33-a559-2dbf810ab42d")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa86de11-b161-480e-894f-07bd47fd195a")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "60019c9e-023a-49fc-9498-17f0ecbf86fa")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2195e240-4279-4a14-b5dd-93ffd406f906")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "391ce281-284f-42c7-9f16-53e0221a3499")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 31 "Net-(D2-A)")
			(pintype "passive")
			(uuid "3df219dc-dcb3-47b1-bfb6-ff0a94fbedb2")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 107 "unconnected-(R14-Pad2)")
			(pintype "passive")
			(uuid "470eeb2c-cc0b-4e3e-9967-96d0c443d6a8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_Push_1P1T_XKB_TS-1187A"
		(layer "F.Cu")
		(uuid "8b6e1249-50b9-44ce-a421-42b4b153d6a0")
		(at 165.09 77.49)
		(descr "SMD Tactile Switch, http://www.helloxkb.com/public/images/pdf/TS-1187A-X-X-X.pdf")
		(tags "SPST Tactile Switch")
		(property "Reference" "SW2"
			(at 0 -3.75 0)
			(layer "F.SilkS")
			(uuid "f413eb6a-644e-4689-a44a-9295bf2174cf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at 0 3.75 0)
			(layer "F.Fab")
			(uuid "e7821490-a42e-4cd9-b754-201609c21c94")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8b2bc345-97ea-4846-bccc-9d6828d1a783")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5719a251-8f10-4ad6-bc22-84ec5e0dab89")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C42420254"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e43d6494-ccfc-476c-bf39-584037c81432")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field6" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c01edd96-e2da-4439-b57c-57d6559f795d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5855783e-235f-4e82-94ba-7534b2d630d7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "38b0972f-6d53-480b-a2de-ca459495dc50")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/7fa70f6d-478c-4413-bca4-f8414a66bc57")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.75 -1)
			(end -2.75 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eb7b3f55-8fcd-478f-993c-6f36a04fd780")
		)
		(fp_line
			(start -1.75 -2.3)
			(end -1.3 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "25f02730-f5c7-47de-be9d-0756220bb40c")
		)
		(fp_line
			(start -1.75 2.3)
			(end -1.3 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "81e8da90-da51-46f9-a4e4-7de1dfaab823")
		)
		(fp_line
			(start -1.3 -2.75)
			(end 1.3 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7fd5a9ee-38c8-4980-a3e5-ea8fee1c87e8")
		)
		(fp_line
			(start -1.3 2.75)
			(end 1.3 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9d910c53-f2a7-45ee-bfdd-7a0aec4d95dc")
		)
		(fp_line
			(start 1.75 -2.3)
			(end 1.3 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "36413fae-3d7e-4006-97a3-ee2681a33989")
		)
		(fp_line
			(start 1.75 2.3)
			(end 1.3 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8ef167e3-cd2c-40ae-a265-706b9bf0ade2")
		)
		(fp_line
			(start 2.75 -1)
			(end 2.75 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9fb18ec1-6d97-4f82-a47f-485e27770195")
		)
		(fp_line
			(start -3.75 -2.8)
			(end 3.75 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "92fe98f0-813c-4cf3-9d9e-7bbb1d56405d")
		)
		(fp_line
			(start -3.75 2.8)
			(end -3.75 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4a9b3393-a35a-47cf-b51f-52621e8ba382")
		)
		(fp_line
			(start 3.75 -2.8)
			(end 3.75 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "631847fb-a308-41e0-829d-d920b210a167")
		)
		(fp_line
			(start 3.75 2.8)
			(end -3.75 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7967dec2-2576-4df5-85f1-80f1dbe524cf")
		)
		(fp_line
			(start -2.9 -2.1)
			(end -2.9 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b3c9f957-776b-4718-bded-74c475806bd4")
		)
		(fp_line
			(start -2.9 2.1)
			(end -2.9 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2cb97742-c6c5-4e96-917b-c4564c1f82a5")
		)
		(fp_line
			(start -2.4 -1.4)
			(end -1.4 -2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "db5cda3f-7fef-4c91-acdc-9cf040f78278")
		)
		(fp_line
			(start -2.4 -1.25)
			(end -2.4 -1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb14630c-df3b-4383-91a0-2cccab94feb4")
		)
		(fp_line
			(start -2.4 1.4)
			(end -2.4 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f42642e1-34aa-4a86-80cf-58ea88cd7e73")
		)
		(fp_line
			(start -1.4 -2.4)
			(end -1.25 -2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "11f504a3-e343-4a5e-b654-68c0d8e8e1ac")
		)
		(fp_line
			(start -1.4 2.4)
			(end -2.4 1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ef9a9c83-8226-4224-bf30-c1d0de8760fd")
		)
		(fp_line
			(start -1.25 2.4)
			(end -1.4 2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d4ef6eb3-89ea-4392-a0aa-018bb0c64e78")
		)
		(fp_line
			(start 1.25 -2.4)
			(end 1.4 -2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54754106-a9b6-471f-bf1c-79b88a65480a")
		)
		(fp_line
			(start 1.4 -2.4)
			(end 2.4 -1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb425387-a234-4b86-81c7-703a0b256d3f")
		)
		(fp_line
			(start 1.4 2.4)
			(end 1.25 2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb8dc681-a635-4211-abc0-f089dbea3ce6")
		)
		(fp_line
			(start 2.4 -1.4)
			(end 2.4 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "facc8304-c496-4acc-93a9-d9419a7e3eab")
		)
		(fp_line
			(start 2.4 1.25)
			(end 2.4 1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e111e10b-7e27-4b95-be7c-dcd6f93861e0")
		)
		(fp_line
			(start 2.4 1.4)
			(end 1.4 2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ea625217-8436-459a-b690-60dc5a57c86d")
		)
		(fp_line
			(start 2.9 -2.1)
			(end 2.9 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2d051750-6458-4d67-ac63-d5517004c191")
		)
		(fp_line
			(start 2.9 2.1)
			(end 2.9 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "79ec9f59-ead6-4fe8-8086-0f4dbcd8d388")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "b0c44dc1-1612-4023-bcc7-345091c6d3ec")
		)
		(fp_poly
			(pts
				(xy -1.7 -2.1) (xy -2.2 -1.6) (xy -3.25 -1.6) (xy -3.25 -2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "7bd2eb79-986a-4f96-b02e-4934a87d0dd2")
		)
		(fp_poly
			(pts
				(xy -1.7 2.1) (xy -2.2 1.6) (xy -3.25 1.6) (xy -3.25 2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "a58ee2f3-0cbd-4c06-8aab-bb10e8a70763")
		)
		(fp_poly
			(pts
				(xy 1.7 -2.1) (xy 2.2 -1.6) (xy 3.25 -1.6) (xy 3.25 -2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "751c2b37-dc35-4219-a0db-8c54287e76c6")
		)
		(fp_poly
			(pts
				(xy 1.7 2.1) (xy 2.2 1.6) (xy 3.25 1.6) (xy 3.25 2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "eba61ba3-3c4a-429f-b72a-f58e3ceafec5")
		)
		(fp_poly
			(pts
				(xy 0.85 -1.85) (xy 1.85 -0.85) (xy 1.85 0.85) (xy 0.85 1.85) (xy -0.85 1.85) (xy -1.85 0.85) (xy -1.85 -0.85)
				(xy -0.85 -1.85)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "8243a36c-9fe1-4866-b787-9fed21fced4a")
		)
		(fp_poly
			(pts
				(xy -1.25 -2.55) (xy 1.25 -2.55) (xy 1.25 -1.975) (xy 1.575 -1.975) (xy 1.975 -1.575) (xy 1.975 -1.25)
				(xy 2.55 -1.25) (xy 2.55 1.25) (xy 1.975 1.25) (xy 1.975 1.575) (xy 1.575 1.975) (xy 1.25 1.975)
				(xy 1.25 2.55) (xy -1.25 2.55) (xy -1.25 1.975) (xy -1.575 1.975) (xy -1.975 1.575) (xy -1.975 1.25)
				(xy -2.55 1.25) (xy -2.55 -1.25) (xy -1.975 -1.25) (xy -1.975 -1.575) (xy -1.575 -1.975) (xy -1.25 -1.975)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "ede6d45a-05ad-4d58-bb10-b064a574fdce")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -3.75 0)
			(layer "F.Fab")
			(uuid "3c43f713-3016-4033-b2f7-f72f7225d56b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -3 -1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(uuid "6c405011-7472-4cfa-b267-d8c95219e031")
		)
		(pad "1" smd rect
			(at 3 -1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(uuid "1f3dd33f-e1ec-46d5-80e4-b6a995ccfc45")
		)
		(pad "2" smd rect
			(at -3 1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "USR_BUTTON")
			(pinfunction "2")
			(pintype "passive")
			(uuid "eb2ce3c4-5b1a-495e-bb28-8d8fc3d1197b")
		)
		(pad "2" smd rect
			(at 3 1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "USR_BUTTON")
			(pinfunction "2")
			(pintype "passive")
			(uuid "df82b95e-dfa3-49e5-9e81-36ad69456d2e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_XKB_TS-1187A.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "F.Cu")
		(uuid "8ca84b92-7de0-4a42-8561-2916bb128ea0")
		(at 158.55 90.35)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q2"
			(at 0 -2.75 0)
			(layer "F.SilkS")
			(uuid "e822526e-922f-4ed0-bd0a-02bb9e4b50b6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PMOS"
			(at 0 2.5 0)
			(layer "F.Fab")
			(uuid "729d5725-aa0f-4f76-93d6-73bb59fc934b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_MOSFETs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "315fdf09-18c8-459a-acb1-77937855c939")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "P-MOSFET transistor, drain/source/gate"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "03e822a0-b58a-49c7-b07a-51cadf0b96b1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "PMOS"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6b91d8af-6833-443f-ba68-55546994d068")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Type" "VDMOS"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "64fa79d7-662d-41f1-8af4-3c5339eb7b41")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=D 2=G 3=S"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "296592c3-b743-42f4-a610-cf0f65009a2d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/16f6fc64-eb5f-4533-a552-1f541d148eb3")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.04 -1.58)
			(end -0.84 -1.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f52c8e68-6348-49f9-868b-aa7e15e3e805")
		)
		(fp_line
			(start -0.04 -1.58)
			(end 0.76 -1.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "32513d0c-42c3-4a6f-93bb-d754e6ae6479")
		)
		(fp_line
			(start 0.76 -1.58)
			(end 0.76 -0.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8401e980-f1ad-4027-a80c-6ca46cb453a7")
		)
		(fp_line
			(start 0.76 1.58)
			(end -0.7 1.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a1d6b02d-5af1-47f3-b84d-a2634b80c002")
		)
		(fp_line
			(start 0.76 1.58)
			(end 0.76 0.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aae2729d-bcdf-4fc9-aec9-01eeb06d4cde")
		)
		(fp_poly
			(pts
				(xy -1.34 -1.61) (xy -1.58 -1.94) (xy -1.1 -1.94) (xy -1.34 -1.61)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "12f8e095-8892-46e8-978b-4dfe2b2b46f2")
		)
		(fp_line
			(start -2.7 -1.75)
			(end 2.7 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c6588774-2893-488d-b777-05750375e58f")
		)
		(fp_line
			(start -2.7 1.75)
			(end -2.7 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7fc5ed91-c5f9-4ce8-a5e5-3c3eab5eb160")
		)
		(fp_line
			(start 2.7 -1.75)
			(end 2.7 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4382dcd6-02ce-40b5-a91d-0818d9558ec1")
		)
		(fp_line
			(start 2.7 1.75)
			(end -2.7 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1edce3ab-0d7e-4a80-8ed1-b4c43be17874")
		)
		(fp_line
			(start -0.7 -0.95)
			(end -0.7 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ec0b6ab-4534-4f4f-b077-13823c2e6bbe")
		)
		(fp_line
			(start -0.7 -0.95)
			(end -0.15 -1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6cb41ba1-5c75-4bf7-ac97-b7e1a713579a")
		)
		(fp_line
			(start -0.7 1.52)
			(end 0.7 1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce11f6e0-1f4b-4b2b-bf01-e6033225dac4")
		)
		(fp_line
			(start -0.15 -1.52)
			(end 0.7 -1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "103f14c5-4f91-4ee0-8a86-ca8c878dea4a")
		)
		(fp_line
			(start 0.7 -1.52)
			(end 0.7 1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e858d52-0062-462c-ad48-f705a3a8a815")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "eb5a573c-0083-46f4-acd0-9343bfbdc2ad")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.075)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5 -0.95)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "Charger Load")
			(pinfunction "D")
			(pintype "passive")
			(uuid "136cb07d-ac4a-44b2-83ec-cdf79dc75560")
		)
		(pad "2" smd roundrect
			(at -1.5 0.95)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(IC2-VG)")
			(pinfunction "G")
			(pintype "input")
			(uuid "5d791c75-6c0b-40c6-9720-1348818aa596")
		)
		(pad "3" smd roundrect
			(at 1.5 0)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(IC2-VCC)")
			(pinfunction "S")
			(pintype "passive")
			(uuid "bcdfbcfd-7f2b-4761-938f-519d5bc2ead1")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "9a65cc58-595e-4826-a8cb-00f07f6d6485")
		(at 144.06 72.54)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C39"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "9c2ae5dc-378c-4223-bd8c-b3db22db0707")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "3a0907af-1e60-4378-99bf-e36438f17f07")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d9823cb2-c776-4b2f-9e29-8b832dac3a18")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "27163074-824b-4460-89fd-d078d48e89af")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a9b40957-bb73-46ad-8d77-e7851f163459")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d25a7958-4698-471c-a14d-56f042a26a49")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1380c129-90dc-4337-a62a-43ca776ad307")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "754e3c34-9b5b-4af8-977c-0c6c7cfc2ae3")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ca288531-f2ae-4783-b8aa-9cf14c8b2bb1")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b5771742-7dcd-4378-9393-afd221917364")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "17b89f23-64de-44fe-8e72-586a47d71ea6")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f81c5542-9087-4fc1-8ae5-5d7b6205580f")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "774e56ad-276f-481c-bb7c-41eeedc77093")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b46f61f-b8ba-4102-a0e7-af52b887d190")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "42974e59-4a9b-4876-a60e-b80151b3a94c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c8acbaa2-9f78-4163-9fc9-9f32025a9caa")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 14 "+4V")
			(pintype "passive")
			(uuid "37995bf3-e403-4691-8ed9-9af585a9ff49")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "9e4d48df-ebff-4692-a121-d755aae702e1")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
		(layer "F.Cu")
		(uuid "9ab1314b-3313-4b5f-843d-5855c4b16520")
		(at 131.75 105.68)
		(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R37"
			(at 0 -2.62 0)
			(layer "F.SilkS")
			(uuid "b7f8f9ae-0741-4ff3-b1bf-6fd7cf33d24d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1"
			(at 0 2.62 0)
			(layer "F.Fab")
			(uuid "c19f4190-2830-418a-a07c-e894588b6f72")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f305b599-17f9-47c1-ae0c-ce7677621ddb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e341b4b3-65e6-4c70-8fd9-46c7101975a7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/ee484925-4472-4702-ae2c-7f9ee40d3d71")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.177064 -1.71)
			(end 2.177064 -1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "868723b0-e680-4819-9281-cb83547d5a63")
		)
		(fp_line
			(start -2.177064 1.71)
			(end 2.177064 1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b0d80c59-7730-4674-b5cc-24ced04c2da2")
		)
		(fp_line
			(start -4 -1.92)
			(end 4 -1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "143a02e6-f880-4565-b516-3ae92346127c")
		)
		(fp_line
			(start -4 1.92)
			(end -4 -1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9f00cfdd-2ada-4a71-bdb4-4445c12d8884")
		)
		(fp_line
			(start 4 -1.92)
			(end 4 1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3af873a5-e96d-472a-9fe1-ca1c10d07a51")
		)
		(fp_line
			(start 4 1.92)
			(end -4 1.92)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b49fc6f2-9489-4229-9aad-78acff7c7c25")
		)
		(fp_line
			(start -3.15 -1.6)
			(end 3.15 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ef77eda4-fd3d-42fe-8319-4422c332c805")
		)
		(fp_line
			(start -3.15 1.6)
			(end -3.15 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d32877fd-d920-4ddb-bb95-7708704f161a")
		)
		(fp_line
			(start 3.15 -1.6)
			(end 3.15 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b0450be1-f86f-4f29-a57e-085e75853f08")
		)
		(fp_line
			(start 3.15 1.6)
			(end -3.15 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "70dfd9e4-55ec-4122-a80f-d8732a4aa21c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "afa7757b-3db3-452d-bfa0-075e8b5a82ba")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -3.05 0)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 94 "Sol Shunt 1")
			(pintype "passive")
			(uuid "221d7304-2442-4ad5-b66d-639cb88705cd")
		)
		(pad "2" smd roundrect
			(at 3.05 0)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 94 "Sol Shunt 1")
			(pintype "passive")
			(uuid "0d6fef56-da13-4c32-9a6e-c2df17ff1ab0")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "9b45ae6f-4a48-478c-aa5c-398ef81c792d")
		(at 124.85 72.33)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R30"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "bd028c69-dc44-47ab-927e-dffad55b8106")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "23.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "e5487741-2966-45a6-baf9-c1acf8d1bffe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "85df5cac-e698-45e3-8214-5400f1aa5c3f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0b72e50c-30b9-496b-86fa-a4ee3f074b5c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/d77e74ad-289f-4869-951b-895aa3e2bfce")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0652b2da-54d6-4216-8ebf-6cc17db15d9d")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7ade4dc0-6b7e-4f26-9dd8-f4a6f6ebe45f")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "91125f57-d0c8-4268-a3dd-b7d8a950f4b5")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6ff2d611-6410-43b5-94ed-6aafa3b8cdb1")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "39edf3b8-2a92-459c-a8f6-1c4850e5c8f3")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "462d3e40-1cb6-45f4-bfb0-fb3879afa983")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c127d2b4-6a3c-4d38-a947-39d7215d4025")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1cdf31ea-6a18-4ae7-a4ed-8e059da16c7b")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2eff8808-d305-42e0-b264-098900e9eca0")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9ea92195-e4c5-4acb-a263-3d0643362095")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1e67ec48-60eb-4397-9f28-7d5bc00334ce")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 87 "VBUS")
			(pintype "passive")
			(uuid "80ff1ad2-1cf4-49fb-a13f-6c47d69b4447")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 117 "Net-(R30-Pad2)")
			(pintype "passive")
			(uuid "7268cdd4-b811-452a-9f02-bddbaf63887d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "9e4573a0-2fa6-4124-8142-185929e5b494")
		(at 120.1 78.23)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R23"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "c4e2fecf-749a-4967-a972-677963454a00")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "51.1k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "7efce5df-a098-436a-ad8a-a9f2dc3122c5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "97813e31-b729-4988-b1e0-f5e61141e17a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5e6663d9-17e5-45fe-acef-21a5e8abda95")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/e451565a-fe1f-4586-a24d-ecc270889779")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "25f11755-5e71-4ecd-a760-dd302c4bb2a8")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e4d88562-cf89-42aa-8781-040eb573ddc8")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0c8aea7b-744a-4297-9a4c-f67a26bb3a5a")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bbc96b47-3606-4c6a-889d-681b5304e2e6")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "92df1771-1b41-4464-a37b-bcccafd5ce83")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "47c2aae7-bdd4-4d41-8ccc-7c96e15d36ae")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ff91f03-e70e-4175-9d56-f2278e22c3ad")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b334ffd7-dd38-41c3-b057-3b694d843105")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be341403-00a5-490b-a7cc-ddab1c011a41")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f2d1c8b5-c686-4e11-8ca6-4b19b69f4e35")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3b017e93-5b12-4da1-a398-be4334ad916d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 112 "unconnected-(R23-Pad1)")
			(pintype "passive")
			(uuid "f2ba98a2-19d7-4d2c-8ac1-2c0d3ef37a9d")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "a88eb1e9-cc76-4b05-846b-bb55c46f9349")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "a00b90af-3ff6-44bb-9fd8-44f45230e0a7")
		(at 110.6 87.08)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "a9c9057b-2e28-4b77-a87d-78c66cbd511a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "9b8da9b4-35e1-448e-8bee-6bb3f1b3bfa4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d71377f3-6cfc-4cee-b977-1c0e33457db0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2e6bf342-ab9a-436d-9a3a-75b8d494f82a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/39b34b28-8ec8-4bb0-a606-ad0e74ec574e")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5a1905da-e585-4911-9283-3581d0eaec7d")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a540fde0-8a85-4b72-be3d-9fc9033ae089")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1da275c6-1c89-4282-aacf-a3076c2f7330")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5af6a7c5-8d3c-49bf-abfa-7c3b85fbefcc")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5da5a97-9620-4be4-9d92-7eb9d86ef10d")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e3764d5a-c543-4df6-8d84-3544c8017a7f")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "39813ed2-6806-4725-ab9a-a0cf6947fe67")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "14c933cf-4041-456a-a392-7d6003845629")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "347d79c8-16b8-497e-bf8a-abc094022cda")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a6973057-2047-445d-94f3-e6b4e1808f91")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b18812ab-8ef2-487f-bcf0-1ef19b1fc51b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 105 "Net-(U1-VFB)")
			(pintype "passive")
			(uuid "bd2f6d54-7aac-4ea7-8b29-d289b98f76c8")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "b98b11cb-7ded-4c4b-a0cb-dc2e17ba431e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "a0e9e2e6-c08b-4088-bb0c-3fc32e29aead")
		(at 142.8 105.09)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C30"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "82d3a35a-5ee4-47c7-8f46-7c4187466a12")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "220pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "fd2b67eb-a8fe-48bf-a4b9-65d3c9f8e061")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d0d3dab8-9ecb-4bae-93a3-92f25f7c9102")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "59410611-865f-4585-b482-675cabbd872a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/94a8d90a-7b4f-41d0-b668-94e38db10a4e")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ba33532c-6a22-475f-adfe-22002fba1289")
		)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e62cebfd-7618-4b4a-a8e3-be012d996b3c")
		)
		(fp_line
			(start -1.65 -0.73)
			(end 1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1e1a3c6b-2668-4afa-ae19-ec1c2139e9c1")
		)
		(fp_line
			(start -1.65 0.73)
			(end -1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "45be1e07-2d07-488b-8905-6d01379fc7aa")
		)
		(fp_line
			(start 1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1cf223a9-6392-4bb6-8120-bc62735301a5")
		)
		(fp_line
			(start 1.65 0.73)
			(end -1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1d0ac82e-141d-493a-a462-4a17b57a5354")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "997463b5-b246-4a64-be3e-43dbcf607d03")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4cc392a4-0428-4cf8-b530-46c90b67f58b")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a6faca7-3a2f-4266-8898-ed68d8424938")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7d40c8fd-6d52-4aea-8d52-25e634402248")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "10dd3e3a-a214-4999-8a22-7cd88a3f9c69")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "3dc46cc5-6394-43ea-ab5c-131d36af7cea")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "4fd4ffbb-3102-4db2-8c39-7819a5d19422")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(uuid "a346fef7-290b-4707-87a8-b8971199051c")
		(at 138.3 118.41)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 -1.998 0)
			(layer "F.SilkS")
			(uuid "6696145e-382d-4242-83ee-3725bd607caa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.Fab")
			(uuid "53ab61b8-ab90-4449-9423-bf2d75a7b60e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8d0e1edb-2cab-4b8f-a176-aedb353aa139")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c1725569-ec1b-4627-9d63-858beeebe279")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/1c94abd4-ca03-4d21-a561-1fcffb32bcaf")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_circle
			(center 0 0)
			(end 0 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "da5f43fc-52f6-40f8-9d47-ffdbf41cccaf")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "472fbe24-87c8-4f23-9c77-522e08de30d6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "5058a2fb-c446-498f-aaf8-5f7e0e4c52ef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 109 "I2C SCL")
			(pinfunction "1")
			(pintype "passive")
			(uuid "ac71fa98-1f23-4cf7-89b9-edf30e53be11")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "a3e6d95f-e5d4-49ed-9f1d-088ffb1631d7")
		(at 142.8 115.13)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C43"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "f5696dd9-b229-4a3f-bfa0-62f868b82a5c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "5deecd4c-3d08-475a-a29a-b4bcc9b45b27")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "36d4f327-9a65-43ac-b714-86d0c7ccd6fe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "40e472a5-7db3-455b-b7e9-7854f64b46a9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/f2039b58-a1b5-4afa-8fcb-c6c3f4f97cfc")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "61bc35af-7df2-4d4f-83e9-6b6f71d1a4f8")
		)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ced9d849-64e6-4c38-ae31-25888fea7d21")
		)
		(fp_line
			(start -1.65 -0.73)
			(end 1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3f16319a-4eab-40b7-9b52-2364678eaf0f")
		)
		(fp_line
			(start -1.65 0.73)
			(end -1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ea917857-8bae-4309-b105-f5cedf9c6a51")
		)
		(fp_line
			(start 1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "24d513d0-123c-4a90-810f-26ca11d0e3c1")
		)
		(fp_line
			(start 1.65 0.73)
			(end -1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eaa7d1b9-5102-4dd8-8989-f43945a03ff2")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b941a18b-858d-44d9-843f-7f914dccdcd2")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00c11aa6-8a05-469f-926f-c13409945cff")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a2edc480-c3bd-47b1-9c8b-f0ec221c8814")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "08adab0f-ac92-42a0-a3ae-1ad5af11f2fd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4c7d283a-7833-446d-b890-fd4bf652591e")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(IC3-TX)")
			(pintype "passive")
			(uuid "9c052c4e-292a-4c3f-9442-2d9d4c2496a6")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(S2-RF1)")
			(pintype "passive")
			(uuid "710cf8b7-8c97-45be-ba68-f22c06f494c0")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "a7c6e786-1e4e-4c95-9b3a-4b5517458f80")
		(at 144.06 66.52)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C37"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "93ce22f7-4651-406e-86d6-73bb5549470d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "b9b3e307-d801-41cf-832d-1da7b4148a8a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8739b85a-509e-4759-938b-6fb4aea66852")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "84f7ed55-0d72-485d-95eb-49fd49843d7d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a40fc250-6817-4fba-989f-dd5bdb7bd3d7")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b7c3295d-9c24-4706-ad9d-25b2b9b6ee86")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7e501e8f-4032-4e72-bf6b-9894c792979b")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "af565ff5-cee9-4574-89a3-db15457692a1")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "897c3fec-c3f0-4aef-b0b0-8041b16f5494")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6050caab-464e-4c88-b409-aacc43b03d73")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0cf89967-94a6-4d40-8522-8828f7f1b939")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5df05587-c5d0-4c43-b8fd-a7e0cba9e381")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ecccf5a8-d7aa-42b7-bcda-5ced332d273d")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8fd4bf16-2e12-4baf-8d5e-8b3424bdcd50")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d24337a8-c521-4e69-9b02-393f68612f91")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c4aa9c41-796d-40b5-ba9c-d93d20146346")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 17 "unconnected-(C37-Pad1)")
			(pintype "passive")
			(uuid "b45facd0-7257-4a6f-b8e7-89aededf3ce7")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "bf7bc580-f5f0-4bfd-b2fd-50eccf02027c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "a7f07841-a8ce-4346-ae88-f64062564eb5")
		(at 110.6 72.33)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "2efad33b-5bc4-496a-b2cc-e2923786d8a7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "6.8k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "bd865eec-e409-4343-b55a-65bb9f9b9d10")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e9f93472-4447-4b7e-ba3e-94ddf9bf9b77")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b874c778-2fdb-4515-99f2-140d6f6b1ac4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/2894f8eb-bc78-4349-846b-395a7a6f5b80")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6189e264-9fe6-45e2-9b00-995f8fb4d5d5")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ba96a22f-90de-4909-81cf-aa2edab79bfd")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "647ed08f-c0bd-4935-942a-b0af421d2209")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cddae788-efb9-442b-8c4b-39ac05b72341")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d6cd8e83-3250-43b3-90a1-915731b9987a")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "33a26924-8d4b-4bad-b146-50202731ab58")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3ff0f594-2aff-4ed5-9e7e-3a027e75d9e8")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ffe765c6-a974-4187-bb1a-bae42394c409")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "661a8698-8f1e-4661-b472-e5a21ce4cd2c")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0d68ba73-ab2a-4751-8f5d-cd254230e28f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "cce54b98-617e-497b-a2bd-375233d85366")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 42 "Net-(IC1-CFG1)")
			(pintype "passive")
			(uuid "86aaf07b-88f6-441a-912b-6e6fbb5d3f84")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "85a033fd-dad1-4e58-b97b-f2c0b50f4922")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "a8b94ee9-6b79-4d15-818f-c69ca0ce4fe8")
		(at 163.235 63.525)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "a992809b-06fb-4d26-a780-331745aa58be")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "d77174ca-3f88-4b0f-b835-f506b7ba76a3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "59c22505-15e8-458b-b976-366fc18a1420")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a482ce00-9c3b-4c3e-8a01-b1e1411da0b2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/2b2b19c4-d737-428d-9c65-e4b12d35ed70")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "76e90c6a-d7c1-4021-9410-9fad319d4046")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad0cb2de-5653-4d01-baa4-cb91e44921e5")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7625eea7-d3a7-445f-8d6d-963fcd0d9f91")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1ad35814-1894-4383-9cde-14f9131e7a5f")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "672a5509-fdaa-4c13-8183-7fc56fdc7a77")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "492ce404-7ac8-44c8-8664-038e6ad91954")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dcbdf3b4-181b-4e99-ba0e-c0c73321300d")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ea061d6-de5d-47fe-9fb9-d8d2b5984ea8")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "041a85ef-0da6-4866-a39b-09cc04573aac")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c674cf4d-9a68-4857-a387-5314b0839c8c")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ee7da9e7-77f2-4f88-8ba2-5e27207f1b81")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e0d41415-00f3-4960-8ed9-a9a6eef62aaa")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "100e8a86-e395-4613-a0a0-8d9d77d95bb2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 29 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "4a5eb765-41c5-4348-92da-df1b6cbbd24c")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 30 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "9fb65244-5928-4778-89e1-8a857749bce8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "a9680c3a-200b-4bad-9523-94fb432c7cde")
		(at 120.1 81.18)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R24"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "f9502a4a-0c0d-4c71-828c-7e72535a2903")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "67aaf9f0-156b-46eb-8061-1e867869a23d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6c3866bd-9711-4840-95cf-bffad3f00e17")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1557d147-f433-44a0-a2e4-4347de9fd355")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/33a0d09e-9c82-4b62-a61b-c4004b740d49")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "164b512c-7596-4943-9e34-6192f9aef1dd")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "27c8ad98-79d7-48af-8dce-c41039024224")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2ef5e199-a74a-430b-b6b8-dcc52922ea6a")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5356595-57c8-49c0-90f5-dbdbb4f19359")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e7f279c-8c04-4be7-a395-6d2f4691fda5")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "973aa517-d428-4840-a97e-9bce508e3234")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f3fde7b9-1562-4803-8697-5c789ee74ab5")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d733bda3-4f36-47c9-8ed9-b77060b2612a")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1291092-9efe-428e-94ce-e3df31e46741")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7abf2823-37b4-4658-a578-1fbeca338a0c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "dae5368c-a63b-4ce0-81ba-40d1b6e30fb6")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "414b29d7-4723-42f6-83c6-5af4d1a617a2")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 113 "USR_BUTTON")
			(pintype "passive")
			(uuid "26636d48-e2d6-4703-85f8-f2b8fa7ef2fb")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_SXN_SMDRI124"
		(layer "F.Cu")
		(uuid "ad3cdd2c-ec21-4b59-8c6b-eefafc39f76e")
		(at 153.64 68.975)
		(descr "Inductor, SXN, SMDRI124, 12.3x12.3x4.5mm, (https://www.sxndz.com/upload/202108/16/202108161607454319.pdf), generated with kicad-footprint-generator gen_inductor.py")
		(tags "Inductor sxn smdri")
		(property "Reference" "L1"
			(at 0 -7.15 0)
			(layer "F.SilkS")
			(uuid "e3ca2fd8-25db-4c49-8808-06adb7d25b31")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2.2uH"
			(at 0 7.15 0)
			(layer "F.Fab")
			(uuid "e9a07c0e-b133-493c-850d-0faa62646563")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0938b627-cf08-44eb-ac44-804e81b94645")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8acf9908-0e54-4496-8019-89304b33d5c6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C2929497"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "157884c7-aa63-4423-a43f-b92ed175d100")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/82f13ee3-6bfb-48e6-a947-d56420d89774")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -6.41 -6.41)
			(end -6.41 -2.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4040e1f2-9fa8-4239-9f1b-8dcec14adfff")
		)
		(fp_line
			(start -6.41 -6.41)
			(end 6.41 -6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "470e111c-6168-4590-815a-6f9c9a1b15fb")
		)
		(fp_line
			(start -6.41 6.41)
			(end -6.41 2.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6a81994c-0bf8-4489-bd72-c8752047fa8e")
		)
		(fp_line
			(start -6.41 6.41)
			(end 6.41 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2f56e75e-9a07-4b63-91eb-b4ff1441b437")
		)
		(fp_line
			(start 6.41 -6.41)
			(end 6.41 -2.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cd2c88c5-7e94-4e25-a457-600075212e41")
		)
		(fp_line
			(start 6.41 6.41)
			(end 6.41 2.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c21a905c-af48-4c26-b539-1162a945e70e")
		)
		(fp_line
			(start -6.65 -6.4)
			(end -6.65 6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b99acd1-bda9-4158-9908-5d506c7c4328")
		)
		(fp_line
			(start -6.65 6.4)
			(end 6.65 6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b64ad9d2-0c90-4ce4-9b45-943179c4a054")
		)
		(fp_line
			(start 6.65 -6.4)
			(end -6.65 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4baf6834-d94a-4d76-8b9f-6cd262525402")
		)
		(fp_line
			(start 6.65 6.4)
			(end 6.65 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "37e29c7d-59cb-4ef0-812d-4df7875dd753")
		)
		(fp_line
			(start -6.15 -6.15)
			(end -6.15 6.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b38044e3-9c25-444d-934b-372ca89626f8")
		)
		(fp_line
			(start -6.15 6.15)
			(end 6.15 6.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f20c8384-6fdf-4e04-baf1-87e4afa2d6de")
		)
		(fp_line
			(start 6.15 -6.15)
			(end -6.15 -6.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0abd57c5-5101-4479-a511-6c91d3374196")
		)
		(fp_line
			(start 6.15 6.15)
			(end 6.15 -6.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0e7daa63-8d87-4c32-90a0-7e02c68ffb89")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9e050b76-6bc7-4fbc-bb98-6bc2d7342b2e")
			(effects
				(font
					(size 0.966667 0.966667)
					(thickness 0.145)
				)
			)
		)
		(pad "1" smd roundrect
			(at -4.95 0)
			(size 2.9 5.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.086207)
			(net 7 "Net-(U1-SW)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "d42b2ecc-74d9-4378-9e28-97756239c26c")
		)
		(pad "2" smd roundrect
			(at 4.95 0)
			(size 2.9 5.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.086207)
			(net 3 "VDD_NRF")
			(pinfunction "2")
			(pintype "passive")
			(uuid "120c76b9-d06e-4f31-ac1e-6848f97af601")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_SXN_SMDRI124.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic:SKY6531321"
		(layer "F.Cu")
		(uuid "af9dd744-f5a5-4092-b227-6ea7c3cd7079")
		(at 151.125 87.275)
		(descr "SKY65313-21-5")
		(tags "Integrated Circuit")
		(property "Reference" "IC3"
			(at -0.3 0 0)
			(layer "F.SilkS")
			(uuid "7124c0df-e3d3-4535-ae64-0848f46d461d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "SKY65313-21"
			(at -0.3 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "cb2d959f-a930-4347-a997-8739443baba8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/1/SKY65313-21.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "902d26f2-ac19-498b-9432-777bc8446a68")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "RF Front End 900MHz TX/RX FEM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "381f214b-e867-4090-9174-e97674a18bc6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "0.9"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "98c5dd48-f191-4b5c-9a68-b38b5392d195")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "Skyworks"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4824d591-d415-4d07-9cd4-e83db6e7fed4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "SKY65313-21"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c8b6da66-3138-40f5-8166-b16a0d3ce142")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" "873-SKY65313-21"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "49393eb8-9963-45cf-9c0b-7e59ee6214a7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Skyworks-Solutions-Inc/SKY65313-21?qs=VxEzYtM1ylfKtczVdpm%252B%252BA%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1e9172c0-94dd-4b65-9796-309d46b0d362")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d1ddb8fd-6f76-45b7-95a0-65bee8efabd3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c96beb27-f468-4b94-866c-2fe9bfb9ea94")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C5144140"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b94491c9-79cb-4ea2-b0c7-3bf0b5b5e580")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5237f824-00b0-49b3-8cca-898eec5a5c39")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "14abad7e-2e29-4584-906c-dea40a23442d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/d5ea5d59-56b0-43bd-8397-a41f8049e541")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.65 -2.8)
			(end -3.65 -2.8)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9d5db31a-39cf-4a95-99ae-d86df30aad41")
		)
		(fp_line
			(start -3.65 -2.6)
			(end -3.65 -2.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6095e8e6-d0f0-4f7e-ad13-729eccee93ad")
		)
		(fp_arc
			(start -3.65 -2.8)
			(mid -3.55 -2.7)
			(end -3.65 -2.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3b8a1c4-85aa-4f56-a459-f0add2b179dc")
		)
		(fp_arc
			(start -3.65 -2.6)
			(mid -3.75 -2.7)
			(end -3.65 -2.8)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dce8bd78-1e77-4157-aab7-a5539b593af0")
		)
		(fp_line
			(start -4.25 -3.65)
			(end 3.65 -3.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6428b0ce-f42d-459a-97e9-96e74ca7d236")
		)
		(fp_line
			(start -4.25 3.65)
			(end -4.25 -3.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0ff5419d-b26c-454e-9470-f7e32f04baef")
		)
		(fp_line
			(start 3.65 -3.65)
			(end 3.65 3.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "94cb5dec-97fb-4921-abbb-89628e2199bf")
		)
		(fp_line
			(start 3.65 3.65)
			(end -4.25 3.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ce3d0e9-61b9-4edb-b105-dc5c4ab2e9bb")
		)
		(fp_line
			(start -3 -3)
			(end 3 -3)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "caa28022-370f-4089-afae-a7ce47aba15a")
		)
		(fp_line
			(start -3 3)
			(end -3 -3)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "567c7193-0e21-4a82-808a-af1f1580cbe2")
		)
		(fp_line
			(start 3 -3)
			(end 3 3)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c422ab5d-7c21-4802-9e83-2afa0745041f")
		)
		(fp_line
			(start 3 3)
			(end -3 3)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63188f22-d695-423c-be10-0f10eed34a2f")
		)
		(fp_text user "${REFERENCE}"
			(at -0.3 0 0)
			(layer "F.Fab")
			(uuid "34f9dbdb-157e-4350-83e2-dc28845b48d6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -2.75 -2.775 90)
			(size 0.75 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_1")
			(pintype "passive")
			(uuid "aa62af15-a09d-4a97-a2aa-deef76d268ca")
		)
		(pad "2" smd rect
			(at -2.75 -1.813 90)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "RADIO TX")
			(pinfunction "CTL1")
			(pintype "passive")
			(uuid "2f1531e1-6f07-4df3-809a-99482e5c3ce9")
		)
		(pad "3" smd rect
			(at -2.75 -1.088 90)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "RADIO C1")
			(pinfunction "CTL2")
			(pintype "passive")
			(uuid "157c76f5-ef50-4a20-9b7c-05c77233bce9")
		)
		(pad "4" smd rect
			(at -2.75 -0.363 90)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "RADIO C2")
			(pinfunction "CTL3")
			(pintype "passive")
			(uuid "d76d365f-35d2-4d29-897e-0aa0506de374")
		)
		(pad "5" smd rect
			(at -2.75 0.362 90)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "VPC")
			(pintype "passive")
			(uuid "4ae30231-f85a-4544-a530-2e61ccf6d08b")
		)
		(pad "6" smd rect
			(at -2.75 1.088 90)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_2")
			(pintype "passive")
			(uuid "e1b5746f-62ba-452f-9408-10d9d8743e94")
		)
		(pad "7" smd rect
			(at -2.75 1.813 90)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(IC3-ANT)")
			(pinfunction "ANT")
			(pintype "passive")
			(uuid "34e46029-71d8-42c2-8c45-7a2c07cdbbbd")
		)
		(pad "8" smd rect
			(at -2.75 2.775 90)
			(size 0.75 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_3")
			(pintype "passive")
			(uuid "5928196c-8935-4eb2-806a-4a41deda8399")
		)
		(pad "9" smd rect
			(at -1.813 2.75)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_4")
			(pintype "passive")
			(uuid "0c0db7e5-68f2-45e5-b49c-3330a7d4876b")
		)
		(pad "10" smd rect
			(at -1.088 2.75)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(IC3-RX1)")
			(pinfunction "RX1")
			(pintype "passive")
			(uuid "b5e38524-3aa0-44b9-bf1a-b3629ab0323e")
		)
		(pad "11" smd rect
			(at -0.363 2.75)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_5")
			(pintype "passive")
			(uuid "1426173a-007c-4eb0-a152-6fcb480b91db")
		)
		(pad "12" smd rect
			(at 0.363 2.75)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_6")
			(pintype "passive")
			(uuid "e58af7eb-3eaa-4234-971d-c6642281802b")
		)
		(pad "13" smd rect
			(at 1.088 2.75)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(IC3-RX1)")
			(pinfunction "RX2")
			(pintype "passive")
			(uuid "8a45a835-bd10-4129-b299-d9bc18e581b1")
		)
		(pad "14" smd rect
			(at 1.812 2.75)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_7")
			(pintype "passive")
			(uuid "83d948f2-6712-4135-9537-01b4cf316761")
		)
		(pad "15" smd rect
			(at 2.75 2.775 90)
			(size 0.75 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_8")
			(pintype "passive")
			(uuid "44dc73a2-0166-48d9-bb85-d649a0d4bf33")
		)
		(pad "16" smd rect
			(at 2.75 1.813 90)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "VDD1")
			(pintype "passive")
			(uuid "01745425-3cdd-4eeb-bc6d-12a206fc2a2c")
		)
		(pad "17" smd rect
			(at 2.75 1.088 90)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "VCC_RX")
			(pintype "passive")
			(uuid "c9707787-e34e-4ecd-9b5b-e2029790a344")
		)
		(pad "18" smd rect
			(at 2.75 0.362 90)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(IC3-RX3)")
			(pinfunction "RX3")
			(pintype "passive")
			(uuid "7e4ba017-553c-49f1-b591-a7a48b5bbbc0")
		)
		(pad "19" smd rect
			(at 2.75 -0.363 90)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_9")
			(pintype "passive")
			(uuid "cc2b1a32-a150-44c5-be1e-55d961605cbb")
		)
		(pad "20" smd rect
			(at 2.75 -1.088 90)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(IC3-TX)")
			(pinfunction "TX")
			(pintype "passive")
			(uuid "e6a714c7-d0fa-4fe4-b8f2-fe4a75096c75")
		)
		(pad "21" smd rect
			(at 2.75 -1.813 90)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_10")
			(pintype "passive")
			(uuid "4bb42607-2b8e-4d4d-8c0f-42b8f6c1981b")
		)
		(pad "22" smd rect
			(at 2.75 -2.775 90)
			(size 0.75 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_11")
			(pintype "passive")
			(uuid "8bd5e001-6e1f-4130-9963-06bf10eefdc5")
		)
		(pad "23" smd rect
			(at 1.812 -2.75)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "USE_ANT_2")
			(pinfunction "VDD2")
			(pintype "passive")
			(uuid "40d255ec-bebd-4d54-9daa-21c240907bd8")
		)
		(pad "24" smd rect
			(at 1.088 -2.75)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "USE_ANT_2")
			(pinfunction "VCC_TX1")
			(pintype "passive")
			(uuid "45d810ce-3c04-4061-8a1a-61a66aaa52e0")
		)
		(pad "25" smd rect
			(at 0.363 -2.75)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "USE_ANT_2")
			(pinfunction "VCC_TX2")
			(pintype "passive")
			(uuid "3d28079d-a174-44ed-9d16-4f9ec00e0eb3")
		)
		(pad "26" smd rect
			(at -0.363 -2.75)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "USE_ANT_2")
			(pinfunction "VCC_TX3")
			(pintype "passive")
			(uuid "1eff239d-f23f-4770-9109-7dd401c75e22")
		)
		(pad "27" smd rect
			(at -1.088 -2.75)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_12")
			(pintype "passive")
			(uuid "b8440aae-d541-4a1a-9884-29c7800096a9")
		)
		(pad "28" smd rect
			(at -1.813 -2.75)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_13")
			(pintype "passive")
			(uuid "57498f76-3bfe-4145-8368-5841e80be293")
		)
		(pad "29" smd rect
			(at -1.502 -1.502 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_14")
			(pintype "passive")
			(uuid "68c1e6e0-a51c-470e-9bd8-bd1dfd8b7056")
		)
		(pad "30" smd rect
			(at -1.502 -0.501 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_15")
			(pintype "passive")
			(uuid "bd312808-c4f3-4a4a-afc8-2978c660be98")
		)
		(pad "31" smd rect
			(at -1.502 0.501 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_16")
			(pintype "passive")
			(uuid "effac4fe-467d-4c87-a412-ec377c721996")
		)
		(pad "32" smd rect
			(at -1.502 1.502 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_17")
			(pintype "passive")
			(uuid "b7132bf2-f318-49ce-9cff-fabf6ef58721")
		)
		(pad "33" smd rect
			(at -0.501 1.502 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_18")
			(pintype "passive")
			(uuid "839fcc5e-7aa2-4fca-a754-7185a13e729a")
		)
		(pad "34" smd rect
			(at 0.501 1.502 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_19")
			(pintype "passive")
			(uuid "77bb69d7-8654-4a16-acbb-85a1933e69d5")
		)
		(pad "35" smd rect
			(at 1.501 1.502 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_20")
			(pintype "passive")
			(uuid "7863d163-2c45-4132-853a-4159c22227d1")
		)
		(pad "36" smd rect
			(at 1.501 0.501 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_21")
			(pintype "passive")
			(uuid "dd828718-7fe1-417f-a4f0-35f7997060e0")
		)
		(pad "37" smd rect
			(at 1.501 -0.501 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_22")
			(pintype "passive")
			(uuid "9dec448e-7563-4c98-ad94-cf0764d87537")
		)
		(pad "38" smd rect
			(at 1.501 -1.502 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_23")
			(pintype "passive")
			(uuid "75980ea0-cd73-4126-b538-a799c17c9442")
		)
		(pad "39" smd rect
			(at 0.501 -1.502 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_24")
			(pintype "passive")
			(uuid "1cf1d489-ee5b-40a4-af95-6d4590311ddb")
		)
		(pad "40" smd rect
			(at -0.501 -1.502 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_25")
			(pintype "passive")
			(uuid "5688d6ba-e723-4a36-8199-8a95b2ec8987")
		)
		(pad "41" smd rect
			(at -0.501 -0.501 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_26")
			(pintype "passive")
			(uuid "5e0dd7eb-f4f6-4015-9e17-e36a5d2a9c72")
		)
		(pad "42" smd rect
			(at -0.501 0.502 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_27")
			(pintype "passive")
			(uuid "33031747-ffd0-4831-965e-bc16340a96f3")
		)
		(pad "43" smd rect
			(at 0.501 0.501 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_28")
			(pintype "passive")
			(uuid "02b6c77d-71c7-437f-b66f-cdacbfe19faa")
		)
		(pad "44" smd rect
			(at 0.501 -0.501 90)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_29")
			(pintype "passive")
			(uuid "feda77cb-a8e3-4616-93ae-68b5630edff0")
		)
		(embedded_fonts no)
		(model "SKY65313-21.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "b06044fb-841b-4265-b478-fd1ee24d6d6a")
		(at 115.35 66.43)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "30a5e40f-6a4c-4129-b951-720867be583d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "37382bf9-264a-484d-b253-7e544f7e4fb4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0c437ee6-a6b9-4317-8499-80b72d8d4df9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bf6c002e-50f5-41b7-a0f3-c76deeff6c18")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/72dcaf5d-1e1b-4e8b-9e7a-ebbcad20dd87")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dfe4e03c-578f-4c55-bdf4-3c3071666c77")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3ee96284-2dfa-4016-bc85-95348be13490")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3c5c6461-f3d6-44fe-9718-1030f99cb7b9")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1cdc1047-c5c1-4c60-9d8d-ca3b3f059bd4")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0a1ab344-a746-4250-b455-de616aec15d4")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aaeafb60-a6de-4b6c-8dcc-eff94f350746")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "24b7bc3e-bb3b-4660-a7f8-85ff53e203b6")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7defebca-01a9-4263-aed1-3a4b74b67913")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d12e2e58-1c98-4687-bd7e-b43aa3ba472c")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37ba7513-bac9-41bc-b64c-d6d581a60197")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "05e4fd93-5d14-4741-aece-78cabeec4db0")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 33 "Net-(D3-A)")
			(pintype "passive")
			(uuid "d64a7fdc-a314-4625-9177-bebc4916dfc4")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 12 "Net-(IC2-VCC)")
			(pintype "passive")
			(uuid "40deb1c0-3a83-4886-8b21-5b74c03ec1a4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(uuid "b4850398-96f6-48d8-a305-c2303745409a")
		(at 142.35 118.41)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 -1.998 0)
			(layer "F.SilkS")
			(uuid "2f62bf10-961e-426f-b856-6944f1e7d5e7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.Fab")
			(uuid "cd1f4ed7-9bbb-4798-a54a-e452b1388d54")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "126e04c6-22f7-45d6-816d-0a53df2915c0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "80600bea-58d6-4b99-919b-030b5d341c79")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/8e878ae7-d51a-44bf-8a99-b75c101c2f5c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_circle
			(center 0 0)
			(end 0 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "2fb79b85-a926-477d-831a-312a0f8b9240")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "54d60aac-b274-439c-bd42-7f5684924bc7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "342ce39f-7f6f-475b-86c3-b7f00c5fe0e7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 87 "VBUS")
			(pinfunction "1")
			(pintype "passive")
			(uuid "34eed3b8-ac7a-45e1-abf7-c21ec25a55ea")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:CP_Elec_4x5.4"
		(layer "F.Cu")
		(uuid "b715bf96-5c89-43df-ba93-8f505bf17783")
		(at 131.1 121.79)
		(descr "SMD capacitor, aluminum electrolytic, Panasonic A5 / Nichicon, 4.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C24"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(uuid "c0be551b-73f4-4c27-bdcf-eb33b4c2dff8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 3.2 0)
			(layer "F.Fab")
			(uuid "f3eebd24-881d-41ad-9ae8-d677efbf6f30")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d8c26871-ed72-4388-9674-41b34d802dfe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7a02f0c2-53a8-468a-bfc9-e21cf7dcb0d4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "CP_*")
		(path "/d30c7ca6-b507-41b1-bc16-e705b5af3ff1")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -3 -1.56)
			(end -2.5 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0d665eca-5539-4444-b224-cfd1abe624ca")
		)
		(fp_line
			(start -2.75 -1.81)
			(end -2.75 -1.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0ca66fdc-191a-4ead-b0ab-f03d678fa67f")
		)
		(fp_line
			(start -2.26 -1.195563)
			(end -2.26 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f846e976-1e5e-4eec-8e32-5c7a57ea1d46")
		)
		(fp_line
			(start -2.26 -1.195563)
			(end -1.195563 -2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9dca84d4-3317-4ad2-9cd5-d19836da0b3f")
		)
		(fp_line
			(start -2.26 1.195563)
			(end -2.26 1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "56db371c-5fba-43ed-bb04-a96c7ecd9c27")
		)
		(fp_line
			(start -2.26 1.195563)
			(end -1.195563 2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4e8d61f9-6492-4b33-bbe2-879524c18da4")
		)
		(fp_line
			(start -1.195563 -2.26)
			(end 2.26 -2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9671dba6-21e6-4e25-8015-b45b516774a0")
		)
		(fp_line
			(start -1.195563 2.26)
			(end 2.26 2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "99ec0e43-67c5-45a4-8223-c862e93eae65")
		)
		(fp_line
			(start 2.26 -2.26)
			(end 2.26 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c03579c0-08c6-4703-89bc-e2f2c8865aeb")
		)
		(fp_line
			(start 2.26 2.26)
			(end 2.26 1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3e5efad5-ce18-4bd1-abcd-88e8ecc4ace7")
		)
		(fp_line
			(start -3.35 -1.05)
			(end -3.35 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c4ba0cfc-35a0-4407-b6c5-70e26d67df90")
		)
		(fp_line
			(start -3.35 1.05)
			(end -2.4 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f6cce6f0-8bf4-40d2-a86c-3a4a7bf059e9")
		)
		(fp_line
			(start -2.4 -1.25)
			(end -2.4 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9f0a940f-ec11-4d3f-ba0c-410f10bd0668")
		)
		(fp_line
			(start -2.4 -1.25)
			(end -1.25 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f07ba669-d153-4b56-9c81-d86ab5d9d02a")
		)
		(fp_line
			(start -2.4 -1.05)
			(end -3.35 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c69663ed-f6aa-48f2-8cd1-2ceddbb2b18c")
		)
		(fp_line
			(start -2.4 1.05)
			(end -2.4 1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "173df4e4-b28b-4189-a888-1350595e6954")
		)
		(fp_line
			(start -2.4 1.25)
			(end -1.25 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fc9d2ff9-9d81-445c-b818-02c871ffac06")
		)
		(fp_line
			(start -1.25 -2.4)
			(end 2.4 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6ff34b88-145f-4239-813e-d1e2112aefbe")
		)
		(fp_line
			(start -1.25 2.4)
			(end 2.4 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3861bf2d-d3ee-4185-8e95-13b7f7900413")
		)
		(fp_line
			(start 2.4 -2.4)
			(end 2.4 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f62d580-cebc-4f90-8ac2-7701611313f2")
		)
		(fp_line
			(start 2.4 -1.05)
			(end 3.35 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "594b5ea2-9bc1-4f21-acb2-aeff067a93c5")
		)
		(fp_line
			(start 2.4 1.05)
			(end 2.4 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b643c914-0eea-4ed2-a13c-84fb34d99668")
		)
		(fp_line
			(start 3.35 -1.05)
			(end 3.35 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "90535070-0136-44f5-a2a6-60e898a663ca")
		)
		(fp_line
			(start 3.35 1.05)
			(end 2.4 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1491bc8a-b6dc-40df-8e2f-329f4379f424")
		)
		(fp_line
			(start -2.15 -1.15)
			(end -2.15 1.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "74ee2966-69d9-4712-8ed8-6fd4a5c5d80d")
		)
		(fp_line
			(start -2.15 -1.15)
			(end -1.15 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "92a0b2ce-8616-4a12-a590-7b331b535f93")
		)
		(fp_line
			(start -2.15 1.15)
			(end -1.15 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "507a5c5c-c3e9-48de-b1d2-c05ff31adbdb")
		)
		(fp_line
			(start -1.574773 -1)
			(end -1.174773 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "569ec186-f6e9-4531-8640-32373101d844")
		)
		(fp_line
			(start -1.374773 -1.2)
			(end -1.374773 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4900551f-a10c-48f5-a04a-6101b0444a32")
		)
		(fp_line
			(start -1.15 -2.15)
			(end 2.15 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "52e48486-07c7-47da-9921-256a15445830")
		)
		(fp_line
			(start -1.15 2.15)
			(end 2.15 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87be1264-4568-466f-8233-427df38c2f4b")
		)
		(fp_line
			(start 2.15 -2.15)
			(end 2.15 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d141d7be-ba4d-4cf1-81fd-508d31504c2b")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "ff060107-92a7-445d-aeee-2b4c5d0669fd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "81a74ca0-6d94-4d1d-b9a6-c8e71854bd78")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.8 0)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 12 "Net-(IC2-VCC)")
			(pintype "passive")
			(uuid "93b7a3cb-d3a6-4e17-9f9b-5ebc7bfa3c89")
		)
		(pad "2" smd roundrect
			(at 1.8 0)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 11 "Net-(IC2-VG)")
			(pintype "passive")
			(uuid "5b18d2f6-224f-4edb-9c04-2f55a7974339")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_4x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "b868c0f7-2027-4677-b7f0-7fb7b78e1592")
		(at 124.85 66.43)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R28"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "63003a2c-1a0d-4213-88e4-60e766a9c454")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "23.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "2b113dc7-7d97-4544-9507-edd63650b741")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "046d8a1f-1846-47ad-a269-ef974935fc9f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d51cdda1-958b-475e-b6ff-71eb09660062")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/9101b906-2ec4-4e50-9448-21fcf78df54d")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7292d949-a085-401a-8a77-882858fee932")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e61060cc-b60d-4db7-9918-6f460f910a7c")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1f50a180-6584-4bf9-bc7e-663f76808beb")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7c83266c-b011-4eeb-85f3-f9ecf2707bdc")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "89a8f2bc-ef8b-419f-bf51-dc1e629690f2")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0e16651b-81a4-4f08-a4b8-297955595e29")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "18d6f3fb-dfe3-4362-a00a-a09edfadc274")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "976b4f11-471e-4e03-bd28-2b1ce4f1b1e6")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a55bc796-c82b-4c07-abb6-d8dd1ea47de4")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4882bfeb-aa5a-4fc3-9bef-13e3a8204d7e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "895e48fb-a534-45f2-af8f-af32d5a949f6")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 87 "VBUS")
			(pintype "passive")
			(uuid "c92915b5-e88a-47b1-8c01-991deded76c1")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 116 "Net-(R28-Pad2)")
			(pintype "passive")
			(uuid "f7954e0d-7d9d-4d0b-8956-2ded644dc38d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "bb99c9dd-519e-4ea0-8180-c4fd60fe90c7")
		(at 129.63 75.55)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "e744d6e5-b2ce-4afc-9177-417562c6c962")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "0ebe2868-4e0c-4b38-a404-67b5243a1330")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cfe02fb0-460f-4a87-8237-1fa676b962a3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "67fa042d-9910-46aa-88fa-4e6735ec0b03")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/fcf0e2d3-1699-4445-9fcb-6107a28dfda8")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "07f66911-51b6-4d35-b150-f20458de080c")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9ae348f4-be39-49f3-9903-b3750b620d84")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "49ccd87b-430f-4adb-b351-4d22781ce869")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "44ec2afa-163c-4865-9f7a-3a4073f99510")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "326ba3ba-5ba8-4267-a60c-2757d3802f22")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c1102756-0284-4b74-920a-1a6589cd4b3f")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da91771f-d569-466e-a349-bc89a61092f5")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "31936965-5dd5-4f2c-adce-4ba05efa61d1")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "637a04a2-b898-483c-b77f-8305412e2bac")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc418abf-d235-4ef3-b09e-6e1d9666eeaa")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f047f499-e079-4a33-a0f5-e2e23b069a1c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "51fdb209-ef15-4136-9e1a-dabd3606ff13")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "ed44d139-cb59-4975-8339-cd24494cbbc8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "bbfc9cb7-a036-4c75-89e0-30899db5e04c")
		(at 129.63 69.53)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "caa20bce-462d-470c-9ff4-174440c8714a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "08eaed12-49ea-4044-8657-fd86bd28a749")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2de1cb0b-32d7-4d71-90bf-69f3db3e409d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c6949d36-e882-4dc8-951a-832ffbaed718")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/2aba3709-1593-4aeb-b114-e94971cd0b98")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "48373dc9-e121-48f7-9cda-c483c3ce7297")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e7ded28-1785-468c-91bd-5dc46e41e26a")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e849b75c-9848-49b4-b51c-04e0a8215c0d")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bf9fd215-27cc-458e-8bc9-f345a2bfaee3")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e824d71a-9570-4302-ad43-2cd9d4c4fa65")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3e98fc65-6404-4387-ae34-c4d46217fc19")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4de10de5-f52a-4c72-8d3e-d87c88285b92")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "090f5085-81f7-4d9d-a4a5-ebd28b5c0856")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b833f019-9b07-4539-9da2-2c6cdaaee3dc")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f94f3fb1-02e7-4293-a0a0-ba67e538177e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "69c2347c-1d8d-4d50-a699-93a610cee09d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "df55347c-f91f-49ed-ba92-a47109dfc9d0")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "503b54ab-cf65-4f21-8507-b1653b2e6da2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "c099dea4-fbc6-4913-b4ca-b36f335e2f9f")
		(at 144.06 63.51)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C35"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "7df554d1-742f-49ca-b39b-97b30627a8b6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "d51677e2-ced5-45b7-a31d-bfec322403b3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ebdd7d16-4577-42ae-8847-e912b152777d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2f162a1f-2f9b-40b2-8de5-6c1e9351e379")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/cf836a19-7ab3-4a3d-8aeb-41aad7a6907c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "59962aab-94e5-40f2-bd17-1351d07b586a")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "382854b2-1613-4708-a6d9-49be4312f367")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "68f41a97-5948-46ab-83cc-93301eac1234")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "43817d05-576f-4e9c-8c77-3e9242086d73")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a9d0d33d-d9ff-43c8-82b2-efd2b57b50d0")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "63ff4a45-05ff-4be9-b872-9dec45037358")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4428eed2-b3a5-46fe-b441-d990338ec93d")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8b385f5a-0d91-495d-8d15-9dd625190553")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "291954c3-df0f-4baf-973a-d0c5d0ae2bd1")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "313a4eff-0f52-4669-9651-6b9b9bb777db")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4100758b-0847-48cb-8fce-5b121505e0ee")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 14 "+4V")
			(pintype "passive")
			(uuid "52cdd796-4661-4d16-b6df-7da1e1764c6d")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "ae474682-c50e-4656-8fae-26e7fb2a8472")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "c3e2e79f-9d15-4acc-ba6b-5795cc77932a")
		(at 134.44 72.54)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C11"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "19b0ebc2-0d92-49ec-a61c-bda7392bae09")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "8ec965ee-e5a3-402f-a58d-20f3ec4b273e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e4afeb05-8daf-4fda-81c7-80031672be72")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9bf3a5e2-776b-4a05-994a-0da3cc41577c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/2aee7a45-9f20-4a9d-9840-e7711dd4db71")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3878622f-0e3b-4ea5-9846-256875c3143b")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f120e5c0-d536-4702-a38c-7b02dd0d3a89")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f3ae766f-af87-4d0e-be7f-957ed374642c")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3755c9f-7a0e-4752-9f85-c1fd2b10fb0c")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7558d2f2-3d8d-4485-b160-813ed8fd334d")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f7fccef0-e650-4c09-9b43-845e19e8f088")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f36f8054-756a-4413-afac-291c10fcebc0")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87ef955b-5f0b-41fe-b02e-8b481d5e2f35")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0df77fba-f9eb-47fc-990a-3c0da234319d")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "93cb0f51-8b0a-449f-ad28-d92bfb7d6724")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bc34b4e6-1156-45df-99a1-225b8529c4c8")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "Net-(U1-VIN)")
			(pintype "passive")
			(uuid "3cfc86ee-bda6-4ebb-b559-571f695917df")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "626dfddb-33b7-4b18-97d3-01b907c3f400")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:Nordic_AQFN-73-1EP_7x7mm_P0.5mm"
		(layer "F.Cu")
		(uuid "c609aca6-6fe2-4017-b854-c7dd71585043")
		(at 166.55 108.86)
		(descr "http://infocenter.nordicsemi.com/index.jsp?topic=%2Fcom.nordic.infocenter.nrf52%2Fdita%2Fnrf52%2Fchips%2Fnrf52840.html")
		(tags "AQFN 7mm ")
		(property "Reference" "U7"
			(at 0 -4.5 0)
			(layer "F.SilkS")
			(uuid "914bbca9-f2b4-49b2-8522-309e5c7fe4dd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "nRF52840"
			(at 0.03 5.72 0)
			(layer "F.Fab")
			(uuid "2968df95-e376-4f3c-8b84-54d4f0ff47f3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://infocenter.nordicsemi.com/topic/com.nordic.infocenter.nrf52/dita/nrf52/chips/nrf52840.html"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "57068bb5-eaf6-4f96-aede-c3ceda335cbd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, AQFN-73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d2ed28c2-e428-4495-a871-7a307a72050f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Nordic*AQFN*1EP*7x7mm*P0.5mm*")
		(path "/f82a1418-c722-433f-bd53-a913a7ebb75b")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.61 -2.48)
			(end -3.61 3.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d84523a1-14aa-4ee5-819d-8f2b6d2f466e")
		)
		(fp_line
			(start -3.61 3.61)
			(end 3.61 3.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1809836b-6eda-4c4b-adc2-33a3a9e5cd43")
		)
		(fp_line
			(start 3.61 -3.61)
			(end -2.48 -3.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49b5a669-5637-4421-8c7d-72a02111c5e4")
		)
		(fp_line
			(start 3.61 3.61)
			(end 3.61 -3.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f14379f5-2f65-467c-94f7-6ab7d491470c")
		)
		(fp_poly
			(pts
				(xy -3.61 -3.61) (xy -4.11 -3.61) (xy -3.61 -4.11) (xy -3.61 -3.61)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "7202d3c8-2bad-4184-b505-6df66bc8171e")
		)
		(fp_rect
			(start 4.5 -4.5)
			(end -4.5 4.5)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "29b80849-8853-4268-a69f-8ca9ef7b393f")
		)
		(fp_line
			(start -3.5 -2.5)
			(end -3.5 3.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ee934bb-5e11-48a0-aa09-fa9f35649cab")
		)
		(fp_line
			(start -3.5 -2.5)
			(end -2.5 -3.5)
			(stroke
				(width 0.1)
				(type default)
			)
			(layer "F.Fab")
			(uuid "44d43957-1e16-49a3-b0ec-cbe1a5097e5a")
		)
		(fp_line
			(start -3.5 3.5)
			(end 3.5 3.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "19d144a0-1c18-4db3-90e1-b23c10213af8")
		)
		(fp_line
			(start -2.5 -3.5)
			(end 3.5 -3.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "247ee0ee-43ee-4ab4-b8bb-75aadd7f412b")
		)
		(fp_line
			(start 3.5 -3.5)
			(end 3.5 3.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "48ad4ae0-2314-4027-bc32-4f88878423fc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "481823ba-9533-4923-8693-dd6908efbcbd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" smd rect
			(at -1.2125 -1.2125 180)
			(size 2 2)
			(layers "F.Paste")
			(uuid "3f7cfb01-4695-466e-b1de-96b30caf4cca")
		)
		(pad "" smd rect
			(at -1.2125 1.2125 180)
			(size 2 2)
			(layers "F.Paste")
			(uuid "10fc73bc-6442-4768-80db-3544cadf4fcd")
		)
		(pad "" smd rect
			(at 1.2125 -1.2125 180)
			(size 2 2)
			(layers "F.Paste")
			(uuid "9f9f56ed-6283-4e28-8cc2-f9394a766101")
		)
		(pad "" smd rect
			(at 1.2125 1.2125 180)
			(size 2 2)
			(layers "F.Paste")
			(uuid "7d0d831b-7e6b-4fdd-bf7d-0e5310af3a1b")
		)
		(pad "A8" smd circle
			(at -1.25 -3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 170 "unconnected-(U7-AIN7{slash}P0.31-PadA8)")
			(pinfunction "AIN7/P0.31")
			(pintype "bidirectional")
			(uuid "8d14bdd4-507f-409e-8236-73c1862feffc")
		)
		(pad "A10" smd circle
			(at -0.75 -3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 173 "unconnected-(U7-AIN5{slash}P0.29-PadA10)")
			(pinfunction "AIN5/P0.29")
			(pintype "bidirectional")
			(uuid "98fbd895-a619-4ada-80d7-7cac0b1763a0")
		)
		(pad "A12" smd circle
			(at -0.25 -3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 146 "unconnected-(U7-AIN0{slash}P0.02-PadA12)")
			(pinfunction "AIN0/P0.02")
			(pintype "bidirectional")
			(uuid "3c2dba84-b75e-40c7-b49e-d009a1ab4633")
		)
		(pad "A14" smd circle
			(at 0.25 -3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 178 "unconnected-(U7-P1.15-PadA14)")
			(pinfunction "P1.15")
			(pintype "bidirectional")
			(uuid "b93d8991-0ae7-49b6-a340-603b54bb2e16")
		)
		(pad "A16" smd circle
			(at 0.75 -3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 128 "unconnected-(U7-P1.13-PadA16)")
			(pinfunction "P1.13")
			(pintype "bidirectional")
			(uuid "0c214dd5-bb79-4343-8037-e7b2f93cc2fa")
		)
		(pad "A18" smd circle
			(at 1.25 -3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 177 "unconnected-(U7-DEC2-PadA18)")
			(pinfunction "DEC2")
			(pintype "passive")
			(uuid "b74edabd-f2f4-454b-bef3-7b33cd8f389a")
		)
		(pad "A20" smd circle
			(at 1.75 -3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "unconnected-(U7-P1.10-PadA20)")
			(pinfunction "P1.10")
			(pintype "bidirectional")
			(uuid "39b2a787-2321-4e82-80bf-0913eb2a3be5")
		)
		(pad "A22" smd circle
			(at 2.25 -3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 137 "Net-(U7-VDD-PadA22)")
			(pinfunction "VDD")
			(pintype "passive")
			(uuid "5ad01964-4bda-4849-a3ae-136e9b6e6f0c")
		)
		(pad "A23" smd circle
			(at 2.75 -3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 131 "unconnected-(U7-XC2-PadA23)")
			(pinfunction "XC2")
			(pintype "input")
			(uuid "136316ab-bc46-40d9-84e0-6bddaa05d36b")
		)
		(pad "AA24" smd circle
			(at 3.25 2.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 126 "unconnected-(U7-SWDCLK-PadAA24)")
			(pinfunction "SWDCLK")
			(pintype "input")
			(uuid "0229242e-8659-4e40-9aee-3fefea2abf0a")
		)
		(pad "AB2" smd circle
			(at -2.75 2.5 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 171 "unconnected-(U7-DCCH-PadAB2)")
			(pinfunction "DCCH")
			(pintype "power_out")
			(uuid "8df82b6c-b643-4e25-9a2f-02e7b86fefbe")
		)
		(pad "AC5" smd circle
			(at -2 2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 175 "unconnected-(U7-DECUSB-PadAC5)")
			(pinfunction "DECUSB")
			(pintype "passive")
			(uuid "ab025c78-6320-4bd5-a787-57dc6ed3c510")
		)
		(pad "AC9" smd circle
			(at -1 2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 166 "unconnected-(U7-P0.14-PadAC9)")
			(pinfunction "P0.14")
			(pintype "bidirectional")
			(uuid "7dadc876-daeb-4187-a461-d485c2ee3f05")
		)
		(pad "AC11" smd circle
			(at -0.5 2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 189 "unconnected-(U7-P0.16-PadAC11)")
			(pinfunction "P0.16")
			(pintype "bidirectional")
			(uuid "ee18f38f-675a-4c41-bba2-c9b55e6b5dff")
		)
		(pad "AC13" smd circle
			(at 0 2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 162 "unconnected-(U7-P0.18{slash}~{RESET}-PadAC13)")
			(pinfunction "P0.18/~{RESET}")
			(pintype "bidirectional")
			(uuid "78d4b1e9-ffdd-43ab-b8d3-a2b5cc99ac8a")
		)
		(pad "AC15" smd circle
			(at 0.5 2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 182 "unconnected-(U7-P0.19-PadAC15)")
			(pinfunction "P0.19")
			(pintype "bidirectional")
			(uuid "cf650211-2942-4472-9c22-cbb24c4cf8ed")
		)
		(pad "AC17" smd circle
			(at 1 2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 153 "unconnected-(U7-P0.21-PadAC17)")
			(pinfunction "P0.21")
			(pintype "bidirectional")
			(uuid "5694c753-38b6-4865-8eed-c01281a8ad31")
		)
		(pad "AC19" smd circle
			(at 1.5 2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 167 "unconnected-(U7-P0.23-PadAC19)")
			(pinfunction "P0.23")
			(pintype "bidirectional")
			(uuid "838bdeda-8bd6-441d-aae8-f79ba98cadb8")
		)
		(pad "AC21" smd circle
			(at 2 2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 172 "unconnected-(U7-P0.25-PadAC21)")
			(pinfunction "P0.25")
			(pintype "bidirectional")
			(uuid "90e76939-6da8-473a-874e-a2ee49c72437")
		)
		(pad "AC24" smd circle
			(at 3.25 2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 180 "unconnected-(U7-SWDIO-PadAC24)")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
			(uuid "c8858bd7-149a-4171-97c7-532a9004a456")
		)
		(pad "AD2" smd circle
			(at -2.75 3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 157 "unconnected-(U7-VBUS-PadAD2)")
			(pinfunction "VBUS")
			(pintype "power_in")
			(uuid "5e95a55d-ac7c-403b-8061-0bff57462b6f")
		)
		(pad "AD4" smd circle
			(at -2.25 3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 143 "unconnected-(U7-D--PadAD4)")
			(pinfunction "D-")
			(pintype "bidirectional")
			(uuid "37e30fc8-91a9-4cc5-a1f5-d8fabe8e77f9")
		)
		(pad "AD6" smd circle
			(at -1.75 3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 139 "unconnected-(U7-D+-PadAD6)")
			(pinfunction "D+")
			(pintype "bidirectional")
			(uuid "276d96eb-dcb1-44ab-aa63-82cec29db3e1")
		)
		(pad "AD8" smd circle
			(at -1.25 3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 134 "unconnected-(U7-P0.13-PadAD8)")
			(pinfunction "P0.13")
			(pintype "bidirectional")
			(uuid "1ba0d218-e213-4f61-98b2-df00ff364337")
		)
		(pad "AD10" smd circle
			(at -0.75 3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 156 "unconnected-(U7-P0.15-PadAD10)")
			(pinfunction "P0.15")
			(pintype "bidirectional")
			(uuid "5b916ba6-dff8-4b9a-b32b-df0816f11e6f")
		)
		(pad "AD12" smd circle
			(at -0.25 3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 186 "unconnected-(U7-P0.17-PadAD12)")
			(pinfunction "P0.17")
			(pintype "bidirectional")
			(uuid "d7b7ee81-bbaf-43a2-a8f3-a2ae2835b5e1")
		)
		(pad "AD14" smd circle
			(at 0.25 3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 137 "Net-(U7-VDD-PadA22)")
			(pinfunction "VDD")
			(pintype "passive")
			(uuid "1fa01ccd-3494-4c2c-97fd-c1c66140dec1")
		)
		(pad "AD16" smd circle
			(at 0.75 3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 133 "unconnected-(U7-P0.20-PadAD16)")
			(pinfunction "P0.20")
			(pintype "bidirectional")
			(uuid "191f7580-e9c0-4bc7-be8a-27f5be9a15e5")
		)
		(pad "AD18" smd circle
			(at 1.25 3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 192 "unconnected-(U7-P0.22-PadAD18)")
			(pinfunction "P0.22")
			(pintype "bidirectional")
			(uuid "f69a2261-2fda-4335-a732-244834b4f3cd")
		)
		(pad "AD20" smd circle
			(at 1.75 3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 163 "unconnected-(U7-P0.24-PadAD20)")
			(pinfunction "P0.24")
			(pintype "bidirectional")
			(uuid "79da44d9-e3a3-43c6-abc2-1e1a4e7ae4be")
		)
		(pad "AD22" smd circle
			(at 2.25 3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 147 "unconnected-(U7-TRACEDATA0{slash}P1.00-PadAD22)")
			(pinfunction "TRACEDATA0/P1.00")
			(pintype "bidirectional")
			(uuid "41b37ec9-50cd-4710-9fde-eac8e3c021df")
		)
		(pad "AD23" smd circle
			(at 2.75 3.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 137 "Net-(U7-VDD-PadA22)")
			(pinfunction "VDD")
			(pintype "passive")
			(uuid "40f1dc71-fc61-4fd4-997c-89aa7f3c0278")
		)
		(pad "B1" smd circle
			(at -3.25 -2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 137 "Net-(U7-VDD-PadA22)")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "adb8be38-2ba1-4736-ae29-f38a60c5160d")
		)
		(pad "B3" smd circle
			(at -2.5 -2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 188 "unconnected-(U7-DCC-PadB3)")
			(pinfunction "DCC")
			(pintype "power_out")
			(uuid "ec3294d7-de47-4522-b9ed-557485b2ae61")
		)
		(pad "B5" smd circle
			(at -2 -2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 169 "unconnected-(U7-DEC4-PadB5)")
			(pinfunction "DEC4")
			(pintype "passive")
			(uuid "8c02fac3-9448-41ef-903e-55f7f13a8cd4")
		)
		(pad "B7" smd circle
			(at -1.5 -2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 129 "Net-(U7-VSS-PadB7)")
			(pinfunction "VSS")
			(pintype "power_in")
			(uuid "a401eb16-c1cd-42cd-9b6c-9506d1189c9f")
		)
		(pad "B9" smd circle
			(at -1 -2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 193 "unconnected-(U7-AIN6{slash}P0.30-PadB9)")
			(pinfunction "AIN6/P0.30")
			(pintype "bidirectional")
			(uuid "fd661280-7fce-4bab-9e3a-99fc8317624f")
		)
		(pad "B11" smd circle
			(at -0.5 -2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 155 "unconnected-(U7-AIN4{slash}P0.28-PadB11)")
			(pinfunction "AIN4/P0.28")
			(pintype "bidirectional")
			(uuid "5aa223f8-51b1-44aa-87b8-b2800648192a")
		)
		(pad "B13" smd circle
			(at 0 -2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 130 "unconnected-(U7-AIN1{slash}P0.03-PadB13)")
			(pinfunction "AIN1/P0.03")
			(pintype "bidirectional")
			(uuid "13131e93-11a9-4daf-b190-f9748de02355")
		)
		(pad "B15" smd circle
			(at 0.5 -2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 165 "unconnected-(U7-P1.14-PadB15)")
			(pinfunction "P1.14")
			(pintype "bidirectional")
			(uuid "7da81d17-42a1-442f-8a7e-35da160ea170")
		)
		(pad "B17" smd circle
			(at 1 -2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 151 "unconnected-(U7-P1.12-PadB17)")
			(pinfunction "P1.12")
			(pintype "bidirectional")
			(uuid "5501954f-38c2-48b5-afbb-66bf1a32cfb9")
		)
		(pad "B19" smd circle
			(at 1.5 -2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 138 "unconnected-(U7-P1.11-PadB19)")
			(pinfunction "P1.11")
			(pintype "bidirectional")
			(uuid "1fa40431-b157-4868-a733-47b69a3d247c")
		)
		(pad "B24" smd circle
			(at 3.25 -2.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 136 "unconnected-(U7-XC1-PadB24)")
			(pinfunction "XC1")
			(pintype "input")
			(uuid "1d99054e-f439-42c2-8618-db67efd58120")
		)
		(pad "C1" smd circle
			(at -3.25 -2.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 140 "unconnected-(U7-DEC1-PadC1)")
			(pinfunction "DEC1")
			(pintype "passive")
			(uuid "292b713e-c9ee-4bb0-95c3-46c8ab27e39c")
		)
		(pad "D2" smd circle
			(at -2.75 -2 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 168 "unconnected-(U7-XL1{slash}P0.00-PadD2)")
			(pinfunction "XL1/P0.00")
			(pintype "bidirectional")
			(uuid "8877c918-5d8e-4b08-964a-b11cbf46eae0")
		)
		(pad "D23" smd circle
			(at 2.75 -2 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 141 "unconnected-(U7-DEC3-PadD23)")
			(pinfunction "DEC3")
			(pintype "passive")
			(uuid "31e3eb90-3620-4188-9931-28e46d465304")
		)
		(pad "E24" smd circle
			(at 3.25 -1.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 179 "unconnected-(U7-DEC6-PadE24)")
			(pinfunction "DEC6")
			(pintype "passive")
			(uuid "c6ebe8a5-f76d-459a-86b8-100d376bbc78")
		)
		(pad "EP" smd rect
			(at 0 0 180)
			(size 4.85 4.85)
			(layers "F.Cu" "F.Mask")
			(net 129 "Net-(U7-VSS-PadB7)")
			(pinfunction "VSS")
			(pintype "passive")
			(uuid "0fc43787-304d-4456-b4d3-13c92b927b64")
		)
		(pad "F2" smd circle
			(at -2.75 -1.5 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 142 "unconnected-(U7-XL2{slash}P0.01-PadF2)")
			(pinfunction "XL2/P0.01")
			(pintype "bidirectional")
			(uuid "33f22a5e-263f-421e-a476-e7e3f7d9da1d")
		)
		(pad "F23" smd circle
			(at 2.75 -1.5 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 158 "unconnected-(U7-VSS_PA-PadF23)")
			(pinfunction "VSS_PA")
			(pintype "power_in")
			(uuid "608a4552-f5fc-4674-b97f-a0d647f24ad3")
		)
		(pad "G1" smd circle
			(at -3.25 -1.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 176 "unconnected-(U7-P0.26-PadG1)")
			(pinfunction "P0.26")
			(pintype "bidirectional")
			(uuid "b6c8c53a-eabb-4623-a087-f910a39080ad")
		)
		(pad "H2" smd circle
			(at -2.75 -1 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 181 "unconnected-(U7-P0.27-PadH2)")
			(pinfunction "P0.27")
			(pintype "bidirectional")
			(uuid "cbb4cf7f-f323-4bd0-8104-2f7a6ee56a80")
		)
		(pad "H23" smd circle
			(at 2.75 -1 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "unconnected-(U7-ANT-PadH23)")
			(pinfunction "ANT")
			(pintype "passive")
			(uuid "03e95496-3b29-40be-9c79-4ddfdc6cc7eb")
		)
		(pad "J1" smd circle
			(at -3.25 -0.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 144 "unconnected-(U7-AIN2{slash}P0.04-PadJ1)")
			(pinfunction "AIN2/P0.04")
			(pintype "bidirectional")
			(uuid "386656dc-baa9-4920-b1a9-4c0684da9cdf")
		)
		(pad "J24" smd circle
			(at 3.25 -0.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 152 "unconnected-(U7-NFC2{slash}P0.10-PadJ24)")
			(pinfunction "NFC2/P0.10")
			(pintype "bidirectional")
			(uuid "55fca93c-744d-4fdc-8ee8-70c9c38de242")
		)
		(pad "K2" smd circle
			(at -2.75 -0.5 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 135 "unconnected-(U7-AIN3{slash}P0.05-PadK2)")
			(pinfunction "AIN3/P0.05")
			(pintype "bidirectional")
			(uuid "1d36d5cc-7682-4b61-b25d-46dc5aa4cc0f")
		)
		(pad "L1" smd circle
			(at -3.25 -0.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 160 "unconnected-(U7-P0.06-PadL1)")
			(pinfunction "P0.06")
			(pintype "bidirectional")
			(uuid "6e32cd7b-4a7b-4d4b-970d-9dde8d9b39db")
		)
		(pad "L24" smd circle
			(at 3.25 -0.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 149 "unconnected-(U7-NFC1{slash}P0.09-PadL24)")
			(pinfunction "NFC1/P0.09")
			(pintype "bidirectional")
			(uuid "4980908d-181b-4363-9f61-3b0e3e3777bd")
		)
		(pad "M2" smd circle
			(at -2.75 0 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 187 "unconnected-(U7-TRACECLK{slash}P0.07-PadM2)")
			(pinfunction "TRACECLK/P0.07")
			(pintype "bidirectional")
			(uuid "dc2ea683-13c6-4abc-a65b-229fc8dffa1e")
		)
		(pad "N1" smd circle
			(at -3.25 0.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 164 "unconnected-(U7-P0.08-PadN1)")
			(pinfunction "P0.08")
			(pintype "bidirectional")
			(uuid "7c57e445-b985-4a51-ab07-63ecb9643eec")
		)
		(pad "N24" smd circle
			(at 3.25 0.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 150 "unconnected-(U7-DEC5-PadN24)")
			(pinfunction "DEC5")
			(pintype "passive")
			(uuid "52af099f-fbbb-439d-a02f-9381faa1549e")
		)
		(pad "P2" smd circle
			(at -2.75 0.5 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 159 "unconnected-(U7-P1.08-PadP2)")
			(pinfunction "P1.08")
			(pintype "bidirectional")
			(uuid "6d1e87df-9d85-4784-b661-ce264601a994")
		)
		(pad "P23" smd circle
			(at 2.75 0.5 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 174 "unconnected-(U7-P1.07-PadP23)")
			(pinfunction "P1.07")
			(pintype "bidirectional")
			(uuid "a6217315-8ece-4441-b551-7aea09ade3bd")
		)
		(pad "R1" smd circle
			(at -3.25 0.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 190 "unconnected-(U7-TRACEDATA3{slash}P1.09-PadR1)")
			(pinfunction "TRACEDATA3/P1.09")
			(pintype "bidirectional")
			(uuid "f232e9bb-922d-4d61-b404-05eb0d7d97f3")
		)
		(pad "R24" smd circle
			(at 3.25 0.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 184 "unconnected-(U7-P1.06-PadR24)")
			(pinfunction "P1.06")
			(pintype "bidirectional")
			(uuid "d1daa962-12a5-4b69-b232-05d1c918cc5b")
		)
		(pad "T2" smd circle
			(at -2.75 1 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 161 "unconnected-(U7-TRACEDATA2{slash}P0.11-PadT2)")
			(pinfunction "TRACEDATA2/P0.11")
			(pintype "bidirectional")
			(uuid "75d03f4b-1d30-492e-a1a5-ec690a135684")
		)
		(pad "T23" smd circle
			(at 2.75 1 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 132 "unconnected-(U7-P1.05-PadT23)")
			(pinfunction "P1.05")
			(pintype "bidirectional")
			(uuid "17b0b71f-56d4-46e4-8adb-9eeba7bac22b")
		)
		(pad "U1" smd circle
			(at -3.25 1.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 125 "unconnected-(U7-TRACEDATA1{slash}P0.12-PadU1)")
			(pinfunction "TRACEDATA1/P0.12")
			(pintype "bidirectional")
			(uuid "01972dd0-46ad-4634-a839-30bbe6d776a4")
		)
		(pad "U24" smd circle
			(at 3.25 1.25 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 183 "unconnected-(U7-P1.04-PadU24)")
			(pinfunction "P1.04")
			(pintype "bidirectional")
			(uuid "d1d26faa-a953-4f40-a354-038c478c8016")
		)
		(pad "V23" smd circle
			(at 2.75 1.5 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 148 "unconnected-(U7-P1.03-PadV23)")
			(pinfunction "P1.03")
			(pintype "bidirectional")
			(uuid "432a1ee0-295d-46dc-bc82-819288057a75")
		)
		(pad "W1" smd circle
			(at -3.25 1.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 137 "Net-(U7-VDD-PadA22)")
			(pinfunction "VDD")
			(pintype "passive")
			(uuid "6a897ab2-8ba5-4376-aa96-2ccc7c3066a9")
		)
		(pad "W24" smd circle
			(at 3.25 1.75 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 154 "unconnected-(U7-P1.02-PadW24)")
			(pinfunction "P1.02")
			(pintype "bidirectional")
			(uuid "584365f3-1b67-48fd-b61f-188de88fbd06")
		)
		(pad "Y2" smd circle
			(at -2.75 2 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 191 "unconnected-(U7-VDDH-PadY2)")
			(pinfunction "VDDH")
			(pintype "power_in")
			(uuid "f51739d5-8ec9-400a-a934-b5688dbb3212")
		)
		(pad "Y23" smd circle
			(at 2.75 2 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 185 "unconnected-(U7-P1.01-PadY23)")
			(pinfunction "P1.01")
			(pintype "bidirectional")
			(uuid "d21c0c0a-78c9-4306-b7d5-cab21bc590c3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Nordic_AQFN-73-1EP_7x7mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "c7f2b87a-d34d-422d-8d96-17d2570f8ff8")
		(at 115.35 87.08)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R17"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "da6924cb-227f-4957-b41d-42b4b2b1f78a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "77fa61e5-078a-4dcd-a142-fe1435c9c38b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ac5d4565-5248-497b-81f7-3efbab53c471")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "445e0888-9a2f-4fae-b67d-4e2f2c0660ec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/3ccd7da3-ea73-4653-b042-b982c6ffcd9c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e598f456-8637-423f-88a2-0c8dd1a0d4b7")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "363f8c9e-809e-4c71-83f5-16d3ea36877b")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "db7bd32e-7b76-49ae-a994-719f98f918c3")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0c64e1ab-450f-4336-8d72-ad64c0112b5c")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "78a17a72-6c5b-4360-826e-e8add63106e3")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "17e6a084-7da1-437c-9c3d-4943ff551842")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb72b237-1ac3-4009-b1f0-898f1c0f940f")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "277f015a-f160-4aac-9c3d-e5685a63b0a7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2a63de87-13f2-4b95-8d7c-89d625aba42a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8df3690d-bbd4-42f0-84d2-df4cc13d66e2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "721c91b1-4a5b-49f8-a2fd-d041c925e1f2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "62d4b9ad-18ec-4927-85c6-504982987137")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 109 "I2C SCL")
			(pintype "passive")
			(uuid "feb1f0e3-e0b6-4bc4-9f53-b91200606dd3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "d066f21d-f808-4a2b-88b6-ece6cb760621")
		(at 115.35 84.13)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R16"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "3fdeadb3-c47f-486d-89e8-34a87f4333b4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "8a8f9248-ca0e-4a35-8962-bda8b27448e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d3552ef0-02cb-4d04-8b59-337860996626")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "16c55c51-9ba8-444b-a8c7-a9d917677c3f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/154c0391-b6ce-4973-9abc-0a85f91031d0")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8976c92c-476a-416b-9f2d-72e2db0513ee")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "03abb37b-9e5a-4d00-b544-73c6ac892871")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2bc21d1-cb3f-4d92-afb4-94e34f9aa667")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d00c663d-a04a-4b29-b737-e63a921f1a75")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "46798ac7-7cbd-467f-8cda-42aa944d2365")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0f276054-3122-4025-a2bf-6f7a48907287")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5dec4e74-27ed-4541-b47e-ffe59d57b778")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "350f3708-2110-4507-b122-0820557a5d18")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "42eb0209-5c23-4b76-beb8-316d996b14b7")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1f72cca2-dbaf-4e30-99f0-0b2db669879f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "01f7a64a-4040-4fa5-9228-51ff55a82cf2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 108 "I2C SDA")
			(pintype "passive")
			(uuid "d1b953a4-4fe6-45ee-b561-c622f5ad3fca")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "fbe4e909-e4e7-4fdb-8838-763c48336b94")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(uuid "d3efd04a-ca5f-43e8-ae43-f923ba31ffe6")
		(at 118.1 122.04)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U6"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "3f292458-3f94-4af8-b1b5-f487e7c90d90")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "USBLC6-2SC6"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "f3ad4c68-873b-4589-baf8-c73718ca292e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/usblc6-2.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1a2515cd-3a5a-4808-927c-9f6f0ce7babb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b3acbe24-97c8-464e-a3e1-bfdf9ab5e7aa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bbf30386-0917-4941-aaf0-57c22c80b865")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2b2165d4-68f0-424d-bb49-aa18af5bcfd5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/778a6fa8-fc79-4871-8fca-1e1eb951d152")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b9f1d315-ac54-4322-9daa-ccca88203394")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "01538847-32b1-488d-9fbd-858280608aa1")
		)
		(fp_line
			(start 0 1.56)
			(end -0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "290b4c03-972f-4337-8f3e-b63b18491117")
		)
		(fp_line
			(start 0 1.56)
			(end 0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1a162a35-27eb-4a9a-b513-e6ee179173f9")
		)
		(fp_poly
			(pts
				(xy -1.3 -1.51) (xy -1.54 -1.84) (xy -1.06 -1.84)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "3fb197d4-7195-4374-8fcf-a17538780e1d")
		)
		(fp_rect
			(start -2.05 -1.7)
			(end 2.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "6de395ae-df09-4aa6-a8fc-5e7425158986")
		)
		(fp_line
			(start -0.8 -1.05)
			(end -0.4 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5c09513c-a0b2-405b-88a8-8cdf6cc62271")
		)
		(fp_line
			(start -0.8 1.45)
			(end -0.8 -1.05)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "12768405-e4ae-411f-9040-295bbe08d3d8")
		)
		(fp_line
			(start -0.4 -1.45)
			(end 0.8 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "95963ed3-a59b-4613-8d52-2c4be69cd9c2")
		)
		(fp_line
			(start 0.8 -1.45)
			(end 0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "403a08e0-f69b-4a83-82e4-f30e9c44bfb4")
		)
		(fp_line
			(start 0.8 1.45)
			(end -0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2eb21d4f-0b11-47d0-bc45-0503bfa96635")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a347ec81-a041-4a93-b348-4aaae46bf823")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "Net-(J1-D--PadA7)")
			(pinfunction "I/O1")
			(pintype "passive")
			(uuid "950f9306-6b2a-4a93-9e42-24fe69fc6626")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "a7a967b1-970d-40e5-a59d-b2fb603b6fb2")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "Net-(J1-D+-PadA6)")
			(pinfunction "I/O2")
			(pintype "passive")
			(uuid "7a55b525-c408-4fb3-a586-d8acc631e22a")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "D+")
			(pinfunction "I/O2")
			(pintype "passive")
			(uuid "c688e2e2-4371-4baf-95bc-2f0b87f420ee")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "eb3cc890-2920-4fe4-8c7d-d8486b9143f4")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "D-")
			(pinfunction "I/O1")
			(pintype "passive")
			(uuid "e740b37c-9000-4c18-93e0-6e9a4012e802")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "d5d6caf7-1b6d-4c65-93ca-3ef7981bfb92")
		(at 138.45 115.13)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C29"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "88ee9784-da15-4ff4-91ed-724349015504")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "c0d73e15-74fb-441a-8d23-991013746353")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9b9788f2-5e58-489c-9532-04dfeefcf60f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2cd539bf-e9ba-4e3a-b0fe-e804dd3d8617")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/e6238dc2-1497-4aa0-b345-6fd9f1f027b3")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "35636d87-e5be-42ed-a154-c0ad65ace7ce")
		)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bfc24ff8-164f-43e0-80cd-2ba83ebfa646")
		)
		(fp_line
			(start -1.65 -0.73)
			(end 1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "005e51dd-9a8b-49be-8560-b9508d4b85da")
		)
		(fp_line
			(start -1.65 0.73)
			(end -1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "01351d71-fe5e-4c63-90e9-fd5005526fa8")
		)
		(fp_line
			(start 1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3067a836-f0a0-44f3-82bc-0be76fd34ae3")
		)
		(fp_line
			(start 1.65 0.73)
			(end -1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2c6c2580-3a8f-4b9c-bc1f-eb41b860861c")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b47bde6-3d6c-4bcc-8311-08197597d2da")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eadb225c-1b67-4092-846b-f23772568e33")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c4f7dd62-31a6-41e4-907a-c111a7cb677d")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d7be425f-999b-4761-9fba-85fd416dd6d1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3bd1de45-1fe9-4627-87b5-75205194d9fb")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "0f50b476-8bde-4275-98b3-72dc320f8b99")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "f62d4ff9-ff28-4e93-9cb8-9e405817e01a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RF_Antenna:Texas_SWRA117D_2.4GHz_Left"
		(layer "F.Cu")
		(uuid "d9429ec7-291e-48b1-9780-2656b7b64792")
		(at 162.2 120.81)
		(descr "http://www.ti.com/lit/an/swra117d/swra117d.pdf")
		(tags "PCB antenna")
		(property "Reference" "AE1"
			(at -4.55 -6.41 0)
			(layer "F.SilkS")
			(uuid "5bc406d3-69ba-4a25-bd0d-4f5d03c58146")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Antenna_Chip"
			(at -3.95 1.21 0)
			(layer "F.Fab")
			(uuid "e79463d9-792a-4e3c-8b95-0248cc670c3c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "64889b61-35c5-45cd-a2e7-0dd1b8b7b19b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Ceramic chip antenna with pin for PCB trace"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9847968a-e219-42de-adf2-fe753b940701")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c82b77a7-7048-4524-8c3f-0010107c6e26")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "659f7a6e-c31f-4f83-a4bf-8eb963b39a0e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/f1e46d7b-dbe8-46bf-86b7-d2ff8765ec4a")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr exclude_from_pos_files)
		(net_tie_pad_groups "1,2")
		(fp_poly
			(pts
				(xy -2.45 -2.51) (xy -4.45 -2.51) (xy -4.45 -5.15) (xy -7.15 -5.15) (xy -7.15 -2.51) (xy -9.15 -2.51)
				(xy -9.15 -5.15) (xy -11.85 -5.15) (xy -11.85 -0.71) (xy -11.35 -0.71) (xy -11.35 -4.65) (xy -9.65 -4.65)
				(xy -9.65 -2.01) (xy -6.65 -2.01) (xy -6.65 -4.65) (xy -4.95 -4.65) (xy -4.95 -2.01) (xy -1.95 -2.01)
				(xy -1.95 -4.65) (xy -0.25 -4.65) (xy -0.25 0.25) (xy 0.25 0.25) (xy 0.25 -4.65) (xy 1.65 -4.65)
				(xy 1.65 0.25) (xy 2.55 0.25) (xy 2.55 0.006785) (xy 2.247583 0.006785) (xy 2.237742 0.054395) (xy 2.213674 0.096797)
				(xy 2.175731 0.129581) (xy 2.167819 0.133935) (xy 2.125156 0.146043) (xy 2.076637 0.1453) (xy 2.031122 0.1324)
				(xy 2.012511 0.121787) (xy 1.978868 0.086553) (xy 1.958309 0.041368) (xy 1.951778 -0.008158) (xy 1.960218 -0.056417)
				(xy 1.977112 -0.088643) (xy 2.012372 -0.121313) (xy 2.057682 -0.141408) (xy 2.107267 -0.147982)
				(xy 2.155353 -0.140092) (xy 2.188245 -0.123186) (xy 2.223185 -0.086416) (xy 2.242847 -0.041622)
				(xy 2.247583 0.006785) (xy 2.55 0.006785) (xy 2.55 -5.15) (xy -2.45 -5.15) (xy -2.45 -2.51)
			)
			(stroke
				(width 0)
				(type solid)
			)
			(fill yes)
			(layer "F.Cu")
			(uuid "715e2c7f-b761-4a5c-9ad5-1ec68415136c")
		)
		(fp_line
			(start -12.15 -0.25)
			(end -12.15 -5.45)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "ab19ec12-3f34-4a57-b5d1-3ce6fd116839")
		)
		(fp_line
			(start 3.05 -5.45)
			(end -12.15 -5.45)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "7a50b5cd-a99b-475d-828b-e680a4f54fc5")
		)
		(fp_line
			(start 3.05 -5.45)
			(end -12.15 -0.25)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "63838c57-c054-4c87-b657-165237ca3587")
		)
		(fp_line
			(start 3.05 -0.25)
			(end -12.15 -5.45)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "470a57ca-f03f-4772-886f-adb63e75a669")
		)
		(fp_line
			(start 3.05 -0.25)
			(end -12.15 -0.25)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "87fbce61-df61-49f4-aa13-9ac2f2b10b88")
		)
		(fp_line
			(start 3.05 -0.25)
			(end 3.05 -5.45)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "4af023a0-2d43-4506-8701-9c7f3506b3c6")
		)
		(fp_line
			(start -12.3 -5.6)
			(end -12.3 0.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9b38eff4-405e-4684-b6ec-0496c4ad9d82")
		)
		(fp_line
			(start -12.3 0.35)
			(end 3.2 0.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c48f693-4da7-46f5-bbe1-64689aa6e94c")
		)
		(fp_line
			(start 3.2 -5.6)
			(end -12.3 -5.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ccaae13f-c513-4811-96d3-193d9f58040e")
		)
		(fp_line
			(start 3.2 0.35)
			(end 3.2 -5.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e99e80b9-d2dc-45ef-ac86-086ac8df2446")
		)
		(fp_line
			(start -12.3 -5.6)
			(end -12.3 0.35)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "76665561-ad6c-48ae-9f69-7856bc6df9d8")
		)
		(fp_line
			(start -12.3 0.35)
			(end 3.2 0.35)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae5cf67d-d4f1-4782-a9ea-6e44a0435bf9")
		)
		(fp_line
			(start 3.2 -5.6)
			(end -12.3 -5.6)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b85bc9ec-d271-49b0-86ef-3a251fa0528b")
		)
		(fp_line
			(start 3.2 0.35)
			(end 3.2 -5.6)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c90aa30-3308-4dff-8bfe-9960e832e712")
		)
		(fp_text user "${REFERENCE}"
			(at -4.55 -6.4 0)
			(layer "F.Fab")
			(uuid "7cd7e3a8-13bc-483c-b5cc-90efbaed9a8d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" connect rect
			(at 0 0)
			(size 0.5 0.5)
			(layers "F.Cu")
			(net 2 "RF_WIFI_BT")
			(pinfunction "FEED")
			(pintype "input")
			(uuid "ff031cef-c6aa-4fee-81e0-ef88dd8ba237")
		)
		(pad "2" thru_hole rect
			(at 2.1 0)
			(size 0.9 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "PCB_Trace")
			(pintype "passive")
			(zone_connect 2)
			(uuid "063a6a7d-da3e-4e2c-9cb2-c318f4250306")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "da7dd6f4-6e20-4516-a484-ed33775be5b6")
		(at 124.85 78.23)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R32"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "0e080e20-3b9e-4ceb-8870-b0b0ec50a279")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "2be0797b-7e2c-441a-a7b4-d9910d5abe86")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4607eba7-98b3-4685-8598-7c0d257ea35b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "92e6a8d1-51d1-4ba0-ab0e-97a865384f47")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1e4b1651-fc91-4961-a779-3c1d5f5635e1")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "208cc665-653b-4d10-9f5a-933a19cdfd7e")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c98ee191-a704-4173-9eeb-fc5e6d9242a4")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e66dea3f-2bac-42f1-ba9b-470eba78fbb0")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "54d79168-f3df-4d8f-bb40-d3c6783d6d56")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "482dd202-2790-4a1a-8ac4-355e34718484")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0f1306d7-ac63-4252-bef3-2b03c0bbab71")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d78ef133-4884-4771-be2d-8bdc1da47394")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "23a95402-e0eb-485f-93db-7f4a9be95d38")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3f158c64-7c52-430f-b4a1-13dcd31776a9")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a7dfdb77-e348-475a-a393-1f1d0d4786e9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a2a4a4d1-323d-49cd-b5b4-d8cb6d881732")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 115 "Net-(R27-Pad2)")
			(pintype "passive")
			(uuid "9517c764-4924-449c-9861-7dfee7b6abba")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "bb002ff4-fe4a-4e31-8af1-b5a59200df2a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "daa5d287-7e10-4836-96ef-a312e53e24cf")
		(at 129.63 81.57)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "a2137190-ff05-4e6b-bc10-17797ce98098")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "d0740c04-280b-4cb7-b610-301d27af66b7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "808adecf-3097-4687-98c4-289899b310d5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "360facdd-f553-4421-bd33-98c62b5735bb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/f038f94e-9ab9-48a2-95a6-396b3a8a8d99")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "01c46d9f-023c-44cf-b6f3-231ea90acfcc")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c071c289-da7b-4bfc-b6c8-b130ca522353")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c34fb631-c83a-4f77-9772-1807e4829b92")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0eba20e1-e83c-4564-83ae-6d38251bdd0a")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b9f38496-3c93-4eb8-bca9-d58331baf05d")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "06e153a4-7eff-4aee-956c-b796cddeb083")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "786ed586-4079-4592-a524-b0e7e2df86f7")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4ec2e3ec-fcc6-411d-bfbe-a6d43ac48380")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "06202834-c97e-466c-9671-520f111d1ee2")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83635121-d328-4696-8e8f-f9190bec5f2a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8b571b4a-85f8-4669-8c0b-9297494eb78b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "01df9b51-b7e1-449c-94c0-fa74d256ef17")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "71f12af2-a84f-4899-b652-a4193bce63d4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "db464fb5-b6f0-4679-b448-5579dc4cadb1")
		(at 115.35 75.28)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "9b99665c-df09-4bcb-abc4-b8c3a5d20e85")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "51k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "d0e3c740-e67f-4f06-a7a8-34bd73956833")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5c5ceb25-7dee-472e-a45e-9e02e91553f4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c909543a-67c1-4e9c-a7cf-4cc877c8d116")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/989e4871-e710-4c31-98f4-e3fdf042549c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d564cff4-a6ee-4c83-99b2-9911b5b363ed")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49c3b514-82a8-4fbe-97a9-1cb5336347a0")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ee8375e9-8d9a-408b-be5d-5ed845cabae7")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "30f530c3-aa9c-4593-bca8-a4dc285e1d86")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c437b445-1cc0-4192-adc3-a9114b410a88")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a0d02f7e-9343-4cb1-bf48-2770433ce11b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "07b1cb91-f308-48b5-b26e-e216c718a8e5")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7d0f0b0c-8ea5-43ef-8bdf-66f7242dded7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6c2f5c1d-a77e-426d-ba0d-8870a5e632e5")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5473a6fd-c036-43f8-b770-a5c13522ad30")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0fbe9d23-3878-4b5f-a87c-7d9a15c095c9")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 103 "Charger Load")
			(pintype "passive")
			(uuid "f9823943-8455-4b37-bf2d-7a715db152c2")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 45 "Net-(IC2-MPPT)")
			(pintype "passive")
			(uuid "920069e9-f7be-46f1-a021-38d9953a2e4e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "dd8239c6-1341-4691-9962-640d22ea6a0a")
		(at 147.15 110.11)
		(descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "fuse handsolder")
		(property "Reference" "F1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "d4d59e1c-de2c-4554-b685-d7146434be9e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Fuse (3A)"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "e54223fc-1c0f-4e80-b9e8-089a6edfe0d6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1e11d52f-f718-4774-98a8-77380b155728")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Fuse"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e7b644f3-5632-45f5-b31a-b3d59f37445d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*Fuse*")
		(path "/15872d8b-470a-4104-924e-cd63363d4b9f")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.171267 -0.51)
			(end 0.171267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "edf4b480-8084-46ea-bee1-63d70c9958d5")
		)
		(fp_line
			(start -0.171267 0.51)
			(end 0.171267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6e6b1767-93ca-4bba-9abf-30ea3b29e7d3")
		)
		(fp_line
			(start -1.65 -0.73)
			(end 1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b91e8359-aaa8-45f2-9d67-98bedda38f9f")
		)
		(fp_line
			(start -1.65 0.73)
			(end -1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4e63f0a9-2905-49ca-b241-db8ddc4b6378")
		)
		(fp_line
			(start 1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b2acdb42-70e0-4d0a-97b9-a039378f9777")
		)
		(fp_line
			(start 1.65 0.73)
			(end -1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6648b4fd-7e5c-4d70-be12-663d46aedbf7")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f89c7465-6323-45eb-a271-d3fbeb3faba0")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "143aa68f-509d-493d-b333-d53c8534a0c6")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46bbbfb3-e383-408a-818f-29bcff88c8bb")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "49b87a81-e2bc-4c51-acac-51762ec904cb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6a162e71-6eec-4cec-b653-d0787b4b6b6a")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.875 0)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "Sys Load")
			(pintype "passive")
			(uuid "3a6dd777-977f-47ff-b7d4-0ce15842d439")
		)
		(pad "2" smd roundrect
			(at 0.875 0)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(U1-VIN)")
			(pintype "passive")
			(uuid "f5ac21b1-bdc7-40a7-9ad9-0f15d4efe68d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "dd858d61-0641-43d7-b391-f86870c641af")
		(at 110.6 69.38)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "inductor handsolder")
		(property "Reference" "L9"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "03ab78f2-fb68-4acc-a4cf-e6d0c62e9879")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7uH"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "3e6ec91d-fe7c-45c8-b7fe-f077e7bc6cd9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9a3eb59f-a4a5-4435-afa7-c9438cf9c2f9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c96bb324-e383-40af-ba5a-d435a83437ef")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/d029387f-dccc-47a2-9396-d08ec1dc8924")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.71)
			(end 0.261252 -0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68f27e82-d9db-4cea-b37b-b9c595bca639")
		)
		(fp_line
			(start -0.261252 0.71)
			(end 0.261252 0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10bdf7f2-407a-41bd-8e5e-3b4f35246adf")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4e4aa523-d92a-45cd-9a0b-dd8fc061ea0e")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cde389a8-2343-4521-932b-eff30ed4d393")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ee9ce129-4f67-4ca9-9fb6-fd1ef3e1623a")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e22a14d4-fdb9-4b03-bff8-7f05d10909d6")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8df2af0c-20ca-4866-87ac-e7c89379e1cb")
		)
		(fp_line
			(start -1 0.6)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "231f30c1-b0b9-447c-9313-a1131089a3ed")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "79b2f0b8-330c-4cef-a68b-6e7bb64babf6")
		)
		(fp_line
			(start 1 0.6)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "740476fd-0e61-4070-b29c-5a3428f5e908")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c4607152-8e19-43f3-bf2f-eb571ec07ab9")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 3 "VDD_NRF")
			(pinfunction "1")
			(pintype "passive")
			(uuid "b9efac7b-53d1-4971-8674-305c244ae806")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 102 "Net-(U3-L)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "f1e8139b-c4c6-441f-a433-fe2956d45eac")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:Texas_R-PDSO-G6"
		(layer "F.Cu")
		(uuid "dfd78c95-1f54-4869-bb1e-07305d12d946")
		(at 168.1 120.56)
		(descr "R-PDSO-G6, http://www.ti.com/lit/ds/slis144b/slis144b.pdf")
		(tags "R-PDSO-G6 SC-70-6")
		(property "Reference" "U3"
			(at 0 -2.25 0)
			(layer "F.SilkS")
			(uuid "61f289f6-fd1b-4ce2-ba08-0b41d81cf0c8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TPS61220DCK"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "8f042aa5-1037-4aec-a81a-5de73cd366f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61220.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d43c3536-5b8d-41be-8919-d89eb1ddbf23")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a03d96ff-3749-4fa7-b490-555fc28f7861")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C116461 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "59f8c20e-48ea-4f7e-8838-df098a489089")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ed3b1980-0982-4419-9a4b-50034d3893af")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2d7f31dd-7729-4e3f-b2c6-f6b2d8bd0bea")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Texas*R*PDSO*G6*")
		(path "/57949f98-963c-4677-a24d-43c4f416800c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.7 -1.16)
			(end 0.7 -1.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "15a06fb1-297d-4fef-b8b7-2a1e5c862072")
		)
		(fp_line
			(start -0.7 1.16)
			(end 0.7 1.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f930ea76-7afa-40a2-ab89-8633e8c0e9c8")
		)
		(fp_poly
			(pts
				(xy -1.12 -1.11) (xy -1.36 -1.44) (xy -0.88 -1.44) (xy -1.12 -1.11)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "7f22b4f8-1ea6-4d1c-ae97-2d3a9e0a5986")
		)
		(fp_line
			(start -1.6 -1.4)
			(end -1.6 1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b4d9d259-36c8-4c74-be6d-c06bb99a9081")
		)
		(fp_line
			(start -1.6 -1.4)
			(end 1.6 -1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8c857675-ad93-473b-acd0-5f1e2adb9792")
		)
		(fp_line
			(start -1.6 1.4)
			(end 1.6 1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7b9cdc3e-4022-4890-abb8-1ff859db1804")
		)
		(fp_line
			(start 1.6 1.4)
			(end 1.6 -1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a3fd934c-7d4b-4678-bce0-0c24716c1dfe")
		)
		(fp_line
			(start -0.675 -0.6)
			(end -0.675 1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4b63214e-e97a-4e5d-8e46-33e39d8cb317")
		)
		(fp_line
			(start -0.175 -1.1)
			(end -0.675 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb561f18-f562-429f-a641-e3c16b311d6e")
		)
		(fp_line
			(start 0.675 -1.1)
			(end -0.175 -1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5cda036c-79a4-4dd4-bf29-7788ca975dc6")
		)
		(fp_line
			(start 0.675 -1.1)
			(end 0.675 1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "faea2429-64c3-4fcb-ba8e-eb0324d5bfa6")
		)
		(fp_line
			(start 0.675 1.1)
			(end -0.675 1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c03fd2f-209f-47b5-a956-aba262a366b9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "2152d17d-9c64-4c3b-a09a-eec694d7c0bd")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.075)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1 -0.65)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VDD_NRF")
			(pinfunction "VIN")
			(pintype "power_in")
			(uuid "28aaabf0-ef7e-40c3-bcf9-7723148b4864")
		)
		(pad "2" smd roundrect
			(at -1.1 0)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "Net-(U3-FB)")
			(pinfunction "FB")
			(pintype "input")
			(uuid "f1ba992a-f455-485f-a107-f7e41c620d83")
		)
		(pad "3" smd roundrect
			(at -1.1 0.65)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "80d12199-15ca-450b-b2b7-247faa949578")
		)
		(pad "4" smd roundrect
			(at 1.1 0.65)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "+4V")
			(pinfunction "VOUT")
			(pintype "power_out")
			(uuid "b23972ac-9c7e-4aa3-b24b-c2491e50c2b4")
		)
		(pad "5" smd roundrect
			(at 1.1 0)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "Net-(U3-L)")
			(pinfunction "L")
			(pintype "power_in")
			(uuid "992dcaa5-8e62-4ebc-9bcf-01eb39ce81c6")
		)
		(pad "6" smd roundrect
			(at 1.1 -0.65)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VDD_NRF")
			(pinfunction "EN")
			(pintype "input")
			(uuid "09ff3de9-3bec-4aa9-b255-5d58f65eb5c8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "e10c70e8-9487-4208-b513-ffc5bd795eca")
		(at 163.235 72.645)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D5"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "bd30a861-0393-4e6b-91db-64a268ca63fe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "f76922f3-c2e1-4290-b199-999a397537e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a3c4e003-94fc-4553-bfce-e22dd0207763")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3acdd9e9-291e-478e-934f-7db7ff9fc55a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/56bc0c52-daf5-4ecb-a971-5c95b80418d4")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4618ecdb-caf2-4555-a2ea-a6733c4af29f")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8231f286-e728-4a5d-a3a1-b1e781c4b2d4")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "acea0834-936d-4d52-a9c0-ac59ec0158d7")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b7c8085f-1fae-42ea-8a73-3669f2ed951b")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fdffeeb6-524a-4cb5-aaf4-7d1afd79c6f6")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "65e5ccfd-3c7e-4621-8342-4ead5737d74a")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6f60a43-c00e-4bd9-807d-2c2d92ddb2fe")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b4d465e-5133-43e1-baec-d5cbeb91955b")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5869aa63-14ae-493e-9060-e97a33c7c3a5")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1d25018-7cfc-4897-8ca0-d3984bb0fd4e")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "939a6d23-028a-4f83-99d9-e55bd809765d")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4efc1744-8aef-4870-825f-ccb684736f8d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2afd43bb-cb25-41ef-b644-3714369cab57")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 34 "Net-(D5-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "e7d6eb59-a8a2-4257-b10b-35b01f832d77")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 33 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "8dc25c47-400a-457d-bb7c-81d8bac985e0")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_EH_S2B-EH_1x02_P2.50mm_Horizontal"
		(layer "F.Cu")
		(uuid "e35c1241-c17a-4cba-b7fd-8aa012489e63")
		(at 140.3 90.8)
		(descr "JST EH series connector, S2B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH horizontal")
		(property "Reference" "J5"
			(at 1.25 -7.9 0)
			(layer "F.SilkS")
			(uuid "76f4ba27-dd82-4303-aaa5-5258f354dddb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.25 2.7 0)
			(layer "F.Fab")
			(uuid "6719430c-8840-4ac1-92dd-10e3a2be8592")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "086e92a9-d7d1-4cb7-bcfa-2870df060a33")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "52b9d0e7-c4c0-4c8d-b166-4b60faa33589")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c3dd85a8-fc5c-431c-88b2-2517edeb091d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e7a89742-1430-4476-b0d7-7906ccf0938d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/c0c3a649-79ab-4678-864b-8669333c8153")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.61 -6.81)
			(end 5.11 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "36439302-40bf-4861-96eb-cfc61a896f92")
		)
		(fp_line
			(start -2.61 -5.59)
			(end -1.39 -5.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7f8ed94b-1da6-485e-a9f7-6ec01b0952e4")
		)
		(fp_line
			(start -2.61 1.61)
			(end -2.61 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84bc373f-7ea7-4449-b4e0-28b18c4e043e")
		)
		(fp_line
			(start -1.39 -5.59)
			(end -1.39 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a75f1b0a-793d-44ce-bfea-bf5827b9a5be")
		)
		(fp_line
			(start -1.39 -1.59)
			(end 3.89 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fd57b0fc-cb5e-455c-9cee-7144b46b0471")
		)
		(fp_line
			(start -1.39 -0.59)
			(end -2.61 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "32f97038-e324-4a68-b0be-dd3ee872b4e9")
		)
		(fp_line
			(start -1.39 -0.59)
			(end -1.39 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "efa19668-bd04-4344-b185-4d92343cb07a")
		)
		(fp_line
			(start -1.39 1.61)
			(end -2.61 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2ce60b88-ec32-4a14-950d-ae0adda446a1")
		)
		(fp_line
			(start -0.32 -5.01)
			(end 0 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e66196bb-4505-41ac-b5bc-a317f4a810dc")
		)
		(fp_line
			(start -0.32 -1.59)
			(end -0.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a7b77c66-a03e-473c-990f-580c01d2fe6e")
		)
		(fp_line
			(start -0.3 2.1)
			(end 0.3 2.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e23f615c-f6e0-4728-82c7-84811177ddca")
		)
		(fp_line
			(start 0 -5.09)
			(end 0.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6a8eac08-e452-4f5c-bb04-c63eed96331a")
		)
		(fp_line
			(start 0 -1.59)
			(end -0.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6de7658e-057b-478f-a39a-50a9842c449e")
		)
		(fp_line
			(start 0 1.5)
			(end -0.3 2.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d58140a-9a50-499a-b3b1-fc747842df0d")
		)
		(fp_line
			(start 0.3 2.1)
			(end 0 1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f14c8664-44e8-46b5-8a3c-d97ae46ed507")
		)
		(fp_line
			(start 0.32 -5.01)
			(end 0.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22e7b54a-f6d7-4f0b-86bc-6ac93529705f")
		)
		(fp_line
			(start 0.32 -1.59)
			(end 0 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9812264c-4df3-46ed-a0d6-a20b2a6ae32a")
		)
		(fp_line
			(start 1.17 -0.59)
			(end 1.33 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "027493f3-c55a-483e-ba99-ded880b56845")
		)
		(fp_line
			(start 2.18 -5.01)
			(end 2.5 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "344a8fcb-fa47-4a09-96a7-92c6ee80d75a")
		)
		(fp_line
			(start 2.18 -1.59)
			(end 2.18 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa8cbbb9-859c-4157-8f2e-3c38492ff92c")
		)
		(fp_line
			(start 2.5 -5.09)
			(end 2.82 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "196f55ac-ae52-4af6-b5c2-7b928ec4bd73")
		)
		(fp_line
			(start 2.5 -1.59)
			(end 2.18 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "13890250-1d41-499f-918b-efc06f396690")
		)
		(fp_line
			(start 2.82 -5.01)
			(end 2.82 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "261af30a-df1e-428d-a72f-65e1f72b81d1")
		)
		(fp_line
			(start 2.82 -1.59)
			(end 2.5 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3ecec0be-cb7f-4c7b-a045-3ceab7a1b939")
		)
		(fp_line
			(start 3.89 -5.59)
			(end 3.89 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b1ebdba-0fa3-40e2-b63f-149e2c8a3f80")
		)
		(fp_line
			(start 3.89 -0.59)
			(end 5.11 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "550d5dd2-6b0f-47c3-b585-511b0d99bbf2")
		)
		(fp_line
			(start 3.89 1.61)
			(end 3.89 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5d8844e0-31ec-4a15-b0b3-0795df747d8b")
		)
		(fp_line
			(start 5.11 -6.81)
			(end 5.11 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f6f0e5d-1f05-4857-829a-57fbb30b8c28")
		)
		(fp_line
			(start 5.11 -5.59)
			(end 3.89 -5.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "98d211eb-0a88-41bf-9156-84b254584cfc")
		)
		(fp_line
			(start 5.11 1.61)
			(end 3.89 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2e6b0604-77de-49f1-b29b-fc09a28e3f20")
		)
		(fp_line
			(start -3 -7.2)
			(end -3 2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8a332688-ad9e-49fa-9d35-220fecc80958")
		)
		(fp_line
			(start -3 2)
			(end 5.5 2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a2de43c2-b28d-4a01-bf03-ffd203d87faa")
		)
		(fp_line
			(start 5.5 -7.2)
			(end -3 -7.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e41e1ad-e17e-48be-a030-9750c26ff33b")
		)
		(fp_line
			(start 5.5 2)
			(end 5.5 -7.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0c994a19-709f-4401-9af7-7a27f97b078b")
		)
		(fp_line
			(start -2.5 -6.7)
			(end 5 -6.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "97000fb7-30b7-4e85-b4c4-25ee1bce3dc1")
		)
		(fp_line
			(start -2.5 1.5)
			(end -2.5 -6.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "95a5e717-4416-499c-850c-375f089ab728")
		)
		(fp_line
			(start -1.5 -0.7)
			(end -1.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "484a5c64-6d5e-41dc-be78-baa502dc9b79")
		)
		(fp_line
			(start -1.5 1.5)
			(end -2.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c9c3541-36fb-4317-b543-8133445f4be4")
		)
		(fp_line
			(start -0.5 -0.7)
			(end 0 -1.407107)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83b947b3-c30d-4aa9-aa27-be813452d763")
		)
		(fp_line
			(start 0 -1.407107)
			(end 0.5 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "79a340fc-21fa-4bc8-be84-c43ca6e2e6a5")
		)
		(fp_line
			(start 4 -0.7)
			(end -1.5 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c0e38c41-67b3-4df0-8604-5e8fb259536e")
		)
		(fp_line
			(start 4 1.5)
			(end 4 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "62655cdf-8a48-4878-a2e6-44fd43389e6f")
		)
		(fp_line
			(start 5 -6.7)
			(end 5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7bfc8168-ecfd-407c-b54c-34dbc05641d7")
		)
		(fp_line
			(start 5 1.5)
			(end 4 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "12364ae7-bbff-4f88-a36d-6ce86ce4c897")
		)
		(fp_text user "${REFERENCE}"
			(at 1.25 -2.6 0)
			(layer "F.Fab")
			(uuid "9fe02c06-554c-4ed3-852d-1a835d0fe0a9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 94 "Sol Shunt 1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "c221996c-3424-49ac-96fd-b92a30561d29")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "8dc3d274-f2d8-47b5-b00a-9f895a497590")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_S2B-EH_1x02_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "e3cfcdeb-281e-47dd-98d1-e20f090429ad")
		(at 139.25 72.54)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C20"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "f063cdb6-5dbf-4c68-a0dd-4ad6cad9a3ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "220nF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "f2ec722c-3e15-49f3-94ae-aa32473cc282")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9a91dacd-42db-4330-8177-8317f78b654a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e3f55cf5-02cb-4674-b8aa-7043b74130c8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/38788ddc-4ba6-4b44-a7a2-2d76cb4fe9f9")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dfe03cf7-05a8-4b61-ae1e-f4b8ce49e069")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9d928b00-8454-43d2-8bc2-16e0cc91a805")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "650a9985-0989-4fdc-a330-89a3b6eb51ea")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ce040182-c6cd-479e-b4e1-031a08a5efd5")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "918174fc-93c0-491d-87bc-08e26e9906b6")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dae6229a-262d-4527-8098-2e4886a9fcbf")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "adc350f1-a4c4-4465-b8c4-fb9b78626a2b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d885ea2b-b036-4740-b070-6b73ac8fea82")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "393cd97b-23da-40fc-bde2-f5a1aba8c2b4")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ffb24b4e-e0ae-47bf-a38a-de266a93edb5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "611700d1-e6fb-4994-a96e-229fe9d12df2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "daa32b6c-40b5-4548-b02f-ad682ee2f69f")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 10 "Net-(C20-Pad2)")
			(pintype "passive")
			(uuid "2a48121d-9a6a-42ab-bfb0-965a1467175d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_C_Receptacle_G-Switch_GT-USB-7010ASV"
		(layer "F.Cu")
		(uuid "e43d06aa-d6b2-4f1c-bd22-a7dbd19e6ed5")
		(at 159.17 98.83)
		(descr "USB Type C, right-angle, SMT, https://datasheet.lcsc.com/lcsc/2204071530_G-Switch-GT-USB-7010ASV_C2988369.pdf")
		(tags "USB C Type-C Receptacle SMD")
		(property "Reference" "J1"
			(at 0 -5.5 0)
			(layer "F.SilkS")
			(uuid "19c095e9-ea73-4faa-921a-5004fcfc3bb2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "USB_C_Receptacle_USB2.0"
			(at 0 5 0)
			(layer "F.Fab")
			(uuid "8efceaf0-f866-4a79-83b0-68f8a6c4caf6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3d521721-10be-47dd-96a8-56a5b2390266")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2e2887fb-e38a-4a6e-aa1b-44344f6a0d4d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(path "/853cd093-ee5d-412d-acaf-339a7c25043c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.58 -1.85)
			(end -4.58 0.07)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bcc69cb5-f846-4caf-8495-6dec9c49ac5e")
		)
		(fp_line
			(start -4.58 3.785)
			(end -4.58 2.08)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "21a2254c-f665-4ba9-9158-30c2a06ff685")
		)
		(fp_line
			(start 4.58 0.07)
			(end 4.58 -1.85)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e9846fd2-b0a7-44f1-8728-4df838496709")
		)
		(fp_line
			(start 4.58 2.08)
			(end 4.58 3.785)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91c45ea7-6b22-4835-a1a3-bace2f1cdb8f")
		)
		(fp_line
			(start 4.58 3.785)
			(end -4.58 3.785)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d97bd258-3a09-4c0e-a02e-65c2013fa6bc")
		)
		(fp_line
			(start -5.32 -4.85)
			(end 5.32 -4.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c52af991-973f-42f0-8ef3-e4fe0405444b")
		)
		(fp_line
			(start -5.32 4.18)
			(end -5.32 -4.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f99b7a67-b16b-412e-a856-1b509b51281b")
		)
		(fp_line
			(start 5.32 -4.85)
			(end 5.32 4.18)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9b002907-1713-4b9d-b370-528502d37c55")
		)
		(fp_line
			(start 5.32 4.18)
			(end -5.32 4.18)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c53152b7-2076-4c90-ae17-6ca2ae883c72")
		)
		(fp_line
			(start -4.47 -3.675)
			(end -4.47 3.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6814f43c-99d4-4c0e-94cd-cf02b4a94401")
		)
		(fp_line
			(start -4.47 -3.675)
			(end 4.47 -3.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7a10b4f-fd71-4ea6-9438-c88c3ebf5962")
		)
		(fp_line
			(start -4.47 3.675)
			(end 4.47 3.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d5b3fa3-1d4b-4f34-b33e-055e412e01a2")
		)
		(fp_line
			(start 4.47 3.675)
			(end 4.47 -3.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5656e83e-6f65-4f86-ac1c-6eba6c01bf80")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "002b5dd7-a93a-41ad-8ed0-4b376d1fd8f2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -2.89 -2.605)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(uuid "d1774aa3-efbb-45eb-8dfa-a277193f2de0")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -2.605)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(uuid "70bfc274-e463-4852-8941-16894b863fb7")
		)
		(pad "A1" smd rect
			(at -3.2 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "f4a1979f-76c9-4216-baef-6e7ff36be153")
		)
		(pad "A4" smd rect
			(at -2.4 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "adc811f8-0cbd-4188-8b99-2e20edc6b12b")
		)
		(pad "A5" smd rect
			(at -1.25 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "CC1")
			(pinfunction "CC1")
			(pintype "bidirectional")
			(uuid "8b991c7a-4c42-4b4d-819e-c103cac8931c")
		)
		(pad "A6" smd rect
			(at -0.25 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "Net-(J1-D+-PadA6)")
			(pinfunction "D+")
			(pintype "bidirectional")
			(uuid "933ba3af-efef-4264-8b30-cb1ab60a0271")
		)
		(pad "A7" smd rect
			(at 0.25 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(J1-D--PadA7)")
			(pinfunction "D-")
			(pintype "bidirectional")
			(uuid "08b1b9aa-03a8-4531-92ff-30cb60167efb")
		)
		(pad "A8" smd rect
			(at 1.25 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "unconnected-(J1-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
			(uuid "4b7b342f-1917-474d-ac86-bb9ffb20199d")
		)
		(pad "A9" smd rect
			(at 2.4 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "160d21c2-acb6-48e9-bb56-742c4303b309")
		)
		(pad "A12" smd rect
			(at 3.2 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "cc74d49e-a429-4fe3-8be8-56a0240083f0")
		)
		(pad "B1" smd rect
			(at 3.2 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "9755e0a4-259a-4709-b986-c880327c259d")
		)
		(pad "B4" smd rect
			(at 2.4 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "2b533fec-2dfb-4945-8ac1-c40e0a9e1ee2")
		)
		(pad "B5" smd rect
			(at 1.75 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "CC2")
			(pinfunction "CC2")
			(pintype "bidirectional")
			(uuid "812dc8ed-5bcf-461b-9aeb-b68ca95dcb14")
		)
		(pad "B6" smd rect
			(at 0.75 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "Net-(J1-D+-PadA6)")
			(pinfunction "D+")
			(pintype "bidirectional")
			(uuid "eb44f4f8-0f50-4cf1-9de3-16421e27122a")
		)
		(pad "B7" smd rect
			(at -0.75 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(J1-D--PadA7)")
			(pinfunction "D-")
			(pintype "bidirectional")
			(uuid "f4a39744-b53e-4c54-af18-fbbc664c8354")
		)
		(pad "B8" smd rect
			(at -1.75 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 90 "unconnected-(J1-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
			(uuid "b12ea455-d8d8-4f48-974b-2e08e1a8a3a3")
		)
		(pad "B9" smd rect
			(at -2.4 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "b9d234c1-761e-4ada-b581-f0e7a11a93db")
		)
		(pad "B12" smd rect
			(at -3.2 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "d04e487a-1441-437c-bc44-e70ee34e43aa")
		)
		(pad "S1" thru_hole oval
			(at -4.32 -3.125)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "f0780fa4-56e7-4e15-8cd8-82c49ffb4570")
		)
		(pad "S1" thru_hole oval
			(at -4.32 1.075)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "6ff911ba-aac8-49ff-a0c2-0c239695b054")
		)
		(pad "S1" thru_hole oval
			(at 4.32 -3.125)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "479e97e0-e150-47d7-9a55-09a3e545fbc4")
		)
		(pad "S1" thru_hole oval
			(at 4.32 1.075)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "dcf540c4-8afa-4590-b47b-692ef7eb812f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_G-Switch_GT-USB-7010ASV.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic:SOT65P210X110-6N"
		(layer "F.Cu")
		(uuid "e4a37f8e-0723-4080-915a-ae9a7c8ae09d")
		(at 167.955 67.63)
		(descr "SC - 70")
		(tags "Switch")
		(property "Reference" "S2"
			(at 0 0 0)
			(layer "F.SilkS")
			(uuid "0ce2d70d-0831-4640-8479-aa2eec31069f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "MASWSS0136TR-3000"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "0f25faa5-b93d-4e38-9cfb-a695ef68de9a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" "https://rs.componentsearchengine.com/Datasheets/1/MASWSS0136TR-3000.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4524f5a3-407a-4014-a0df-afb92612dc2d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "RF Switch ICs DC-3.0GHz ISO 27dB IL .4dB @2.4GHz"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "28d17121-528e-464e-a6b9-3028d0b0706a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "1.1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3507333c-4bb9-445e-8c44-168bf443a8ff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "MACOM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "27f89fb7-766a-4495-a777-b5c9c682731f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "MASWSS0136TR-3000"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "141f7f67-ae3c-4c86-a05e-24c9b6e9acfc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" "937-MASWSS0136-T"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1d9af397-9a4c-4784-aaeb-8036992961b5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/MACOM/MASWSS0136TR-3000?qs=3Wmz%2FrCSAaHZLGvANOUDKw%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7c75ec58-2e4d-46ef-abd6-9e06b906d43b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "faa642c9-544a-4f92-9edf-7ae5b055502d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a59962b9-045d-45c3-8e31-73302adafe02")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/4edca5e9-b778-49a2-af05-55e7448a9b06")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.575 -1.2)
			(end -0.425 -1.2)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d7fd3f8e-83d0-4460-ae05-cfa60e792689")
		)
		(fp_line
			(start -0.075 -1)
			(end 0.075 -1)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49c44a8e-8328-4816-9541-a6281fc67eeb")
		)
		(fp_line
			(start -0.075 1)
			(end -0.075 -1)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "71be2105-92a0-494a-b846-2b072f2644f0")
		)
		(fp_line
			(start 0.075 -1)
			(end 0.075 1)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a309241c-c984-4b67-b312-792f038d4e1b")
		)
		(fp_line
			(start 0.075 1)
			(end -0.075 1)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c9ae280e-12fc-4700-a4bc-0e7d21f84ceb")
		)
		(fp_line
			(start -1.825 -1.35)
			(end 1.825 -1.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ead1c8fd-09db-4d5e-a38b-5134dbe8e341")
		)
		(fp_line
			(start -1.825 1.35)
			(end -1.825 -1.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7bec18c6-d757-47e7-b998-265f4e29bcb8")
		)
		(fp_line
			(start 1.825 -1.35)
			(end 1.825 1.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dfa1903c-3927-4f72-97e5-1784c864c53c")
		)
		(fp_line
			(start 1.825 1.35)
			(end -1.825 1.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8a5f6814-d30c-4f1b-8488-3814e1644350")
		)
		(fp_line
			(start -0.625 -1)
			(end 0.625 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f30b51a8-9dd5-421e-94a6-d8b92ae7554e")
		)
		(fp_line
			(start -0.625 -0.35)
			(end 0.025 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e47a19cc-cf8e-4bb6-97c9-e2fb605e0cbf")
		)
		(fp_line
			(start -0.625 1)
			(end -0.625 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f8ed4c5-d892-4473-adbb-4cc2f21a0a44")
		)
		(fp_line
			(start 0.625 -1)
			(end 0.625 1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "91f2de73-afb1-4545-bcdf-36294214d1fe")
		)
		(fp_line
			(start 0.625 1)
			(end -0.625 1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d2b33741-7273-41ec-8769-15a4df6c81fd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "860afae7-5e19-4739-acb9-d1783c6cfe87")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -1 -0.65 90)
			(size 0.4 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(S2-RF1)")
			(pinfunction "RF1")
			(pintype "bidirectional")
			(uuid "fcc36a61-3db4-4255-90d3-0041c1d92e55")
		)
		(pad "2" smd rect
			(at -1 0 90)
			(size 0.4 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "c3d906e3-b2c5-4f2e-8e49-39cd5abee174")
		)
		(pad "3" smd rect
			(at -1 0.65 90)
			(size 0.4 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(S2-RF2)")
			(pinfunction "RF2")
			(pintype "passive")
			(uuid "ab98c8c5-09e5-489d-a73c-1fbfab471d6a")
		)
		(pad "4" smd rect
			(at 1 0.65 90)
			(size 0.4 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 118 "RADIO RX")
			(pinfunction "V2")
			(pintype "input")
			(uuid "0fe7e844-3b9e-415f-acde-e60d5edae2f9")
		)
		(pad "5" smd rect
			(at 1 0 90)
			(size 0.4 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(S2-RFC)")
			(pinfunction "RFC")
			(pintype "bidirectional")
			(uuid "44c51a72-3f63-41e2-a49d-dca73e1deca9")
		)
		(pad "6" smd rect
			(at 1 -0.65 90)
			(size 0.4 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "RADIO TX")
			(pinfunction "V1")
			(pintype "input")
			(uuid "94d76b37-9cde-4073-8987-5169a6374fce")
		)
		(embedded_fonts no)
		(model "MASWSS0136TR-3000.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "e569dba5-fffe-4c42-8e04-f9465cac507a")
		(at 124.85 63.48)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R27"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "f783b594-8289-43e3-a011-622974502d40")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "23.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "ec85aea3-c834-4882-8e77-ef144861a797")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "026f120e-c404-4761-8cef-7eb073c4bc4c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "97008435-343e-42fb-b2d1-0d35b9a9ceeb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/ec5b8e2a-c0a4-4c3a-8f84-ad1f8af688f8")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cc5cb7d7-5d5f-4010-bd68-08491d3e97a8")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49b0ea94-43bd-4534-aaed-481d9e36c2c7")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "387d795a-3545-473e-9fe5-b630e8f6a50a")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "78b012b8-803b-44d0-bb86-c8f0e05a1961")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8560e25d-4532-4f71-9c8d-d832191fccf4")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2a8d10ac-ef20-4ddb-ae9a-5c0b1ebdcf75")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a602585b-ac5a-47c7-8d8f-bb69b17acd29")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d38e558-8aad-4ce7-bee2-508f30c10e15")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0159815c-55af-453d-a27c-134a085b26cc")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "88e8a209-2038-417e-b15b-19ccf0625992")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "06a18d04-6e1a-49af-91ba-24657e442522")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 8 "Bat Shunt 1")
			(pintype "passive")
			(uuid "8f0c9c54-1ea3-4809-bef1-365c2fba736b")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 115 "Net-(R27-Pad2)")
			(pintype "passive")
			(uuid "1fd357e5-3c7c-4d7e-86f6-5906b7c54f61")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(uuid "e6ff602f-1048-40b5-8847-d7e0f627ec20")
		(at 123.04 95.17)
		(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
		(tags "sma edge")
		(property "Reference" "J3"
			(at -1.5 7 0)
			(layer "F.SilkS")
			(uuid "91497d83-7b96-473e-a35d-8f0ea8ff922f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_Coaxial_Small"
			(at -1.72 -7.11 0)
			(layer "F.Fab")
			(uuid "bf0652c6-bb7a-429e-b96c-47630d7c2912")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dcdf7a36-44f0-4661-a04a-c3fddc5e8e88")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "small coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a4fd748d-b318-4a6b-8e94-ce0689dacb5d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(path "/a7ac3701-5e8c-4217-b013-0d1ec42aee30")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start 2 0)
			(end 2.5 -0.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91442011-c2b0-4ed8-8c39-540e9fe7dbd2")
		)
		(fp_line
			(start 2.5 -0.25)
			(end 2.5 0.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9812da49-4673-4911-8de4-c5af8df281cb")
		)
		(fp_line
			(start 2.5 0.25)
			(end 2 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b6765a6d-e825-4b38-b597-302cab7daf26")
		)
		(fp_line
			(start -14.29 -6.09)
			(end -14.29 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "53b40a4d-347e-4dff-924e-6aed5c2ccec3")
		)
		(fp_line
			(start -14.29 -6.09)
			(end 2.71 -6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "a5aa2b9a-8d33-4d1f-a57f-3f25a5a12f8b")
		)
		(fp_line
			(start -14.29 6.09)
			(end 2.71 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "7daf6b0a-6a00-4649-8cc5-00ff9d0bff84")
		)
		(fp_line
			(start 2.71 -6.09)
			(end 2.71 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "86112aa3-ebb5-4601-81fe-ae4fc2171c64")
		)
		(fp_line
			(start -14.29 -6.09)
			(end -14.29 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07bda8de-c4a6-4c70-8ba8-8c5175cd027e")
		)
		(fp_line
			(start -14.29 6.09)
			(end 2.71 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a4e2fd4f-4ce8-4251-ade1-33cacc7615ed")
		)
		(fp_line
			(start 2.71 -6.09)
			(end -14.29 -6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "05b94731-16ae-4073-9039-7c952991d27e")
		)
		(fp_line
			(start 2.71 -6.09)
			(end 2.71 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f6535b29-9b27-49d5-bdec-70f0c823c3c5")
		)
		(fp_line
			(start -13.79 -2.65)
			(end -13.79 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "604f40d0-75bd-4e02-bb35-21d7a1327b9a")
		)
		(fp_line
			(start -13.79 -2.65)
			(end -5.91 -2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da1b0efa-286f-4290-862a-4e4b7ed877d5")
		)
		(fp_line
			(start -13.79 2.65)
			(end -5.91 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "445b04d0-a2c7-4a49-b5cc-998ed2890069")
		)
		(fp_line
			(start -5.91 -4.76)
			(end -5.91 4.76)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de6b74bf-b400-4ac6-9719-602cb747aaa8")
		)
		(fp_line
			(start -5.91 4.76)
			(end 0.49 4.76)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "94eee473-4c3b-4914-ada4-c0359a009001")
		)
		(fp_line
			(start -4.76 -3.75)
			(end -4.76 3.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6caa497d-9f52-4d20-a16a-cd739456dd01")
		)
		(fp_line
			(start -4.76 -3.75)
			(end 0.49 -3.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b14f46dc-0e85-4334-938c-d673c467e34d")
		)
		(fp_line
			(start -4.76 -0.38)
			(end 0.49 -0.38)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c18aef7-66a4-44b1-8da7-f476f6ebbc0d")
		)
		(fp_line
			(start -4.76 0.38)
			(end 0.49 0.38)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0466eb89-d75b-421d-bdad-827564704572")
		)
		(fp_line
			(start -4.76 3.75)
			(end 0.49 3.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a297da69-504c-4e54-9644-4f5d95a9c5f8")
		)
		(fp_line
			(start 0.49 -4.76)
			(end -5.91 -4.76)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d396252f-ab2b-4477-8512-1693916876bc")
		)
		(fp_line
			(start 0.49 -4.76)
			(end 0.49 -3.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "29d00bd2-f0d0-4170-b90e-1a463e46724f")
		)
		(fp_line
			(start 0.49 -0.38)
			(end 0.49 0.38)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17418c08-0680-43e6-8aa2-c9888ca77e24")
		)
		(fp_line
			(start 0.49 3.75)
			(end 0.49 4.76)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d41238c-c4e4-46ef-b147-99b96ecefd4b")
		)
		(fp_line
			(start 2 0)
			(end 2.5 0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4af3fecc-4b60-4816-a295-9f89bbf23f4c")
		)
		(fp_line
			(start 2.5 -0.25)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9c2ac913-6c43-4dc6-88b9-20d90129b386")
		)
		(fp_line
			(start 2.5 0.25)
			(end 2.5 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c07fa23a-836d-4bc6-bd93-5855b0fd5d8b")
		)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 0)
			(layer "F.Fab")
			(uuid "724de8b6-cbd7-4ad6-a0b4-2fda180222a1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -1.72 0)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(J3-In)")
			(pinfunction "In")
			(pintype "passive")
			(uuid "814f529e-d3d4-435c-8876-0a3446e54f3e")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "e4a2b64a-34ee-4c42-b13e-e1691e23bee3")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "0367c163-d129-4338-87a2-c7f862314746")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "98402110-f76e-42a7-a33d-3a828e3ec76c")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "40e82f2e-8a06-4ee3-9cea-7cc1920bb32d")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "4f55e213-6581-4768-981b-43b5bc56532e")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "88869841-12a7-4137-99e7-b850247e1701")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "3f18642b-0c19-45ce-bc70-59eb04cff6c6")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "6956d8e1-27f6-43f2-84f7-a1d434bd6b14")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "c34fe25f-f712-4b76-b6af-ba2670886db9")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "ae990316-c4a9-49f5-8245-874d83e7d38a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "e8c9ba63-9770-4226-bc24-2a63b976a7f2")
		(at 142.8 110.11)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C41"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "fb9c7cb0-8c01-4de3-8e05-0c755fb4de45")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "3c162b87-0337-4130-9c29-b70dc12486e3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "31417cb9-1d67-4e8b-8240-c425b178b9c0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "977658dc-ffc9-4071-9389-27ec9d7ea5bb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/6273f0e3-803a-4b77-95be-6ece6b380a79")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "936a4628-e2ab-4443-89d5-0eafe9b333df")
		)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e128ee0e-9180-4218-84cb-f8245e137834")
		)
		(fp_line
			(start -1.65 -0.73)
			(end 1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "993f095e-be31-4305-891f-d228b8faa0b9")
		)
		(fp_line
			(start -1.65 0.73)
			(end -1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fc50673a-259f-4bd5-8e62-924a09aa5c79")
		)
		(fp_line
			(start 1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bc84bede-690c-4d24-b43c-e2b7fb4b2104")
		)
		(fp_line
			(start 1.65 0.73)
			(end -1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6c9bcf28-68f0-4afe-9598-962326c4f230")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ffdaf797-4024-4f09-b221-177ddb1b49c1")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "65a57d9f-bb76-42fc-949b-efbff21629da")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d27bf877-7f4e-4d16-80a4-7c1548439163")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81d8214c-2e36-46d9-b48c-65ed7f4e6aac")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "159542d4-7a4f-4aa8-9d65-d7208881a46c")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(S1-RF2)")
			(pintype "passive")
			(uuid "42a866b5-b903-421b-bfe8-ac5247c2caeb")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(S2-RFC)")
			(pintype "passive")
			(uuid "bc02653a-dce8-43cc-b936-66d8c79bb13d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "ead047e2-3a61-4f7b-b61b-04091c0a6d9c")
		(at 110.6 63.48)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "inductor handsolder")
		(property "Reference" "L2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "2808f918-7887-4d1c-8eaf-24ee7a5d32b1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uH"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "dc49c852-e3cd-4c04-90f3-587b90b1b425")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4dd489e3-3733-4d79-989f-12aa57d419e2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "645097ee-7ac3-4657-b91b-cbbd1a9cc5ef")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/379428d7-d65e-424e-af84-990a0ccbcc2f")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.71)
			(end 0.261252 -0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "619b1acb-00d6-4185-a9d0-1b295342acf2")
		)
		(fp_line
			(start -0.261252 0.71)
			(end 0.261252 0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "55b58d5b-8df2-448b-981e-dfa80ae8042b")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8a2db4b-011b-452c-a28e-bcbd42501abd")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ca04fe8a-d85e-46b0-ac15-ab557381a6f3")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f3e2f49b-8490-409c-8e2b-ee1b26adf854")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bf7a903e-e132-4f64-9c15-f6af514a72c3")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3a804c19-20b5-4f81-bd90-771cfd775968")
		)
		(fp_line
			(start -1 0.6)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4b58d0ac-9fcc-4ca7-bfc4-8c0a6fa670d1")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f7f8c16-a7b4-468f-b737-49ce7c885a74")
		)
		(fp_line
			(start 1 0.6)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "05d4baf8-c003-43e3-8f45-04150d5eeae5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b0d9b1be-1b9b-4b6d-b89a-473e3a13f305")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 35 "Net-(D6-K)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "991f27b5-2ab5-4385-8621-85cb14bd78fe")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 47 "Net-(IC2-CSP)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "426cd8e4-3082-4eef-9281-b6e40f2e184d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "ec7bcc93-e184-401f-8aa8-9d39c73f4d08")
		(at 120.1 75.28)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R22"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "c142ea27-a4c7-4388-b643-6d5a3314dbd7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "c3e0215c-e991-4812-80c8-30b2e49a9114")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "153f1ee5-aa7d-49ee-9d1f-795bbb3d4b2d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b6db20c1-24cb-43db-9807-6cd99118d775")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/fcf2334e-e740-45e3-82e6-22af6b28ce73")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "973a41d2-00ad-44eb-89df-0fd3b7f446fb")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b8a7c99f-981f-417a-891b-b79ef8ee918e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "57f3f46b-3ae2-462d-b135-2437df83e2b0")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e9715794-1b0f-43af-a48e-4e2febbea460")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4cf6de52-de9b-4d62-a105-3b062dd36c0b")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ba9b520b-4d12-4b8a-93a5-c89a5f762801")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ff96ed8-b18c-44e8-a79a-4b0990351ad5")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7e2395d1-42d9-40fe-863a-29d0db54a33f")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4b473b23-6089-4ba4-a3b3-fd140a5ffa14")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "704fc359-d86e-4644-a11e-3591a1af058d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "17c4a493-ad4b-4136-8143-0b60e019ccfc")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 111 "USE_ANT_1")
			(pintype "passive")
			(uuid "f1b51d96-ecc3-4ddf-9443-a682556c7342")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "c952d56f-83cc-4e42-8dab-fb99fae58ee7")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "ef32d8bd-195d-43c1-b13e-4afbe1c386e5")
		(at 110.6 78.23)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "0ba402c1-139b-4ed5-9108-22cf86a5014b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "44c6d1c5-23be-47f6-8b44-5b2ef96a7623")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bfb6a619-de1e-4c4e-a476-f038d8e6dc79")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cecaed4b-22bb-44d2-9d50-180a0c409db7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/a4f26091-217a-4fcb-9585-739b8cb48c50")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49452a58-2208-4d9f-a20d-d984015e0475")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e86e155f-67d3-4b24-82e4-2d4c9461ef59")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c693ea1e-131c-4073-ab9b-ceb4eec80eda")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bd687ea9-4085-43e8-9dcb-32520fca8dfa")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "90d403be-dfe5-42c0-922b-0da3b4a9b981")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "be47cd23-6100-4f56-a93b-e7d20d846b2d")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d0ed50ad-bf29-4f48-adae-6805d05a24ef")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "03af6699-b58c-4b61-8f58-bc0f282d529a")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "65c2583a-5761-4932-9f3c-1571697bb6b1")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5e5def46-ed9a-4b02-bdd8-be3eccd78388")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "82246e20-758d-4876-8bcf-552157b51315")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 4 "Net-(IC1-VDD)")
			(pintype "passive")
			(uuid "113f1c16-6566-4f00-aef7-c3255003f6cb")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 30 "Net-(D1-A)")
			(pintype "passive")
			(uuid "4831d312-c486-4b61-8443-88bb0450977d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "eff72b5a-0d25-42d6-b554-94cbb97df7cc")
		(at 120.1 66.43)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R19"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "b0eff83e-35f3-489e-906b-6fe4aa9b7b45")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "85ebacda-c11b-4cd6-99ce-02377ab34e61")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6141465d-4270-4b3d-931b-99ebe2acc462")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "85f6ea06-0094-4994-9603-4b066aec4866")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/0a7f186c-c5d1-43dc-8b61-ead9cb92ffad")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "30b19390-4e9a-4164-9320-ecd89650aea8")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "324d9e62-d3b7-4527-9c55-e6e706bcab61")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "66c7390b-8751-4412-8a3d-8976f5f85d33")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b4202a1e-84c6-48e4-bdbc-fd443788ccbd")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7ec6a993-5e50-4271-8d4f-677f5107020c")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0b1e0faa-0f64-4c67-ab02-ab8a79c22971")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "71f613df-806b-4fbf-9483-6a2228d2952f")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5ccfb97f-e877-43e8-8cc2-0b44be302d9e")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cbf977c8-d575-40b9-9b14-833e3733874e")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2567e293-3f2a-4849-8fe5-74d8974bd949")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "34d11d97-ca2b-4483-8208-638d363359d0")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "aede7716-32ed-4425-b203-6a2a5bc9b8de")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 13 "USE_ANT_2")
			(pintype "passive")
			(uuid "767ee249-f72b-493f-8fd3-06b549e40b9e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "f0dd0dd3-3802-4d0a-be56-a9e38fb4ae13")
		(at 120.1 72.33)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R21"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "a301bd41-d5aa-440d-89c3-61a5af1a7277")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "700k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "d7257ce7-2fa5-4616-8137-5d77c1fce058")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e68f2387-e64c-4127-87bd-eeae608f9ae8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4868d889-6bfc-4bcf-a032-d904e3a6fa05")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/3685251d-c1a7-4ba5-96e8-2fa61160a79c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "566bd423-e148-4f41-9658-12dd6ad4d756")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a7407a47-b997-4997-970b-dd92048f48e2")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b1575c6-bfba-4ab3-bd81-e51ce0f3d719")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f00ea180-1415-445d-aca3-7bf0d0aa032c")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5ab6d287-e777-4e7e-ace0-d66e42306000")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c2fe92c5-ed9c-445c-adbe-1688547c935f")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f5caad38-f8a2-46ae-8bf8-a19f0b1590ad")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "efcbcb33-5026-400d-962e-38b3207d780f")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9d3236e-b10c-4351-beed-fbf560bc1322")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ce1f949-0468-4831-a929-03d72d57d76d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "21c28acf-6aad-4c30-9e4c-fd1b23e9e3cc")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 14 "+4V")
			(pintype "passive")
			(uuid "c8e6a9a8-3075-4199-8a1a-876709bf3502")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 110 "Net-(U3-FB)")
			(pintype "passive")
			(uuid "bd040c61-26df-434e-aba7-2cd320fda743")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "f46166d1-b005-4ff8-a36b-6293a26a611a")
		(at 142.8 107.6)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C36"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "43b09109-7b15-4ffc-9b86-c0487e8f1b96")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "daa9f0cb-d793-4038-b3f6-cb92cb11052d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6db2b4ae-061a-49e6-aa01-17283deb237a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "fc69a1c6-885f-40f3-8b78-d9e77b79f053")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/9ddf98a3-81fc-45d8-971f-a8860352e810")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5343aa2b-ebe9-4b71-8513-9588ead112b1")
		)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b605e378-26eb-4c4d-ad26-7bc54e1eb4f0")
		)
		(fp_line
			(start -1.65 -0.73)
			(end 1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ca063987-95c1-423c-8e45-44f9d8a189d4")
		)
		(fp_line
			(start -1.65 0.73)
			(end -1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ba43250-f9c4-4611-97fa-8a27bbce2ae0")
		)
		(fp_line
			(start 1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a69ff2de-ce69-4ea9-8727-24750c4b9fd2")
		)
		(fp_line
			(start 1.65 0.73)
			(end -1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "523fe2ca-37d0-4e6b-aa84-2cf0a8f47805")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46fff28f-9947-4af8-a4c9-9f515714fb6c")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e84d1087-1245-437a-80f2-2b7af0022cc3")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "89c4b012-7404-468d-a5d6-f4c96a796737")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be8d4ceb-2e72-4961-bab0-c407f8188072")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "42af189a-572e-446b-9977-2b5146e0c1db")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "RF_LORA")
			(pintype "passive")
			(uuid "7ca21621-b778-4a72-9e26-44ac723b0be3")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(S1-RFC)")
			(pintype "passive")
			(uuid "39b5949f-95b2-4770-b224-066edbe6cd8f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic:SOP100P600X180-11N"
		(layer "F.Cu")
		(uuid "f50cca02-c71a-4ea2-9326-473fa4c57c2f")
		(at 150.69 79.245)
		(descr "ESSOP10 (5*3.9mm)")
		(tags "Integrated Circuit")
		(property "Reference" "IC1"
			(at 0 0 0)
			(layer "F.SilkS")
			(uuid "f36c7d05-9fef-49b1-9ad8-e7579ba152d8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "CH224K"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "f270a071-61b2-4fd8-8f68-2408fffdd63e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2204251615_WCH-Jiangsu-Qin-Heng-CH224K_C970725.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a7b2ac5a-c33a-427a-b8a5-a62be193ce78")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "ESSOP-10 USB ICs ROHS"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f418acd3-2b6a-453b-947e-463207690ec0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "1.8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e646fadc-3561-4ba9-9709-296ee2e3e1d5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "WCH"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "989c3956-f46b-43fd-9a65-2152e927dbd3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "CH224K"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b09550d1-4056-4518-849a-b8768440e332")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f313dd20-ab50-4182-af2d-9e417564eebf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d775756e-1ccd-4817-a210-fb2cf8469026")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0046811d-fd27-473c-b3c2-3a7802d850f3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d41af79a-a491-4fe7-8526-ad9ff0cf3c81")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C970725"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6dbbd846-e83f-4b90-949e-3709aecd69f3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/e54b9406-6388-4ea0-9a3c-ff1d4e346d52")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.45 -2.7)
			(end -2.05 -2.7)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "78d1a29b-b503-48fd-b59a-fe60f2235160")
		)
		(fp_line
			(start -3.7 -2.75)
			(end 3.7 -2.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2dddced2-7e17-456f-ba64-0ea0c1a8cb18")
		)
		(fp_line
			(start -3.7 2.75)
			(end -3.7 -2.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "67d2636d-ace0-426b-b42e-ba85f2ab5cbc")
		)
		(fp_line
			(start 3.7 -2.75)
			(end 3.7 2.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7d21e75b-dcff-4f12-9f8e-45d43a860c5f")
		)
		(fp_line
			(start 3.7 2.75)
			(end -3.7 2.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1a82bbe8-ada0-4b79-b7ea-73f6a6396734")
		)
		(fp_line
			(start -1.95 -2.5)
			(end 1.95 -2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0634f25f-153a-4a24-b142-4ebe1e0d1c2b")
		)
		(fp_line
			(start -1.95 -1.5)
			(end -0.95 -2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ea76bd3a-97b1-4cf9-9d10-ffedd1606ed9")
		)
		(fp_line
			(start -1.95 2.5)
			(end -1.95 -2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cce03c9e-8aae-4764-8e09-d3143488abf4")
		)
		(fp_line
			(start 1.95 -2.5)
			(end 1.95 2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4291b1be-52d2-43fc-8606-34a9b4e87c44")
		)
		(fp_line
			(start 1.95 2.5)
			(end -1.95 2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a82eaefd-2f37-4453-8f00-1abffcbadd7f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b9a2bb16-b499-4b3d-b24a-13aa1b089050")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -2.75 -2 90)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(IC1-VDD)")
			(pinfunction "VDD")
			(pintype "passive")
			(uuid "84714467-ee8e-4eef-8491-edbea7182541")
		)
		(pad "2" smd rect
			(at -2.75 -1 90)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "unconnected-(IC1-CFG2-Pad2)")
			(pinfunction "CFG2")
			(pintype "passive+no_connect")
			(uuid "a77742d2-a9fe-436e-898d-e3890ff8a8d3")
		)
		(pad "3" smd rect
			(at -2.75 0 90)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "unconnected-(IC1-CFG3-Pad3)")
			(pinfunction "CFG3")
			(pintype "passive+no_connect")
			(uuid "a549dbdb-61b3-4e9b-b4da-0dfef58f5696")
		)
		(pad "4" smd rect
			(at -2.75 1 90)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "D+")
			(pinfunction "DP")
			(pintype "passive")
			(uuid "47102e1c-6358-4145-809f-6001532444fe")
		)
		(pad "5" smd rect
			(at -2.75 2 90)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "D-")
			(pinfunction "DM")
			(pintype "passive")
			(uuid "d15d3c2b-412b-47a6-b933-8f7f14aaa7b2")
		)
		(pad "6" smd rect
			(at 2.75 2 90)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "CC2")
			(pinfunction "CC2")
			(pintype "passive")
			(uuid "d3fc62ac-97c5-4027-a6fc-69f83827c6f3")
		)
		(pad "7" smd rect
			(at 2.75 1 90)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "CC1")
			(pinfunction "CC1")
			(pintype "passive")
			(uuid "7f4fbb21-1442-4d2e-8374-64bafcbc4052")
		)
		(pad "8" smd rect
			(at 2.75 0 90)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "Net-(IC1-VBUS)")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "ab92d746-fd5f-4650-abf1-1fcb76c6e7ed")
		)
		(pad "9" smd rect
			(at 2.75 -1 90)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "Net-(IC1-CFG1)")
			(pinfunction "CFG1")
			(pintype "passive")
			(uuid "bce01b3f-7ce7-4acb-b185-983b7f73341c")
		)
		(pad "10" smd rect
			(at 2.75 -2 90)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(D1-K)")
			(pinfunction "PG")
			(pintype "passive")
			(uuid "a16fcc91-841c-41dc-baae-2c4aee264b3c")
		)
		(pad "11" smd rect
			(at 0 0)
			(size 2.3 3.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "69c98d93-96db-4bfd-8185-dbe4761df7b2")
		)
		(embedded_fonts no)
		(model "CH224K.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "f702af8c-00d3-44bc-bf55-0bca78847d55")
		(at 134.44 75.55)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C12"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "676d0d80-43ca-41b5-8b11-2bc29e680b20")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "e4cddb7a-eaf0-49d5-91bf-d66223700c1c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ca4e55a4-23cd-47c7-b213-dd77602bd0ae")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e854cdce-699b-413c-9b1b-2867d0075960")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/89dfac6b-c1b2-4fc1-b664-4f6afbbf8739")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4c70b50c-cefe-4e12-b730-461631c0ef89")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2eb47637-c3b5-4826-984c-5c5e5cd82246")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1e961be9-40e2-4f36-8538-8c9cb55d3cf7")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7a2878ec-5942-420b-b9b4-ad8821a0c838")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a289f7e2-64b9-473a-93ad-a456dc893953")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cc69ff2c-6b65-4a50-a902-c87f526ba93e")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a53b5456-72c8-45d9-9a77-3a54ab71397c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2108b6b5-5c3f-4c78-a06d-c0a63de2a2a9")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f9a1d15-d717-4545-a9b2-beae9cfd63e6")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "94acbf65-ccbb-4f4a-a686-3c2d8bd15d2d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4d082c09-9022-47f0-b7f1-e156ca1b3fc5")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "Net-(U1-VIN)")
			(pintype "passive")
			(uuid "b90afbfe-1058-4498-b73c-ba9f93ee5958")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "3ff5058f-5d7a-4bd7-a282-b363392fdc07")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic:SOP100P600X175-10N"
		(layer "F.Cu")
		(uuid "f79be3fd-2082-46b2-bf6f-cc9b12b5dac0")
		(at 166.025 86.4)
		(descr "CN3791")
		(tags "Integrated Circuit")
		(property "Reference" "IC2"
			(at 0 0 0)
			(layer "F.SilkS")
			(uuid "a71bec6d-77dc-4d8e-8d90-b9b2a40efa95")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "CN3791"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "4388dd37-f1ca-43f5-b765-d9dec8c1243b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" "http://www.consonance-elec.com/pdf/datasheet/DSE-CN3791.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6379aec0-8e04-435d-9311-15a248ac642c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "ic"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "99ec19ed-14b1-42d3-8bb7-27a5a95c2965")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "1.75"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c42e6536-09a2-471d-afdb-757cd81897fe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "Consonance"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "769b237f-1b9b-4457-899a-b0971d8451a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "CN3791"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0befd9b-46e8-47d7-8274-f3da6e813c73")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "408f23eb-8d0f-44df-a425-331933e8104c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6d47f3a5-66c4-4c8e-86c3-d2f569605f88")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8f9da7ad-91dd-4d99-ad16-9da48bc94c00")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3648525e-61b5-4d8e-a0cd-3a90486929ea")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C154992"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b8571f35-8514-40ac-8e6c-fa76ba86f8bf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a9f8b2cc-cdf9-487f-97af-b67b618bc2ba")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1ab6c454-c2bc-4040-a090-9e5ebed71bdb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/714c827e-f961-4794-94bb-bb28cdcf6f2e")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.475 -2.675)
			(end -1.95 -2.675)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b8f796ae-be86-487c-9d83-f2e91dff543f")
		)
		(fp_line
			(start -1.6 -2.45)
			(end 1.6 -2.45)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c16ef475-f152-44ed-9474-d1774698bf91")
		)
		(fp_line
			(start -1.6 2.45)
			(end -1.6 -2.45)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4930b30d-03c2-469d-a734-ca7bd122f457")
		)
		(fp_line
			(start 1.6 -2.45)
			(end 1.6 2.45)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c64942e7-711a-4e51-8a7f-b8f261b6a566")
		)
		(fp_line
			(start 1.6 2.45)
			(end -1.6 2.45)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b689cdf1-6a45-42a6-a343-3072b7038107")
		)
		(fp_line
			(start -3.725 -2.8)
			(end 3.725 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "343abc28-1b78-457e-aac6-81d185d00725")
		)
		(fp_line
			(start -3.725 2.8)
			(end -3.725 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0c686304-1317-4b09-be99-994097cd3951")
		)
		(fp_line
			(start 3.725 -2.8)
			(end 3.725 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "79ec7703-3d2d-4fac-b917-5806218d19d9")
		)
		(fp_line
			(start 3.725 2.8)
			(end -3.725 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b8d784a9-24b8-435e-9661-48e284f6f1b9")
		)
		(fp_line
			(start -1.95 -2.45)
			(end 1.95 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "afd5d70f-236a-4676-8b6a-4af9cad4aa2c")
		)
		(fp_line
			(start -1.95 -1.45)
			(end -0.95 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "18fe1ee6-5b17-4047-97fc-6be312a61a28")
		)
		(fp_line
			(start -1.95 2.45)
			(end -1.95 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5b602347-99df-41f4-969a-94bf6cd820d2")
		)
		(fp_line
			(start 1.95 -2.45)
			(end 1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6e8cbb4-1300-43ea-b23d-1a43b2b0624a")
		)
		(fp_line
			(start 1.95 2.45)
			(end -1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc2b99b8-70ad-4805-beaa-a3343b084847")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "51441eb1-2da7-47c1-9cbb-1aad97323f24")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -2.712 -2 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(IC2-VG)")
			(pinfunction "VG")
			(pintype "passive")
			(uuid "04b30f6e-e725-40e2-a71b-3918f3d332bc")
		)
		(pad "2" smd rect
			(at -2.712 -1 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "1f6ad2ae-ac96-4b68-a1bf-2b27945736bb")
		)
		(pad "3" smd rect
			(at -2.712 0 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "Net-(D3-K)")
			(pinfunction "~{CHRG}")
			(pintype "passive")
			(uuid "681aac82-9813-4a6b-b055-3d6dc2337793")
		)
		(pad "4" smd rect
			(at -2.712 1 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(D5-K)")
			(pinfunction "~{DONE}")
			(pintype "passive")
			(uuid "cb141ccd-e2c7-4001-b1f9-99a6229afc41")
		)
		(pad "5" smd rect
			(at -2.712 2 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(IC2-COM)")
			(pinfunction "COM")
			(pintype "passive")
			(uuid "594e0265-3014-48fa-bf2a-6355ab9e1e7d")
		)
		(pad "6" smd rect
			(at 2.712 2 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "Net-(IC2-MPPT)")
			(pinfunction "MPPT")
			(pintype "passive")
			(uuid "20c10a1c-5c12-4604-87e1-9bf4597f5db4")
		)
		(pad "7" smd rect
			(at 2.712 1 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Bat Shunt 1")
			(pinfunction "BAT")
			(pintype "passive")
			(uuid "97981deb-4d4d-4daa-b497-e4ad3bdc98b4")
		)
		(pad "8" smd rect
			(at 2.712 0 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "Net-(IC2-CSP)")
			(pinfunction "CSP")
			(pintype "passive")
			(uuid "7396f03d-9e5a-40f2-be36-c7304265478a")
		)
		(pad "9" smd rect
			(at 2.712 -1 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(IC2-VCC)")
			(pinfunction "VCC")
			(pintype "passive")
			(uuid "579f0c39-aaa5-4499-8eb7-fa9fecee9f92")
		)
		(pad "10" smd rect
			(at 2.712 -2 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "Net-(IC2-DRV)")
			(pinfunction "DRV")
			(pintype "passive")
			(uuid "a1d825e2-1e9a-4cf5-b11b-d82dbe735d8f")
		)
		(embedded_fonts no)
		(model "CN3791.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "f9c607a8-cd3e-4b55-bf61-620909cfac54")
		(at 142.8 112.62)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C42"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "a33f2c90-9b6f-491e-8cd1-20e108dc2aaf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "25cdb419-642c-42dc-915a-424ac97992d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "aed9bd4d-4c2c-49fc-8af9-71adf2b2ece6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ed43f687-1b5b-438b-84bd-270f8fae5fea")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/beaf1a65-5243-45ee-b3f0-f6e822a84775")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8ae9f454-b7b0-4ef7-9420-fe3eeee85ccb")
		)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "71c61f9b-821a-42c0-ac4b-92d3fee59d51")
		)
		(fp_line
			(start -1.65 -0.73)
			(end 1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "15b2fbd4-8894-4e1f-a387-9d18d8fef320")
		)
		(fp_line
			(start -1.65 0.73)
			(end -1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8c3c361a-54ef-4bcd-b2e2-4cbe0a9f07b9")
		)
		(fp_line
			(start 1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f777eca9-9ace-4320-b810-09c05f53531a")
		)
		(fp_line
			(start 1.65 0.73)
			(end -1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f4e7c145-2669-4a0e-a7ab-d29c632b71be")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f6a7f21-f391-4b18-8d49-b1b2f1b2ce85")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6994e0e-2e8c-4da6-b209-1c4db8a7686f")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9d708176-ad07-4161-b8f0-c1349ed0328b")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f7012bf4-287e-4c12-81b9-7278eaff5e21")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f1389196-d9ad-4d7d-bfba-bfa354c3b63d")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(J7-In)")
			(pintype "passive")
			(uuid "87bcf5fb-e49f-4955-b1c2-ffac863acaaa")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(S1-RF1)")
			(pintype "passive")
			(uuid "907b1b0b-77a7-4c00-8d68-d2d29d4dfe84")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(uuid "fa34dd1e-d5fa-40b6-a91b-2cfb0703bec7")
		(at 138.3 122.46)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 -1.998 0)
			(layer "F.SilkS")
			(uuid "924df810-0c67-4169-9845-ef646fdad51a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.Fab")
			(uuid "9e49ab5a-0244-4eff-a748-9662e3d38930")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "856d4cd5-7566-4bf6-bcc6-b53021b7e7fc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5656288c-72c0-498a-9440-7cf4cf3c35a5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/da71199a-a76b-48b5-8cfd-f9c0a33d6d61")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_circle
			(center 0 0)
			(end 0 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "d4b5b0af-200c-4010-a871-99312b784ef4")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "8ec7d7a9-65b2-4d0c-94e3-ca23aede7435")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "50679a45-f581-4895-a3e3-f0e6014eb5a2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 108 "I2C SDA")
			(pinfunction "1")
			(pintype "passive")
			(uuid "9b8ed9cc-220b-45df-abfe-e6771946f20b")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(uuid "faf583db-1503-4ad7-a579-8a1b31395e06")
		(at 142.35 122.46)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 -1.998 0)
			(layer "F.SilkS")
			(uuid "4990a9d9-abc6-485c-8675-86fea3062b00")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.Fab")
			(uuid "7715eefc-7ebf-4a03-8c51-61c33975bb29")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "19fbd6ed-0ad1-473e-ba4e-c02274c2833f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b418123f-de51-45cd-a757-ffc4f5655b4e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/4e9b4119-64dd-4708-a871-9172dda61a32")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_circle
			(center 0 0)
			(end 0 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "f8f476de-7f0d-40bf-b9f7-142cbb30e026")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "56844e37-bac4-47d5-a83f-2f92a208df1a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "a914c0fe-2e8a-4bfa-a3d0-e62c7e69d61d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 94 "Sol Shunt 1")
			(pinfunction "1")
			(pintype "passive")
			(uuid "bec74716-4b69-4c9b-9d5c-64c5c6807bad")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "fd356628-5341-42b8-9161-884f66ee290b")
		(at 120.1 63.48)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R18"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "f088b697-cf01-488c-8f6d-83be1fdb983b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "5094d963-1bc5-491f-b166-f463a68bdfa2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "590ba5fc-30e9-4d59-8cfe-7a56a337991c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6c4fd4a5-7afb-4fe9-8201-3edb51cb9440")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/f9f9b350-ceb2-4685-abe3-a2b246ef02bb")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc97e962-9535-4e5f-b168-d3b5fbaf5f90")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d0a89783-6c27-403e-a7c8-c029f40f5f45")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "daaa294c-dadf-43b8-a55f-02e3a19b6b72")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "123a8577-4d36-414c-8b7a-50ca17668073")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "437c9765-ff59-4b0a-8d90-9262dc5c624c")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "463e0523-5978-4138-aa37-466b4401ba85")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "284c3817-af59-46a8-8fdf-77589ed5c36d")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "84c9cd9e-e779-4620-852a-a26d8b9612eb")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "11fb7cda-088e-423a-933f-cfdf767e87bd")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "efbebab8-bc7b-4b34-b257-f15082ae7451")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "73ee6c4e-6a34-4d30-b28e-e056dfb719d7")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 11 "Net-(IC2-VG)")
			(pintype "passive")
			(uuid "55cdb589-7489-46d5-86f0-b42d5e89f780")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 12 "Net-(IC2-VCC)")
			(pintype "passive")
			(uuid "1f5bf64e-3192-472d-80eb-852c185c61be")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "fdfbd100-adc6-4967-99e6-dce9fac68c70")
		(at 138.45 105.09)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C25"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "3a5bc2e4-9396-40e1-8251-aae5c17887ad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "220pF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "21a76cb8-0fae-432a-ba29-360ed0f4b5c2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bdae14d6-56c6-40cd-95a3-ce47d3c4f191")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e03ac4d6-80e3-4eae-bd84-164622895aea")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/74b2a195-63b3-426e-86a3-393512917391")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "722c6030-c42e-4599-87b2-7f00a20ebef9")
		)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8e7ef349-bf6b-432a-8275-dece65aa51c9")
		)
		(fp_line
			(start -1.65 -0.73)
			(end 1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9c566351-6263-42b5-8c50-a2e2c7df5a88")
		)
		(fp_line
			(start -1.65 0.73)
			(end -1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7856bb6f-37f6-4445-8b83-e8854703ccc9")
		)
		(fp_line
			(start 1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dfdd0f8f-8c20-46cb-9f88-9da20b1ec074")
		)
		(fp_line
			(start 1.65 0.73)
			(end -1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6f46a6ad-d62f-48c2-8428-250e9820a7ac")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b84c17f2-eff6-496e-b214-36e79948f4f6")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a00bd08c-1a8c-47b4-80e4-fa7ca34d4246")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb10d5b8-9736-4710-bdf6-26542a2e4ac8")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15b8549b-014b-4825-a33d-bb67c989bc1b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d77f1ff7-7dfd-4f19-aca4-e9a0107809b1")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "USE_ANT_2")
			(pintype "passive")
			(uuid "5e574396-2def-4100-8d2c-33982878656e")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(uuid "ce1444e6-1e6e-456b-a825-9ee8ae2c1094")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "F.Cu")
		(uuid "fe7ac98d-67f7-4ee4-a2f9-fcd008a50184")
		(at 158.55 85.575)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q1"
			(at 0 -2.75 0)
			(layer "F.SilkS")
			(uuid "cb89442d-f71c-4d9e-a5e3-03d604072cd0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PMOS"
			(at 0 2.5 0)
			(layer "F.Fab")
			(uuid "5ae548e4-eec7-4c80-b3e9-b8adc238ebde")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_MOSFETs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "756d5b5b-3f6f-4dbe-89f9-412b74ac3cbf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "P-MOSFET transistor, drain/source/gate"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "327be07f-9d99-45f1-8090-3f135b5cafbc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "PMOS"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "14c439ed-87f6-4669-9a58-ab5117b4cf5e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Type" "VDMOS"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1f5ad0fc-477a-4df4-a7a0-2b626be88932")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=D 2=G 3=S"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8689900a-3279-4752-8efe-d538b898c96a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/8c139557-19ed-4448-b687-400c822f12e7")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.04 -1.58)
			(end -0.84 -1.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0c57003b-66d3-4c38-88f0-df72c5d8ab9a")
		)
		(fp_line
			(start -0.04 -1.58)
			(end 0.76 -1.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3a555fb9-171d-43c5-bdd9-b481754ad027")
		)
		(fp_line
			(start 0.76 -1.58)
			(end 0.76 -0.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ebc8e798-9c46-40ec-9ab9-658e5a89c431")
		)
		(fp_line
			(start 0.76 1.58)
			(end -0.7 1.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7eca70e4-f31b-4ab5-8a3c-2ae603cde5eb")
		)
		(fp_line
			(start 0.76 1.58)
			(end 0.76 0.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "88f226e5-f416-4ee0-8920-5aa2f7d7ab41")
		)
		(fp_poly
			(pts
				(xy -1.34 -1.61) (xy -1.58 -1.94) (xy -1.1 -1.94) (xy -1.34 -1.61)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "7296bfdd-80c5-43d4-97c9-9a7a392e658e")
		)
		(fp_line
			(start -2.7 -1.75)
			(end 2.7 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9dc4526c-1a3b-4d84-a018-20052f331543")
		)
		(fp_line
			(start -2.7 1.75)
			(end -2.7 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5e0782e-fa40-4b08-9a5b-d54af86071c9")
		)
		(fp_line
			(start 2.7 -1.75)
			(end 2.7 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fa5546aa-0c87-4b4a-b0e9-3359fba10109")
		)
		(fp_line
			(start 2.7 1.75)
			(end -2.7 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f5b0ee6-1e77-472a-a816-64445a832b88")
		)
		(fp_line
			(start -0.7 -0.95)
			(end -0.7 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f5899bf2-800d-4688-936b-84489529680a")
		)
		(fp_line
			(start -0.7 -0.95)
			(end -0.15 -1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "431ee2b9-c17d-414d-9845-52e4e676ca9e")
		)
		(fp_line
			(start -0.7 1.52)
			(end 0.7 1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb46a33d-3894-45db-b18c-9354c90ace8f")
		)
		(fp_line
			(start -0.15 -1.52)
			(end 0.7 -1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0342b348-154a-4e2a-9d5d-22a816af2ec9")
		)
		(fp_line
			(start 0.7 -1.52)
			(end 0.7 1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa56e281-3712-419b-af4b-51eae264ffb2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "493a3c10-c1da-481c-a09b-1d30663d291f")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.075)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5 -0.95)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(IC2-VCC)")
			(pinfunction "D")
			(pintype "passive")
			(uuid "57e13f1b-c02e-4b30-85de-da6bbb646455")
		)
		(pad "2" smd roundrect
			(at -1.5 0.95)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "Net-(IC2-DRV)")
			(pinfunction "G")
			(pintype "input")
			(uuid "056bdb7a-329d-4fc7-8e36-1124c6d1d690")
		)
		(pad "3" smd roundrect
			(at 1.5 0)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "Net-(D6-K)")
			(pinfunction "S")
			(pintype "passive")
			(uuid "7c57c21f-3468-4fab-9195-4eb9edf2869d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(uuid "ff7b5f9b-4cc6-4220-8802-48329a1bdf35")
		(at 118.1 117.415)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "df002fbc-84ca-4e8e-8e5f-f2124628e52e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TPS565208"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "5ac0505c-7b19-4149-a48b-2ef544898fd4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps565208.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "da251546-28b0-45d3-ae6c-4733fb9b6d76")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "5A Synchronous Step-Down Voltage Regulator, Adjustable Output Voltage, 4.5-17V Input Voltage, SOT-23-6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f6fcedce-13e6-4568-a07f-0b100452464d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C2650336"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "02618a45-607c-48ef-9309-442f400ced85")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a537b171-5339-4143-a4bf-58a1b66df9f2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2803803b-728f-444d-b9d7-6592a155a2c7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/eeb008f6-cb32-4f6e-80e9-84b8ed52bcf6")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c40f4895-3ffb-4432-a5af-93384ef3545a")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "be8679d9-f7fe-45d5-b938-1d5e30b25da1")
		)
		(fp_line
			(start 0 1.56)
			(end -0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eb96adb4-e3e8-491d-b228-b39c52aad3d8")
		)
		(fp_line
			(start 0 1.56)
			(end 0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8b20bdb8-7346-4180-890e-56d9a15dbfe1")
		)
		(fp_poly
			(pts
				(xy -1.3 -1.51) (xy -1.54 -1.84) (xy -1.06 -1.84)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "97d1137c-d1bb-4899-80b7-0318fb538763")
		)
		(fp_rect
			(start -2.05 -1.7)
			(end 2.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "0e41a374-66bd-418a-aeab-8cd2e98723ed")
		)
		(fp_line
			(start -0.8 -1.05)
			(end -0.4 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b4bac3ae-903e-4029-a3d1-87c52b93a272")
		)
		(fp_line
			(start -0.8 1.45)
			(end -0.8 -1.05)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "34f21b07-55ad-47f8-a8af-02b871f00fa6")
		)
		(fp_line
			(start -0.4 -1.45)
			(end 0.8 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aad6609d-56b2-488c-9fbb-266a9815daef")
		)
		(fp_line
			(start 0.8 -1.45)
			(end 0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "148a5ab7-ad16-4029-b6ac-570be52bb807")
		)
		(fp_line
			(start 0.8 1.45)
			(end -0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f9523f7-9857-44bf-952b-4ec33b55d778")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "364a5450-63ff-4420-9a44-2cade0e77e93")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "da8d3532-db97-4168-8ef4-1742718fe90d")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U1-SW)")
			(pinfunction "SW")
			(pintype "output")
			(uuid "a945679e-3c5f-44ce-9131-33d969b1614f")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(U1-VIN)")
			(pinfunction "VIN")
			(pintype "power_in")
			(uuid "24bb5ca7-4350-442f-9886-4193e4c9c8b9")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "Net-(U1-VFB)")
			(pinfunction "VFB")
			(pintype "input")
			(uuid "5a715f5d-a79e-4a41-996f-bfc7a9b27af0")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "Net-(U1-EN)")
			(pinfunction "EN")
			(pintype "input")
			(uuid "f84a63e2-5db9-45ca-9eb8-838fe98690d7")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U1-VBST)")
			(pinfunction "VBST")
			(pintype "passive")
			(uuid "4bbfa8ed-57a0-495b-bf48-2cd3c1cc46b4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(embedded_fonts no)
)
