(footprint "SATA_Data" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at -8.8 3.7 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 87bdc13f-63b6-46f8-bd8c-273d2f9e7675)
  )
  (fp_text value "SATA_Data" (at 0.3 3.6 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 23f1ffd3-d236-472a-a2eb-dd72e7574b0a)
  )
  (fp_text user "${REFERENCE}" (at 0.3 5.1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0c977436-3f08-4e0b-aedb-129497bbd7da)
  )
  (fp_line (start -11.81 -3.2) (end -9.81 -3.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4facbec5-c82a-469d-aa41-627be140b56a))
  (fp_line (start -11.81 2.2) (end -11.81 -3.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp da69e63f-fde8-4a09-bbfd-d02bb2627a61))
  (fp_line (start -9.81 -4.2) (end 2.39 -4.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7bdba5a1-17bc-4499-8e16-ed6151405421))
  (fp_line (start -9.81 -3.2) (end -9.81 -4.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f83883ee-79d2-45f4-b398-3db993f04dd5))
  (fp_line (start 2.39 -4.2) (end 2.39 -3.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a7e46aa0-379c-464c-87ef-99fd68926b4a))
  (fp_line (start 2.39 -3.3) (end 3.39 -3.3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b13b1e2e-96f2-414b-92ba-426502095c9f))
  (fp_line (start 3.39 -3.3) (end 3.39 -3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3a3344ae-e6c6-41ef-8d07-c10dd8eae8fd))
  (fp_line (start 3.39 -3) (end 4.19 -3)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d7334e59-4d03-4fb6-9ed5-64db9b94d423))
  (fp_line (start 3.39 1.4) (end 3.39 2.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b0c35aa5-dd0f-4444-813b-2c1b36620430))
  (fp_line (start 3.39 2.2) (end -11.81 2.2)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0ca58e43-7785-4bac-ad30-9bd0248e09db))
  (fp_line (start 4.19 -3) (end 4.19 1.4)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eb44df39-76e0-43d8-bf0e-c20dfbe22e7d))
  (fp_line (start 4.19 1.4) (end 3.39 1.4)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 06bc17a4-8a36-4310-8cf2-40da0f10ff60))
  (fp_rect (start -7.75 1.54) (end -7.55 2.14)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 95b19a30-386f-4f03-89f8-3c14176c7ab2))
  (fp_rect (start -11.91 2.3) (end 4.29 -4.3)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 936e0d75-fe5f-4ee3-b05f-87d0fc88d6d9))
  (fp_line (start -7.61 -1.9) (end 0.69 -1.9)
    (stroke (width 0.2) (type solid)) (layer "F.Fab") (tstamp 420493c6-743e-4d9e-b8c7-6b4ba355ee80))
  (fp_line (start -7.61 0.8) (end -7.61 -1.9)
    (stroke (width 0.2) (type solid)) (layer "F.Fab") (tstamp 4f91b00b-fb32-4b81-b5ea-c0af4d98533e))
  (fp_rect (start -11.81 2.2) (end 4.19 -4.2)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp e3a9c96f-1a77-4d82-998e-e5115b4731ee))
  (pad "" thru_hole circle (at -10.29 -0.5) (size 2.2 2.2) (drill 1.6) (layers "*.Cu" "*.Mask") (tstamp ca9be034-b2d8-4fc3-bd77-eda31cfd26d4))
  (pad "" thru_hole circle (at 2.67 -0.5) (size 2.2 2.2) (drill 1.6) (layers "*.Cu" "*.Mask") (tstamp c16ac3bd-7ec4-4f54-afb1-d7044563e1d8))
  (pad "1" thru_hole oval (at 0 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp 5facd3fa-56e6-40e6-9b1c-71f6657868b1))
  (pad "2" thru_hole oval (at -1.27 -1) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp fe60c4ef-c0df-447a-9dc3-459ce1f3a9b9))
  (pad "3" thru_hole oval (at -2.54 -1) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp 5482cbf6-fac3-4d1e-aeb5-c454a5e96ad7))
  (pad "4" thru_hole oval (at -3.81 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp f12463a0-b9aa-4ba9-883f-f03f20993262))
  (pad "5" thru_hole oval (at -5.08 -1) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp c528117f-5b6f-4fb2-af86-164fe876b761))
  (pad "6" thru_hole oval (at -6.35 -1) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp 1de39d65-b53a-4fe0-9f24-35ff24f6b3ba))
  (pad "7" thru_hole oval (at -7.62 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp c93cb002-bc48-47cc-8273-54c6582a4a05))
  (model "${KIPRJMOD}/libs/3d/data.stp"
    (offset (xyz -31 -22.2 10.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 0 90))
  )
)
