(module LED_D3.0mm (layer F.Cu) (tedit 5B965EC7)
  (descr "LED, diameter 3.0mm, 2 pins")
  (tags "LED diameter 3.0mm 2 pins")
  (fp_text reference D72 (at 1.27 -2.96) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value LED_3mm (at 1.27 2.96) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0 0) (end 0 -1.524) (layer F.SilkS) (width 0.15))
  (fp_arc (start 0 0) (end -1.5 -1.16619) (angle 284.3) (layer F.Fab) (width 0.1))
  (fp_circle (center 0 0) (end 1.5 0) (layer F.Fab) (width 0.1))
  (fp_line (start -1.5 -1.16619) (end -1.5 1.16619) (layer F.Fab) (width 0.1))
  (fp_line (start -2.42 -2.25) (end -2.42 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.42 2.25) (end 2.43 2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.43 2.25) (end 2.43 -2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.43 -2.25) (end -2.42 -2.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.5 -1.25) (end 2.5 -1.25) (layer B.SilkS) (width 0.15))
  (fp_line (start 2.5 -1.25) (end 2.5 1.25) (layer B.SilkS) (width 0.15))
  (fp_line (start 2.5 1.25) (end -2.5 1.25) (layer B.SilkS) (width 0.15))
  (fp_line (start -2.5 1.25) (end -2.5 -1.25) (layer B.SilkS) (width 0.15))
  (pad 1 thru_hole rect (at -1.27 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu B.Mask))
  (pad 2 thru_hole circle (at 1.27 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu B.Mask))
  (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 0.393701 0.393701 0.393701))
    (rotate (xyz 0 0 0))
  )
)
