(module MX-Alps_Switch_Cutout-1u_1.25u-3u-wide (layer F.Cu) (tedit 5971FE21)
  (fp_text reference REF** (at 0.25 10.05) (layer Eco2.User) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value MX-Alps_Switch_Cutout (at 0 -15.24) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -9.5 -9.5) (end 9.5 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.5 9.5) (end -9.5 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.5 9.5) (end -9.5 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.5 -9.5) (end 9.5 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.5 9.5) (end -9.5 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.5 -9.5) (end 9.5 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.5 9.5) (end -9.5 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.5 -9.5) (end 9.5 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.55 9.5) (end 9.55 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.55 -9.5) (end 28.55 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.55 9.5) (end 9.55 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 28.55 9.5) (end 9.55 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 28.55 -9.5) (end 28.55 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 28.55 9.5) (end 9.55 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.55 -9.5) (end 28.55 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 28.55 -9.5) (end 28.55 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -28.55 9.5) (end -28.55 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -28.55 -9.5) (end -9.55 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -28.55 9.5) (end -28.55 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.55 9.5) (end -28.55 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.55 -9.5) (end -9.55 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.55 9.5) (end -28.55 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -28.55 -9.5) (end -9.55 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.55 -9.5) (end -9.55 9.5) (layer Dwgs.User) (width 0.15))
  (pad "" np_thru_hole oval (at 6.85 6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 7.325 6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 7.325 -6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 6.85 -6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -6.85 -6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -7.325 -6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -7.325 6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -6.85 6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 7.8 0) (size 0.3 12.8) (drill oval 0.3 12.8) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -7.8 0) (size 0.3 12.8) (drill oval 0.3 12.8) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 0 7) (size 14 0.3) (drill oval 14 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 0 -7) (size 14 0.3) (drill oval 14 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 7.325 6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 7.325 -6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 7.8 0) (size 0.3 12.8) (drill oval 0.3 12.8) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 6.85 -6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 6.85 6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 0 7) (size 14 0.3) (drill oval 14 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -6.85 -6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -7.325 -6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -7.8 0) (size 0.3 12.8) (drill oval 0.3 12.8) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -7.325 6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -6.85 6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 0 -7) (size 14 0.3) (drill oval 14 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 12.2 -6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 25.9 -6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 12.2 -6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 19.05 7) (size 14 0.3) (drill oval 14 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 19.05 7) (size 14 0.3) (drill oval 14 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 25.9 -6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 19.05 -7) (size 14 0.3) (drill oval 14 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 19.05 -7) (size 14 0.3) (drill oval 14 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 11.725 -6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 11.725 6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 12.2 6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 11.725 -6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 11.25 0) (size 0.3 12.8) (drill oval 0.3 12.8) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 11.725 6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 11.25 0) (size 0.3 12.8) (drill oval 0.3 12.8) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 12.2 6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 26.85 0) (size 0.3 12.8) (drill oval 0.3 12.8) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 25.9 6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 26.375 -6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 26.375 6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 26.375 -6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 26.375 6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 26.85 0) (size 0.3 12.8) (drill oval 0.3 12.8) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 25.9 6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -25.9 -6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -12.2 -6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -25.9 -6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -19.05 7) (size 14 0.3) (drill oval 14 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -19.05 7) (size 14 0.3) (drill oval 14 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -12.2 -6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -19.05 -7) (size 14 0.3) (drill oval 14 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -19.05 -7) (size 14 0.3) (drill oval 14 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -26.375 -6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -26.375 6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -25.9 6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -26.375 -6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -26.85 0) (size 0.3 12.8) (drill oval 0.3 12.8) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -26.375 6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -26.85 0) (size 0.3 12.8) (drill oval 0.3 12.8) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -25.9 6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -11.25 0) (size 0.3 12.8) (drill oval 0.3 12.8) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -12.2 6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -11.725 -6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -11.725 6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -11.725 -6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -11.725 6.25) (size 1.25 0.3) (drill oval 1.25 0.3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -11.25 0) (size 0.3 12.8) (drill oval 0.3 12.8) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -12.2 6.625) (size 0.3 1.05) (drill oval 0.3 1.05) (layers *.Cu *.Mask))
)
