(footprint "vik-module-connector-horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 5.12 -3.56 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6a24f8c0-aeb6-4acc-9c9e-28fc44782c17)
  )
  (fp_text value "vik-module-connector-horizontal" (at 0.1 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c70d6d6a-d6fc-495d-9524-6faba107174f)
  )
  (fp_text user "3v3" (at 3.3 -2.7 unlocked) (layer "F.SilkS")
      (effects (font (size 0.75 0.75) (thickness 0.15)) (justify left bottom))
    (tstamp 4b11a486-b108-4ffc-8af7-1f570059679e)
  )
  (fp_text user "VIK IN" (at -2.36 -3.42 unlocked) (layer "F.SilkS" knockout)
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp 680dee3f-61a6-4e55-8e3f-51c2eda13336)
  )
  (fp_text user "C479750" (at 0 0.75) (layer "User.2")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f5c1073f-d475-4492-a36d-fb0b7148e8a1)
  )
  (fp_line (start -5.5 -2.2) (end -3.131 -2.2)
    (stroke (width 0.254) (type solid)) (layer "F.SilkS") (tstamp e9c3c16c-d370-46bb-8ec2-bcf5a670a865))
  (fp_line (start -5.5 -0.539) (end -5.5 -2.2)
    (stroke (width 0.254) (type solid)) (layer "F.SilkS") (tstamp 432687d1-f599-4763-a3a1-716eb5338f19))
  (fp_line (start -5.5 4.295) (end -5.5 1.912)
    (stroke (width 0.254) (type solid)) (layer "F.SilkS") (tstamp 500be781-dcbb-4d71-aa39-5dc1c0b2a28b))
  (fp_line (start 5.5 -2.2) (end 3.131 -2.2)
    (stroke (width 0.254) (type solid)) (layer "F.SilkS") (tstamp d62be2f6-d1e3-4136-a34b-7d2f16211654))
  (fp_line (start 5.5 -0.539) (end 5.5 -2.2)
    (stroke (width 0.254) (type solid)) (layer "F.SilkS") (tstamp aff7b656-725d-4a36-bd1d-dfb618d9818f))
  (fp_line (start 5.5 4.295) (end -5.5 4.295)
    (stroke (width 0.254) (type solid)) (layer "F.SilkS") (tstamp 60ebbfd5-fbba-4ecf-91e2-3418f75fdb23))
  (fp_line (start 5.5 4.295) (end 5.5 1.912)
    (stroke (width 0.254) (type solid)) (layer "F.SilkS") (tstamp 6bfda8d1-d217-4924-ba4e-8c2698453f37))
  (fp_circle (center -3.429 -2.708) (end -3.302 -2.708)
    (stroke (width 0.254) (type solid)) (fill none) (layer "F.SilkS") (tstamp 23c8b252-36ac-4d51-ab48-29ba0dc7cb7f))
  (fp_line (start -3.5 2) (end -3.5 4.5)
    (stroke (width 0.12) (type default)) (layer "Cmts.User") (tstamp 98fc752f-6329-4116-b170-1697d5789616))
  (fp_line (start 3.5 2) (end 3.5 4.5)
    (stroke (width 0.12) (type default)) (layer "Cmts.User") (tstamp d61faa52-f880-4bf1-bb18-952e3ddbb395))
  (pad "1" smd rect (at -2.75 -2.038) (size 0.28 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp a9addef9-1afc-4014-a229-a9de062d5ae2))
  (pad "2" smd rect (at -2.25 -2.038) (size 0.28 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8403a7e1-7cbc-4e22-b921-5c769088b17b))
  (pad "3" smd rect (at -1.75 -2.038) (size 0.28 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp c6b94f95-8e7b-4bd7-9237-c62c44f7b5b0))
  (pad "4" smd rect (at -1.25 -2.038) (size 0.28 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 04e12e25-b35e-401a-aad1-426d496578f1))
  (pad "5" smd rect (at -0.75 -2.038) (size 0.28 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 9aa84185-be6d-436f-a468-aa048b10c536))
  (pad "6" smd rect (at -0.25 -2.038) (size 0.28 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp a8b34486-19e6-4cdb-8904-d8c5a0dbcbd4))
  (pad "7" smd rect (at 0.25 -2.038) (size 0.28 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b448983c-3629-4ddb-8567-d84b93ef2ced))
  (pad "8" smd rect (at 0.75 -2.038) (size 0.28 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 05792805-de7b-4fb3-befc-a6ed057194a8))
  (pad "9" smd rect (at 1.25 -2.038) (size 0.28 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 46512633-de25-4f9f-be65-79a3f5141146))
  (pad "10" smd rect (at 1.75 -2.038) (size 0.28 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp e81a27d8-8637-4524-870a-4b523b84e211))
  (pad "11" smd rect (at 2.25 -2.038) (size 0.28 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 39220a33-8dec-43c5-a397-9878d2b9ba0c))
  (pad "12" smd rect (at 2.75 -2.038) (size 0.28 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 9c5ad9f7-41f1-47a5-af74-cfe9c6f2bd63))
  (pad "13" smd rect (at 4.55 0.686) (size 1.8 2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ac0050f6-430d-46d0-afc7-4653652e0e29))
  (pad "14" smd rect (at -4.55 0.686) (size 1.8 2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp dd32776b-07a6-490f-a260-1a414ce7f65a))
)
