(module Triple-Dual-1u-LED-flip (layer F.Cu) (tedit 5A12ED03)
  (fp_text reference CHERRY (at 0 3.175) (layer F.SilkS) hide
    (effects (font (size 1.27 1.524) (thickness 0.2032)))
  )
  (fp_text value MX (at 0 5.08) (layer F.SilkS) hide
    (effects (font (size 1.27 1.524) (thickness 0.2032)))
  )
  (fp_text user + (at 1.26 3.5) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user - (at -1.27 3.5) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user + (at 1.26 3.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user - (at -1.27 3.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -6.35 -6.35) (end 6.35 -6.35) (layer Cmts.User) (width 0.1524))
  (fp_line (start 6.35 -6.35) (end 6.35 6.35) (layer Cmts.User) (width 0.1524))
  (fp_line (start 6.35 6.35) (end -6.35 6.35) (layer Cmts.User) (width 0.1524))
  (fp_line (start -6.35 6.35) (end -6.35 -6.35) (layer Cmts.User) (width 0.1524))
  (fp_line (start -9.398 -9.398) (end 9.398 -9.398) (layer Dwgs.User) (width 0.1524))
  (fp_line (start 9.398 -9.398) (end 9.398 9.398) (layer Dwgs.User) (width 0.1524))
  (fp_line (start 9.398 9.398) (end -9.398 9.398) (layer Dwgs.User) (width 0.1524))
  (fp_line (start -9.398 9.398) (end -9.398 -9.398) (layer Dwgs.User) (width 0.1524))
  (fp_line (start -6.985 -6.985) (end 6.985 -6.985) (layer Eco2.User) (width 0.1524))
  (fp_line (start 6.985 -6.985) (end 6.985 6.985) (layer Eco2.User) (width 0.1524))
  (fp_line (start 6.985 6.985) (end -6.985 6.985) (layer Eco2.User) (width 0.1524))
  (fp_line (start -6.985 6.985) (end -6.985 -6.985) (layer Eco2.User) (width 0.1524))
  (pad 2 smd oval (at 2.52 -4.79 356.055) (size 2 2.581378) (layers F.Cu F.Paste F.Mask))
  (pad 2 thru_hole circle (at 2.5 -4.5 330.95) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 2.54 -5.08 330.95) (size 2 2) (drill 1.2) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2.5 -4 330.95) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
  (pad HOLE np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu))
  (pad HOLE np_thru_hole circle (at -5.08 0) (size 1.8 1.8) (drill 1.8) (layers *.Cu))
  (pad HOLE np_thru_hole circle (at 5.08 0) (size 1.8 1.8) (drill 1.8) (layers *.Cu))
  (pad 1 thru_hole circle (at -3.81 -2.54) (size 2 2) (drill oval 1.2) (layers *.Cu *.Mask))
  (pad 2 smd oval (at 3.155 -3.27 221.9) (size 1.5 3.961556) (layers B.Cu B.Paste B.Mask))
  (pad 1 smd oval (at -3.155 -3.27 138.1) (size 2 3.961556) (layers B.Cu B.Paste B.Mask))
  (pad 2 thru_hole circle (at 2.5 -4) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 3.81 -2.54 311.9) (size 2 1.5) (drill 1.2) (layers *.Cu *.Mask))
  (pad 1 smd oval (at -2.52 -4.79 3.945) (size 2 2.581378) (layers B.Cu B.Paste B.Mask))
  (pad 1 thru_hole circle (at -2.5 -4.5 330.95) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2.54 -5.08 330.95) (size 2 2) (drill 1.2) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 1.27 5.08) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 4 thru_hole rect (at -1.27 5.08) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 1 smd oval (at -3.155 -3.27 138.1) (size 2 3.961556) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd oval (at -2.52 -4.79 3.945) (size 2 2.581378) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at 3.155 -3.27 221.9) (size 1.5 3.961556) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at 2.52 -4.79 356.055) (size 2 2.581378) (layers B.Cu B.Paste B.Mask))
  (pad 2 thru_hole circle (at 0 -5.9) (size 2 2) (drill 1.2) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -5 -3.8 138.1) (size 2 2) (drill 1.2) (layers *.Cu *.Mask))
  (pad 1 thru_hole oval (at 5 -3.8 221.9) (size 1.4 2) (drill 1.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 5.5 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu))
  (pad "" np_thru_hole circle (at -5.5 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu))
  (model /Users/danny/Documents/proj/custom-keyboard/kicad-libs/3d_models/mx-switch.wrl
    (at (xyz 0.294 0.294 0.234))
    (scale (xyz 0.4 0.4 0.4))
    (rotate (xyz 270 0 180))
  )
  (model /Users/danny/Documents/proj/custom-keyboard/kicad-libs/3d_models/SA-R3-1u.wrl
    (at (xyz 0 0 0.47))
    (scale (xyz 0.394 0.394 0.394))
    (rotate (xyz 270 0 0))
  )
)
