(module "TQFP-44_10x10mm_Pitch0.8mm" (layer F.Cu) (tedit 5DD97FAA)
  (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
  (tags "QFP 0.8")
  (attr smd)
  (fp_text reference "REF**" (at 0 -7.45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value "TQFP-44_10x10mm_Pitch0.8mm" (at 0 7.45) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center -4.064 -4.064) (end -3.81 -3.81) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.08 -4.064) (end -4.064 -5.08) (layer F.SilkS) (width 0.15))
  (fp_text user "%R" (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4 -5) (end 5 -5) (layer F.Fab) (width 0.15))
  (fp_line (start 5 -5) (end 5 5) (layer F.Fab) (width 0.15))
  (fp_line (start 5 5) (end -5 5) (layer F.Fab) (width 0.15))
  (fp_line (start -5 5) (end -5 -4) (layer F.Fab) (width 0.15))
  (fp_line (start -5 -4) (end -4 -5) (layer F.Fab) (width 0.15))
  (fp_line (start -6.7 -6.7) (end -6.7 6.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.7 -6.7) (end 6.7 6.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.7 -6.7) (end 6.7 -6.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.7 6.7) (end 6.7 6.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.175 -5.175) (end -5.175 -4.6) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.175 -5.175) (end 5.175 -4.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.175 5.175) (end 5.175 4.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.175 5.175) (end -5.175 4.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.175 -5.175) (end -4.5 -5.175) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.175 5.175) (end -4.5 5.175) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.175 5.175) (end 4.5 5.175) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.175 -5.175) (end 4.5 -5.175) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.175 -4.6) (end -6.45 -4.6) (layer F.SilkS) (width 0.15))
  (pad "44" smd rect (at -4 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "43" smd rect (at -3.2 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "42" smd rect (at -2.4 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "41" smd rect (at -1.6 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "40" smd rect (at -0.8 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "39" smd rect (at 0 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "38" smd rect (at 0.8 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "37" smd rect (at 1.6 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "36" smd rect (at 2.4 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "35" smd rect (at 3.2 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "34" smd rect (at 4 -5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "33" smd rect (at 5.7 -4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "32" smd rect (at 5.7 -3.2) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "31" smd rect (at 5.7 -2.4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "30" smd rect (at 5.7 -1.6) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "29" smd rect (at 5.7 -0.8) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "28" smd rect (at 5.7 0) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "27" smd rect (at 5.7 0.8) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "26" smd rect (at 5.7 1.6) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "25" smd rect (at 5.7 2.4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "24" smd rect (at 5.7 3.2) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "23" smd rect (at 5.7 4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "22" smd rect (at 4 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "21" smd rect (at 3.2 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "20" smd rect (at 2.4 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "19" smd rect (at 1.6 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "18" smd rect (at 0.8 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "17" smd rect (at 0 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "16" smd rect (at -0.8 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "15" smd rect (at -1.6 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "14" smd rect (at -2.4 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "13" smd rect (at -3.2 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd rect (at -4 5.7 90) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd rect (at -5.7 4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at -5.7 3.2) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at -5.7 2.4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at -5.7 1.6) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at -5.7 0.8) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at -5.7 0) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at -5.7 -0.8) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -5.7 -1.6) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -5.7 -2.4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -5.7 -3.2) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "1" smd rect (at -5.7 -4) (size 1.5 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-44_10x10mm_P0.8mm.wrl"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
