(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "vik-keyboard-connector" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 17.78 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "" (at 0 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "vik-keyboard-connector_1_1"
      (pin power_out line (at 0 13.97 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 -8.89 0) (length 2.54)
        (name "SPI_CS" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 -11.43 0) (length 2.54)
        (name "MISO" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 -13.97 0) (length 2.54)
        (name "SCLK" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 0 11.43 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 8.89 0) (length 2.54)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 6.35 0) (length 2.54)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 3.81 0) (length 2.54)
        (name "RGB_LED_OUT" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 0 1.27 0) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 -1.27 0) (length 2.54)
        (name "GPIO_AD1" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 -3.81 0) (length 2.54)
        (name "MOSI" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 0 -6.35 0) (length 2.54)
        (name "GPIO_AD2" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "vik-module-connector" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 17.78 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "" (at 0 6.35 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 6.35 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "vik-module-connector_1_1"
      (pin input line (at 0 13.97 0) (length 2.54)
        (name "SCLK" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -8.89 0) (length 2.54)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -11.43 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -13.97 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 11.43 0) (length 2.54)
        (name "MISO" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 8.89 0) (length 2.54)
        (name "SPI_CS" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 6.35 0) (length 2.54)
        (name "GPIO_AD2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 3.81 0) (length 2.54)
        (name "MOSI" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 1.27 0) (length 2.54)
        (name "GPIO_AD1" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 0 -1.27 0) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -3.81 0) (length 2.54)
        (name "RGB_LED_IN" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 0 -6.35 0) (length 2.54)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
