(module "C_0402" (layer F.Cu) (tedit 5DB0AA19)
  (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
  (tags "capacitor 0402")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.27) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text value "C_0402" (at 0 1.27) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "%R" (at 2.667 0) (layer F.Fab)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.1))
  (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.1))
  (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.1))
  (fp_line (start 1.016 -0.47) (end -1.016 -0.47) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.016 0.47) (end 1.016 0.47) (layer F.SilkS) (width 0.12))
  (fp_line (start -1 -0.4) (end 1 -0.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1 -0.4) (end -1 0.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1 0.4) (end 1 -0.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1 0.4) (end -1 0.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.016 -0.47) (end 1.016 0.47) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.016 -0.47) (end -1.016 0.47) (layer F.SilkS) (width 0.12))
  (pad "2" smd rect (at 0.55 0) (size 0.6 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "1" smd rect (at -0.55 0) (size 0.6 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
