(module Resistor (layer F.Cu) (tedit 5957E680)
  (fp_text reference Ref** (at 0 0) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (fp_text value VAL** (at 0 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (fp_line (start 3 0) (end 4.2 0) (layer B.SilkS) (width 0.15))
  (fp_line (start -2.8 0.8) (end -3 0) (layer B.SilkS) (width 0.15))
  (fp_line (start -2.6 1) (end -2.8 0.8) (layer B.SilkS) (width 0.15))
  (fp_line (start -2.2 1) (end -2.6 1) (layer B.SilkS) (width 0.15))
  (fp_line (start -2 0.8) (end -2.2 1) (layer B.SilkS) (width 0.15))
  (fp_line (start 2 0.8) (end -2 0.8) (layer B.SilkS) (width 0.15))
  (fp_line (start 2.2 1) (end 2 0.8) (layer B.SilkS) (width 0.15))
  (fp_line (start 2.6 1) (end 2.2 1) (layer B.SilkS) (width 0.15))
  (fp_line (start 2.8 0.8) (end 2.6 1) (layer B.SilkS) (width 0.15))
  (fp_line (start 3 0) (end 2.8 0.8) (layer B.SilkS) (width 0.15))
  (fp_line (start 2.8 -0.8) (end 3 0) (layer B.SilkS) (width 0.15))
  (fp_line (start 2.6 -1) (end 2.8 -0.8) (layer B.SilkS) (width 0.15))
  (fp_line (start 2.2 -1) (end 2.6 -1) (layer B.SilkS) (width 0.15))
  (fp_line (start 2 -0.8) (end 2.2 -1) (layer B.SilkS) (width 0.15))
  (fp_line (start -2 -0.8) (end 2 -0.8) (layer B.SilkS) (width 0.15))
  (fp_line (start -2.2 -1) (end -2 -0.8) (layer B.SilkS) (width 0.15))
  (fp_line (start -2.6 -1) (end -2.2 -1) (layer B.SilkS) (width 0.15))
  (fp_line (start -2.8 -0.8) (end -2.6 -1) (layer B.SilkS) (width 0.15))
  (fp_line (start -3 0) (end -2.8 -0.8) (layer B.SilkS) (width 0.15))
  (fp_line (start -4.2 0) (end -3 0) (layer B.SilkS) (width 0.15))
  (fp_line (start 3 0) (end 4.2 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.2 0) (end -3 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.2 -1) (end -2 -0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.6 -1) (end -2.2 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.8 -0.8) (end -2.6 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 0) (end -2.8 -0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.8 0.8) (end -3 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.6 1) (end -2.8 0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.2 1) (end -2.6 1) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 0.8) (end -2.2 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 0.8) (end -2 0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.2 1) (end 2 0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.6 1) (end 2.2 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.8 0.8) (end 2.6 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 3 0) (end 2.8 0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.8 -0.8) (end 3 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.6 -1) (end 2.8 -0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.2 -1) (end 2.6 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start 2 -0.8) (end 2.2 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 -0.8) (end 2 -0.8) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole circle (at -5.08 0) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask))
  (pad 2 thru_hole circle (at 5.08 0) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask))
  (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
    (at (xyz -0.2 0 0))
    (scale (xyz 0.525 0.525 0.525))
    (rotate (xyz 0 0 0))
  )
)
