(module TRRS-PJ-320A-dual (layer F.Cu) (tedit 5970F8E5)
  (fp_text reference REF** (at 0 14.2) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value TRRS-PJ-320A-dual (at 0 -5.6) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user PJ-320A (at 4 5.25 270) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user PJ-320A (at -4 5.25 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 5.1 0) (end 5.1 -2) (layer B.SilkS) (width 0.15))
  (fp_line (start -0.5 -2) (end 5.1 -2) (layer B.SilkS) (width 0.15))
  (fp_line (start -0.5 0) (end -0.5 -2) (layer B.SilkS) (width 0.15))
  (fp_line (start -0.75 12.1) (end 5.35 12.1) (layer B.SilkS) (width 0.15))
  (fp_line (start 5.35 0) (end 5.35 12.1) (layer B.SilkS) (width 0.15))
  (fp_line (start -0.75 0) (end 5.35 0) (layer B.SilkS) (width 0.15))
  (fp_line (start -0.75 0) (end -0.75 12.1) (layer B.SilkS) (width 0.15))
  (fp_line (start 0.5 -2) (end -5.1 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.1 0) (end -5.1 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.5 0) (end 0.5 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.35 0) (end -5.35 12.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.75 0) (end 0.75 12.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.75 12.1) (end -5.35 12.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.75 0) (end -5.35 0) (layer F.SilkS) (width 0.15))
  (pad "" np_thru_hole circle (at 2.3 8.6) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 2.3 1.6) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole oval (at 4.6 11.3) (size 1.6 2.2) (drill oval 0.9 1.5) (layers *.Cu *.Mask))
  (pad 1 thru_hole oval (at -4.6 11.3) (size 1.6 2.2) (drill oval 0.9 1.5) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 10.2) (size 1.6 2.2) (drill oval 0.9 1.5) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 0 3.2) (size 1.6 2.2) (drill oval 0.9 1.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -2.3 8.6) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -2.3 1.6) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 0 6.2) (size 1.6 2.2) (drill oval 0.9 1.5) (layers *.Cu *.Mask))
)
