(module SolderJumperRight (layer F.Cu) (tedit 591E0DF4)
  (fp_text reference REF** (at 1.016 -2.04) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Val** (at 1.016 -3.04) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user GND (at -2.54 1.778) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user VCC (at -2.54 -1.778) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user GND (at -2.54 1.778) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VCC (at -2.54 -1.778) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 3 thru_hole rect (at 0 1.778) (size 1.524 1.524) (drill 0.3) (layers *.Cu *.Mask))
  (pad 2 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.3) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 -1.778) (size 1.524 1.524) (drill 0.3) (layers *.Cu *.Mask))
)
