(module "SW_SPST_TL3342" (layer F.Cu) (tedit 5EA282C8)
  (descr "Low-profile SMD Tactile Switch, https://www.e-switch.com/system/asset/product_line/data_sheet/165/TL3342.pdf")
  (tags "SPST Tactile Switch")
  (attr smd)
  (fp_text reference "REF**" (at 0 -3.75) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text value "SW_SPST_TL3342" (at 0 3.75) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "%R" (at 0 -3.75) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3.2 2.1) (end 3.2 1.6) (layer F.Fab) (width 0.1))
  (fp_line (start 3.2 -2.1) (end 3.2 -1.6) (layer F.Fab) (width 0.1))
  (fp_line (start -3.2 2.1) (end -3.2 1.6) (layer F.Fab) (width 0.1))
  (fp_line (start -3.2 -2.1) (end -3.2 -1.6) (layer F.Fab) (width 0.1))
  (fp_line (start 2.7 -2.1) (end 2.7 -1.6) (layer F.Fab) (width 0.1))
  (fp_line (start 1.7 -2.1) (end 3.2 -2.1) (layer F.Fab) (width 0.1))
  (fp_line (start 3.2 -1.6) (end 2.2 -1.6) (layer F.Fab) (width 0.1))
  (fp_line (start -2.7 -2.1) (end -2.7 -1.6) (layer F.Fab) (width 0.1))
  (fp_line (start -1.7 -2.1) (end -3.2 -2.1) (layer F.Fab) (width 0.1))
  (fp_line (start -3.2 -1.6) (end -2.2 -1.6) (layer F.Fab) (width 0.1))
  (fp_line (start -2.7 2.1) (end -2.7 1.6) (layer F.Fab) (width 0.1))
  (fp_line (start -3.2 1.6) (end -2.2 1.6) (layer F.Fab) (width 0.1))
  (fp_line (start -1.7 2.1) (end -3.2 2.1) (layer F.Fab) (width 0.1))
  (fp_line (start 1.7 2.1) (end 3.2 2.1) (layer F.Fab) (width 0.1))
  (fp_line (start 2.7 2.1) (end 2.7 1.6) (layer F.Fab) (width 0.1))
  (fp_line (start 3.2 1.6) (end 2.2 1.6) (layer F.Fab) (width 0.1))
  (fp_line (start -1.7 2.3) (end -1.25 2.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.7 2.3) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.7 -2.3) (end 1.25 -2.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.7 -2.3) (end -1.25 -2.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -2 -1) (end -1 -2) (layer F.Fab) (width 0.1))
  (fp_line (start -1 -2) (end 1 -2) (layer F.Fab) (width 0.1))
  (fp_line (start 1 -2) (end 2 -1) (layer F.Fab) (width 0.1))
  (fp_line (start 2 -1) (end 2 1) (layer F.Fab) (width 0.1))
  (fp_line (start 2 1) (end 1 2) (layer F.Fab) (width 0.1))
  (fp_line (start 1 2) (end -1 2) (layer F.Fab) (width 0.1))
  (fp_line (start -1 2) (end -2 1) (layer F.Fab) (width 0.1))
  (fp_line (start -2 1) (end -2 -1) (layer F.Fab) (width 0.1))
  (fp_line (start 2.75 -1) (end 2.75 1) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.25 2.75) (end 1.25 2.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.75 -1) (end -2.75 1) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.25 -2.75) (end 1.25 -2.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.6 -1.2) (end -2.6 1.2) (layer F.Fab) (width 0.1))
  (fp_line (start -2.6 1.2) (end -1.2 2.6) (layer F.Fab) (width 0.1))
  (fp_line (start -1.2 2.6) (end 1.2 2.6) (layer F.Fab) (width 0.1))
  (fp_line (start 1.2 2.6) (end 2.6 1.2) (layer F.Fab) (width 0.1))
  (fp_line (start 2.6 1.2) (end 2.6 -1.2) (layer F.Fab) (width 0.1))
  (fp_line (start 2.6 -1.2) (end 1.2 -2.6) (layer F.Fab) (width 0.1))
  (fp_line (start 1.2 -2.6) (end -1.2 -2.6) (layer F.Fab) (width 0.1))
  (fp_line (start -1.2 -2.6) (end -2.6 -1.2) (layer F.Fab) (width 0.1))
  (fp_line (start -4.25 -3) (end 4.25 -3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.25 -3) (end 4.25 3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.25 3) (end -4.25 3) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.25 3) (end -4.25 -3) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
  (pad "2" smd rect (at 3.15 1.9) (size 1.7 1) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -3.15 1.9) (size 1.7 1) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "1" smd rect (at 3.15 -1.9) (size 1.7 1) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "1" smd rect (at -3.15 -1.9) (size 1.7 1) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_TL3342.step"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
