(module SW_PG1350_reversible (layer F.Cu) (tedit 5DD501D8)
  (descr "Kailh \"Choc\" PG1350 keyswitch, able to be mounted on front or back of PCB")
  (tags kailh,choc)
  (fp_text reference REF** (at 0 -8.255) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SW_PG1350_reversible (at 0 8.255) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 6 -7) (end 7 -7) (layer F.SilkS) (width 0.15))
  (fp_line (start 7 -7) (end 7 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start 7 6) (end 7 7) (layer F.SilkS) (width 0.15))
  (fp_line (start 7 7) (end 6 7) (layer F.SilkS) (width 0.15))
  (fp_line (start -6 7) (end -7 7) (layer F.SilkS) (width 0.15))
  (fp_line (start -7 7) (end -7 6) (layer F.SilkS) (width 0.15))
  (fp_line (start -7 -6) (end -7 -7) (layer F.SilkS) (width 0.15))
  (fp_line (start -7 -7) (end -6 -7) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.6 -3.1) (end 2.6 -3.1) (layer Eco2.User) (width 0.15))
  (fp_line (start 2.6 -3.1) (end 2.6 -6.3) (layer Eco2.User) (width 0.15))
  (fp_line (start 2.6 -6.3) (end -2.6 -6.3) (layer Eco2.User) (width 0.15))
  (fp_line (start -2.6 -3.1) (end -2.6 -6.3) (layer Eco2.User) (width 0.15))
  (fp_line (start -7 -6) (end -7 -7) (layer B.SilkS) (width 0.15))
  (fp_line (start -7 -7) (end -6 -7) (layer B.SilkS) (width 0.15))
  (fp_line (start -6 7) (end -7 7) (layer B.SilkS) (width 0.15))
  (fp_line (start -7 7) (end -7 6) (layer B.SilkS) (width 0.15))
  (fp_line (start 7 6) (end 7 7) (layer B.SilkS) (width 0.15))
  (fp_line (start 7 7) (end 6 7) (layer B.SilkS) (width 0.15))
  (fp_line (start 6 -7) (end 7 -7) (layer B.SilkS) (width 0.15))
  (fp_line (start 7 -7) (end 7 -6) (layer B.SilkS) (width 0.15))
  (fp_line (start -6.9 6.9) (end 6.9 6.9) (layer Eco2.User) (width 0.15))
  (fp_line (start 6.9 -6.9) (end -6.9 -6.9) (layer Eco2.User) (width 0.15))
  (fp_line (start 6.9 -6.9) (end 6.9 6.9) (layer Eco2.User) (width 0.15))
  (fp_line (start -6.9 6.9) (end -6.9 -6.9) (layer Eco2.User) (width 0.15))
  (fp_line (start -7.5 -7.5) (end 7.5 -7.5) (layer B.Fab) (width 0.15))
  (fp_line (start 7.5 -7.5) (end 7.5 7.5) (layer B.Fab) (width 0.15))
  (fp_line (start 7.5 7.5) (end -7.5 7.5) (layer B.Fab) (width 0.15))
  (fp_line (start -7.5 7.5) (end -7.5 -7.5) (layer B.Fab) (width 0.15))
  (fp_text user %R (at 0 -8.255) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user %V (at 0 8.255) (layer B.Fab)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_line (start -7.5 -7.5) (end 7.5 -7.5) (layer F.Fab) (width 0.15))
  (fp_line (start 7.5 7.5) (end -7.5 7.5) (layer F.Fab) (width 0.15))
  (fp_line (start 7.5 -7.5) (end 7.5 7.5) (layer F.Fab) (width 0.15))
  (fp_line (start -7.5 7.5) (end -7.5 -7.5) (layer F.Fab) (width 0.15))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer B.Fab)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (pad "" np_thru_hole circle (at -5.22 -4.2) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 5 3.8) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0 0) (size 3.429 3.429) (drill 3.429) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -5 3.8) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 0 5.9) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 5.22 -4.2) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 5.5 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -5.5 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
)
