(module "USB-C-12-Pin-MidMount" (layer F.Cu) (tedit 5EB3A296)
  (fp_text reference "REF**" (at 0 9) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text value "USB-C-12-Pin-MidMount" (at 0 -2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 7 0) (end 4.64 0) (layer F.SilkS) (width 0.2))
  (fp_line (start -7 0) (end -4.64 0) (layer F.SilkS) (width 0.2))
  (fp_line (start -4.64 6.66) (end 4.64 6.66) (layer F.SilkS) (width 0.2))
  (fp_line (start -4.64 6.66) (end -4.64 0) (layer F.SilkS) (width 0.2))
  (fp_line (start 4.64 6.66) (end 4.64 0) (layer F.SilkS) (width 0.2))
  (pad "13" thru_hole oval (at 5.62 6.1) (size 1 1.8) (drill oval 0.6 1.4) (layers *.Cu *.Mask))
  (pad "13" thru_hole oval (at -5.62 6.1) (size 1 1.8) (drill oval 0.6 1.4) (layers *.Cu *.Mask))
  (pad "13" thru_hole oval (at -5.62 2.1) (size 1 2.2) (drill oval 0.6 1.8) (layers *.Cu *.Mask))
  (pad "13" thru_hole oval (at 5.62 2.1) (size 1 2.2) (drill oval 0.6 1.8) (layers *.Cu *.Mask))
  (pad "6" smd rect (at 0.25 7.235) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at -0.25 7.235) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at 0.75 7.235) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at -0.75 7.235) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at 1.25 7.235) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at 1.75 7.235) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at -1.75 7.235) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at -1.25 7.235) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 2.45 7.235) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "1" smd rect (at 3.225 7.235) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd rect (at -2.45 7.235) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd rect (at -3.225 7.235) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask"))
)
