(module SolderJumper (layer F.Cu) (tedit 592809B7)
  (fp_text reference REF** (at 0.5 0) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Val** (at 0.5 -3) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user Right (at 4 1.5) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user Left (at 3.5 -1.5) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user Right (at 4 1.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user Left (at 3.5 -1.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 2 thru_hole rect (at 1 1.5) (size 1.524 1.524) (drill 0.3) (layers *.Cu *.Mask))
  (pad 3 thru_hole rect (at -1 1.5) (size 1.524 1.524) (drill 0.3) (layers *.Cu *.Mask))
  (pad 2 thru_hole rect (at 1 -1.5) (size 1.524 1.524) (drill 0.3) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at -1 -1.5) (size 1.524 1.524) (drill 0.3) (layers *.Cu *.Mask))
)
