(footprint "vik-keyboard-connector-vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 4.25 -3 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1f223643-2caf-4a56-89a5-0d0e5d7690f1)
  )
  (fp_text value "vik-keyboard-connector-vertical" (at 0 3 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 73fd7c8b-a7c4-42a1-8f18-947babcd56dc)
  )
  (fp_text user "3v3" (at -5.4 2.77 unlocked) (layer "F.SilkS")
      (effects (font (size 0.75 0.75) (thickness 0.15)) (justify left bottom))
    (tstamp 2164bb7b-bdf1-4a11-bca3-780a9facf731)
  )
  (fp_text user "VIK OUT" (at -3.02 -2.67 unlocked) (layer "F.SilkS" knockout)
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp 2486f5fb-9a01-45e4-b241-2da1787cb49f)
  )
  (fp_text user " C262499" (at -4 3.75 unlocked) (layer "User.2")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp 28c590ba-629f-42b9-af0d-f890495ced4d)
  )
  (fp_line (start -5.8 -1.5) (end -5.8 -0.75)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 5b7222ab-fa7a-4ae2-8ba1-186e65a3a903))
  (fp_line (start -5.8 -1.5) (end -5.05 -1.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 4ce5f806-7e91-46cb-ab95-931dae256ce1))
  (fp_line (start -5.8 1.5) (end -5.8 0.75)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 9bb56868-a5b6-4f12-84f4-f657cb62d622))
  (fp_line (start -5.8 1.5) (end -5.05 1.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 484a4e07-e9bc-45e1-a392-b3f0ce6ae893))
  (fp_line (start 5.8 -1.5) (end 5.05 -1.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 80915f11-65be-4766-a924-f671d4f1586c))
  (fp_line (start 5.8 -1.5) (end 5.8 -0.75)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 05fab351-c95a-42d4-95f4-2079df99266d))
  (fp_line (start 5.8 1.5) (end 5.05 1.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 13553c16-9c62-4aff-aa9d-c0be057d1698))
  (fp_line (start 5.8 1.5) (end 5.8 0.75)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp aa457871-977d-4c85-92b7-cbdd143c0ce5))
  (fp_circle (center -2.773 2.15) (end -2.646 2.15)
    (stroke (width 0.254) (type solid)) (fill none) (layer "F.SilkS") (tstamp 3a607dd4-b6f6-4e2f-90a0-da29060a800f))
  (fp_rect (start -5.8 -1.5) (end 5.8 1.5)
    (stroke (width 0.12) (type default)) (fill none) (layer "Cmts.User") (tstamp fa46dca5-3c7b-4e82-9189-58ea6e969cff))
  (fp_circle (center -2.773 2.15) (end -2.646 2.15)
    (stroke (width 0.254) (type solid)) (fill none) (layer "F.Fab") (tstamp fbe15807-99e8-43c5-8a18-6a36f5ae3f46))
  (pad "" smd rect (at -4.35 0) (size 1.8 2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 97f175f0-ce93-42c1-9ded-c4ebe0fed459))
  (pad "" smd rect (at 4.35 0) (size 1.8 2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 1e86b112-86a1-49c1-891c-a2bbe7090cb4))
  (pad "1" smd rect (at -2.75 1) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 52ba868a-44b3-4f10-b69e-01557684c6f5))
  (pad "2" smd rect (at -2.25 -1) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 72686d1f-2dee-4a23-8bfd-858ac8b2ad0a))
  (pad "3" smd rect (at -1.75 1) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp a3cf5e54-c93f-4273-b17a-4c4c391b4a75))
  (pad "4" smd rect (at -1.25 -1) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 04462577-9626-4b92-87e2-8b345fb53324))
  (pad "5" smd rect (at -0.75 1) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 2e1725ea-493c-4844-89c1-bd24111dcb4e))
  (pad "6" smd rect (at -0.25 -1) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp b119f5c7-0dbc-4cdc-9b76-f0f11e2a4d1b))
  (pad "7" smd rect (at 0.25 1) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 0d68b5d2-a09e-4f8d-a6a3-62c6e11a6e75))
  (pad "8" smd rect (at 0.75 -1) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 7ec4dc3a-8b14-4cc9-b833-caa6366f18f4))
  (pad "9" smd rect (at 1.25 1) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp c8ce7f80-6077-403d-8a4b-ba94004f89e3))
  (pad "10" smd rect (at 1.75 -1) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp dc7f30ac-e402-41c4-9c22-ae74f88e5c1e))
  (pad "11" smd rect (at 2.25 1) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp b004f436-cb22-4ecf-b189-fa367cb62b93))
  (pad "12" smd rect (at 2.75 -1) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 52e7a7e3-fc54-446b-b199-5e68450b3778))
)
