(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(AE3-A)")
	(net 3 "VDD_NRF")
	(net 4 "Net-(IC1-VDD)")
	(net 5 "Sys Load")
	(net 6 "Net-(U1-SW)")
	(net 7 "Net-(U1-VBST)")
	(net 8 "Net-(C20-Pad2)")
	(net 9 "+4V")
	(net 10 "Net-(C31-Pad1)")
	(net 11 "Net-(S1-RFC)")
	(net 12 "RF_LORA")
	(net 13 "Net-(IC4-SS)")
	(net 14 "+5V")
	(net 15 "Net-(IC7-SS)")
	(net 16 "Net-(D1-A)")
	(net 17 "Net-(D1-K)")
	(net 18 "D+")
	(net 19 "D-")
	(net 20 "CC2")
	(net 21 "unconnected-(J1-SBU2-PadB8)")
	(net 22 "CC1")
	(net 23 "unconnected-(J1-SBU1-PadA8)")
	(net 24 "Net-(D2-A)")
	(net 25 "Net-(D3-K)")
	(net 26 "RST")
	(net 27 "Net-(D3-A)")
	(net 28 "Net-(D5-K)")
	(net 29 "Net-(IC4-OV1)")
	(net 30 "Charger Load")
	(net 31 "Net-(IC4-ILIM)")
	(net 32 "Net-(IC4-OV2)")
	(net 33 "Net-(U2-L)")
	(net 34 "VBUS")
	(net 35 "Sol Shunt 1")
	(net 36 "Net-(IC7-OV1)")
	(net 37 "Net-(IC7-OV2)")
	(net 38 "unconnected-(IC7-CP2-Pad3)")
	(net 39 "Net-(IC7-ILIM)")
	(net 40 "Bat Shunt 1")
	(net 41 "GPS_EN")
	(net 42 "GPS_TX")
	(net 43 "GPS_RX")
	(net 44 "Net-(IC3-ANT)")
	(net 45 "unconnected-(J6-NC{slash}TDI-Pad8)")
	(net 46 "unconnected-(J6-SWO{slash}TDO-Pad6)")
	(net 47 "unconnected-(J6-KEY-Pad7)")
	(net 48 "SWDIO")
	(net 49 "SWDCLK")
	(net 50 "Net-(IC2-CSP)")
	(net 51 "Net-(D6-K)")
	(net 52 "RF_WIFI_BT")
	(net 53 "Net-(U3-L)")
	(net 54 "Net-(IC2-DRV)")
	(net 55 "Net-(IC2-VCC)")
	(net 56 "Net-(IC2-VG)")
	(net 57 "Net-(IC1-CFG1)")
	(net 58 "Net-(IC1-VBUS)")
	(net 59 "Net-(U1-EN)")
	(net 60 "Net-(U1-VFB)")
	(net 61 "Net-(IC2-COM)")
	(net 62 "Net-(IC2-MPPT)")
	(net 63 "Net-(IC5-P0.03)")
	(net 64 "I2C SDA")
	(net 65 "I2C SCL")
	(net 66 "USE_ANT_2")
	(net 67 "Net-(U3-FB)")
	(net 68 "USE_ANT_1")
	(net 69 "USR_BUTTON")
	(net 70 "RADIO TX{slash}RX")
	(net 71 "unconnected-(U5-PV-Pad10)")
	(net 72 "unconnected-(U5-A0-Pad5)")
	(net 73 "unconnected-(U5-EP-Pad17)")
	(net 74 "unconnected-(U5-TC-Pad13)")
	(net 75 "unconnected-(U5-CRITICAL-Pad9)")
	(net 76 "unconnected-(U5-WARNING-Pad8)")
	(net 77 "Net-(U1-VIN)")
	(net 78 "unconnected-(IC1-CFG2-Pad2)")
	(net 79 "unconnected-(IC1-CFG3-Pad3)")
	(net 80 "Net-(IC3-RX3)")
	(net 81 "Net-(IC3-RX1)")
	(net 82 "unconnected-(IC5-P0.30-Pad15)")
	(net 83 "unconnected-(IC5-P0.16-Pad26)")
	(net 84 "unconnected-(IC5-P0.11-Pad25)")
	(net 85 "unconnected-(IC5-LR_DIO7-Pad24)")
	(net 86 "unconnected-(IC5-P0.09-Pad59)")
	(net 87 "unconnected-(IC5-ANT_WIFI-Pad65)")
	(net 88 "unconnected-(IC5-P0.06-Pad32)")
	(net 89 "unconnected-(IC5-P0.00-Pad29)")
	(net 90 "unconnected-(IC5-P1.09-Pad34)")
	(net 91 "unconnected-(IC5-P0.17-Pad43)")
	(net 92 "unconnected-(IC5-P0.15-Pad42)")
	(net 93 "unconnected-(IC5-P0.08-Pad33)")
	(net 94 "unconnected-(IC5-P0.27-Pad16)")
	(net 95 "unconnected-(IC5-P1.03-Pad56)")
	(net 96 "unconnected-(IC5-P0.04-Pad31)")
	(net 97 "unconnected-(IC5-P1.08-Pad20)")
	(net 98 "unconnected-(IC5-P0.01-Pad30)")
	(net 99 "unconnected-(IC5-P0.13-Pad39)")
	(net 100 "unconnected-(IC5-P0.14-Pad38)")
	(net 101 "unconnected-(IC5-ANT_GNSS-Pad67)")
	(net 102 "unconnected-(IC5-P1.02-Pad55)")
	(net 103 "unconnected-(IC5-P0.02-Pad12)")
	(net 104 "unconnected-(IC5-P0.26-Pad18)")
	(net 105 "unconnected-(IC5-P0.23-Pad53)")
	(net 106 "unconnected-(IC5-LR_DIO8-Pad23)")
	(net 107 "unconnected-(IC5-P0.10-Pad60)")
	(net 108 "unconnected-(IC5-LR_DIO9-Pad11)")
	(net 109 "unconnected-(IC5-P0.05-Pad17)")
	(net 110 "unconnected-(IC5-P0.31-Pad10)")
	(net 111 "unconnected-(IC5-P0.25-Pad52)")
	(net 112 "unconnected-(IC5-P0.19-Pad61)")
	(net 113 "unconnected-(IC5-P0.28-Pad14)")
	(net 114 "unconnected-(IC5-P0.18-Pad36)")
	(net 115 "unconnected-(IC5-P0.12-Pad35)")
	(net 116 "unconnected-(IC5-P0.21-Pad49)")
	(net 117 "unconnected-(IC5-P0.07-Pad19)")
	(net 118 "unconnected-(IC5-P0.29-Pad9)")
	(net 119 "Net-(J1-D+-PadA6)")
	(net 120 "Net-(J1-D--PadA7)")
	(net 121 "Net-(AE1-A)")
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "0241f412-0dd4-44e8-8dd2-08df96938d8d")
		(at 167.475 96.03)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "1457ed92-cf54-4ef2-9dbd-043c9f26e916")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "c5698a85-991d-4a73-b6d5-56a3862674ae")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7400693b-7ba5-4097-92a0-4e248f664291")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b7c74ff1-2ae3-4391-90cc-6109e645d1fd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/38d60f25-e00c-4565-b040-4604500ef45c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cfeae6c3-a27f-484f-bc98-1cc10b6cb003")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9834058c-bf11-44a0-afdb-3adb3d4a4cc7")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "70afbb0a-c907-47e8-be53-1ba8791b1bef")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "32cf4ffc-c543-4d5e-b553-6168acbdb9bd")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7b877ab9-4658-45aa-b375-d5d6c2729813")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "956ce667-ffc6-45fa-9f28-5521cc48a7cc")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d3abe234-6f47-4e12-9013-9b6600c5cc7a")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ff4e714e-f69b-49ab-833a-c74567de0f5d")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6fe31a76-2a62-4c9c-9cda-7f1b74bde258")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c24e824f-506d-42a1-be88-94720524c023")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "495e4fd1-873e-4106-8d97-f9bec16ffca6")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ebc37b43-c038-4e1d-8c7f-9bbe618edb40")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a1b15287-8efa-49b1-8c8d-804c9ec7b0fe")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "9a9e7c9e-ae6b-4f87-b849-aa5e29aa2f0b")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 24 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "b2ce71c8-e994-4d7b-88f2-90bd44a61263")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(uuid "029ca115-dc59-471c-8611-311086adcc8b")
		(at 144.95 108.5 90)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(uuid "737bef25-27c7-4f3d-af66-e4b8c3d9ba8d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(uuid "f0245eea-eb14-4dc2-aa74-cbd4b8bf4a8f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2df68c0c-f936-4d25-8ed6-e744878de79a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b5073e14-2638-40dd-a292-7f648b2a0dcc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/1c94abd4-ca03-4d21-a561-1fcffb32bcaf")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_circle
			(center 0 0)
			(end 0 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "3d83a28c-e913-4a91-867a-f2b639d2e665")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "be433fe2-a5d2-4029-a10b-f76df685588f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
			(uuid "18572d10-7e55-4399-8b41-46d9f1d307e3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 65 "I2C SCL")
			(pinfunction "1")
			(pintype "passive")
			(uuid "271c8668-608f-43c2-b98a-3c2b57cf7847")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "030df2d2-0871-482a-8247-3eb5348dd0d6")
		(at 59.47 128.0375 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C14"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "da615a95-d6e4-4b79-859f-a25fc53c67bd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "1a13b0a0-3f0c-4ef1-a9b9-2f1190d9075a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c2c776c2-d8da-4f64-8b4c-def7438bb57c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5c009297-db3e-45b9-ab53-a77dbc4b5880")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/3a72942d-8d10-4780-ba77-05e4c7e0c89f")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "da7b3f3e-00d2-40bf-87bc-dfa9d3e2623f")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "51127693-d78f-47f1-9ddb-e1b656db07e4")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d7f4e953-4ec9-44a7-b458-a72c49cec8c6")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f6c0044d-8a4b-449d-9060-ae7d549df115")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a1567e05-f2c7-451b-90c9-a066aeadc2ae")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d96bc10e-19c2-438e-9595-b7fa1c5d7b9f")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4a4c7045-5d8c-4193-9d39-84e2036b7389")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9589d83a-b0ad-48f8-99ae-3a4ac3944da4")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dbf8df39-2811-4a83-a398-d1ea57d65625")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6ae6690c-de85-42c1-bf93-e9d499a672f2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "5b2cad25-0d37-4736-b105-9abbd85b3c82")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "57ea4b9f-135d-4551-a926-36915b8d1acb")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "e179d0f1-950d-45cb-a94b-f9a9926d5ecd")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "0509464c-8562-4ede-9131-78ad03a7d014")
		(at 127.25 105.7)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R31"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "088ba73c-8cdb-4108-b32c-112a89c6190c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "696dbc2b-0f39-4b91-8924-d0ff537afa48")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7b265756-566d-4ce0-ad2f-41741e487dad")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9156814a-1d5f-4a55-a0c5-8238990055fc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1a822f60-b17c-4df0-98d1-22ceac6a2d4f")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "477dd62e-a167-4d5c-8ab2-9700cd28916a")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dfd23dc4-9fe9-4363-b41d-48e46c44928e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f453aef8-f50d-4b7c-93be-a6b45e607d44")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c409c088-76c6-42e0-9976-0b7a05126b60")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7eb74e70-3a75-4e1d-8666-b198a20d5538")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3ebbf88-fa60-42ea-bd11-5587d50dae4e")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "533ce892-9d20-47f6-abd2-1175df5a066f")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5ce47c4a-7a0f-4140-9cbf-5aa1b7ef83a8")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "035d26b9-174d-49f9-b2d6-e80bf0c00186")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9ab59be-24d2-4bdf-8c11-2d86fc6e896c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "26c615f4-3468-4fb9-8be7-caa39ccb74f9")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 36 "Net-(IC7-OV1)")
			(pintype "passive")
			(uuid "d9fa66c6-6090-4c28-9055-57d32cfe69be")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "fa66fd39-b963-48bb-b363-8533bac20232")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "0d421c58-f71f-46e3-96e8-d9967fe4f0b1")
		(at 127.25 102.75)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R30"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "68e74abb-a27c-4d84-8fa0-6751966309d4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "23.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "9510c333-c412-46b6-8f9a-2ffb46e68f91")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "79ec76a6-42aa-4690-a015-6a01d8b2ffec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ed8b5c1e-e0d6-4876-9a96-98d60c69e7a3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/d77e74ad-289f-4869-951b-895aa3e2bfce")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "547e400f-ed23-4679-ba01-699260657dc5")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d902f23-a67d-4959-bbf2-6bb9013ffd3c")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3208d094-c60f-4052-999c-615a140319cf")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8b592831-413a-41e0-a084-d2a6acb5a2dd")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "21589df8-a27c-495b-8a3a-9c63b014bdf8")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2fe30c4e-158c-4754-966e-63a346151e2c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f32552e8-39b7-4983-9b8f-60467beaf082")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9344202-c9e3-4eb7-b1c8-67b0f0bbbd93")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b25a2d27-26a0-4a0b-a1e4-809d87d2bb51")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "13241369-a569-4ca8-ae80-cba2e0c6f1d1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "7759c82f-7ef1-470c-8e3f-0d6d58eb3f52")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 34 "VBUS")
			(pintype "passive")
			(uuid "26f2d040-9634-4cd8-8c55-6e04676e84b8")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 36 "Net-(IC7-OV1)")
			(pintype "passive")
			(uuid "60bb3201-d983-4f6e-9594-5fbf94641d20")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "0d502196-7dc9-40a1-82c4-71ff9d3f7736")
		(at 193 122)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R22"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "9375a57c-41cf-4561-acfa-3ea1bc592284")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "b7120c22-b57b-462c-8724-16e1de4d80a8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f4c48bed-cbde-4ab5-b8c1-efbc20799d9a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d02ea77d-4742-43f2-bd95-1b41a5897424")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/fcf2334e-e740-45e3-82e6-22af6b28ce73")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a7026459-47d4-461a-9d4f-35c526fbc545")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c9533944-3be7-4e42-8e87-32e88343aecd")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4a9f5928-e232-479d-bb1f-6fc9952143ca")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ee8c37bf-54e0-4805-a69d-0b49f84723f3")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "774c3f2e-ea74-48eb-b7e9-d2d7a7787e2b")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d059925e-6d21-4289-b6b7-d44dcffbc4bb")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "571c070e-c19d-4ea4-a012-6962d12b8c2c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "75a43a37-8885-484c-a0ae-8d2d1763c467")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e87d92fd-f95a-4542-8648-747eae907f9a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cdf25003-e5eb-4e22-8602-dcec80509f46")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "71d8c446-ad2c-40a7-a042-d8893d89c734")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 68 "USE_ANT_1")
			(pintype "passive")
			(uuid "2811f0ca-8a08-4322-b039-3e088fc308e9")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "a4d82aa1-77f4-442b-affd-d6dccb66071f")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "10270a71-ea9d-4d4b-af6a-5b3d403971c8")
		(at 68.05 104.1375 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R20"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(uuid "2a6bdd32-2280-41b7-ac69-8afd1cfd5bc3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "9d190a29-6cc0-46d7-a64c-3241fb6cfc68")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e96aba80-7c92-465f-8193-05efabe03728")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "086e5ebe-8b76-4429-96ae-65e6d84d4f2e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/9aa206f9-44a1-4d19-bc8c-36f9838954c7")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d953643-ed86-45d4-94fa-204d6b9725b6")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49e96df9-f891-4af2-8cfd-24cf29416bbe")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "117ade29-e1f9-411d-95e8-84b17441120f")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5e355367-0c33-411b-8b98-32281e494bd7")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c15c78cf-a6ad-4a31-99fb-1984ee6a59c8")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "18c225be-25dd-4b29-95f2-d33b3fe0c9c6")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b611cf82-8573-4979-850d-09da7bd9b32f")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b63c94b6-e8ee-4e2b-bfa1-ccf4b73fc8d2")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "11663a04-0af9-433d-b382-2c40f8bc61eb")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a1e979f-0de4-496c-89c1-dddc5d5020fc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "89d7d0ce-441a-4770-9452-19673f2a5721")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 67 "Net-(U3-FB)")
			(pintype "passive")
			(uuid "06dab136-e30a-4770-976a-956097bb5c2c")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "5541aa82-001b-49a9-b076-95da271f782e")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "1232e229-341d-48e8-8916-8b73894b6eb2")
		(at 188.0375 110.98)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C25"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "bf718e70-477e-4e69-8abf-4692ea5e1c3a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "220pF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "7fd3b94e-77db-4df2-9a50-536fe1b5c74f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "94f32599-d62c-4132-a91f-ce0ec87390dc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "051f38eb-8ad0-46ce-8d99-1e7a58739c28")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/74b2a195-63b3-426e-86a3-393512917391")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "752604d8-28ea-40b6-9b8a-09eab2725d02")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "00338009-7ad3-451d-af1d-6500a19ec526")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "750dfb72-2dde-4938-b5e1-5f28f8f1cb85")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ecca0d47-8a22-43c0-bf30-6a60c27939b7")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e29bdc98-e93c-44dc-b161-6b2456c1ddc3")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8b36a0d1-608e-467c-88da-28669e844c5b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cd4a7151-41d8-4318-8710-a54d9d3e9ba9")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a3e52350-72cc-4ba0-873d-a22809523f6f")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51778b01-8b84-41d8-86b0-5346c4e28a8b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "015f3011-1163-43a0-8e04-3724a1defb3b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1c504c0e-c241-4290-a3e1-c3aaa02fa20d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 9 "+4V")
			(pintype "passive")
			(uuid "2a634e05-cbc7-474e-96e3-84c0f5a105da")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "90d680c1-4e55-4e7c-a9df-f51fc23a542b")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "1702821f-e740-4319-ba4c-31b9b437ea4e")
		(at 177.5 100.49)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "432d6355-e688-4001-9624-82fa59a7124a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "d50ae243-2026-40f8-82f3-4586544c54de")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "eeb5da18-def1-4d4b-9642-80228aaa79f7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d4cd10c6-2414-4af8-b0ed-99a29eaa45ed")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/31502cff-abd5-4e7b-94dc-a1acf0f3ad7c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "844d7bf1-456d-4a1d-abf6-be861bd61686")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "77d821e5-ebb2-4c0c-8297-5addca2e63f5")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f433a188-faeb-4001-aa81-21efd7c63c89")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0a77f2ca-ebb0-449d-bd2a-fc0a5792790b")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5df8e0a9-3563-476f-87ee-9e860934934c")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "781a3702-82a0-4cd5-98f8-960bd5c30782")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3bb365ce-7ef2-47ab-8c96-9ef5f48bd4f4")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15b1be83-1499-4a55-9766-448ae12f8bb7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17e18857-ee1b-44e2-bab1-6771c284bd50")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "417902a0-ad75-421a-8b52-fb81bf64f013")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4c9ba43a-eaaf-4056-9d0e-5966e3cdf266")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "f929215e-3fae-44e3-a710-bb459585f9bb")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "aaa25318-f684-4c05-9e0f-2f5752f47f1f")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_SXN_SMDRI124"
		(layer "F.Cu")
		(uuid "1aca88f2-f134-4a69-8bbc-3daef51b85bd")
		(at 78 101.5 90)
		(descr "Inductor, SXN, SMDRI124, 12.3x12.3x4.5mm, (https://www.sxndz.com/upload/202108/16/202108161607454319.pdf), generated with kicad-footprint-generator gen_inductor.py")
		(tags "Inductor sxn smdri")
		(property "Reference" "L1"
			(at 0 -7.15 90)
			(layer "F.SilkS")
			(uuid "8bf634eb-7eeb-415c-b5cf-f8eeed6acd89")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2.2uH"
			(at 0 7.15 90)
			(layer "F.Fab")
			(uuid "2538a3e4-9ab7-4fee-8260-9e3f212810af")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "b47528f1-aa95-4232-a88b-60291943ba4d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "dcd0f447-c5f8-4366-907c-9766b62066c1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C2929497"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e46f568c-6e68-45b3-b5b0-8d60c69f54b9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/82f13ee3-6bfb-48e6-a947-d56420d89774")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start 6.41 -6.41)
			(end 6.41 -2.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "43ba11c1-3f1d-4c8b-88da-287173ed9dbe")
		)
		(fp_line
			(start -6.41 -6.41)
			(end 6.41 -6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "74fa89b9-b07f-4bfd-8d22-ebe44c86363a")
		)
		(fp_line
			(start -6.41 -6.41)
			(end -6.41 -2.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8d96029a-b45e-445d-a248-8528f6626ffd")
		)
		(fp_line
			(start 6.41 6.41)
			(end 6.41 2.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a931f81-8fb3-4c4a-aa94-38868221a763")
		)
		(fp_line
			(start -6.41 6.41)
			(end -6.41 2.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9ce7f9be-2f68-40b7-8d8c-d49a9c33f92e")
		)
		(fp_line
			(start -6.41 6.41)
			(end 6.41 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc346d3f-6547-4938-9bf9-6b3890d91d95")
		)
		(fp_line
			(start 6.65 -6.4)
			(end -6.65 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aa3df6ce-e577-4c2f-9dbd-3f832d18ef2d")
		)
		(fp_line
			(start -6.65 -6.4)
			(end -6.65 6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8c9dfadb-aab4-4ec2-901e-07243de44516")
		)
		(fp_line
			(start 6.65 6.4)
			(end 6.65 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3ada46e2-50e0-45c7-9986-4fec45fc797f")
		)
		(fp_line
			(start -6.65 6.4)
			(end 6.65 6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8a42b5ec-2a96-476c-98f5-8ef9e8041719")
		)
		(fp_line
			(start 6.15 -6.15)
			(end -6.15 -6.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57237a72-52b6-419f-8dd9-7527a264185a")
		)
		(fp_line
			(start -6.15 -6.15)
			(end -6.15 6.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "663b3729-8b8b-40fa-bd56-23f4dafac62a")
		)
		(fp_line
			(start 6.15 6.15)
			(end 6.15 -6.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b852c99-dde2-4fe6-9213-c73d8cb93beb")
		)
		(fp_line
			(start -6.15 6.15)
			(end 6.15 6.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1590cfe-3132-4acb-b709-10bf4222ed3d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "88d22d43-9475-449b-a6d2-7eb6158043f9")
			(effects
				(font
					(size 0.966667 0.966667)
					(thickness 0.145)
				)
			)
		)
		(pad "1" smd roundrect
			(at -4.95 0 90)
			(size 2.9 5.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.086207)
			(net 6 "Net-(U1-SW)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "b069a4af-f042-4427-9de2-f1e3edf4d351")
		)
		(pad "2" smd roundrect
			(at 4.95 0 90)
			(size 2.9 5.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.086207)
			(net 3 "VDD_NRF")
			(pinfunction "2")
			(pintype "passive")
			(uuid "7c856946-2b71-4499-bc8d-aa27bbe97040")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_SXN_SMDRI124.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:Texas_R-PDSO-G6"
		(layer "F.Cu")
		(uuid "26b9b1be-ac7c-4b93-9ac5-3f7665d810ee")
		(at 68.62 121.4 90)
		(descr "R-PDSO-G6, http://www.ti.com/lit/ds/slis144b/slis144b.pdf")
		(tags "R-PDSO-G6 SC-70-6")
		(property "Reference" "U2"
			(at 0 -2.25 90)
			(layer "F.SilkS")
			(uuid "16f10bd6-5581-400d-89e3-9235d95ed03d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TPS61222DCK"
			(at 0 2 90)
			(layer "F.Fab")
			(uuid "b439dfb4-4cc1-4c15-9d5d-346e44020fd9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61220.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f41ab996-d95a-4e40-b63b-85aa406fa15d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "49fd031e-41e0-45fd-a54f-e8807bb382a4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C116461"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c356c55e-90b7-4716-a0a3-f1b789e4711e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Texas*R*PDSO*G6*")
		(path "/88898e51-2e9a-44c4-b336-70a2f81aebb1")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.7 -1.16)
			(end 0.7 -1.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "af70df03-3d27-4a40-aa15-db078d6d46bc")
		)
		(fp_line
			(start -0.7 1.16)
			(end 0.7 1.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0769b283-c4dd-4f39-91f3-00a1b8eee537")
		)
		(fp_poly
			(pts
				(xy -1.12 -1.11) (xy -1.36 -1.44) (xy -0.88 -1.44) (xy -1.12 -1.11)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "3d237bda-a6d3-4589-8ede-7118c9462b81")
		)
		(fp_line
			(start -1.6 -1.4)
			(end 1.6 -1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d0f0780e-881e-4d8a-a20c-6864e91b43f7")
		)
		(fp_line
			(start -1.6 -1.4)
			(end -1.6 1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "420c7384-f936-48ba-b26f-1aa7f6a00492")
		)
		(fp_line
			(start 1.6 1.4)
			(end 1.6 -1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "36480067-e132-456c-b588-1f217ec9e7d8")
		)
		(fp_line
			(start -1.6 1.4)
			(end 1.6 1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3349d3c-520a-4fb1-b1ab-ec706a334c9e")
		)
		(fp_line
			(start 0.675 -1.1)
			(end -0.175 -1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a2f88e97-f3b9-4d30-95d3-68c2bba20119")
		)
		(fp_line
			(start 0.675 -1.1)
			(end 0.675 1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "03d9af9e-8704-4637-8065-7aa712e5cced")
		)
		(fp_line
			(start -0.175 -1.1)
			(end -0.675 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8732ad77-45bc-45a7-a761-eaf51dcc9e97")
		)
		(fp_line
			(start -0.675 -0.6)
			(end -0.675 1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "68f2e77e-9c98-468c-8b97-b426775c50e2")
		)
		(fp_line
			(start 0.675 1.1)
			(end -0.675 1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e17924a9-06b8-49ab-8a8b-a061918e41a8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "28e59760-b7be-4f63-b7a5-872c3d704220")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.075)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1 -0.65 90)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VDD_NRF")
			(pinfunction "VIN")
			(pintype "power_in")
			(uuid "0f5c3f50-d472-45ce-ae05-f3f0d0bfc8a5")
		)
		(pad "2" smd roundrect
			(at -1.1 0 90)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "+5V")
			(pinfunction "FB")
			(pintype "input")
			(uuid "31106abf-f16b-4357-afd7-75bb8caed248")
		)
		(pad "3" smd roundrect
			(at -1.1 0.65 90)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "956d1de3-9559-46a8-91d8-80015abf37b3")
		)
		(pad "4" smd roundrect
			(at 1.1 0.65 90)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "+5V")
			(pinfunction "VOUT")
			(pintype "power_out")
			(uuid "c81adc70-c7af-4eac-ac74-158c69cdec61")
		)
		(pad "5" smd roundrect
			(at 1.1 0 90)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Net-(U2-L)")
			(pinfunction "L")
			(pintype "power_in")
			(uuid "be7027d9-1e4f-41cc-9363-9f6f5c365c31")
		)
		(pad "6" smd roundrect
			(at 1.1 -0.65 90)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VDD_NRF")
			(pinfunction "EN")
			(pintype "input")
			(uuid "1a609968-34dd-4497-9033-4b0c13e9c342")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(uuid "28a68239-a45e-4be1-8d23-78151fdec9d6")
		(at 144.95 100.4 90)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(uuid "a3bd59b9-d499-4eae-8734-9e829fc88a7b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(uuid "1404ce2a-41b8-4754-8fc1-7c68de71b521")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f59442d1-d927-4442-8c00-21b25740b024")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "45f78aca-934c-4b43-815f-0572f599bd29")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/5c91fc53-c07f-4cfc-a479-3e45d9a2734b")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_circle
			(center 0 0)
			(end 0 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "3f9b0c54-840c-402a-be54-14defca74af9")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "ed4ae7f0-c447-4028-acf5-397a0908ca94")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
			(uuid "6181fd11-e05b-403d-8611-4b2fb86a04bc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 5 "Sys Load")
			(pinfunction "1")
			(pintype "passive")
			(uuid "af9633fc-b96e-4a73-a616-5e8f3f6b1166")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "28ae58f6-b46a-407a-8bed-5d303d0530ea")
		(at 117.75 99.8)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "96749292-8eb1-4871-91d5-7a61b5ceed67")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "51k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "a8edb314-10b2-483b-a80b-9f3fdcefe171")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c22c0e6a-419b-46eb-ba7f-a6ec999f8c7f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "921424c5-8742-4120-99df-8673d3d26c93")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/989e4871-e710-4c31-98f4-e3fdf042549c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b5df7c55-4165-4c38-a01e-ef4d218f3341")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7a839cc-301d-4a86-94bc-557b88416848")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0edf43d3-0a14-43b6-829f-7fbd805ec0af")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "df515215-d454-403b-92e7-16bc504b2c8b")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "476616c0-bb7d-49b9-b18c-d46d015be9c6")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "65ff4915-6cfa-4d82-a1ec-fdc7db2ecea8")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6605652c-c2a6-4391-81e3-d62fd34e196b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "073e3ff6-e4aa-4ee6-8435-6be8aa1d013f")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "90411b1d-9797-42c9-b7e1-1cce2d0443bc")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "90dbfbf2-5f3c-4142-bc1a-de86951d1d51")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d873588c-67b0-4584-9c11-deab79950b2d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 30 "Charger Load")
			(pintype "passive")
			(uuid "24c3b5a0-ee1e-49d0-aeaa-5b03addc1016")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 62 "Net-(IC2-MPPT)")
			(pintype "passive")
			(uuid "d4906eb8-a5e8-4562-ac24-f60a6936b682")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(uuid "28e79c97-3409-4da6-ba56-c2930e6fd4a3")
		(at 149 104.45 90)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(uuid "c80825d9-515c-4673-b2c3-40d8fd6fda11")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(uuid "1c710eab-5e63-473e-910e-589ade1fc673")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "08cf419f-82dd-4373-92a9-0feabd0cc4bc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c4fea6ce-8e97-443f-a62a-df48a25d9ffa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/4e9b4119-64dd-4708-a871-9172dda61a32")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_circle
			(center 0 0)
			(end 0 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "94134dc9-15c5-4e16-b937-71fea7f6f999")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "2856ceb8-2d84-45fe-9e3b-e4ddeca48477")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
			(uuid "0f2d3e2a-a8b7-4dbd-a138-bb2fde7f3586")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 35 "Sol Shunt 1")
			(pinfunction "1")
			(pintype "passive")
			(uuid "e0feb448-ba3f-4a71-adff-ce4318b56da6")
		)
		(embedded_fonts no)
	)
	(footprint "Package_DFN_QFN:Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
		(layer "F.Cu")
		(uuid "29632d0b-9a7b-4973-b606-442d1403160a")
		(at 132.78 101.48)
		(descr "Texas RGV0016A VQFN, 16 Pin (http://www.ti.com/lit/ds/symlink/ina3221.pdf#page=44), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "Texas VQFN NoLead")
		(property "Reference" "U5"
			(at 0 -3.33 0)
			(layer "F.SilkS")
			(uuid "c75cdbcd-27a3-4cf4-9cf4-3a1a14050c1f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "INA3221"
			(at 0 3.33 0)
			(layer "F.Fab")
			(uuid "4911e515-04d9-4ee4-8c23-db7bc4eb8024")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina3221.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "56c162ee-696d-47a8-9b39-62e0d53fd441")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Triple-Channel High-Side Shunt and Bus Voltage Monitor with I2C and SMBUS Compatible Interface, QFN-16"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9cf3e4bc-b6d5-4d6f-851b-1d9d147dce65")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C181255"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b35fb02c-e07b-4dc6-b1fc-0b066b414e0d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field6" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "78729e69-559b-4c9b-ba5e-7d5ae665bf1f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Texas*RGV0016A*")
		(path "/baa3bafb-eaa8-4edd-b990-34769c6f289b")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.11 -1.41)
			(end -2.11 -1.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f5fbb318-1235-4815-826d-6d9eca379318")
		)
		(fp_line
			(start -2.11 2.11)
			(end -2.11 1.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a3f9dd79-f4d3-4c8d-a0d9-30495e5ac5e6")
		)
		(fp_line
			(start -1.41 -2.11)
			(end -1.81 -2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "58846b56-3a76-4165-a028-4318086c017a")
		)
		(fp_line
			(start -1.41 2.11)
			(end -2.11 2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9a27eaed-27da-4536-aa20-999174a8648a")
		)
		(fp_line
			(start 1.41 -2.11)
			(end 2.11 -2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "80c45b49-0193-40bb-98a7-076afa138283")
		)
		(fp_line
			(start 1.41 2.11)
			(end 2.11 2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd9f2c4d-deae-4a50-90aa-5b4bc58a0511")
		)
		(fp_line
			(start 2.11 -2.11)
			(end 2.11 -1.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a5c6439e-c48f-413f-80dd-be647a66014a")
		)
		(fp_line
			(start 2.11 2.11)
			(end 2.11 1.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10bbb852-1c8b-4aed-99e5-ac6c8d06de5b")
		)
		(fp_poly
			(pts
				(xy -2.11 -2.11) (xy -2.35 -2.44) (xy -1.87 -2.44) (xy -2.11 -2.11)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "6bbcca5a-99d3-4e16-93f3-c02f2107fe11")
		)
		(fp_line
			(start -2.63 -2.63)
			(end -2.63 2.63)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dfcb5b1f-d187-45b5-9f42-93bfc49478c0")
		)
		(fp_line
			(start -2.63 2.63)
			(end 2.63 2.63)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "65e82838-7bad-4e8b-844b-55071cd63907")
		)
		(fp_line
			(start 2.63 -2.63)
			(end -2.63 -2.63)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b630401b-f1c5-419e-afc6-8dee463c760a")
		)
		(fp_line
			(start 2.63 2.63)
			(end 2.63 -2.63)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7729b00e-5bdd-4399-8ab9-1939b86c717e")
		)
		(fp_line
			(start -2 -1)
			(end -1 -2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb8effd2-aded-4cf4-a3a8-4b369a0582ad")
		)
		(fp_line
			(start -2 2)
			(end -2 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15ce8b85-5207-4ebd-97d4-e22bd89deace")
		)
		(fp_line
			(start -1 -2)
			(end 2 -2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "113b9aab-7d71-419c-9782-ef6c57ac1fae")
		)
		(fp_line
			(start 2 -2)
			(end 2 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3e7d1263-2ffa-4a16-90cf-9b105efea93b")
		)
		(fp_line
			(start 2 2)
			(end -2 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "528d4bd5-8daa-40e5-9a47-c2f67ed2fe52")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a92bf5e1-2a5a-4a22-8759-6fddd72af74d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" smd roundrect
			(at -0.525 -0.525)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "e37eea74-b2e4-4132-ac9a-d2970f979439")
		)
		(pad "" smd roundrect
			(at -0.525 0.525)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "216a513c-c2aa-4920-9a0a-fa933d40c87c")
		)
		(pad "" smd roundrect
			(at 0.525 -0.525)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "9ee46616-83b7-4dcc-aa05-a636c075e78a")
		)
		(pad "" smd roundrect
			(at 0.525 0.525)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "e8662ba9-807b-4ec5-a603-ab6775c514a3")
		)
		(pad "1" smd roundrect
			(at -1.8625 -0.975)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Sys Load")
			(pinfunction "IN-3")
			(pintype "input")
			(uuid "f2675e44-7a1b-4d98-9ac8-eeaae4fedc22")
		)
		(pad "2" smd roundrect
			(at -1.8625 -0.325)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Sys Load")
			(pinfunction "IN+3")
			(pintype "input")
			(uuid "19c48686-3e98-44c3-9748-724c9bfede7c")
		)
		(pad "3" smd roundrect
			(at -1.8625 0.325)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "029f5e8d-1472-47f9-be23-eb09cce0d6c6")
		)
		(pad "4" smd roundrect
			(at -1.8625 0.975)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VDD_NRF")
			(pinfunction "VS")
			(pintype "power_in")
			(uuid "9ec4b9e3-231d-41ca-bcd5-d9d2e8bf5567")
		)
		(pad "5" smd roundrect
			(at -0.975 1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "unconnected-(U5-A0-Pad5)")
			(pinfunction "A0")
			(pintype "input+no_connect")
			(uuid "8be97812-e196-49c7-9e21-48c345b4f56d")
		)
		(pad "6" smd roundrect
			(at -0.325 1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "I2C SCL")
			(pinfunction "SCL")
			(pintype "input")
			(uuid "44bc0102-de50-4997-ae88-26ec07b60ee3")
		)
		(pad "7" smd roundrect
			(at 0.325 1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "I2C SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
			(uuid "b876d330-029a-4996-99af-dd4815cda264")
		)
		(pad "8" smd roundrect
			(at 0.975 1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "unconnected-(U5-WARNING-Pad8)")
			(pinfunction "WARNING")
			(pintype "open_collector+no_connect")
			(uuid "d15d30f4-473d-472c-8007-a17e8ce5b51b")
		)
		(pad "9" smd roundrect
			(at 1.8625 0.975)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "unconnected-(U5-CRITICAL-Pad9)")
			(pinfunction "CRITICAL")
			(pintype "open_collector+no_connect")
			(uuid "b3267988-ed92-4efd-ac93-971bced81ace")
		)
		(pad "10" smd roundrect
			(at 1.8625 0.325)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "unconnected-(U5-PV-Pad10)")
			(pinfunction "PV")
			(pintype "open_collector+no_connect")
			(uuid "84421935-835e-45e3-9b18-8c46188cc247")
		)
		(pad "11" smd roundrect
			(at 1.8625 -0.325)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "Bat Shunt 1")
			(pinfunction "IN-1")
			(pintype "input")
			(uuid "06696362-0db5-4bae-b265-db15e0c1569e")
		)
		(pad "12" smd roundrect
			(at 1.8625 -0.975)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "Bat Shunt 1")
			(pinfunction "IN+1")
			(pintype "input")
			(uuid "0988b45f-19f2-45b9-8765-07b1bfe25431")
		)
		(pad "13" smd roundrect
			(at 0.975 -1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "unconnected-(U5-TC-Pad13)")
			(pinfunction "TC")
			(pintype "open_collector+no_connect")
			(uuid "976b616c-75a2-4923-b8d5-a3d7cc5286b4")
		)
		(pad "14" smd roundrect
			(at 0.325 -1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "Sol Shunt 1")
			(pinfunction "IN-2")
			(pintype "input")
			(uuid "13ae2fc5-b994-4acf-a69b-acb891492ca5")
		)
		(pad "15" smd roundrect
			(at -0.325 -1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "Sol Shunt 1")
			(pinfunction "IN+2")
			(pintype "input")
			(uuid "c5bca089-7489-4a7e-8c69-7daddcbd28a0")
		)
		(pad "16" smd roundrect
			(at -0.975 -1.8625)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VDD_NRF")
			(pinfunction "VPU")
			(pintype "power_in")
			(uuid "2a0d2df5-2ac3-488f-bac6-ac1a0ad66ad8")
		)
		(pad "17" smd rect
			(at 0 0)
			(size 2.1 2.1)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 73 "unconnected-(U5-EP-Pad17)")
			(pinfunction "EP")
			(pintype "passive+no_connect")
			(zone_connect 2)
			(uuid "8e8ea4f2-6ec8-413f-a9fa-869c3dba613c")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "30482443-c56c-4780-bee2-cc87c664b357")
		(at 113 117.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "e7ec2cf9-54cb-4b1d-8056-095b79702204")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "120"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "d01d0ddb-e995-4032-93fd-47c7c86569e2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "53724105-bb0c-416b-b262-14c6e70e154c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ff8dfa9f-fda1-459a-b4d2-c15db7a0401a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/34f90ef6-cdeb-49a0-b801-1a46978c2982")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "acce5009-c262-4995-8225-28b36724dce8")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "813187d1-8c71-4ef0-856d-f1356b5e8c27")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "22a083a4-6e05-4bb1-9cdd-0d9c9b3d34bc")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4143600c-c0cf-401f-b126-536158d27259")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c3436cb8-5b64-476b-bb48-7f20c08f1a46")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c3e49c4d-f19b-4c29-93ac-ca49eb3200f0")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "50a0a7e5-ede1-48c3-8109-e112845d7af8")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80f7f8c5-94e3-4699-8da9-98e4fb5b39fc")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a2eaaec6-d962-4dac-add4-9ac7186444a6")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3a217f4c-dd5d-4763-a3d1-dcd4af79d090")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f7361101-12e1-4e7d-93ab-bd0089b10ead")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 61 "Net-(IC2-COM)")
			(pintype "passive")
			(uuid "b29269e1-24f7-4611-af09-1e3c05a4f46c")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 8 "Net-(C20-Pad2)")
			(pintype "passive")
			(uuid "9c886013-41b5-44ec-bd9a-b2ee493e8e4c")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "33a717c9-bb82-4893-a3a3-b3d1a3d3aa77")
		(at 129.5595 125.435)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D3"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "aa70675a-c944-40c6-8c5c-59c3f7d06d5b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "120afc91-e453-4bad-bf2d-9c6370f90acb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "73d3d265-aa10-4e34-8c44-f17cb68e7a83")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ab3c02b9-fff7-4b14-931c-04efa1d3f192")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/a43975a2-00d5-4ed2-9ce3-de26a28fb474")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eb45467a-bc95-4a97-8cf6-b6231a840f16")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6b6e3f14-f781-43bc-b245-63f90003eaa4")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9385ba0d-6ee1-4664-8645-5a489aea077c")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50160a26-1294-4c38-8392-8c8bcfcea4d0")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0d3e2cb8-d076-43cd-8050-0a7b0020c28e")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d50a175d-db36-40a9-9217-d2252bab05b1")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ef7b2cfe-188d-44ad-a1be-c59062e4a01f")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c254689-1805-4ea7-84ed-dadc1af5e20c")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b05990c4-82cc-48c9-923d-4a00a2d753e6")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a43f6ad2-d88a-43dd-a378-94b410604b8f")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f0fa9eaa-9c65-400a-8184-a72687f68efb")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d7d8ba6-1da7-4d00-b2b0-6daf894bcb4a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f04e8059-e9c3-4384-832b-7c0122ea1411")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 25 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "61c3bd96-2ed9-44a9-aaaa-c47231289581")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 27 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "a78bd78c-e820-40ab-9b01-88d7c0166c01")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "3541fddc-b59d-4380-9464-e6385d21c45a")
		(at 53.45 128.0375 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C12"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "f0899002-37ea-4425-bbc3-3eac1733a887")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "5299a120-e2f2-4187-96db-f32daca5e397")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a2187c8e-d9d3-49d8-919d-cdda54c691c9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "460bedf2-5921-410f-99e5-f2bb67a8d9c3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/89dfac6b-c1b2-4fc1-b664-4f6afbbf8739")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "66a335e7-c567-48a1-84d4-0046cf43ac62")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "41de304f-97e3-401d-af2d-80b01afffde4")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ae30fa84-c69d-4556-959c-9b6e03f7d2c6")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f473474e-07bb-45a3-84f0-7e47523ce088")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7aecebe1-2a09-49a0-bbe2-b54d31eb53ce")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "74e6ae07-68bf-418f-a7c9-5c8066bf4e3d")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6eced67f-2c8b-44d6-8315-1c26e3def489")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5d7c5a1a-a7ad-4fae-93db-3210c482a58c")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "05f1937c-f737-449b-b87a-63a7a054e2f3")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "550fd58b-7ac8-4903-a9b5-3a2771fbb110")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "e9a299bd-bd35-4f83-9a10-8e2cb1b03589")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 77 "Net-(U1-VIN)")
			(pintype "passive")
			(uuid "d4f58a30-2deb-486d-9d30-9ec05cc15e58")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "8196ecd0-1899-4e4b-84ad-fe0b2577d28b")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:Texas_R-PDSO-G6"
		(layer "F.Cu")
		(uuid "357a890b-56c8-4575-a289-924c1325e856")
		(at 72.545 121.4 90)
		(descr "R-PDSO-G6, http://www.ti.com/lit/ds/slis144b/slis144b.pdf")
		(tags "R-PDSO-G6 SC-70-6")
		(property "Reference" "U3"
			(at 0 -2.25 90)
			(layer "F.SilkS")
			(uuid "31c59d90-074a-40eb-afd2-0ca77afa4754")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TPS61222DCK"
			(at 0 2 90)
			(layer "F.Fab")
			(uuid "98511f89-36b6-4d84-a3f6-83b2d67bd9d9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61220.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "634b7752-1aea-40cf-a169-646d887f6ba0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3490f9b4-03df-4b3a-956c-cc9fc3543397")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C116461 "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0c465e5c-7627-47c2-b2b0-67b2a94c6a22")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Texas*R*PDSO*G6*")
		(path "/57949f98-963c-4677-a24d-43c4f416800c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.7 -1.16)
			(end 0.7 -1.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1a86b5ca-59b3-4ee5-bd64-5068d7758466")
		)
		(fp_line
			(start -0.7 1.16)
			(end 0.7 1.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e89ebe81-1d57-43cf-8e21-254db1959fa0")
		)
		(fp_poly
			(pts
				(xy -1.12 -1.11) (xy -1.36 -1.44) (xy -0.88 -1.44) (xy -1.12 -1.11)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "e18817ea-b636-4cf3-a177-a7e2200e0dda")
		)
		(fp_line
			(start -1.6 -1.4)
			(end 1.6 -1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d56693bc-6bfa-4e2a-ab10-1e77366617a0")
		)
		(fp_line
			(start -1.6 -1.4)
			(end -1.6 1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b70284a6-319d-4f90-ae20-a8a012e2a34f")
		)
		(fp_line
			(start 1.6 1.4)
			(end 1.6 -1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "226e576d-06d1-4241-a86f-c903bcf3188e")
		)
		(fp_line
			(start -1.6 1.4)
			(end 1.6 1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bc220fc4-22f5-4227-934c-23988f3e6886")
		)
		(fp_line
			(start 0.675 -1.1)
			(end -0.175 -1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc4bb2e0-82f6-475a-8f02-6029bbd664e9")
		)
		(fp_line
			(start 0.675 -1.1)
			(end 0.675 1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb0b766e-89bd-471a-ab12-847d4ec34745")
		)
		(fp_line
			(start -0.175 -1.1)
			(end -0.675 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dda01315-a8e9-4729-8818-ccab144db4b3")
		)
		(fp_line
			(start -0.675 -0.6)
			(end -0.675 1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9ea80e1e-9b4e-444b-a133-d37bc9f1a081")
		)
		(fp_line
			(start 0.675 1.1)
			(end -0.675 1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7bfb908f-2aee-4080-8894-ccdbe7967c7e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "790110df-c165-4e97-ad51-c43dd33098e6")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.075)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1 -0.65 90)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VDD_NRF")
			(pinfunction "VIN")
			(pintype "power_in")
			(uuid "0191f834-0628-4a5d-bf4c-e3aee97b02ef")
		)
		(pad "2" smd roundrect
			(at -1.1 0 90)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "Net-(U3-FB)")
			(pinfunction "FB")
			(pintype "input")
			(uuid "e86ae8b2-ceb9-46d9-bcb4-d6026ff542b3")
		)
		(pad "3" smd roundrect
			(at -1.1 0.65 90)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "4d28c65e-f377-4a35-bf6c-909175a922aa")
		)
		(pad "4" smd roundrect
			(at 1.1 0.65 90)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "+5V")
			(pinfunction "VOUT")
			(pintype "power_out")
			(uuid "302a70bf-6d84-483b-89d1-32fb0f0fe4f4")
		)
		(pad "5" smd roundrect
			(at 1.1 0 90)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "Net-(U3-L)")
			(pinfunction "L")
			(pintype "power_in")
			(uuid "ec6b6ef9-4866-4abf-822b-13d029209457")
		)
		(pad "6" smd roundrect
			(at 1.1 -0.65 90)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VDD_NRF")
			(pinfunction "EN")
			(pintype "input")
			(uuid "cbbf6064-2fb9-4b19-b9f8-f04edbe67981")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(uuid "3d1bce5d-ee4f-4b70-917c-dff9b8ca1416")
		(at 139.57 135.8 90)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U6"
			(at 0 -2.4 90)
			(layer "F.SilkS")
			(uuid "9d023434-d2f4-435e-a328-d68bd93eee81")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "USBLC6-2SC6"
			(at 0 2.4 90)
			(layer "F.Fab")
			(uuid "ea9596d1-514a-4a8a-9b1d-d002dadaca8a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/usblc6-2.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "feb49a87-5584-42b8-b869-469dbdad47f8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "cea3c1f3-0cd8-4c2f-a2ab-50e757dc36be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/778a6fa8-fc79-4871-8fca-1e1eb951d152")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end 0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fee42222-7186-4598-9887-05b82e9dedcd")
		)
		(fp_line
			(start 0 -1.56)
			(end -0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "db0fcc3d-d9cb-4949-8455-e48afb7a611a")
		)
		(fp_line
			(start 0 1.56)
			(end 0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2ed88734-e420-4c85-9055-029aa1c2f3bb")
		)
		(fp_line
			(start 0 1.56)
			(end -0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "851d39cc-91fc-4d5e-8e1d-d829c1617f72")
		)
		(fp_poly
			(pts
				(xy -1.3 -1.51) (xy -1.54 -1.84) (xy -1.06 -1.84)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "5faef7bb-580f-4ed6-9a3c-10c69e685859")
		)
		(fp_rect
			(start -2.05 -1.7)
			(end 2.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "63ceaea1-fe9c-4c75-8fb5-b966b920f81f")
		)
		(fp_line
			(start 0.8 -1.45)
			(end 0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2fbba14f-c774-4b70-bfae-a578af467d6a")
		)
		(fp_line
			(start -0.4 -1.45)
			(end 0.8 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0e4e321f-51de-41fd-a127-60605eb1cb3a")
		)
		(fp_line
			(start -0.8 -1.05)
			(end -0.4 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "88183fb3-65d4-4b3b-a0c2-afb1637f89fb")
		)
		(fp_line
			(start 0.8 1.45)
			(end -0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8213e743-ab60-433f-9bbb-35a1f72690bd")
		)
		(fp_line
			(start -0.8 1.45)
			(end -0.8 -1.05)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb641c69-ef78-4d8f-8ecd-7efb2ff9f59e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "ba16d1b4-bcec-4e87-a032-e84c6710aa8a")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 120 "Net-(J1-D--PadA7)")
			(pinfunction "I/O1")
			(pintype "passive")
			(uuid "f6a09e2e-6443-4b72-97ab-602fb75a33b8")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "65b1e3e1-2c9f-4dd1-b33e-5a4ca7bbccc6")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "Net-(J1-D+-PadA6)")
			(pinfunction "I/O2")
			(pintype "passive")
			(uuid "2c28b4ee-14d4-4ba9-ab5b-26a8aa412cda")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "D+")
			(pinfunction "I/O2")
			(pintype "passive")
			(uuid "1c78cff2-7405-4ce5-b901-3e0da7381e71")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "9ac8f212-cc15-4f0b-af28-38d500e82d65")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "D-")
			(pinfunction "I/O1")
			(pintype "passive")
			(uuid "0924bc28-2486-447e-bd97-8f0f89e37553")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "3d3afd1f-4a76-422f-91b8-e7645857bf9e")
		(at 53.3 108.8875 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(uuid "e9447f35-3325-4ab1-857e-d5745aa081c3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "f27c5135-3f10-43c6-a4c8-f946a1bd9088")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4ff633c0-d9f3-407b-83b2-4214c7034f8f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5c5f3f88-fc3d-4e31-bb1c-c4528a19dac7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/39b34b28-8ec8-4bb0-a606-ad0e74ec574e")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8ffe2480-9c32-46de-8c14-5618ffc802ba")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "06fd1840-8db9-4165-812b-050fb96ecc5e")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72b14a8f-8eb3-4a8f-9c5f-5d1ce655e513")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7beac073-8301-4a8e-94ac-d7f29086a779")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "76e0aa76-8c70-45c5-bfe7-907ed1c63993")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "644f80dc-b948-49fd-b9cc-413c0eca8306")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a259124-be61-4846-84a2-fcaef4864e76")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "239a8feb-f215-499c-b1b8-e28984323303")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bf5a2f5e-9955-4aa2-9990-0c625d11126f")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "edd2b56d-ed73-417d-9494-651985127a77")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "a0b9ab38-8aa6-418e-b8e7-b7a5352ded35")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 60 "Net-(U1-VFB)")
			(pintype "passive")
			(uuid "b9314d83-2b2f-41da-a441-d8f0db119c6b")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "7205c3e5-f32b-40be-bd76-79085ccf0a17")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(uuid "3ed9b7c1-a333-4676-afef-28b78928c984")
		(at 210.71 115 180)
		(descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
		(tags "sma edge")
		(property "Reference" "J3"
			(at -1.5 7 0)
			(layer "F.SilkS")
			(uuid "fa206d84-0c88-4001-9da6-bb5661d5edde")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_Coaxial_Small"
			(at -1.72 -7.11 0)
			(layer "F.Fab")
			(uuid "48a74040-c19f-41e7-8951-2abca3d557d4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9d7912f9-a878-4437-9c1f-ab2cd0388a7a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "small coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "567dbe76-d9fb-4a90-be43-8c0495e3c679")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(path "/a7ac3701-5e8c-4217-b013-0d1ec42aee30")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start 2.5 0.25)
			(end 2 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3c4b28b5-2ff3-4e0f-9732-faa725a720d2")
		)
		(fp_line
			(start 2.5 -0.25)
			(end 2.5 0.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cb881a1e-916c-4c62-80ee-24d40e228985")
		)
		(fp_line
			(start 2 0)
			(end 2.5 -0.25)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c3d4f083-43c4-4315-9750-0f8cf8f19dd3")
		)
		(fp_line
			(start 2.71 -6.09)
			(end 2.71 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "52142779-0402-4e90-a203-58eb9717e900")
		)
		(fp_line
			(start -14.29 6.09)
			(end 2.71 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "8d6b53c1-94be-4229-8665-a89163b5bbe6")
		)
		(fp_line
			(start -14.29 -6.09)
			(end 2.71 -6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5b44c6aa-9994-408d-8970-9afd18a7aba1")
		)
		(fp_line
			(start -14.29 -6.09)
			(end -14.29 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "a99376e6-80fe-4f8a-b72d-02aa0c83d872")
		)
		(fp_line
			(start 2.71 -6.09)
			(end 2.71 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "68425a76-a9b3-41b6-a453-753fe7455648")
		)
		(fp_line
			(start 2.71 -6.09)
			(end -14.29 -6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "92458cf4-01b3-4ea5-ba7d-b7e4b025098c")
		)
		(fp_line
			(start -14.29 6.09)
			(end 2.71 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6823fb25-fa60-4443-bc01-5fb5ed75cb0d")
		)
		(fp_line
			(start -14.29 -6.09)
			(end -14.29 6.09)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7a68d1a0-b91c-454b-83f5-1044b0b5a391")
		)
		(fp_line
			(start 2.5 0.25)
			(end 2.5 -0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a7797961-17c9-4128-9145-8f1481a040e6")
		)
		(fp_line
			(start 2.5 -0.25)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "161610c1-a5b5-4904-b422-0b7895b120f8")
		)
		(fp_line
			(start 2 0)
			(end 2.5 0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9614775-29ae-418b-9656-c4377caa7173")
		)
		(fp_line
			(start 0.49 3.75)
			(end 0.49 4.76)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4612fa48-f765-488d-ad14-aa864a391048")
		)
		(fp_line
			(start 0.49 -0.38)
			(end 0.49 0.38)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32a25aab-6dfd-4cac-a05b-16e6386e23a0")
		)
		(fp_line
			(start 0.49 -4.76)
			(end 0.49 -3.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b30decf4-59e4-4bfc-bea4-e1c9496de22f")
		)
		(fp_line
			(start 0.49 -4.76)
			(end -5.91 -4.76)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9328492b-1395-4ad7-a109-50c1190dc322")
		)
		(fp_line
			(start -4.76 3.75)
			(end 0.49 3.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dafbfe61-d6c2-4faa-a9c6-f18d04eac7b0")
		)
		(fp_line
			(start -4.76 0.38)
			(end 0.49 0.38)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "096630ad-0ea9-47cd-b1fc-3c6e8c9aaddc")
		)
		(fp_line
			(start -4.76 -0.38)
			(end 0.49 -0.38)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "523fb2e6-5847-4110-b610-bf739cc03ef0")
		)
		(fp_line
			(start -4.76 -3.75)
			(end 0.49 -3.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6e9351b0-c2f7-47c3-bfd7-d422910727f4")
		)
		(fp_line
			(start -4.76 -3.75)
			(end -4.76 3.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "800014ac-6855-4c94-baf6-804317d8594a")
		)
		(fp_line
			(start -5.91 4.76)
			(end 0.49 4.76)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "04600ac2-cde3-4c29-8aee-91a3f1d58bdb")
		)
		(fp_line
			(start -5.91 -4.76)
			(end -5.91 4.76)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ef699454-de13-457f-97a0-7adb8f16dfda")
		)
		(fp_line
			(start -13.79 2.65)
			(end -5.91 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "333e75ba-fd90-429b-8e8a-6915d8fee541")
		)
		(fp_line
			(start -13.79 -2.65)
			(end -5.91 -2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc647ded-4cd5-4102-8c88-ce67d38bbf15")
		)
		(fp_line
			(start -13.79 -2.65)
			(end -13.79 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f840391b-ca6e-4166-99e4-3ff7708719af")
		)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 0)
			(layer "F.Fab")
			(uuid "034216e3-7e07-4039-902c-379541ee7ee8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -1.72 0 180)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(IC3-ANT)")
			(pinfunction "In")
			(pintype "passive")
			(uuid "c7315f71-9dc9-499c-832f-f61724222c0f")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 180)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "18970c58-4e73-486d-bed7-df45899258c4")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 180)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "36657f73-625f-49a4-83c0-2caedea4ad47")
		)
		(pad "2" smd rect
			(at -1.72 4.38 180)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "b49c0dae-aca3-4280-93db-02f147ae3454")
		)
		(pad "2" smd rect
			(at -1.72 4.38 180)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "22b9be51-f4e7-4003-bc1f-a58ea8afd6c7")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 180)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "7b06539e-2cba-4edc-998b-3995706a6d96")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 180)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "3f963cfd-1e3a-4ed3-95f5-eeef81ca0456")
		)
		(pad "2" smd rect
			(at 1.27 4.38 180)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "d390f4ef-da39-4c4d-8551-4acbbc5ad481")
		)
		(pad "2" smd rect
			(at 1.27 4.38 180)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "5babaaba-94f2-4b9c-a719-474967c8b596")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38 180)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "021d8045-889f-4575-bd8a-7d5fd093af99")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38 180)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
			(uuid "b4504ebe-5208-4217-9405-098e78dd1806")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "F.Cu")
		(uuid "3eeff084-3f11-45af-ae48-0a74d00299ed")
		(at 135.1545 120.335)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q1"
			(at 0 -2.75 0)
			(layer "F.SilkS")
			(uuid "860f1027-5d2d-4bf3-90ca-7b473cde08e7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PMOS"
			(at 0 2.5 0)
			(layer "F.Fab")
			(uuid "d1d5894c-2fa4-4a69-8efe-434840fa3bcf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_MOSFETs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "117f11c6-88a6-42f6-aca0-d365cf50bc77")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "P-MOSFET transistor, drain/source/gate"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "abd421c5-37c2-4478-8c8a-61fa2bffc8bd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "PMOS"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f373fad7-6aba-4003-8b62-5d514644f60a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Type" "VDMOS"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9b584396-95e1-4447-b501-2f90c992f1ef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=D 2=G 3=S"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "95158987-e48a-49dd-8b0f-a850f735c875")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/8c139557-19ed-4448-b687-400c822f12e7")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.04 -1.58)
			(end -0.84 -1.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "66b653a6-e43b-4f4b-a4fe-e98eba7bc27d")
		)
		(fp_line
			(start -0.04 -1.58)
			(end 0.76 -1.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "26e87987-d005-4a8c-8683-a5d0de9a043f")
		)
		(fp_line
			(start 0.76 -1.58)
			(end 0.76 -0.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e1c541a4-edda-4380-b533-6e96dfa98455")
		)
		(fp_line
			(start 0.76 1.58)
			(end -0.7 1.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "44500b03-ea42-49b0-9fbc-265f2adb22b2")
		)
		(fp_line
			(start 0.76 1.58)
			(end 0.76 0.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dbd2b7a8-f470-49bf-8146-1f7fc981efa5")
		)
		(fp_poly
			(pts
				(xy -1.34 -1.61) (xy -1.58 -1.94) (xy -1.1 -1.94) (xy -1.34 -1.61)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "55825c20-2f26-4c06-885b-4a18bfbdb5fa")
		)
		(fp_line
			(start -2.7 -1.75)
			(end 2.7 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "48bf5d59-60a0-4573-a7ed-e4af1abd5176")
		)
		(fp_line
			(start -2.7 1.75)
			(end -2.7 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b07e0c53-9b7c-4ee1-a4da-b9a3a554903a")
		)
		(fp_line
			(start 2.7 -1.75)
			(end 2.7 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4cd3b9e9-e353-4261-95ca-544ca5ff2c7e")
		)
		(fp_line
			(start 2.7 1.75)
			(end -2.7 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9c8e76d5-45d1-42ef-86f0-af3707b23842")
		)
		(fp_line
			(start -0.7 -0.95)
			(end -0.7 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b7c8d5fa-bb10-4a92-b277-ec1cc90923f1")
		)
		(fp_line
			(start -0.7 -0.95)
			(end -0.15 -1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1dc8e319-0c2b-4913-b91b-0b962e3489d5")
		)
		(fp_line
			(start -0.7 1.52)
			(end 0.7 1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6a9bfc31-4871-4f3d-baca-9d1fdc545226")
		)
		(fp_line
			(start -0.15 -1.52)
			(end 0.7 -1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f98f307-11c9-418b-8612-f89844b67b4f")
		)
		(fp_line
			(start 0.7 -1.52)
			(end 0.7 1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "064ce294-9955-4222-82e5-80ec05a60b74")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "c626e193-a15e-4152-9beb-2ed23189fba3")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.075)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5 -0.95)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "Net-(IC2-VCC)")
			(pinfunction "D")
			(pintype "passive")
			(uuid "b9e46a0b-a016-4dd6-afde-7c95b8087cd9")
		)
		(pad "2" smd roundrect
			(at -1.5 0.95)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "Net-(IC2-DRV)")
			(pinfunction "G")
			(pintype "input")
			(uuid "37e82787-d774-4183-a71c-802f16e0f982")
		)
		(pad "3" smd roundrect
			(at 1.5 0)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "Net-(D6-K)")
			(pinfunction "S")
			(pintype "passive")
			(uuid "62fd0ef9-bc17-430a-924b-4acc62743710")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical"
		(layer "F.Cu")
		(uuid "3f4524a4-3af8-4495-ab53-d21f9f88a0f5")
		(at 181.23 98.19)
		(descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
		(tags "Through hole pin header THT 2x05 1.27mm double row")
		(property "Reference" "J6"
			(at 0.635 -1.695 0)
			(layer "F.SilkS")
			(uuid "a3174a8e-39d0-4ce5-8252-57cdcc4d05d2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_ARM_JTAG_SWD_10"
			(at 38.835 39.265 180)
			(layer "F.Fab")
			(uuid "e90b69d0-d1b0-4e84-a379-5a2ba87a990d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7c625e93-0a47-45d9-85b0-e81e93f6c788")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5829fe28-3e49-4989-bd55-2e90e33bfb9c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "PinHeader?2x05?P1.27mm*")
		(path "/8d551d4a-caea-4f37-aa1a-447ca7746a77")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.13 -0.76)
			(end 0 -0.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b430deb4-d831-4859-a3f6-3f6a9c184e24")
		)
		(fp_line
			(start -1.13 0)
			(end -1.13 -0.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "433fd6a3-d83c-42e2-89f9-296c3baa8572")
		)
		(fp_line
			(start -1.13 0.76)
			(end -1.13 5.775)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "88d91d92-69ff-4f4e-a0c3-2446272b47e7")
		)
		(fp_line
			(start -1.13 0.76)
			(end -0.563471 0.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "db322971-41e4-4183-ad18-a9c2d8f4f6f1")
		)
		(fp_line
			(start -1.13 5.775)
			(end -0.30753 5.775)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b1adbc49-285b-4e2a-8958-ec7c319f7382")
		)
		(fp_line
			(start 0.30753 5.775)
			(end 0.96247 5.775)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f18d99d2-653e-4e2a-8d40-68cd0fa78df1")
		)
		(fp_line
			(start 0.563471 0.76)
			(end 0.706529 0.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7db8f7d1-4341-45f1-b1f6-be4083a98555")
		)
		(fp_line
			(start 0.76 -0.695)
			(end 0.96247 -0.695)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5108cdcd-535f-472c-bedd-03c7704a8bb7")
		)
		(fp_line
			(start 0.76 -0.563471)
			(end 0.76 -0.695)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cd35bda3-e507-41ac-aa24-e2654583eb58")
		)
		(fp_line
			(start 0.76 0.706529)
			(end 0.76 0.563471)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7c01b9f4-0b85-4b2a-891b-0c2ea5953656")
		)
		(fp_line
			(start 1.57753 -0.695)
			(end 2.4 -0.695)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a3eac9b1-463f-4b79-be1e-174fdd6946ca")
		)
		(fp_line
			(start 1.57753 5.775)
			(end 2.4 5.775)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0fe699fa-1de5-4b1e-92a8-7a2fea6cd4f2")
		)
		(fp_line
			(start 2.4 -0.695)
			(end 2.4 5.775)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9bb8b815-53bc-4729-b423-693f37560ceb")
		)
		(fp_line
			(start -1.6 -1.15)
			(end -1.6 6.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ed1be7d-b98d-46cd-8571-1ca7e0a147f4")
		)
		(fp_line
			(start -1.6 6.25)
			(end 2.85 6.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a457ead4-b7aa-4842-8a59-d0b44d4b5445")
		)
		(fp_line
			(start 2.85 -1.15)
			(end -1.6 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ac0d5113-b3df-4375-8d11-1f8d6f2b5e74")
		)
		(fp_line
			(start 2.85 6.25)
			(end 2.85 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ea3a355f-63bd-40f0-86e2-18b448909f6f")
		)
		(fp_line
			(start -1.07 0.2175)
			(end -0.2175 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e96e7a83-0a42-47a4-973c-481f692d042a")
		)
		(fp_line
			(start -1.07 5.715)
			(end -1.07 0.2175)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f93f16df-4cc3-4367-a9b3-53ae95d4bab8")
		)
		(fp_line
			(start -0.2175 -0.635)
			(end 2.34 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0b786719-f3a3-4350-add6-2c5f8aac047d")
		)
		(fp_line
			(start 2.34 -0.635)
			(end 2.34 5.715)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bf395e9a-2f62-409c-b05a-e747f2c212aa")
		)
		(fp_line
			(start 2.34 5.715)
			(end -1.07 5.715)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dda4f186-c21e-4913-9780-d7fdd65ce082")
		)
		(fp_text user "${REFERENCE}"
			(at 0.635 2.54 90)
			(layer "F.Fab")
			(uuid "1bb63f82-9c27-427a-ae27-dcca7229859f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VDD_NRF")
			(pinfunction "VTref")
			(pintype "power_in")
			(uuid "1288692f-5896-484d-b892-966e3a5a4a4b")
		)
		(pad "2" thru_hole oval
			(at 1.27 0)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "SWDIO")
			(pinfunction "SWDIO/TMS")
			(pintype "bidirectional")
			(uuid "ddf19391-54d7-4449-98fa-afa60d7ba915")
		)
		(pad "3" thru_hole oval
			(at 0 1.27)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "0157451f-5ef5-4c8e-a792-0e84d3ce2ef4")
		)
		(pad "4" thru_hole oval
			(at 1.27 1.27)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "SWDCLK")
			(pinfunction "SWCLK/TCK")
			(pintype "output")
			(uuid "e060df9f-0419-4273-91c2-380fd13a7059")
		)
		(pad "5" thru_hole oval
			(at 0 2.54)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "ab6b85c3-c829-4b8e-99e1-76e5822b8dca")
		)
		(pad "6" thru_hole oval
			(at 1.27 2.54)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "unconnected-(J6-SWO{slash}TDO-Pad6)")
			(pinfunction "SWO/TDO")
			(pintype "input+no_connect")
			(uuid "b526d651-af38-4685-a34c-374736792d66")
		)
		(pad "7" thru_hole oval
			(at 0 3.81)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "unconnected-(J6-KEY-Pad7)")
			(pinfunction "KEY")
			(pintype "no_connect")
			(uuid "b725c83e-405c-4481-8550-6b902b96af15")
		)
		(pad "8" thru_hole oval
			(at 1.27 3.81)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(J6-NC{slash}TDI-Pad8)")
			(pinfunction "NC/TDI")
			(pintype "output+no_connect")
			(uuid "6292b921-f106-4c46-8a32-0103a72c7b23")
		)
		(pad "9" thru_hole oval
			(at 0 5.08)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GNDDetect")
			(pintype "passive")
			(uuid "d8210b10-e5d6-46bb-ae8e-ee9c7cbc1c8a")
		)
		(pad "10" thru_hole oval
			(at 1.27 5.08)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "RST")
			(pinfunction "~{RESET}")
			(pintype "open_collector")
			(uuid "f479b857-3f12-497d-9b96-7bfa4d42bd41")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "40514f6c-2043-4a80-921d-05b7f16fc854")
		(at 177.5 94.47)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "2dd25dfc-139a-445c-a13b-2806c790f18d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "e3e0b196-b092-42ec-90fc-16a0e6790288")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f0046a39-69ad-4ed0-a67e-9ce4a61f8cec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "753d3c48-b783-45e0-b0a9-ba75b97f48ee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/66a4540a-823d-4b19-bde4-4ed77ffc0f84")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7dae0850-6975-49f4-8c3b-07d69ca9a15f")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a9fee04e-7ac4-4c53-aa6a-9337bf1157cc")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e0621a26-90ae-4df5-a4a2-b48035e3268f")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "db71c613-028c-4e6b-bc19-18aa4cd0daa6")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a043b1ce-f981-403b-b50b-d7be09a03217")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f0a03f01-04ec-4c15-b224-c89f72f7c29b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2c263ba8-b596-4b09-9974-b7d09f6b5f27")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab5a3bf9-4819-402a-be16-65add962e51b")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2e19042b-f2a9-4883-9737-a17e1ac374e7")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0f89e31e-c2fc-4aa0-87cd-08f8e935394c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "97e1ee03-a210-4f47-a478-218e8ddf4642")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "cab73b8c-66ab-486b-b5b8-090d5459fb12")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "bf30d997-1386-46b7-9533-49083d55eb21")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "41280926-96b9-46c8-b3c5-bfd494079ea4")
		(at 108.25 99.8)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "inductor handsolder")
		(property "Reference" "L2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "999cd7b9-c000-49ea-829a-9f4d46ef45a2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uH"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "aa76debe-4607-4902-8826-796c3c1f78e2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2a3d7689-3731-425c-98db-b604726f6383")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9875ea01-f974-40a6-aa94-c2eeb2b7f32a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/379428d7-d65e-424e-af84-990a0ccbcc2f")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.71)
			(end 0.261252 -0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a148266a-e657-404a-8226-10d4f965559a")
		)
		(fp_line
			(start -0.261252 0.71)
			(end 0.261252 0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b718f3b6-9283-4331-9711-15c551470089")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9f6fa88b-3fe5-4ac7-b6b6-84ee16466d29")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf59906a-0578-49b0-b079-051160960f4d")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "644f7786-08c7-419e-ae4a-1ea413ca9b0a")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3550009b-2b9c-433a-a9f5-2b215676ae7c")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b403d2c2-3b0b-4259-83e1-7c4eeff273f8")
		)
		(fp_line
			(start -1 0.6)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fa69b145-e8c7-419d-8925-3525448f9628")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a2848a6b-70ba-4c26-b141-c94e9992fbc5")
		)
		(fp_line
			(start 1 0.6)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b21757b-5b2c-490b-a1bb-165d15ab0976")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "27012e51-0769-4073-ad23-9b279ac5c973")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 51 "Net-(D6-K)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "b221c713-3f22-4f9c-a737-7dceeb4ee1bb")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 50 "Net-(IC2-CSP)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "17722e26-8915-461d-97ab-dd297728d35b")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "4479fda6-3303-4de5-9f04-6ebc49d16197")
		(at 122.5 111.6)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R25"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "0dcdf7b0-0553-4c2f-972b-87b329e35849")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "772d0120-744d-45be-b1a4-b87d32b0304f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3c634ccb-52d5-49e3-97f0-ed71629e76a0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2a19efed-31bc-4381-ba10-3c653188d940")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/c09b3889-cb3c-4877-bf7b-1da6db861c17")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f8d4a27c-65bf-40d4-9c27-d860eb9a8943")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "83156e17-7192-4ff9-9220-99c2c303b567")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f52d1bd2-c7cb-49a5-b5a2-b06799bcf79c")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "567b7499-215d-4a7f-90cb-7951dd7c5256")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8470be93-490c-40f3-8db0-6f617b041497")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "14b006a7-194b-4063-8ec7-6acbd10c4f41")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3a2968f9-7511-4b08-954b-66b497574f41")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1eae17eb-c315-485e-a8c1-ce3b2d3e239f")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3f50849f-c7a7-427b-8845-0e0a0f5c8001")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d70f3695-e68d-4f67-b80e-0a94dcd605d2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5bc43150-5c86-492b-863b-f6b3be9cafd4")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "Net-(IC4-OV2)")
			(pintype "passive")
			(uuid "6ac72a01-9a7f-4747-9d5a-a2654b10d682")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "1c97e0d8-a4db-43e2-a9e9-9ee7a07ddd18")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "44a3b97c-2366-4376-bccd-dac218489eb6")
		(at 56.25 108.8875 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(uuid "b04c7e7d-1003-4ee7-8924-4bdf965d32b5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "33.2k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "d617aa60-b6e3-4652-9075-a67470961dce")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "26a0db35-ae54-4061-a175-25be8bfc44af")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1faf2353-9e34-4325-8ea8-4ec0351f3357")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/ae453145-5347-4639-bc75-c1f10260037b")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "484451ca-0ba3-434b-954a-7cf9c00d8d5c")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a4b0ae4f-5aac-4b43-b127-6c6c1ca965ef")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0d9e8f6a-0909-4e22-8127-5dc31e830e96")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e80780b0-09ee-476a-af6f-10862845accc")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "60c8768b-4fd9-4483-a208-811547d91937")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f9c31070-b993-4239-ace6-cecfcee11806")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5bea4147-4f07-4cbd-8ed5-9a39e77b7b7e")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "72769faa-d29a-42c8-bbd9-75545e8d7173")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37f4e811-6949-4def-aef3-f815b6efd17a")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1bcd7eff-9bea-46f9-a924-f6140bfad38c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "6d79b0de-289a-444b-8fbc-075ec9f391aa")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "fc0d8738-eed2-409b-9f75-8ab402f7e937")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 60 "Net-(U1-VFB)")
			(pintype "passive")
			(uuid "960274e7-c062-4310-b3e5-4819f6bbdd28")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "4901990a-ce42-4b0b-884f-4a4b10dff7bd")
		(at 192.8475 110.98)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C36"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "9bb94a66-cd27-4d58-8995-487aa5322823")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100pF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "fec62476-7cc8-4f73-929c-17c84baa988d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "80ab0419-eda5-4506-aeaf-7d17ee5c3604")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d4eb814c-5205-43fd-ba50-7410e640165c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/9ddf98a3-81fc-45d8-971f-a8860352e810")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "17503e53-afad-4233-8033-79d6d0b6d472")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5a310037-a24a-4093-8b51-1af315f38500")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ccbe04a-e2f5-443c-ace3-9c05c705b31f")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "175dbba4-c0e6-4670-a688-43a7524e20ba")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "29a86586-c45b-41b3-872a-8ddef4122f30")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5469020c-5a4b-42d5-98a2-54907c67d417")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "40b528d4-c900-4909-a584-574390fce03c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2d6d15ac-f736-4d65-bbe5-df858d5de548")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb457948-a327-4e43-abea-761b41379204")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e96cff7a-9936-43cc-951a-77cd6a75014f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "22652a4c-1c76-4889-9913-64b0b4a41a68")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 12 "RF_LORA")
			(pintype "passive")
			(uuid "2aa481e1-30ce-44df-a6d9-8e7dfd1a7889")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 11 "Net-(S1-RFC)")
			(pintype "passive")
			(uuid "13d13a4e-d92a-4fc6-8b43-d67eab3bc74b")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "4d9731db-50cb-4991-a7be-bbaad7465b24")
		(at 171.0375 87.56)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "ecd6aa79-43f5-4448-b643-de18aacf76b0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "ed706138-aaa6-47a9-964e-8058850769c8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "849d6eae-92cf-42fb-b114-9c9534c96272")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8ff4878a-7ef5-4b40-825d-cceac5c97a31")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/f038f94e-9ab9-48a2-95a6-396b3a8a8d99")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f54f142b-aec1-4abe-8d01-fa6c79827c61")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c91f12bf-43f8-45a9-aaa9-245b984ce4c0")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4014597d-f48a-4b63-8b39-308de378ddca")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c9eee628-bad2-4f71-af58-2b7f87410154")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3ec9e19-41ba-4b5c-9d5d-afc32b06695e")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "652581e8-4a76-456d-b3e7-d94d0de18072")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "86862afc-35f5-4be9-ba33-9fd164877653")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "578d6f60-8b58-41e5-b029-e47fa816f15e")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "966e8c33-33e3-4c6a-952c-1891c6c459ed")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17a88229-a50a-427a-abd0-05a00997c08b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c1d78a00-0014-488e-b7d9-cceca8a3e949")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "5f52e8c4-5bf8-41e1-a64f-2d589729a80d")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "9d6e3835-5cfe-4c5f-85c3-bfb3d2f514c7")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPS:TPS2121RUXT"
		(layer "F.Cu")
		(uuid "4e3d4dfa-c83d-4b5f-b4c9-4702ded593eb")
		(at 111.5395 133.765)
		(descr "RUX0012A")
		(tags "Integrated Circuit")
		(property "Reference" "IC4"
			(at 0 0 0)
			(layer "F.SilkS")
			(uuid "5db66204-dce8-4564-897f-0d5164ab672b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "TPS2121RUXT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7ac21b4a-63a7-4d15-acc7-28e6ccf541ec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" "https://www.arrow.com/en/products/tps2121ruxt/texas-instruments"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "963c9982-0593-46be-a481-d39626f41259")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Power Switch ICs - Power Distribution 2.7-22V, 56mG , 4.5A, Priority Power MUX with Seamless Switchover 12-VQFN-HR -40 to 125"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "287af29b-7ff2-400e-b11a-6ca2399a7be7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6a5cd81b-fb0a-4b94-aa0c-c917a9169f15")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "16da4c34-7476-47ee-b574-cf5e8cae0ccc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "TPS2121RUXT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d1ffd2da-7f4b-479e-b55e-055d1dbc1714")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" "595-TPS2121RUXT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "da9d355c-118e-4e39-8f3d-899c5f22c503")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/TPS2121RUXT?qs=l7cgNqFNU1i6abJCbO5ulQ%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8174331f-0168-4b69-a38f-b6ea15035fff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Part Number" "TPS2121RUXT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6f0225a3-ebfd-4d53-8ef0-291b1ad7de3e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/tps2121ruxt/texas-instruments?utm_currency=USD&region=nac"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c31fde54-1ae5-446c-badf-e79168915173")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C2156025"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5ffd5a76-010a-47be-8293-ba94e7fa0ea8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/7b9ddaa1-48bb-430a-b98e-3d80e7c674fa")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.6 -0.4)
			(end -1.6 -0.4)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3892174c-8f41-442f-bf90-5a0d1d392811")
		)
		(fp_line
			(start -1.5 -0.4)
			(end -1.5 -0.4)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "58c605fd-b659-4ba9-8787-d0c3622877fa")
		)
		(fp_arc
			(start -1.6 -0.4)
			(mid -1.55 -0.45)
			(end -1.5 -0.4)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3d36c099-cac4-4cb8-b704-198bd1a6e1f6")
		)
		(fp_arc
			(start -1.5 -0.4)
			(mid -1.55 -0.35)
			(end -1.6 -0.4)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cdb6530e-e977-4be0-8d5c-188c934e17b9")
		)
		(fp_line
			(start -1.9 -2.15)
			(end 1.9 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e6c0c54-9e63-468d-b9ed-9981bfdb96ec")
		)
		(fp_line
			(start -1.9 2.15)
			(end -1.9 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ea38e55-8b20-4622-9014-bf59731e9d2e")
		)
		(fp_line
			(start 1.9 -2.15)
			(end 1.9 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a4a76927-7207-48d7-8e4b-5457cdeeedf5")
		)
		(fp_line
			(start 1.9 2.15)
			(end -1.9 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "013c7b1e-b031-45df-a292-6681c9f2b3c4")
		)
		(fp_line
			(start -1 -1.25)
			(end 1 -1.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "03f1cb7d-b0ea-409b-8668-c44ed1752377")
		)
		(fp_line
			(start -1 1.25)
			(end -1 -1.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c11e68ac-b960-4f3b-9009-638c6d9ddd6c")
		)
		(fp_line
			(start 1 -1.25)
			(end 1 1.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "05ff5c7f-6ae5-429c-8a70-2ac8631d334b")
		)
		(fp_line
			(start 1 1.25)
			(end -1 1.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8b797abe-a7cb-4228-b333-fe76660878d2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ed22ae8a-f2d9-440a-839d-e9d3eddd3288")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -0.675 -0.35 90)
			(size 0.4 1.05)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "Charger Load")
			(pinfunction "OUT_1")
			(pintype "passive")
			(uuid "7446e377-692c-4d3e-bd45-aaa98c55a359")
		)
		(pad "2" smd rect
			(at -0.675 0.35 90)
			(size 0.4 1.05)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "Sol Shunt 1")
			(pinfunction "IN2")
			(pintype "passive")
			(uuid "e8d3ff55-5fb7-4855-8c5a-7eb613f3afe3")
		)
		(pad "3" smd rect
			(at -0.75 1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "CP2")
			(pintype "passive")
			(uuid "f573e4ea-93df-4e3d-8740-c0fbed229473")
		)
		(pad "4" smd rect
			(at -0.25 1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "Net-(IC4-OV2)")
			(pinfunction "OV2")
			(pintype "passive")
			(uuid "7a74fb8f-498f-4060-9108-9bdb471d0c99")
		)
		(pad "5" smd rect
			(at 0.25 1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(IC4-OV1)")
			(pinfunction "OV1")
			(pintype "passive")
			(uuid "2ad582a5-c7bd-4fda-8e46-074fa85602b7")
		)
		(pad "6" smd rect
			(at 0.75 1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "PR1")
			(pintype "passive")
			(uuid "fb5611d5-f77b-4e19-a2d1-965c064c4d9e")
		)
		(pad "7" smd rect
			(at 0.675 0.35 90)
			(size 0.4 1.05)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "VBUS")
			(pinfunction "IN1")
			(pintype "passive")
			(uuid "86975ace-02b0-4afe-9094-5a67d35e05a8")
		)
		(pad "8" smd rect
			(at 0.675 -0.35 90)
			(size 0.4 1.05)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "Charger Load")
			(pinfunction "OUT_2")
			(pintype "passive")
			(uuid "3514b754-71d5-4e10-882b-a9ea7a791da0")
		)
		(pad "9" smd rect
			(at 0.75 -1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "ST")
			(pintype "passive")
			(uuid "ea9fdcc1-9ff4-4c63-9e04-ffaff173538b")
		)
		(pad "10" smd rect
			(at 0.25 -1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(IC4-ILIM)")
			(pinfunction "ILIM")
			(pintype "passive")
			(uuid "385c0c66-6497-4847-b82b-bf2d9525d5e0")
		)
		(pad "11" smd rect
			(at -0.25 -1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(IC4-SS)")
			(pinfunction "SS")
			(pintype "passive")
			(uuid "43e9444b-3184-4ab8-acf6-900991537b24")
		)
		(pad "12" smd rect
			(at -0.75 -1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "471bc131-3957-4d93-9194-e6aaa6c0d794")
		)
		(embedded_fonts no)
		(model "TPS2121RUXT.stp"
			(offset
				(xyz 0 0 0.999999985)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "4f85ed18-4d33-4e4b-ac67-5a5b8cad7b89")
		(at 50.44 118.4175 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C35"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "70950fa7-fd6a-42fe-9fa0-b4a4c8957c31")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "cc287932-1ef8-4994-af87-a708b8688db2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fc44915f-87e7-45d5-8ab7-9e3511dfecb6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9609e683-c1fa-4c2d-b629-0821ab59aaa0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/cf836a19-7ab3-4a3d-8aeb-41aad7a6907c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb9ca6be-9f53-4e6b-ac0f-8773b9b960c6")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "adf54e63-7f6b-4469-a6bf-b4c5b43afd27")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "64d11482-b35a-4804-91e4-4392f1a5778e")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "073c5225-c517-47e1-b90f-e7f516b82da3")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9a95f4e5-46cd-42ed-971f-c21122243846")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "efb86975-27f2-4b11-9bef-5114d3cff1ac")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9d970c27-8c65-4cb7-acb4-b25abc411420")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6915d8f6-2805-4486-ba80-f86513c51df7")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a846667c-63fb-4204-a8ff-00f74e5040fb")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2951abab-09c8-4173-9e64-d9aa49a446eb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "3db7be13-6673-4831-8fa3-8c9b57e9b382")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 14 "+5V")
			(pintype "passive")
			(uuid "159d1579-0c1c-4ffc-bf64-441c73aaba34")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "9add72a1-b0f0-42ec-b769-061aae6e1fc2")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_EH_S2B-EH_1x02_P2.50mm_Horizontal"
		(layer "F.Cu")
		(uuid "508f4418-7c52-4df1-979e-c004b47a6021")
		(at 160 92)
		(descr "JST EH series connector, S2B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH horizontal")
		(property "Reference" "J5"
			(at 1.25 -7.9 0)
			(layer "F.SilkS")
			(uuid "5eabc865-efb4-4df1-8680-f5458ae0681a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2d95cf9d-0d89-4b1b-a961-da787499bb51")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "456e4ab3-bebe-4c48-807d-1a146afc6ded")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "125a37e2-a72a-4bfe-987c-adf218cec656")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/c0c3a649-79ab-4678-864b-8669333c8153")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.61 -6.81)
			(end 5.11 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ae8739b9-0400-46a4-8ab4-6c64926b879e")
		)
		(fp_line
			(start -2.61 -5.59)
			(end -1.39 -5.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "826adc35-bc7c-4f41-937c-9a9480f44205")
		)
		(fp_line
			(start -2.61 1.61)
			(end -2.61 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97a4845a-ba9b-4d34-acd7-7980de3af36e")
		)
		(fp_line
			(start -1.39 -5.59)
			(end -1.39 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5746bc47-218f-4a7d-a7ec-a046d2246d1b")
		)
		(fp_line
			(start -1.39 -1.59)
			(end 3.89 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "995f6e52-c80f-4d05-96ba-7dda33d8a20d")
		)
		(fp_line
			(start -1.39 -0.59)
			(end -2.61 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b164fc6a-00dd-41f8-9c00-93b69d18624d")
		)
		(fp_line
			(start -1.39 -0.59)
			(end -1.39 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8647685d-5ad4-4462-bf62-5c113794179c")
		)
		(fp_line
			(start -1.39 1.61)
			(end -2.61 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2eacb21f-b779-41a4-a492-29f0ec0d9de8")
		)
		(fp_line
			(start -0.32 -5.01)
			(end 0 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6aef6e65-a679-48b1-9e98-9ae6c09fd224")
		)
		(fp_line
			(start -0.32 -1.59)
			(end -0.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "29f49252-7492-4d6a-a87c-93705c7a7694")
		)
		(fp_line
			(start -0.3 2.1)
			(end 0.3 2.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2ae76899-efd4-4145-b00e-4f8daa71a949")
		)
		(fp_line
			(start 0 -5.09)
			(end 0.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2eeb0172-fc23-489f-a4a2-128e9949db48")
		)
		(fp_line
			(start 0 -1.59)
			(end -0.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2af416c-b703-41fa-a390-ac4ec9ec69bb")
		)
		(fp_line
			(start 0 1.5)
			(end -0.3 2.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "167bf302-62f9-4276-bf9b-f78470e694d0")
		)
		(fp_line
			(start 0.3 2.1)
			(end 0 1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2cebe0f8-2ef0-4d2f-a781-841169a7f071")
		)
		(fp_line
			(start 0.32 -5.01)
			(end 0.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f58087ff-dd27-4d08-a74c-a5d12421f2e0")
		)
		(fp_line
			(start 0.32 -1.59)
			(end 0 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "00704db6-4292-4b87-90e8-35c56c0e6cdb")
		)
		(fp_line
			(start 1.17 -0.59)
			(end 1.33 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a28c0cfe-8974-40a5-af78-e2f885d94938")
		)
		(fp_line
			(start 2.18 -5.01)
			(end 2.5 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "77c1de1c-0930-41b0-8d1c-6bda433390f5")
		)
		(fp_line
			(start 2.18 -1.59)
			(end 2.18 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6744009d-c58f-4dab-bc3b-5042623ad626")
		)
		(fp_line
			(start 2.5 -5.09)
			(end 2.82 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e9223be1-1aaf-4d9f-83e7-e661fe2e80b6")
		)
		(fp_line
			(start 2.5 -1.59)
			(end 2.18 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2d10cbbf-4b86-4bcc-b2b3-70f49b4da660")
		)
		(fp_line
			(start 2.82 -5.01)
			(end 2.82 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c895b067-24d5-49d6-9988-a0583da9bced")
		)
		(fp_line
			(start 2.82 -1.59)
			(end 2.5 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "43de7873-aa3d-43b5-8e88-20e7337b8e86")
		)
		(fp_line
			(start 3.89 -5.59)
			(end 3.89 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8055cfe1-e31a-4175-997d-b9fbd7e6d996")
		)
		(fp_line
			(start 3.89 -0.59)
			(end 5.11 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "52e9fa4d-c856-436c-8695-fcd9d8a42463")
		)
		(fp_line
			(start 3.89 1.61)
			(end 3.89 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3f5992c4-a1eb-4079-ba4e-1e4b53c4b30a")
		)
		(fp_line
			(start 5.11 -6.81)
			(end 5.11 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a4f6adc9-26a0-4171-858b-1c35bccf99e3")
		)
		(fp_line
			(start 5.11 -5.59)
			(end 3.89 -5.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cc7821b5-5241-4213-bbfd-c43113c70c8a")
		)
		(fp_line
			(start 5.11 1.61)
			(end 3.89 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a526c2de-d43f-44f7-84a0-a21a75efbfb8")
		)
		(fp_line
			(start -3 -7.2)
			(end -3 2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "77149a96-68ef-4047-8437-4215a1199804")
		)
		(fp_line
			(start -3 2)
			(end 5.5 2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fa968092-1711-411c-97cb-c47174dfc167")
		)
		(fp_line
			(start 5.5 -7.2)
			(end -3 -7.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "521d64d9-1669-4cb4-8128-cf4e98190eae")
		)
		(fp_line
			(start 5.5 2)
			(end 5.5 -7.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aed36f6f-6dc6-49ca-a6d0-ee3373539463")
		)
		(fp_line
			(start -2.5 -6.7)
			(end 5 -6.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8e79ede6-8972-4cf5-85b9-9057c0daf1b8")
		)
		(fp_line
			(start -2.5 1.5)
			(end -2.5 -6.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87e988df-63d3-4fbb-8f2b-31e99aadd370")
		)
		(fp_line
			(start -1.5 -0.7)
			(end -1.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f315e0eb-3386-4174-a168-b19a2776b289")
		)
		(fp_line
			(start -1.5 1.5)
			(end -2.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c65e5799-e36a-4481-bae3-d0cda8bf3357")
		)
		(fp_line
			(start -0.5 -0.7)
			(end 0 -1.407107)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "211ba4a5-350f-4280-b0e3-2ae0434187b9")
		)
		(fp_line
			(start 0 -1.407107)
			(end 0.5 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ac507eb-ada8-4f80-9d50-c3f9ebe05e8e")
		)
		(fp_line
			(start 4 -0.7)
			(end -1.5 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "66ba7616-6000-4f78-8e77-9e349d0655ca")
		)
		(fp_line
			(start 4 1.5)
			(end 4 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be1eac67-89de-4c0e-806a-27fbead69351")
		)
		(fp_line
			(start 5 -6.7)
			(end 5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a1a71745-37ce-4360-b37b-a1edd044e6f2")
		)
		(fp_line
			(start 5 1.5)
			(end 4 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3034bc3f-5786-4413-ad98-e3f6b2bd7f14")
		)
		(fp_text user "${REFERENCE}"
			(at 1.25 -2.6 0)
			(layer "F.Fab")
			(uuid "1b31fb4d-a669-46b7-8f20-ebbaff9b7a33")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 35 "Sol Shunt 1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "f9e6863d-0064-49de-a51d-06b1d6cbd2d8")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "c8d0aeb1-3599-4aed-ae9b-b8a38b8075b8")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_S2B-EH_1x02_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:CP_Elec_4x5.4"
		(layer "F.Cu")
		(uuid "513e07dc-b66a-4676-b27c-f736a597044b")
		(at 94.313 112.71)
		(descr "SMD capacitor, aluminum electrolytic, Panasonic A5 / Nichicon, 4.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C17"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(uuid "6e81b3b2-0dfb-480b-ad2e-fd3ba58165a9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 3.2 0)
			(layer "F.Fab")
			(uuid "7eb359b5-49d1-4a18-a6d2-822d7535812a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3ed59991-009a-4b58-90f8-24fdc6ba840d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "97f2f6f1-7a87-484f-ade8-042506213ba8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "CP_*")
		(path "/f0e06aae-9fe4-4f0a-a301-b4c7a46c9e6a")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -3 -1.56)
			(end -2.5 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f4367b3a-8175-44db-8453-42c66ad0c5ea")
		)
		(fp_line
			(start -2.75 -1.81)
			(end -2.75 -1.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "16faccd9-3374-4b4e-b28e-c6c3bd18ed76")
		)
		(fp_line
			(start -2.26 -1.195563)
			(end -2.26 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b31f9681-43d7-4634-80cb-1445b1ba9ece")
		)
		(fp_line
			(start -2.26 -1.195563)
			(end -1.195563 -2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a688c5c4-4ee2-4201-b61f-b1be7f7ad7bc")
		)
		(fp_line
			(start -2.26 1.195563)
			(end -2.26 1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b90525dd-277a-43f2-b055-02c68a31ed2e")
		)
		(fp_line
			(start -2.26 1.195563)
			(end -1.195563 2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0fe0f914-de5a-4a8e-a106-5c77f41d9e63")
		)
		(fp_line
			(start -1.195563 -2.26)
			(end 2.26 -2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3aa38297-48de-43c8-b669-c33cd4071f30")
		)
		(fp_line
			(start -1.195563 2.26)
			(end 2.26 2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e0cce78d-a405-486a-8872-3224ad7d3931")
		)
		(fp_line
			(start 2.26 -2.26)
			(end 2.26 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b69766d4-a388-4538-afa3-33683f8dfe86")
		)
		(fp_line
			(start 2.26 2.26)
			(end 2.26 1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd156cb4-e6e1-4c77-be5b-a824fad4ad67")
		)
		(fp_line
			(start -3.35 -1.05)
			(end -3.35 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1c4fa52d-bf5a-46b5-911d-484767329403")
		)
		(fp_line
			(start -3.35 1.05)
			(end -2.4 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d13c2c4c-9e1c-49f3-a48d-8445cc8a7bb5")
		)
		(fp_line
			(start -2.4 -1.25)
			(end -2.4 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ba6f1305-cdab-4979-91d6-4b98dc1bf8ba")
		)
		(fp_line
			(start -2.4 -1.25)
			(end -1.25 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f0ea8696-2f04-4258-b036-b657836d41e3")
		)
		(fp_line
			(start -2.4 -1.05)
			(end -3.35 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d4905871-b042-46bb-abe1-fa320ba9a69d")
		)
		(fp_line
			(start -2.4 1.05)
			(end -2.4 1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5fd1049c-ea46-465a-8b12-84c27b08a8c6")
		)
		(fp_line
			(start -2.4 1.25)
			(end -1.25 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5b196c27-f8f9-4304-bedd-16d68a31e3ce")
		)
		(fp_line
			(start -1.25 -2.4)
			(end 2.4 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0d92fa79-5274-4634-8ce6-2a9c735024af")
		)
		(fp_line
			(start -1.25 2.4)
			(end 2.4 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4d75dee7-41c8-4abb-88c4-8e7e9640ec32")
		)
		(fp_line
			(start 2.4 -2.4)
			(end 2.4 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e85d1eec-0bb3-49f6-82d6-33f2e1da1512")
		)
		(fp_line
			(start 2.4 -1.05)
			(end 3.35 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d941e168-3d41-4bf5-b485-dcf754753207")
		)
		(fp_line
			(start 2.4 1.05)
			(end 2.4 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "312f2644-a6d8-4e6f-8f78-d0cd2f343905")
		)
		(fp_line
			(start 3.35 -1.05)
			(end 3.35 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4274ac6b-8524-4564-9973-5258f206d22b")
		)
		(fp_line
			(start 3.35 1.05)
			(end 2.4 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "67de7c7c-0440-4e9a-a327-8891f79ae714")
		)
		(fp_line
			(start -2.15 -1.15)
			(end -2.15 1.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4be656be-ca16-4868-8d71-798a06cd31ca")
		)
		(fp_line
			(start -2.15 -1.15)
			(end -1.15 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5d7fdcd4-0234-4e2c-b042-2b4d8484de23")
		)
		(fp_line
			(start -2.15 1.15)
			(end -1.15 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb5117a9-ec2a-4c40-a15a-d320093bb4f1")
		)
		(fp_line
			(start -1.574773 -1)
			(end -1.174773 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "515c526a-393f-44fd-b69b-5ad3f462e2a4")
		)
		(fp_line
			(start -1.374773 -1.2)
			(end -1.374773 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b8e2dde2-4c78-450c-ad05-bb867e81add1")
		)
		(fp_line
			(start -1.15 -2.15)
			(end 2.15 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fdc2475e-112a-4350-9593-41eace6c60a3")
		)
		(fp_line
			(start -1.15 2.15)
			(end 2.15 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c28f8ad8-7eb3-4175-8f33-8c07a72f8a70")
		)
		(fp_line
			(start 2.15 -2.15)
			(end 2.15 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cdac3158-774d-4049-8e64-2c228a93d40d")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "85b24525-92a4-4036-b6fa-e40541b2a333")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b51f8e0a-1d57-40c9-9965-2d97ad8cb33e")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.8 0)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 40 "Bat Shunt 1")
			(pintype "passive")
			(uuid "38e67e51-a4c6-4873-98f7-44b910a5cf1e")
		)
		(pad "2" smd roundrect
			(at 1.8 0)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 1 "GND")
			(pintype "passive")
			(uuid "11b3c3fb-d8b3-4e98-b1d6-931a0b7a3c53")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_4x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "51613e34-18a8-4e42-88c4-4301f35234f3")
		(at 122.5 105.7)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R23"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "bf504faf-91ab-48de-86a7-d950b3834eab")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "51.1k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "ca1fa160-7669-4880-895d-6facb0410c80")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "93fbe99e-7cb6-40c8-ae1a-a4e9648afa07")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "919e596a-e94a-4fa6-add4-6dc68be3d10e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/e451565a-fe1f-4586-a24d-ecc270889779")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "570e5f40-3ce9-4b11-829d-6ef9a8a7198a")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a59266f8-5abe-465a-aa48-ff369af3bb9e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3415a1d3-afb0-4b3c-9376-85989ceafb98")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "75855f13-8f07-4392-b307-78be1ca9aad6")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9356bf8e-0adf-48d2-b02d-cafdb992569b")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "74fb8ef0-9450-4b1d-b346-8fd1b6d0e7f0")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "162ccae0-4e33-4a90-a26a-0a70698afcf7")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2549df1f-5815-419c-a1aa-711f8b088129")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eab686f0-19a9-4a6a-86a9-e51ef4942df1")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a4e0843-f2ec-45f6-b0f1-a90b59d122c9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a23c34bc-a7f3-4e59-bcd0-6273c47ab3fc")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 39 "Net-(IC7-ILIM)")
			(pintype "passive")
			(uuid "46ed65f4-bdfc-4679-8db9-6bbb8d3b914e")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "131c52a8-00c0-42cb-ac31-4ee300a73edc")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "5263a01e-bbb6-4773-8ebd-58da5fe8ebbe")
		(at 65.1 113.6375 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(uuid "8f731fd7-c6a0-4e94-9b50-e2b5a5e68bc3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "610feecc-b967-4948-97f8-48aed4c3d2b0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d4b333de-54e0-40ce-b294-1f1cde76f8f8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d2a8e8a7-d291-43c5-8695-dc4a163b19e9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/c064599d-eb2f-41e7-9521-e7d37647e88f")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5319a323-380a-4d73-afb8-42f302dd90bf")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "13e94ae0-8490-4f4b-8768-889dd7bfa2c7")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1fc1eccc-0c42-4910-9560-e16ac478bfb6")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "70efba6e-9605-4062-ae95-b4fef1a12e5e")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07ba783d-23b4-4be9-8bec-de3ad634d4fb")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3130ed9e-67a7-4cbd-900a-74aa4be4c45d")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "398842f1-1ce0-4a74-b863-609b7027e9a7")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fbac390d-02a4-45f3-99f8-5e7daf29c983")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77a825d8-ca56-4b02-8b4e-0f78306ac8ff")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "278828d5-dae7-46d2-8681-c52a15c941c3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "d3f7f02a-497c-40ad-b75d-289941cc7547")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 34 "VBUS")
			(pintype "passive")
			(uuid "3e85c469-9093-42df-8459-3af27c2db393")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 4 "Net-(IC1-VDD)")
			(pintype "passive")
			(uuid "d478cc9d-847b-4b70-9fdb-b73302fa0eb7")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(uuid "53f21816-b5e7-48cf-8495-d16819fc5349")
		(at 97.458 130.93)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D6"
			(at 0 -2.5 0)
			(layer "F.SilkS")
			(uuid "e35eda8d-93c3-4653-8cdc-a78dac1d5f55")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "D_Schottky"
			(at 0 2.6 0)
			(layer "F.Fab")
			(uuid "a2d5239d-44e0-4129-9187-5f5056cac229")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "38e36e2d-8591-480b-b81d-239c72e2b472")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Schottky diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9ae88721-6694-4b6f-b6f0-145d04bb4ee9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/44adfc12-e24b-4e03-b51b-197393e705f6")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.51 -1.65)
			(end -3.51 1.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d4e03305-bb34-4d0b-a851-eec3151dbf29")
		)
		(fp_line
			(start -3.51 -1.65)
			(end 2 -1.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "29a9c3dc-02ab-4696-92e7-913d20fff79e")
		)
		(fp_line
			(start -3.51 1.65)
			(end 2 1.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1669d74b-04bc-4348-a846-0c24599396c1")
		)
		(fp_line
			(start -3.5 -1.75)
			(end 3.5 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "23a42554-88aa-4f5b-8329-523e70811abc")
		)
		(fp_line
			(start -3.5 1.75)
			(end -3.5 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "302b0add-84d4-4f15-a097-0c03d8304a38")
		)
		(fp_line
			(start 3.5 -1.75)
			(end 3.5 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "01ca23ed-9180-4d10-8a89-daf08ee62623")
		)
		(fp_line
			(start 3.5 1.75)
			(end -3.5 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eaedf6d4-4138-41b9-b617-bbf8d9d8be0b")
		)
		(fp_line
			(start -2.3 1.5)
			(end -2.3 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "40677b0e-fad1-437c-b5e2-7abe51016d07")
		)
		(fp_line
			(start -0.64944 -0.79908)
			(end -0.64944 0.80112)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "75f6245e-01c3-4393-b959-976d98054553")
		)
		(fp_line
			(start -0.64944 0.00102)
			(end -1.55114 0.00102)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d197aa8d-09e7-4ccc-b822-7fd493198820")
		)
		(fp_line
			(start -0.64944 0.00102)
			(end 0.50118 -0.79908)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0e7201d9-19d0-44bd-a3e3-fb0bbc04cc49")
		)
		(fp_line
			(start -0.64944 0.00102)
			(end 0.50118 0.75032)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7be4eada-004e-49d6-959e-11bad6bebd27")
		)
		(fp_line
			(start 0.50118 0.00102)
			(end 1.4994 0.00102)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb78d11c-2d84-4df1-a166-af6b31c1a7e9")
		)
		(fp_line
			(start 0.50118 0.75032)
			(end 0.50118 -0.79908)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a12dddd6-431a-4ec4-b740-b79aa9e74cea")
		)
		(fp_line
			(start 2.3 -1.5)
			(end -2.3 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b8496fd0-0aa5-4cd2-9954-8d87d65f0769")
		)
		(fp_line
			(start 2.3 -1.5)
			(end 2.3 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "68b92901-0406-4f97-a368-b7a9927ee6f1")
		)
		(fp_line
			(start 2.3 1.5)
			(end -2.3 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "353182eb-5dc0-40e4-bd2b-3a34eefffcfe")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(layer "F.Fab")
			(uuid "f10bd623-a57f-4cc8-979d-7f3e62832f5b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2 0)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net 51 "Net-(D6-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "e0a05f65-ff1f-44d4-840a-9e5886596247")
		)
		(pad "2" smd roundrect
			(at 2 0)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "6b1416d5-7c76-4319-b390-263acf553ff4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "5564ba31-04e7-4daa-b1b2-f4ac0dd6a470")
		(at 188.0375 129.04)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C31"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "0c2fe432-76bf-461c-a9a2-ab60732328bb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1.0pF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "284f076b-f39b-4e75-bd88-fbf3d74b55ad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dd0609cf-1894-4aa9-8604-9112c7a4c5ef")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "816b390e-18ba-45fe-a3f4-2c2cdc4a5302")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5b0ccd8b-c1ff-4957-b52c-fb05af365599")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "89c4d128-3f25-4c27-b290-1e4de72ab836")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4963b04c-7c15-475f-97a5-39602831b319")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "11504a11-62db-4bc1-a9ac-e89e6f0cf907")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "29824de8-19ed-4c92-9338-28662860a2f1")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "43a3a31e-3df5-4943-90c1-af74d7a911fc")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6e112ef2-b627-47ff-ba19-4199ea8f8de1")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d42e0147-411b-4bca-b45c-045b52609bc9")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4bbcb21f-8d3f-41e3-a495-0d817f886bcd")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fa7dd4fd-dce0-41fb-a77c-995e5b7daaa5")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "22d824d5-8f8f-4b22-9515-50a3bec9bdbb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bb6ffa7f-3a4f-4165-942b-0652b480f425")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 10 "Net-(C31-Pad1)")
			(pintype "passive")
			(uuid "c0625cff-cb1e-4b23-8858-9acef32d9457")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "ad2262d2-7363-45b0-815b-5efaf861425b")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "55be7567-0956-4510-a2cb-2157f6ab9a1c")
		(at 188.0375 126.03)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C30"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "d4bf31aa-72c0-4509-a0c4-b8ca549a2c7e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "220pF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "ca5fc135-5ad3-4272-8d73-cbc2bf02eaa7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d0314828-be50-4883-aeb4-263924c2515f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9d0224b0-fe90-415a-b0a8-324065e90d66")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/94a8d90a-7b4f-41d0-b668-94e38db10a4e")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb6c25ca-db7b-4c5a-b45b-06a2d2942ec2")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b8fe50b-a779-4e56-a902-b05941ed8035")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ae4ef87-8a2a-4579-8d10-10ee066fbfde")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "86e74d7b-89cf-4e0a-815c-6affb494f523")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1a7eeee9-8472-4a85-bf83-f51bece07d06")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4b3952fe-dd5f-4fbc-9846-5e2fe11fc5e1")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "02bf6c4e-3ec3-4bee-a942-ff89e9ac8272")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "59e25a85-a8aa-4059-a09a-b3948248ee82")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8857e017-cd30-4b40-9890-bc4ef3ab651a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "70a1841a-1c2c-440f-9b24-6d8b0c6b6005")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "91e1ef82-4961-4a6e-9872-15a1a35f782c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "9f479bdc-4596-4193-8abf-dfb1d1b04531")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "da0764dc-6bbc-4b51-a90e-ab5b82dec043")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "58aade41-1ef3-41d1-b840-f8219d5f4930")
		(at 188.0375 120.01)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C28"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "dd1d4c37-162b-4d3c-b8a7-6801244df2ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.047uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "b31f3140-f932-4cb1-ab39-1a94df6373c6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4dfa458d-ba3f-4528-be79-876170b13232")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "82d81107-7700-4772-a277-af33d8e73dc8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/ff9598cd-0bb9-4b77-921e-804b10875021")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fef52690-2586-420f-a1a3-be8102e4a381")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "883314ff-fe23-4714-ad05-f0c20dc0950c")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b337a244-cb9b-4341-ab82-efc5ae25f9f7")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "63b79653-e9cb-4c56-ad79-65073910e379")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "98364fd0-76b0-43ec-9438-43af247c1797")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6d1c0806-7f92-494d-ac9c-22021d2f1c47")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa12428e-94fa-454a-baca-82d6e5319fcd")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a719b0fc-41f6-4f24-8b68-c56f241ff519")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f84f3992-2d35-462b-b2e1-29cb60be9a50")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15a37912-d526-4234-96d9-fb3667d175c1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "64e81b72-9fb5-422b-a202-f11abe9c7239")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 9 "+4V")
			(pintype "passive")
			(uuid "9857115c-695d-44e4-a431-fc2b71d97ced")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "cfcbb5f4-42c6-4d81-bff2-9531a799e073")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic:SS3235SL3"
		(layer "F.Cu")
		(uuid "5a223f8a-3a0d-4c3c-b888-d08b47ad07d1")
		(at 189.5 142.5)
		(descr "SS-3235S-L3")
		(tags "Switch")
		(property "Reference" "SW3"
			(at 0 0 0)
			(layer "F.SilkS")
			(uuid "6955e53d-6efc-4bf3-a996-a0dfa88b381c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "SW_DPDT_x2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "ee73d707-de3a-4442-a8c8-fadf9fdb8ad6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cb438698-27d8-49b4-9615-9f33fd67ba4b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Switch, dual pole double throw, separate symbols"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "fd3941c4-0e73-4f79-90b2-1cab4a52b1cb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C381098"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7b52076c-d77b-487d-8a60-0ce91461da27")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field6" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a003fec7-106a-47b1-beb3-37886a1b006f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SW*DPDT*")
		(path "/25f5c15c-0d18-4403-8564-3038978e4c9d")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.6 -3.25)
			(end -4.6 -3.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1661e0e5-6a7f-4e65-95e8-791ee3e22606")
		)
		(fp_line
			(start -4.6 -3.25)
			(end -4.6 -3.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1fb88bd8-8ac6-41a9-982b-e6f3668cc835")
		)
		(fp_line
			(start -4.55 -1.775)
			(end -4.55 1.775)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7ea5775-86ad-40a6-8e89-fd21e43838d7")
		)
		(fp_line
			(start -4.55 1.775)
			(end 4.55 1.775)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "afd899d3-07b7-441e-afdb-aaf253494254")
		)
		(fp_line
			(start -4.5 -3.25)
			(end -4.5 -3.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91b86000-c2c4-4ac2-870a-e11dc9d1cf19")
		)
		(fp_line
			(start 4.55 -1.775)
			(end -4.55 -1.775)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "07c942de-9d08-4358-8b9a-00ad56fd0ba3")
		)
		(fp_line
			(start 4.55 1.775)
			(end 4.55 -1.775)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "52a8fcec-00a5-4aff-8e58-1bb3c2845d6c")
		)
		(fp_arc
			(start -4.6 -3.25)
			(mid -4.55 -3.3)
			(end -4.5 -3.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d321af72-3bae-430b-a1da-4342f2d7cbf5")
		)
		(fp_arc
			(start -4.5 -3.25)
			(mid -4.55 -3.2)
			(end -4.6 -3.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "258b1d29-2a85-4dd3-a995-8d40961b3e91")
		)
		(fp_arc
			(start -4.5 -3.25)
			(mid -4.55 -3.2)
			(end -4.6 -3.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "52d6b42a-c4ec-4ce1-b360-d9a2283b58c2")
		)
		(fp_line
			(start -5.55 -4.85)
			(end 5.55 -4.85)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d1a5838a-fb01-44e2-acde-45a656dfd918")
		)
		(fp_line
			(start -5.55 4.85)
			(end -5.55 -4.85)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5816b4c1-ba06-4a08-ac63-2e7ed3cbd3f8")
		)
		(fp_line
			(start 5.55 -4.85)
			(end 5.55 4.85)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "51c56183-427a-41cd-bcb4-7e6f1e886c59")
		)
		(fp_line
			(start 5.55 4.85)
			(end -5.55 4.85)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "422ed81a-4871-4f63-8d98-5ba10ce49eb6")
		)
		(fp_line
			(start -4.55 -1.775)
			(end -4.55 1.775)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "04b2e384-7390-4e5e-869c-c41a97f4cc9b")
		)
		(fp_line
			(start -4.55 1.775)
			(end 4.55 1.775)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "33a1d75e-ed5f-44f8-bd75-5abc0a2b2f6c")
		)
		(fp_line
			(start 4.55 -1.775)
			(end -4.55 -1.775)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d18f02a3-684c-42d2-af84-453a5ae9684b")
		)
		(fp_line
			(start 4.55 1.775)
			(end 4.55 -1.775)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c9eacb0f-4d4f-4e2f-8a62-382e34f7c9a5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a29d810a-517d-42b9-b93c-fe1e49a59602")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -2.5 -3.25)
			(size 0.7 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "USE_ANT_1")
			(pinfunction "A")
			(pintype "passive")
			(uuid "81bd4de1-2e01-432b-a9fe-efc31187604a")
		)
		(pad "2" smd rect
			(at 0 -3.25)
			(size 0.7 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "B")
			(pintype "passive")
			(uuid "9e7a5647-6de1-4e43-a9e1-d4aa187828b8")
		)
		(pad "3" smd rect
			(at 2.5 -3.25)
			(size 0.7 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "USE_ANT_2")
			(pinfunction "C")
			(pintype "passive")
			(uuid "c1908cd7-e6a4-45cc-90e1-28a1ce91cee9")
		)
		(pad "4" smd rect
			(at -2.5 3.25)
			(size 0.7 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(uuid "b254ca22-e4be-4068-8815-227a6da9c7e9")
		)
		(pad "5" smd rect
			(at 0 3.25)
			(size 0.7 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(uuid "0f35aa99-86d4-4ae5-ae57-bdbe40e1f6b0")
		)
		(pad "6" smd rect
			(at 2.5 3.25)
			(size 0.7 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(uuid "78daf6e9-c0c3-406d-9a28-ee542e07ece6")
		)
		(embedded_fonts no)
		(model "SS-3235S-L3.stp"
			(offset
				(xyz 0 0 0.3499999888)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "5cea41a3-ac15-4b7b-93dd-18ed2c9c88d9")
		(at 47.4 99.3875 90)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D1"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(uuid "ff6951f9-98ac-4806-a1fc-c41b2b1d3537")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "39240693-4b19-48c0-b22e-d08e5d7cc1a2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3597d8f5-71ba-48af-87b9-3c6bca597218")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "12abd80e-4e18-45b9-a4d2-9675313310cb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/2b2b19c4-d737-428d-9c65-e4b12d35ed70")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2c35f17f-c450-4de0-87f8-dcaf965ed705")
		)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6fd96771-06a3-4bb1-ac75-07853f449929")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "edbda56e-9685-49dc-b550-f2debfa16007")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9769eae4-1a31-493c-9b5c-99e2b3817ae9")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cc8fe7e1-6c36-4d78-af75-b3fa37fb23b0")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7a76e0ac-4e55-43f3-9144-e3e8ab836e30")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3b0faff8-07d3-4be6-a1fb-8ec1e702acf0")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fcc49487-bd5f-403e-91a1-285629f44b90")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5bae8371-150f-4167-a26b-073e20567d74")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a8a1c040-7b1b-43a0-a4c9-2b2f70d4e1f1")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1241abb8-d232-4d3d-a196-525bb1f74e9d")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c783cff0-66fc-4b0c-a7b0-16c68ffb73eb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "9f5073b8-989a-4626-b340-396eb89b9632")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0 90)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 17 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "f6b59f55-b3c3-4150-b0e5-a8a0cb4782a8")
		)
		(pad "2" smd roundrect
			(at 1.025 0 90)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 16 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "8f8c9d5b-69de-4a5b-903a-e89e8587ad4e")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "5ff8bf81-3ef2-4398-a81a-9f067038e201")
		(at 185.4625 106.89)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R17"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "e7bca807-126a-437e-9730-dce2ca59af92")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "ece6e341-7ad4-4d20-8cde-1931ac3738b4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "06b675e0-deed-4883-adb7-d78c33c90e03")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "64f86a7e-3ada-40f0-9eac-5effaa529a89")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/3ccd7da3-ea73-4653-b042-b982c6ffcd9c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8060d546-2ac9-4c83-939f-ee6645c33e26")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "38ef5830-ff89-4eda-97c1-6fc35c48a3cb")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1c5fbb31-aad8-44df-b0eb-8a66744e1a7d")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f13ce1d-d9ff-44b0-b139-0f12d747dd0f")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "74f74c6e-4ec7-4e73-84a2-b04c68c516da")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "60722266-37d1-4582-9a33-d5f8e3518180")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b6f3e34-59fc-4d57-a57b-4376eed13494")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e998c133-b987-4663-9ec1-d8c918018dbb")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "93dba269-82e5-4c0a-a307-43dd385bd989")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c07b2dfc-cef2-4b60-b874-2a299b8c8e7a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "39329d6a-c08d-4d23-afd2-a9fc80192b97")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "6c8cfd8b-8749-478b-a3d0-67a421064a49")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 65 "I2C SCL")
			(pintype "passive")
			(uuid "67b748c5-65dc-42b4-8d36-1aaa8dc6af54")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "6070021d-8fb6-4fe7-aead-848e1ec2e785")
		(at 197.6275 113.78)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "inductor handsolder")
		(property "Reference" "L7"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "cc6526ea-a1ad-4446-b756-43eeb453f8c5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7nH"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "aa14347e-78ef-4908-b39e-365973d073af")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "983c3584-e74d-46ef-b5b3-db77fd683d36")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "054b6c47-fe39-4c0c-9446-c3ed39e78cf6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/ddfa3310-1df8-4f37-9f15-c0d0b84115ff")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.71)
			(end 0.261252 -0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c9862c0f-4a9e-4dcd-aeb6-87aad8af47d7")
		)
		(fp_line
			(start -0.261252 0.71)
			(end 0.261252 0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6789bc65-ada5-41c5-ae39-c42418d8f866")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d951994a-b2bd-46de-91e8-cae97e09c4d7")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2c63e4c1-d43b-465b-a9ff-bcdbacb04813")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1f126216-5fce-4390-9ba6-edffb95fa475")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c8831bf9-0f5e-4491-809b-f8c3e4aac552")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "380a539c-cfa9-464a-bb08-84225af1cfd4")
		)
		(fp_line
			(start -1 0.6)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57941ffb-2fd9-494f-8262-038d4ae88dbf")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4b7b2fef-5c1a-4818-b216-d7fd766c3943")
		)
		(fp_line
			(start 1 0.6)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c0d7216-32d7-435e-9c79-47025d766d2e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f79d4452-018e-4d8c-bf92-2458190f2190")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 10 "Net-(C31-Pad1)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "01a32dea-9b85-46bc-8979-10cd3c18d7fb")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "Net-(AE3-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "747d164c-5e24-48ff-8b9f-5e97093caf2b")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_EH_S5B-EH_1x05_P2.50mm_Horizontal"
		(layer "F.Cu")
		(uuid "6581e15c-751f-4271-828a-b4e4f207f2c1")
		(at 173 140.4675 180)
		(descr "JST EH series connector, S5B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH horizontal")
		(property "Reference" "J2"
			(at 5 -8.0325 0)
			(layer "F.SilkS")
			(uuid "ad1b6c7a-a2ac-42fb-81b7-7b20aa7a1d39")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x05_Socket"
			(at 5 2.7 0)
			(layer "F.Fab")
			(uuid "d1a99cbc-8c01-4bca-9dc3-f28ccea1795d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "67f2ad60-8d1e-40e1-90a7-6d27cf0cb7fe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "35b97e7d-dd67-45e6-93e5-fb30f5d8d84d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/855dc855-fadd-46fb-a7fe-1cc286f51387")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 12.61 1.61)
			(end 11.39 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eb786691-cbe5-4890-9643-362c436ae6e5")
		)
		(fp_line
			(start 12.61 -5.59)
			(end 11.39 -5.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "acf70627-753e-4f33-bb07-0d76e74539e9")
		)
		(fp_line
			(start 12.61 -6.81)
			(end 12.61 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "54d603f8-dd6f-408e-a62a-57e5f67476db")
		)
		(fp_line
			(start 11.39 1.61)
			(end 11.39 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "25b39541-e405-4931-a761-68eda4076b45")
		)
		(fp_line
			(start 11.39 -0.59)
			(end 12.61 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c83b4b25-1f0a-434d-83b3-a3c76d0864ee")
		)
		(fp_line
			(start 11.39 -5.59)
			(end 11.39 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0e900b37-8f3e-4739-a3ac-2782aec8c2dd")
		)
		(fp_line
			(start 10.32 -1.59)
			(end 10 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3154b9c3-18d5-4ba1-9a96-004b2e3ce185")
		)
		(fp_line
			(start 10.32 -5.01)
			(end 10.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73dcd71d-3889-413c-aa99-f613bac482d0")
		)
		(fp_line
			(start 10 -1.59)
			(end 9.68 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fd6eb60a-7b37-434a-9973-f23e4e2eb81e")
		)
		(fp_line
			(start 10 -5.09)
			(end 10.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2cb671d2-865d-44bb-af0a-4ac12036d57b")
		)
		(fp_line
			(start 9.68 -1.59)
			(end 9.68 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "43848300-e065-4d22-acac-cfb45a8873de")
		)
		(fp_line
			(start 9.68 -5.01)
			(end 10 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6b49faa3-d50d-4c1b-b5fb-2770440e921f")
		)
		(fp_line
			(start 8.67 -0.59)
			(end 8.83 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c7504fa5-9664-4bc9-ad81-8de26d64a128")
		)
		(fp_line
			(start 7.82 -1.59)
			(end 7.5 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "693ec186-cc08-495e-b4e0-2458ee9f1cf8")
		)
		(fp_line
			(start 7.82 -5.01)
			(end 7.82 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5a383ed3-f703-4eaf-b65f-9c84e86d83de")
		)
		(fp_line
			(start 7.5 -1.59)
			(end 7.18 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9167cac4-f0cf-4fcb-ab24-b174a6bf1d12")
		)
		(fp_line
			(start 7.5 -5.09)
			(end 7.82 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9fcbccc7-16e8-4403-a684-18296f15133a")
		)
		(fp_line
			(start 7.18 -1.59)
			(end 7.18 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e466b93c-5ec9-4b11-ac3a-c52e3e4b10b2")
		)
		(fp_line
			(start 7.18 -5.01)
			(end 7.5 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a3fc3e8f-0dd9-4198-bc78-762c922f91c3")
		)
		(fp_line
			(start 6.17 -0.59)
			(end 6.33 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d36c872d-1333-4bd9-bedc-b849f7e19040")
		)
		(fp_line
			(start 5.32 -1.59)
			(end 5 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "152dfac3-8760-4b78-bc1f-fd1ea5ab68c8")
		)
		(fp_line
			(start 5.32 -5.01)
			(end 5.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "175eb485-ca78-4dac-842c-9dca79cd5904")
		)
		(fp_line
			(start 5 -1.59)
			(end 4.68 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac772573-4dd7-46de-ae56-ca11ae747c05")
		)
		(fp_line
			(start 5 -5.09)
			(end 5.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d811c6c6-1a7e-4ffc-8a31-fb7caa998219")
		)
		(fp_line
			(start 4.68 -1.59)
			(end 4.68 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c57a6120-572e-49f7-906c-8e7fbe44ba4d")
		)
		(fp_line
			(start 4.68 -5.01)
			(end 5 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b2c30181-0810-4448-aea4-f9a96caf1cc5")
		)
		(fp_line
			(start 3.67 -0.59)
			(end 3.83 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e71745da-295c-444d-ae12-b12fdbc82f81")
		)
		(fp_line
			(start 2.82 -1.59)
			(end 2.5 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "51c10211-7f8f-4fa7-8eed-80abafd1de25")
		)
		(fp_line
			(start 2.82 -5.01)
			(end 2.82 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e48970a-a800-4fe4-8aa5-e15d24c5c67a")
		)
		(fp_line
			(start 2.5 -1.59)
			(end 2.18 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0abb58b3-71b0-4320-b11c-6dc0dbc93463")
		)
		(fp_line
			(start 2.5 -5.09)
			(end 2.82 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2eb46bd3-d1a2-4638-a625-5672fe8fcf79")
		)
		(fp_line
			(start 2.18 -1.59)
			(end 2.18 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "08211a34-750b-4b11-8dfc-57771a6338db")
		)
		(fp_line
			(start 2.18 -5.01)
			(end 2.5 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9f2dd645-53aa-46ef-996e-dfc020eb27d4")
		)
		(fp_line
			(start 1.17 -0.59)
			(end 1.33 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "433e7b92-c8f8-4e0a-b86c-760352c8499b")
		)
		(fp_line
			(start 0.32 -1.59)
			(end 0 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a5854cc2-199a-4707-ae67-ed1e0de6650d")
		)
		(fp_line
			(start 0.32 -5.01)
			(end 0.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed3d8035-73dd-4b05-89fe-a2961add4237")
		)
		(fp_line
			(start 0.3 2.1)
			(end 0 1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b3ef1eb6-56e8-4937-a468-71f57a2d2722")
		)
		(fp_line
			(start 0 1.5)
			(end -0.3 2.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c05c7411-cdd9-4c02-bb5a-e4481fdeea39")
		)
		(fp_line
			(start 0 -1.59)
			(end -0.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "44c80996-c42d-4598-987c-15d54f8041d9")
		)
		(fp_line
			(start 0 -5.09)
			(end 0.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c7f3741c-ca72-4dd1-8532-0f640b15b094")
		)
		(fp_line
			(start -0.3 2.1)
			(end 0.3 2.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "37f911ec-a243-4d47-8c61-6c1286aa7b5e")
		)
		(fp_line
			(start -0.32 -1.59)
			(end -0.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c7c4ae96-b4e1-4770-8951-e2e2bb0100f5")
		)
		(fp_line
			(start -0.32 -5.01)
			(end 0 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f0e680f0-a426-4bff-b93f-413b27e93fab")
		)
		(fp_line
			(start -1.39 1.61)
			(end -2.61 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9b87dca3-a429-4312-ad75-cba7334bd288")
		)
		(fp_line
			(start -1.39 -0.59)
			(end -1.39 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a179015a-a24a-495f-86c5-ebe4e207e3a5")
		)
		(fp_line
			(start -1.39 -0.59)
			(end -2.61 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c1aeba70-ce0a-4348-bea2-9856db65959e")
		)
		(fp_line
			(start -1.39 -1.59)
			(end 11.39 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eb828071-c4cb-4878-babf-31a7d26a7848")
		)
		(fp_line
			(start -1.39 -5.59)
			(end -1.39 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "09f9eafe-d441-4a7a-83c9-17b10f31b31b")
		)
		(fp_line
			(start -2.61 1.61)
			(end -2.61 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a66bd2b0-09ec-41cd-956f-1da1f3bdaf0c")
		)
		(fp_line
			(start -2.61 -5.59)
			(end -1.39 -5.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f5351498-9b20-4ee3-9023-4284d4830ebe")
		)
		(fp_line
			(start -2.61 -6.81)
			(end 12.61 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc96e993-0754-4514-9987-38aa4246abd8")
		)
		(fp_line
			(start 13 2)
			(end 13 -7.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b73548b7-c766-400b-8c24-e02f13ce2764")
		)
		(fp_line
			(start 13 -7.2)
			(end -3 -7.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2c75b56d-7935-4f71-a210-e57ff5aea7b1")
		)
		(fp_line
			(start -3 2)
			(end 13 2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d8a61cd4-c11c-4a3d-b5f0-daa4fc85ab50")
		)
		(fp_line
			(start -3 -7.2)
			(end -3 2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0494abea-addb-41ab-beb5-c7a251ede2c1")
		)
		(fp_line
			(start 12.5 1.5)
			(end 11.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "97ca59b4-3199-45d3-8d8b-639fda528997")
		)
		(fp_line
			(start 12.5 -6.7)
			(end 12.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "94a5393a-2abb-4ed9-96e4-7a5be7fcfcff")
		)
		(fp_line
			(start 11.5 1.5)
			(end 11.5 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c8d45bc9-6b88-4271-be41-40a72bcf719b")
		)
		(fp_line
			(start 11.5 -0.7)
			(end -1.5 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d428665a-6771-4f6a-8b1e-50ef90be43e4")
		)
		(fp_line
			(start 0 -1.407107)
			(end 0.5 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "10e26ba7-0bf0-44d3-9e75-649b40830716")
		)
		(fp_line
			(start -0.5 -0.7)
			(end 0 -1.407107)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87dc88a1-5503-4eb3-8215-4a53b5fee3de")
		)
		(fp_line
			(start -1.5 1.5)
			(end -2.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5c2eed92-8fdb-4570-8c62-4841d854f1a3")
		)
		(fp_line
			(start -1.5 -0.7)
			(end -1.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6c201a11-f122-4cd0-b9a7-8ea4266cc539")
		)
		(fp_line
			(start -2.5 1.5)
			(end -2.5 -6.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "50c085f4-a351-4498-b1c4-191a9e30cf68")
		)
		(fp_line
			(start -2.5 -6.7)
			(end 12.5 -6.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b136bc8b-6144-4120-8963-2114ec89a2b2")
		)
		(fp_text user "${REFERENCE}"
			(at 5 -2.6 0)
			(layer "F.Fab")
			(uuid "91b38a1e-9747-409b-9b6b-1a4c0e8e105d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 3 "VDD_NRF")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "937617af-96d1-4e6a-85c0-0df1f8009c3f")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "GPS_EN")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "441bfde5-4600-432f-abc1-ebdf20cf5324")
		)
		(pad "3" thru_hole oval
			(at 5 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "GPS_TX")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "5ac99f24-c151-441e-99d6-ad829cfffdeb")
		)
		(pad "4" thru_hole oval
			(at 7.5 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "GPS_RX")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "dc8a5820-61a3-4fe4-9a3a-2a1e735f6a0d")
		)
		(pad "5" thru_hole oval
			(at 10 0 180)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "ba7cd3c2-2f6d-4e56-b782-e576838e17a4")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_S5B-EH_1x05_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "6746e8ae-e6a9-4db0-90c7-889b2672815c")
		(at 191 95.99)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C22"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "04b57fb0-a8c0-4cb9-bcca-86e0d475ff80")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "c00e261f-2d37-4754-976f-fb4c90c7f9bd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4956f8b3-f6fe-4acc-9123-90f4df596ea5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bf20caaf-4480-4676-bc21-895e5681f225")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/36c7bd9c-372a-453e-a6c5-cf249c3874d7")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6091339d-854c-4ebd-82f1-a64763320022")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b608067-1dd6-4304-ac17-ab148f5ab582")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c1aa582a-173b-4f30-99d3-76f57272756d")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "036148e1-8474-4ee0-b2de-70b81892c2ea")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5be57591-3c56-489d-93a5-d18020e9552a")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "979b2478-a74d-4127-9562-2eafa1144194")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cf8e6530-3824-45ca-8ec6-90c549d2bee7")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ad1a6174-7358-42ff-bc36-b70d42390f3c")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ccabdfec-5fac-45ef-b919-c6d18b9e7669")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "045b91b6-09ae-4a61-8df6-6bb214ccc23f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2e8175ad-2fa6-434c-a809-4207e55794fe")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "6e428f2b-97ba-4bf7-a427-058ca3ea949d")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "2e4c6c89-855a-42b4-8473-7177392c7e16")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "7532e81b-518c-47a0-ae39-d7baa5f76333")
		(at 127.25 111.6)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R36"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "e3f5bbc4-58fe-4cb2-8180-731ae164688a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "c24d2069-f8fb-4211-932c-58705896e081")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b6d510af-a10a-411b-8313-9ad31f4c4da0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5ded2205-63d2-495a-a794-121c395377f6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/728def05-04b3-4581-8e79-23d03058df83")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "372836e0-9e33-4fb4-a781-d3cbbc0d2fd2")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e13a5e3c-a33e-4a79-ba4d-ddba7f4193c8")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "92e16d47-e9e4-453c-8dd6-e32e6f329acc")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf185b10-e858-40d2-ab6f-6479c001bcda")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0e2bccde-1df9-4bdc-b749-e5d92901da72")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "afb5e300-5e51-4e53-94d0-1ef0f8bd515b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f9946deb-c61e-4083-ad90-95fc3a1b50f5")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32e852fa-e874-400f-a5ed-d39a0a9b01a7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "21ab7801-2f8d-4300-8b49-a9cb636aba72")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "399d43ec-b361-447d-a6e5-f6cce8327fce")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "fd74b206-8c36-4a05-b486-f014419a60ca")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 50 "Net-(IC2-CSP)")
			(pintype "passive")
			(uuid "dba6b29d-3ea9-4c66-a07b-f25443616a2c")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 40 "Bat Shunt 1")
			(pintype "passive")
			(uuid "449491e6-4c26-4477-a9ea-a426c8821586")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(uuid "77d37a00-64d3-4c05-b7a2-4337fae1b755")
		(at 149 108.5 90)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(uuid "7303040e-49a3-45ad-92ab-8bc6539d7212")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(uuid "71082d7f-2030-4c34-ae1f-498fe0722636")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a4908db0-0961-425f-8877-18efba84f2f9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "528f8556-8047-46a9-ad1a-63296e9c9464")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/da71199a-a76b-48b5-8cfd-f9c0a33d6d61")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_circle
			(center 0 0)
			(end 0 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "b3d37c19-2d27-410c-b838-3f5c4eda047b")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "c355a47f-4422-4566-b98d-1aae9ff21dc3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
			(uuid "b434b882-25a3-481c-bf44-bb4a69feb8f3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 64 "I2C SDA")
			(pinfunction "1")
			(pintype "passive")
			(uuid "2a3ce361-f4a9-497f-b1fe-0857e68f6e18")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "7835b9d2-b5de-4504-96a8-9da838554b62")
		(at 122.5 114.55)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R26"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "c8389fff-6475-48a2-b193-e84211e83517")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "23.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "a500c287-d376-466b-a845-73a8d6c5deff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7d0d73dd-04b3-4021-b573-6b0c9361cc38")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6f57be25-cd84-49d5-af00-a142b2a921ee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5bb0c5dc-2ea7-4f9c-83a5-c9b77fb41be9")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "265cb0c9-51db-4c74-9e5d-9dfe34583936")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "54c79562-938b-4521-9e45-4952494b427e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ffde0ae2-bcbc-4246-b748-9cf96b51d934")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2ad72a69-0ada-474d-a43d-1878efe43db7")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "125fe4de-d23f-4baa-a923-e6cbb5b8676a")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bb7467df-62e1-4769-8da0-01e84d5e7bd1")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9afa70a6-8b26-4ad9-afdf-b164f2eadeb1")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "01e7b7cd-f7f7-491f-b048-93bbddf27cb9")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9c2c5864-cab7-4ff5-b119-b3ecd5ad2803")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "544f1ffe-e002-4721-938a-cefcef5e91aa")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f1db9b85-9086-4c88-b0d5-1264a7d7601a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 35 "Sol Shunt 1")
			(pintype "passive")
			(uuid "e7cb8afe-b216-484c-abd7-c08c38c06b00")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "Net-(IC4-OV2)")
			(pintype "passive")
			(uuid "aae51634-6104-49e5-ab5e-cf6394e0e100")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "7cc36bcf-0828-4074-b6bc-c570861bc8f5")
		(at 117.75 102.75)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R13"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "c4fb6423-40de-4321-8ef0-faf0e51bf8cc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "51.1k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "941fb3aa-04b6-48d7-97ec-3d56cf68db99")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9ea60a0c-8801-41bd-a8a0-eeb3b4387794")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6814812c-a8f2-4386-a53b-0048161d69eb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/bd3a0d81-f29b-42ea-ab95-f86bff260041")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "08f5c471-a4c4-4b66-8e56-4faad9d9beea")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "546c9190-cc97-41bb-9380-0c19c60077c3")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "98304a11-6d44-47d4-a7f8-bb89d2711362")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "475b3a1a-2ee4-4e92-bacd-ee824aa52b72")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ba2548de-7aea-4fda-8d65-61074bd4e950")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5358704-9c1b-4c3a-966f-da2336171720")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1f71258-c4f9-44e7-abc4-cc053768e288")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8af2adcf-a7c9-4bcf-842b-5bc1f6cdef1e")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "af9097c8-9511-4795-a429-7ea0bf601b0c")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "33f2a624-60e1-4a54-8391-4c718f0370b1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "281c8b6b-997d-4a31-bdc0-14486d303650")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 31 "Net-(IC4-ILIM)")
			(pintype "passive")
			(uuid "f5aa0cbd-1b0c-42e0-9e7c-d3f5eef9e310")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "8b922d24-63fa-44de-a8cc-9b3603d26154")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "7d904ddc-fbeb-4320-a0b5-cf9754dbc5a2")
		(at 127.25 108.65)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R32"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "b9afa835-b47e-46b9-8fcc-374d3ed13861")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "ba8a4b86-d1ed-49bf-b6dd-944fc555a8aa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d93d3ac9-ef7c-4be5-b0ad-651ba8ee1d53")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e2262544-b321-4326-b7e3-960ff3bc54b6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1e4b1651-fc91-4961-a779-3c1d5f5635e1")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0ac27ba7-248b-4987-9fd1-4c09aa460353")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c616acec-a8a6-4462-9d8e-864b2a326b96")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "589ebd73-12b2-4829-8e41-e65fd81fe138")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1856aa52-bb3c-406d-a2b0-592045605dde")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "91c74261-ff7b-404f-b2cf-1735463b74d3")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8a2f1c4-39fc-4398-ae4d-4c957295c78c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "788812ff-ba14-40c9-862a-cbc0ce3c5944")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "69076eb1-360f-4c3d-8c56-c979e784da70")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "647675c2-bcaa-4f79-b220-e943f7c2956a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5e211622-9318-4679-afae-ff771bf36f98")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c4fd6a54-6704-46d6-9984-895d340ca5e6")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 37 "Net-(IC7-OV2)")
			(pintype "passive")
			(uuid "9f793dee-9506-4eff-81c7-0f641d300d1a")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "988ee89f-4a11-462f-9a71-1d1eb591d8a2")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "7f3b7432-8e12-4cb2-a249-532b1e83cbce")
		(at 129.5595 128.475)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D5"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "5cda1077-2556-4190-bc1a-66b2ae2b25fd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "8ece0dc5-3495-4b4d-9b90-5ed348ce6446")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e1d15e0e-7296-4f86-8d9a-ac3ec5c5dd60")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f2f716a5-b464-41f8-a7e8-809048fbd2b9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/56bc0c52-daf5-4ecb-a971-5c95b80418d4")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "48a643ba-eb86-4b0c-b4c7-8121cda4c175")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5488f1c8-eb6e-429d-8794-726d16d04c8d")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f87ead33-96e5-4451-89c1-3e9eeb7ec69c")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2cee2d74-0e34-4692-a488-6471e3c45230")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "255192e4-52aa-4c51-be15-a020e3478824")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "575fbdff-e39d-496f-93e0-67e4e4bb38f3")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2199415-a16d-4c1c-9d82-87dad01fd2ae")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "551c044e-1063-4406-9b4c-6de4aac30e93")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b77ceb73-1ed8-42e1-a036-b27c1e895b3c")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "582adf07-c7ac-459d-a40b-3067ee9b8e35")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "178155e6-5adc-4ea6-bc1d-15d0980dc973")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "85a0b68d-db62-495d-acaa-8654ff19e34b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6f6c559e-b574-40ef-bf00-fe70c9163264")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 28 "Net-(D5-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "e1d2d7d2-c073-4269-9e51-3bc66d6d1a47")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 27 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "0b9e272b-a837-4386-bb63-31d1d3813202")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "815db7dd-fa43-43c8-9c4f-382840476113")
		(at 62.48 128.0375 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C16"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "b2837a12-5929-45e5-8301-9951595c9ba1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "4f04865e-ea23-474f-b11b-8638604bd260")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "98c62d88-1f8a-49ee-9390-408a1f828402")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4785ff9c-2a86-4792-b359-a7f91efbfa34")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/903308f2-98ff-4200-9c95-f1638ce4c5c8")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f4c7414b-eeba-42b2-a797-7fda71debe5f")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "93a9cc27-61b5-4f7a-8c8c-2e57f24cb87e")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "502057ec-66fc-47a9-8cf3-7c8e5417eae2")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b9d5fee7-9513-4074-9a12-1aef2e9642e0")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c55cf856-5ff3-4691-9eee-d662878e084c")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d6fb1d97-e77b-42f0-a405-67a290d00876")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4fb0bd5d-c593-456d-af3c-5afcdf1cc204")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc0f09cb-623b-445b-907d-7904aeb2540e")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2aef5f13-8406-4e48-a87b-892f5ed280c1")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ecc832ad-e4c1-4093-ab66-a548a098cff0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "17da2a0d-96a7-404a-a88d-8822ae048014")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 7 "Net-(U1-VBST)")
			(pintype "passive")
			(uuid "fe9e82db-1741-4d84-ab85-b2cfeba5d2b4")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 6 "Net-(U1-SW)")
			(pintype "passive")
			(uuid "0cd5bda3-edb6-4223-ab35-0b94c5ae4d67")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "857c045a-1222-4ddf-94fc-741501be3330")
		(at 59.47 118.4175 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C38"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "ba36b6cf-57a7-4b3c-ba9b-903873a7ec4e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "83f94497-3d6f-437a-adf0-3266c83999e3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2d503f43-0332-48e5-83ec-271be3aca8b2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4c1aa4f1-2cd3-4847-869a-cc6a8ed11302")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/fd7dc787-8086-4619-91fb-46344c752fb7")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8a80542e-7bb5-4760-83b2-e89889d7e096")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "621e3c7b-983c-457b-9aff-0df8c8c78697")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8897825-476e-4a0e-8b04-c78dd0296bae")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "318ee0d5-278d-41fd-b1c8-3d386e4a619e")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c7431b66-a7f6-4373-8b2e-bb2f39ee4d52")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a5728904-7f26-42e3-a782-feb9b0b506c7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51c0b963-ec0f-4634-93a2-8239f8fc5b93")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6b114c1a-0fee-4a20-b668-1f6d7cbc86cf")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6b505429-bf20-4276-b99d-942013cbbffe")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb090bee-c347-4af0-a99b-eb9a9f8210de")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "8fa59dd5-f7b5-4983-9da3-59dac1c35e20")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 14 "+5V")
			(pintype "passive")
			(uuid "edc60ef3-23ea-49fe-9f4c-2a9d4d471fb2")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "55b30ff5-cc7a-48c9-a042-ac0aa65d56af")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_Push_1P1T_XKB_TS-1187A"
		(layer "F.Cu")
		(uuid "8f57386b-86ae-44a7-a6b9-6aca30b48818")
		(at 146 117.625)
		(descr "SMD Tactile Switch, http://www.helloxkb.com/public/images/pdf/TS-1187A-X-X-X.pdf")
		(tags "SPST Tactile Switch")
		(property "Reference" "SW2"
			(at 0 -3.75 0)
			(layer "F.SilkS")
			(uuid "067aba10-0378-4f91-beff-db618526166b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at 0 3.75 0)
			(layer "F.Fab")
			(uuid "9b4001c8-d563-4194-b38e-d24f734a4c0f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f4f7f307-6f86-4e89-ac86-db19e6bc7e71")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2f274340-7e09-487e-8e8d-953e71c14c44")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C42420254"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1e2f063c-67d4-473a-86d6-30e770ec8e29")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field6" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "58701e3c-56cc-4c63-8639-d0ce4e2673dc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/7fa70f6d-478c-4413-bca4-f8414a66bc57")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.75 -1)
			(end -2.75 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2ade452d-d679-4f6a-b175-dc7b3d27c3ea")
		)
		(fp_line
			(start -1.75 -2.3)
			(end -1.3 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9d832e76-f0fd-49d0-a112-c7c4b2bbe02f")
		)
		(fp_line
			(start -1.75 2.3)
			(end -1.3 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f6dd47e7-4360-4b75-9ec4-8f339990ace6")
		)
		(fp_line
			(start -1.3 -2.75)
			(end 1.3 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9f95595c-6ea7-438d-95e9-f9b1e9f082bd")
		)
		(fp_line
			(start -1.3 2.75)
			(end 1.3 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9f314471-64be-4315-8932-65b1a5906ff3")
		)
		(fp_line
			(start 1.75 -2.3)
			(end 1.3 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "216d6a64-ee48-4a18-8d42-4872bf511ef8")
		)
		(fp_line
			(start 1.75 2.3)
			(end 1.3 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5c527dc3-a6cb-4f0d-b52f-c5049accbd00")
		)
		(fp_line
			(start 2.75 -1)
			(end 2.75 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "54ef5cc8-2c99-4e14-bed0-6b1002fbf294")
		)
		(fp_line
			(start -3.75 -2.8)
			(end 3.75 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fe6e70ff-b373-4f85-8b08-b0bee909ff84")
		)
		(fp_line
			(start -3.75 2.8)
			(end -3.75 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e092b32d-9064-4214-8ced-7f8233b0d733")
		)
		(fp_line
			(start 3.75 -2.8)
			(end 3.75 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2266b5db-c16c-4159-8e0c-26529c30f20f")
		)
		(fp_line
			(start 3.75 2.8)
			(end -3.75 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eba465c1-20dd-46ce-9e52-5298e9ece82c")
		)
		(fp_line
			(start -2.9 -2.1)
			(end -2.9 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "16cd3db3-e54b-4ba7-8d5c-b561dd6f184c")
		)
		(fp_line
			(start -2.9 2.1)
			(end -2.9 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "38fd403a-cbd6-4c4d-96f8-e9a5cc96e1dd")
		)
		(fp_line
			(start -2.4 -1.4)
			(end -1.4 -2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c93b8cef-c7f1-42a9-a99c-2f275a865f6d")
		)
		(fp_line
			(start -2.4 -1.25)
			(end -2.4 -1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bdbee52b-cb93-4f07-a6d6-786fc9770f9f")
		)
		(fp_line
			(start -2.4 1.4)
			(end -2.4 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2279e953-ab31-439c-91d5-9f1c8a66c60b")
		)
		(fp_line
			(start -1.4 -2.4)
			(end -1.25 -2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57831014-5a0d-45d8-b3a6-c1ef91f87651")
		)
		(fp_line
			(start -1.4 2.4)
			(end -2.4 1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5aa7b4e5-2a97-42cf-95b6-7a38160bb15c")
		)
		(fp_line
			(start -1.25 2.4)
			(end -1.4 2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae9609d0-17e1-4991-8d77-4904fadecdb5")
		)
		(fp_line
			(start 1.25 -2.4)
			(end 1.4 -2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "91528b74-1c69-47d1-b462-466c3b230950")
		)
		(fp_line
			(start 1.4 -2.4)
			(end 2.4 -1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "754cc6e4-bc13-4d39-8fcf-d5f18cb55113")
		)
		(fp_line
			(start 1.4 2.4)
			(end 1.25 2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4b7abc0c-554c-41ba-8b41-c4e04a010840")
		)
		(fp_line
			(start 2.4 -1.4)
			(end 2.4 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2d9151f6-8760-4db5-a22a-41b76f3dc966")
		)
		(fp_line
			(start 2.4 1.25)
			(end 2.4 1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "255b6773-4734-4d4a-b52b-2946db6e7d87")
		)
		(fp_line
			(start 2.4 1.4)
			(end 1.4 2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "10194c3a-339f-4b03-95f6-e22fce0da374")
		)
		(fp_line
			(start 2.9 -2.1)
			(end 2.9 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b8e25c8-482d-4d97-b5f1-60c7e5d3c015")
		)
		(fp_line
			(start 2.9 2.1)
			(end 2.9 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "31076d72-151d-4d2e-9489-3be99e492de5")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "3ec817bb-f367-4523-bfa3-4a263c52fc9d")
		)
		(fp_poly
			(pts
				(xy -1.7 -2.1) (xy -2.2 -1.6) (xy -3.25 -1.6) (xy -3.25 -2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "28601af9-ae2b-4f20-a7ad-5e3ce9c58724")
		)
		(fp_poly
			(pts
				(xy -1.7 2.1) (xy -2.2 1.6) (xy -3.25 1.6) (xy -3.25 2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "66ccdfdf-5edf-4089-bad0-c0b2f22580d1")
		)
		(fp_poly
			(pts
				(xy 1.7 -2.1) (xy 2.2 -1.6) (xy 3.25 -1.6) (xy 3.25 -2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "859c90d4-3ef3-4de3-adc3-e13ae9cded96")
		)
		(fp_poly
			(pts
				(xy 1.7 2.1) (xy 2.2 1.6) (xy 3.25 1.6) (xy 3.25 2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "3daf31e5-d3ad-4423-a173-9b32efcda26c")
		)
		(fp_poly
			(pts
				(xy 0.85 -1.85) (xy 1.85 -0.85) (xy 1.85 0.85) (xy 0.85 1.85) (xy -0.85 1.85) (xy -1.85 0.85) (xy -1.85 -0.85)
				(xy -0.85 -1.85)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "3ceaa6fc-effb-4f05-a76d-dd4214d91a94")
		)
		(fp_poly
			(pts
				(xy -1.25 -2.55) (xy 1.25 -2.55) (xy 1.25 -1.975) (xy 1.575 -1.975) (xy 1.975 -1.575) (xy 1.975 -1.25)
				(xy 2.55 -1.25) (xy 2.55 1.25) (xy 1.975 1.25) (xy 1.975 1.575) (xy 1.575 1.975) (xy 1.25 1.975)
				(xy 1.25 2.55) (xy -1.25 2.55) (xy -1.25 1.975) (xy -1.575 1.975) (xy -1.975 1.575) (xy -1.975 1.25)
				(xy -2.55 1.25) (xy -2.55 -1.25) (xy -1.975 -1.25) (xy -1.975 -1.575) (xy -1.575 -1.975) (xy -1.25 -1.975)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "cc81e44d-d3a7-4ee6-92c7-92dec5126d06")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -3.75 0)
			(layer "F.Fab")
			(uuid "4b6c5f7a-3f49-4524-b03d-48c8d02a98d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -3 -1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(uuid "1416bc48-f9be-4ae9-98b7-78f613480edc")
		)
		(pad "1" smd rect
			(at 3 -1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(uuid "0687ab18-67cb-4839-8f10-bc52868243f3")
		)
		(pad "2" smd rect
			(at -3 1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "USR_BUTTON")
			(pinfunction "2")
			(pintype "passive")
			(uuid "4c4c9960-3565-443f-8544-d6c63f3ec96e")
		)
		(pad "2" smd rect
			(at 3 1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "USR_BUTTON")
			(pinfunction "2")
			(pintype "passive")
			(uuid "ba65f55f-98a7-4bc4-b79b-8d0cab542c29")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_XKB_TS-1187A.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "8f6c6689-7e02-4732-95c7-0eabfd8dfa67")
		(at 103.47 117.89)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C40"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "f6dc9f13-2e88-41d8-9d88-7638e0746329")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "766b8af7-6dfe-43ff-9fd8-1315231e58c6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "531a16b8-4eea-4ad8-9ed7-139521ac2100")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6ddbc705-635b-4350-a169-e98249ed463c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/4e291f0a-24a9-4b0c-abec-2ec656891ecf")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "be674daf-402f-4c02-9db3-0e40df57a9a3")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c6a76066-5fac-4037-af09-99f4fe26836d")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f9ac7934-f67c-433a-84ef-0d9ef000fba8")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d28d9f7d-25ff-4d18-93f5-ffe3e152bdbc")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "023a00d5-dbda-4004-a6c4-a6599f17b2fc")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "24467d90-b6df-4232-ab31-459fa7f8fb7a")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c56b2681-862a-49d7-9c09-ca4d50e412e0")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c8c565d-95b5-4658-8f96-639f4ab64c33")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cd00b575-d49b-44db-9f63-efe92bdb2753")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc382afe-898f-4ef5-8b40-a8acb24f6f24")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "93f237cb-400a-40d2-bf90-572be8522777")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 15 "Net-(IC7-SS)")
			(pintype "passive")
			(uuid "a3c5bfd3-82de-4028-a115-d56bf367d515")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "0d2a9c3a-7b81-4567-ac35-b38401073fb9")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RF_Antenna:Texas_SWRA117D_2.4GHz_Right"
		(layer "F.Cu")
		(uuid "8fb126e8-64e8-43e7-a034-264d24ebaca0")
		(at 191.45 92.125)
		(descr "http://www.ti.com/lit/an/swra117d/swra117d.pdf")
		(tags "PCB antenna")
		(property "Reference" "AE3"
			(at 4.55 -6.41 0)
			(layer "F.SilkS")
			(uuid "1063d8ea-b359-4167-ad4d-ce5fe13843be")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Antenna_Shield"
			(at 4.55 1.21 0)
			(layer "F.Fab")
			(uuid "f2873e48-231f-4247-8c6d-28c453da489b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3f03f522-cfb0-4454-a598-ad5be6c06a8c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Antenna with extra pin for shielding"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0cddd11b-3515-4d15-9fbf-a991be646b3b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/acf37f56-fc09-4f1f-8e65-a7dfa1fbf430")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr exclude_from_pos_files)
		(net_tie_pad_groups "1,2")
		(fp_poly
			(pts
				(xy 2.45 -2.51) (xy 4.45 -2.51) (xy 4.45 -5.15) (xy 7.15 -5.15) (xy 7.15 -2.51) (xy 9.15 -2.51)
				(xy 9.15 -5.15) (xy 11.85 -5.15) (xy 11.85 -0.71) (xy 11.35 -0.71) (xy 11.35 -4.65) (xy 9.65 -4.65)
				(xy 9.65 -2.01) (xy 6.65 -2.01) (xy 6.65 -4.65) (xy 4.95 -4.65) (xy 4.95 -2.01) (xy 1.95 -2.01)
				(xy 1.95 -4.65) (xy 0.25 -4.65) (xy 0.25 0.25) (xy -0.25 0.25) (xy -0.25 -4.65) (xy -1.65 -4.65)
				(xy -1.65 0.25) (xy -2.55 0.25) (xy -2.55 0.006785) (xy -2.247583 0.006785) (xy -2.237742 0.054395)
				(xy -2.213674 0.096797) (xy -2.175731 0.129581) (xy -2.167819 0.133935) (xy -2.125156 0.146043)
				(xy -2.076637 0.1453) (xy -2.031122 0.1324) (xy -2.012511 0.121787) (xy -1.978868 0.086553) (xy -1.958309 0.041368)
				(xy -1.951778 -0.008158) (xy -1.960218 -0.056417) (xy -1.977112 -0.088643) (xy -2.012372 -0.121313)
				(xy -2.057682 -0.141408) (xy -2.107267 -0.147982) (xy -2.155353 -0.140092) (xy -2.188245 -0.123186)
				(xy -2.223185 -0.086416) (xy -2.242847 -0.041622) (xy -2.247583 0.006785) (xy -2.55 0.006785) (xy -2.55 -5.15)
				(xy 2.45 -5.15) (xy 2.45 -2.51)
			)
			(stroke
				(width 0)
				(type solid)
			)
			(fill yes)
			(layer "F.Cu")
			(uuid "a08c2eac-d119-46f2-801d-cadaa8a19031")
		)
		(fp_line
			(start -3.05 -5.45)
			(end 12.15 -5.45)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "28bdfefb-d858-4961-8d77-9e63bc07f0f9")
		)
		(fp_line
			(start -3.05 -5.45)
			(end 12.15 -0.25)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "2efa2e08-8f9f-4b12-a42f-011879d648b7")
		)
		(fp_line
			(start -3.05 -0.25)
			(end -3.05 -5.45)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "3b0807b7-d2a4-48bf-a80b-74726ced3cb2")
		)
		(fp_line
			(start -3.05 -0.25)
			(end 12.15 -5.45)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "f6af1a5e-1fe4-4580-9500-bceb64e23664")
		)
		(fp_line
			(start -3.05 -0.25)
			(end 12.15 -0.25)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "99091930-772c-43ce-a327-26586ccebe46")
		)
		(fp_line
			(start 12.15 -0.25)
			(end 12.15 -5.45)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "62999a6b-ede5-4464-b0ef-24537c3b5e91")
		)
		(fp_line
			(start -3.2 -5.6)
			(end 12.3 -5.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "94ac5427-0909-4216-92a3-0cdb41b75f46")
		)
		(fp_line
			(start -3.2 0.35)
			(end -3.2 -5.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "226ca794-fd7f-4021-8a8b-85943c1ba2dc")
		)
		(fp_line
			(start 12.3 -5.6)
			(end 12.3 0.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "713c25f2-a2a0-406e-a6c7-5b4f5ecb9a41")
		)
		(fp_line
			(start 12.3 0.35)
			(end -3.2 0.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "10670827-be06-4c61-b76c-1ad9a57ddb85")
		)
		(fp_line
			(start -3.2 -5.6)
			(end 12.3 -5.6)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d7ea68af-054c-4759-926a-642fe355bb98")
		)
		(fp_line
			(start -3.2 0.35)
			(end -3.2 -5.6)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d30cf383-1fec-45bd-a45c-bed536aa16d1")
		)
		(fp_line
			(start 12.3 -5.6)
			(end 12.3 0.35)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bdf1a7c6-4e6d-42a3-82e8-e26a2611844b")
		)
		(fp_line
			(start 12.3 0.35)
			(end -3.2 0.35)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e7aeabc3-c152-44af-98f6-0e6770b0c85b")
		)
		(fp_text user "${REFERENCE}"
			(at 4.55 -6.4 0)
			(layer "F.Fab")
			(uuid "65a46eb5-ee13-4a90-ab0f-6fb0d8773ba8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" connect rect
			(at 0 0)
			(size 0.5 0.5)
			(layers "F.Cu")
			(net 2 "Net-(AE3-A)")
			(pinfunction "A")
			(pintype "input")
			(uuid "decf9801-fff8-4ca3-938b-0094e592dca8")
		)
		(pad "2" thru_hole rect
			(at -2.1 0)
			(size 0.9 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Shield")
			(pintype "input")
			(zone_connect 2)
			(uuid "a52a7e26-b3bc-4655-b253-a096905a1593")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "9586a013-2c69-49c3-9a63-bc9f79530c6a")
		(at 127.25 99.8)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R29"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "fc51a7a0-f26c-4770-aad6-e77318e2aa30")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "a198feea-c82f-4f0a-af10-3adbe2678d20")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e09c0548-27bd-4208-beff-361a4521b1de")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "07f78e95-2eb1-4776-83ef-28bb73b71369")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/71bc0379-5e69-458d-967a-dba477305b50")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf005326-f1ac-419d-b299-fa4f117383fa")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "996dc3d8-50d3-4386-aae1-cab028d2c6cb")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "556ea797-ae2f-4a8e-8d15-928c5ff31d67")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "613e7b11-9bb3-4c12-8f61-3bb9703eec41")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "63eca0c8-1d5d-433f-b2af-46486bd6176a")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2f93a61b-09c0-4fed-96b2-255d6f7c4bb4")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fbe3b2a8-1e5d-4ce4-88da-a27c4348aea6")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a66c4a62-3465-45f9-b68e-c95d54bdb262")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb4efee3-4302-4117-bfef-a40d0340d5f6")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dd64b173-6f97-4561-a3fc-3e552d9598a1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c5789754-c99e-4ed1-9a67-6bdf501d4599")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 29 "Net-(IC4-OV1)")
			(pintype "passive")
			(uuid "e305acac-ca72-4617-930c-02b4a242cc8e")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "70350556-ae3f-4dce-b6e6-da7e52295907")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "969243ed-8c03-4c2f-8b87-ccb24e766747")
		(at 113 120.45)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "3154c0c2-2649-453e-93e8-9cb1613bbcfd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "2599df0b-9fe9-4c97-b6bb-158f3424ce94")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "926245b0-28a5-4d8a-8b0a-11c81f07a361")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f72ce40d-1349-4886-b693-d40753891b8f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1ded191a-4224-4a14-b3f0-f55062cc2bda")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd77b58c-5941-4d89-80b0-a2a4ae8a4108")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aa992476-67e4-4fa3-8a6c-2b12f8c78714")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9c576a7d-1fb6-4fa0-b123-ca6d697e6739")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "04d9a400-bf99-4119-8be8-4ad24529b40f")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c38bb10-bf60-4397-b041-ad2f7c61ec46")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "83c705e3-2f45-4198-beac-669f284f2096")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "257dcfc8-ce5e-4441-a68b-c775f9acf000")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "963b521a-321e-479f-9997-d5df160fd6ef")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6448effd-5110-4d16-9398-e019b5ff1fc1")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4c8ff3b-c783-466a-8a65-eec720550f1b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2b2cd040-9c06-43d3-90e5-ac057f09df71")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "5dafd549-e371-464f-906a-e3c9e133150d")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 62 "Net-(IC2-MPPT)")
			(pintype "passive")
			(uuid "5d3e9e7f-890c-4d1f-806e-d002291b0a17")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "9c22d567-c8ef-4c3d-8e25-33de462ca0d5")
		(at 50.35 113.6375 90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "inductor handsolder")
		(property "Reference" "L5"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(uuid "bf7b665d-c14a-49fe-a27b-6a557512ff70")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7uH"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "1273a131-f543-4bf3-8b50-114636c541d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "79fb9184-26bb-4a59-94b1-63ae0e619861")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "99927fa6-9a4a-4bef-b42f-acdcd7667e08")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/6a374a2d-4d1e-4970-bd77-c0c3a850d984")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.71)
			(end 0.261252 -0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a9145ebd-3ab3-4b9c-bd87-286544d12106")
		)
		(fp_line
			(start -0.261252 0.71)
			(end 0.261252 0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fbc8c06b-eb32-430b-b845-22d0175a67d2")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7fb02897-4d03-4ae9-a3a9-bf45958fd51f")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "db242041-541c-487c-9fe9-daf11c916cb6")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9e2387fb-e2a2-400a-81eb-0705e9fe8885")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "19a930a9-20e5-4d65-9d8a-b65d27226f0d")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b182a826-8058-49d5-9a8f-2b2a7180d9a4")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "572d35d9-c490-4f04-9f62-c94e41c6a20f")
		)
		(fp_line
			(start 1 0.6)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4159f99a-3c03-4cc4-8f5d-f233a9388e1c")
		)
		(fp_line
			(start -1 0.6)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "209e9afe-31bd-4093-96fb-f940d466e50b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "943fee2c-01b0-41d4-856e-0ae4be45b944")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0 90)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 3 "VDD_NRF")
			(pinfunction "1")
			(pintype "passive")
			(uuid "007fdb9a-2e50-4b70-847c-710392376591")
		)
		(pad "2" smd roundrect
			(at 1.025 0 90)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 33 "Net-(U2-L)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "2fc9ae51-9287-4ada-96b4-1260f84fff45")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "9e0f2fd3-b908-4a53-b90e-983804f6bb79")
		(at 193 122)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C27"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "76b36fdf-ce4f-4925-9038-18d9b307185c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4700pF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "cdf30b78-89c4-4141-ba91-a9cd9e238025")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "83daa936-190f-4453-9c5b-7bb8c652eb25")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "61c7848c-7341-43f6-884e-315c9eb7ce1d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/11f7620f-f2d0-48ca-b25e-5e3aa6e598b8")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac1c1dd8-0bfb-45b1-b8cc-b9acfe6e98bd")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "751c56a3-5722-4939-94b2-05fe80af7141")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c7fd353b-960a-48c4-a10f-6105a560fb5b")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "df928428-7bab-4170-8ce9-ae781daa5ce2")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50101e66-f5aa-4330-a338-3ea2bf576c9f")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "516a9aad-be1d-4ed6-b309-871666dad329")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab8d3832-9028-41cf-bebb-aa436ce87ea6")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aede6565-67ef-4981-92a4-1947ece4a90f")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1094d624-645e-44a7-915b-930db516006a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4011b6b4-326f-4719-acbb-de94b7494acb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0fa57627-006f-45e6-ab90-3a52b889e354")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 9 "+4V")
			(pintype "passive")
			(uuid "b40c73ea-0cd1-478f-b6e1-e9a99f78f9aa")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "0351d6df-8bc0-496b-82d6-a9e17a7dede3")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "a19dcd5b-640b-4fbd-ad39-8a337e0e1cec")
		(at 113 114.55)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "e9df7e11-76f1-452a-82f4-9a65f72aed17")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "4aca4c02-3090-4727-b930-dca01f74b832")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "758e50f5-245a-4053-a347-486c8740e59c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "22957a5f-625e-4229-84ad-4a73c57ac81a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/72dcaf5d-1e1b-4e8b-9e7a-ebbcad20dd87")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "03b65461-4727-4998-812d-c1b4b9222811")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5247db60-c76b-4e3f-9078-3ae7bca592fa")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9c998990-e1d6-41ff-94ee-d3b46f63e024")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7aafda0b-3600-4a11-bffe-652985170263")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "06a12bc6-023d-4f5f-8c52-70fb4b5af987")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3cd0a20b-54e3-433b-8d9d-90596149f358")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "debb9f2c-165b-4a33-a582-0904a72badc2")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6e403d3c-2f7b-4a83-9656-ce73611ab6f2")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3a0118f6-b784-4231-9b25-651d36bd7016")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0792acc2-25c9-4778-8082-3b4b79a67a33")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "89ad80a5-34d9-4d55-8e87-1595aab55bd8")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 27 "Net-(D3-A)")
			(pintype "passive")
			(uuid "2b22938e-348f-4849-a9d6-f71cbd7c241f")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 55 "Net-(IC2-VCC)")
			(pintype "passive")
			(uuid "3a00629c-bd8f-4050-a17b-489a8e4daadc")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "a95df513-27b5-4196-9e38-8b0870d8413a")
		(at 177.5 91.46)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "f22acb6b-ca4f-4143-932a-5dc1c94d53d0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "2f07bd64-20f0-47e7-a9f0-8b7cb83ada9f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b01a493e-81bb-4957-b013-868f2b30ccf1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "874a9d34-598d-4183-9fa4-d9ee15c58e96")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/b5865098-a11e-4708-8e9d-eb317f39a27b")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e98a9cc6-22cd-4f68-b524-e8cc245e3493")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "261f2508-169b-46e9-883d-8655798c7bf4")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bf41368b-9491-4a79-8d41-8de48ef2a35f")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ecbfd76a-734e-4f29-ae48-f9a0fd3ce879")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7a92c182-ca27-4d42-9a95-c0c58e3d19fb")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5eab0d97-cb6f-43b4-b061-66e3029f3723")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e67c6c5-c94d-4c5f-8d27-2dac46b8de13")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "64282b09-8835-43b5-99b4-69af2cc06638")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ee2f7d13-33a7-4e33-9cd8-0c1c3f79a9ef")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1f0f7952-42be-4cdb-a3e7-04d8d078be6e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5151c55d-cb95-410f-abaa-184dfe0085ee")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "9f989872-1f31-4da4-a483-91aea884579f")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "3233cd16-5165-4865-9c5b-e0745c1531d8")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(uuid "ab20f076-5b87-4ea7-81ff-dc033b539e9b")
		(at 144.95 104.45 90)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(uuid "c456829e-5ea6-4af8-addd-61e39fc5cdb5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(uuid "ce2dd1f6-7559-49af-a268-c378180f7765")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "62b70c65-b9e4-4c08-8864-f624ab1996e4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "56a3515f-ba11-4782-b1fe-79dc4af6a71f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/8e878ae7-d51a-44bf-8a99-b75c101c2f5c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_circle
			(center 0 0)
			(end 0 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "2ea6fbc1-bd44-4fe9-9693-ed9cc71c14e0")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "e8a30ece-7082-4a0f-b76d-8532a8fc2159")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
			(uuid "817a4b6d-666f-4bfc-a292-981b7f2d1392")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 34 "VBUS")
			(pinfunction "1")
			(pintype "passive")
			(uuid "20d9f7ea-acf6-4415-8031-01a15944df3e")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "ad261687-4f1d-4187-8255-d087714b09da")
		(at 47.43 118.4175 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C34"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "1723899c-ea10-4606-9ca3-8e15bc5b4f37")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "95f4ebac-6622-4192-a5dc-4e0ffab65d1a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8cf607e7-7c4f-4f3f-856a-47deb6c4e565")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2d473226-3e05-4b08-aca4-42bd58654901")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/45a12d5e-c3b2-4a0f-8c5c-df015225923d")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e629d4e2-1c2b-4849-8159-95232f6089fd")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4f7a1eb3-3cc9-4524-a45a-23ec88ca32b0")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c26b1cc1-dc49-442e-9317-5dc4658000ba")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "71499833-ff44-4088-a7f2-ab67e10c8e0c")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07b34176-ea7f-4b91-9587-eea72ed9e2b3")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4529c21b-2b1f-4ac4-bbf1-fab29bcfabeb")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d528af80-0608-4db4-a1e7-fde22479cb9b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4e92ee6-271a-4ea6-9231-1d1cae8372c4")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ae341c4-e93c-499c-b1ef-c730bea0ad7c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3398c356-2e3d-41fd-af29-b55656e7f9ca")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "06c57d62-7bb4-480c-815b-dc95af02459e")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "6b6fb865-d69e-4702-aa0d-8ddf16ecbc78")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "00c3975e-f9c3-4a3c-a59a-3ed27a459f18")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "ae907f5f-7396-4a5c-8465-0233bc9e3391")
		(at 185.4625 100.99)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R14"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "b76f2fa0-5324-4bb2-9124-37cb560f70a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "edd6646e-441f-4143-8f26-470bc7665981")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3364ca85-8702-4778-8f03-0ab8909ae153")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4a08454d-dd5f-40f7-8ab0-a72152d3c0c6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/577adf80-b429-4250-a9e3-dfe0ab9169cc")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3324caf2-398b-4256-a77c-6cdeaec33e47")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cef2e3cf-a071-4949-a92f-fde4a2811df5")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6805c2f-8156-4328-8bfe-4c8b53a4936b")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3ce4bb43-8a8b-433d-8bc3-9ef03eed03a8")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cdfee8fe-34cb-4a31-950a-2f4cffec38ab")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e889d1a0-558c-446d-9a71-ed7e657573e4")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2c8ffd6f-9017-4775-9847-e49afdc63802")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5fb5e5b5-b5b0-405f-a4bd-12e5e845e18d")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51453069-230e-4e33-9d29-1c6c6e0ae0fe")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a954479c-3611-479a-9f10-64267d303bfc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "814228e6-6705-4d3a-b5ab-d5e19e3407f1")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 24 "Net-(D2-A)")
			(pintype "passive")
			(uuid "0cede855-8a47-4db0-ae34-a5d626eb7d26")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 63 "Net-(IC5-P0.03)")
			(pintype "passive")
			(uuid "3c3ee566-323d-4c0f-8757-5bcbc028fb18")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "af57fcf5-ef02-421f-95cc-2d04f75958ec")
		(at 103.47 108.86)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C37"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "15abcd36-2065-45c0-b492-37301b943830")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "65a920b1-0ca4-4ecb-8fd1-df7cfbbc649d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f1ff1468-d372-4578-bc53-d22531fe27ba")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b248d7d2-6ab1-4216-bb54-7b49347dbd4c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a40fc250-6817-4fba-989f-dd5bdb7bd3d7")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "098af375-493a-4eec-bfa2-b17c96c6a92e")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "65c6eabc-4027-4e1a-a332-5c516d55e885")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fd79df66-21aa-42c7-b02a-c3b118421622")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f904c28-5552-492a-b9ee-68e19e3427ee")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8d660bb9-7ba3-42fa-bb3e-ba21fa5894c0")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12c55dfe-dbb4-45df-90eb-61c987b8233b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "92dc1ddf-e4a3-43df-b351-5292b28e9e15")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fbc20464-0cd9-48b9-8031-0e052e31c40b")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4860efd5-dd0a-4c89-aed8-771255ab1c75")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6eb5dc74-99da-4c92-878a-10694e58b697")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2d96858b-5223-477e-b95e-0439950eed3e")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 13 "Net-(IC4-SS)")
			(pintype "passive")
			(uuid "9d2bd512-df17-4c45-87f5-fba6cd094097")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "fe9edcaa-652b-4289-aade-33d945d8d731")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(uuid "af9a3483-c7b0-4286-87ba-468a605b3381")
		(at 82 111.3625 90)
		(descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at 0 -2.4 90)
			(layer "F.SilkS")
			(uuid "fe18fd0b-1cca-4ce1-a6dc-8282bc94e413")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TPS565208"
			(at 0 2.4 90)
			(layer "F.Fab")
			(uuid "75d55570-4da5-4e54-b20a-318eb6c62344")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps565208.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "76fd0039-791c-4931-ad9d-0a640da955a9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "5A Synchronous Step-Down Voltage Regulator, Adjustable Output Voltage, 4.5-17V Input Voltage, SOT-23-6"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fe64ac8d-253f-4406-a534-55c934435f70")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C2650336"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e9ce9193-6328-4541-b19b-6ed85d246eac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/eeb008f6-cb32-4f6e-80e9-84b8ed52bcf6")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end 0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f132080-ae05-4014-a315-03747d2b9e47")
		)
		(fp_line
			(start 0 -1.56)
			(end -0.8 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3e5eea84-690d-4255-b33d-e54f4cf4c4a1")
		)
		(fp_line
			(start 0 1.56)
			(end 0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "739142ec-953c-40e1-acd4-a425041b3a8f")
		)
		(fp_line
			(start 0 1.56)
			(end -0.8 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a9399b6-6e9f-4449-82f3-87f1dd7e8534")
		)
		(fp_poly
			(pts
				(xy -1.3 -1.51) (xy -1.54 -1.84) (xy -1.06 -1.84) (xy -1.3 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "56b50e10-3107-4ba9-ad49-f861c412da6e")
		)
		(fp_line
			(start 2.05 -1.7)
			(end -2.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3a4ebb2f-67c7-4280-9f92-ab28354537b6")
		)
		(fp_line
			(start -2.05 -1.7)
			(end -2.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f408bcd3-2e40-4d93-85b4-df3cb7898e3c")
		)
		(fp_line
			(start 2.05 1.7)
			(end 2.05 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "93c49055-7e72-4ccc-90b3-8238beddddad")
		)
		(fp_line
			(start -2.05 1.7)
			(end 2.05 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9b56ca2e-d6ba-465b-83ff-5c8e9753f917")
		)
		(fp_line
			(start 0.8 -1.45)
			(end 0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "acac1a8a-82c3-4dbf-b9a8-1dacc1972aa0")
		)
		(fp_line
			(start -0.4 -1.45)
			(end 0.8 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "62ae0085-46ef-48e1-b509-1effb72670e5")
		)
		(fp_line
			(start -0.8 -1.05)
			(end -0.4 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4145795a-2511-4e42-bc62-136abe756b57")
		)
		(fp_line
			(start 0.8 1.45)
			(end -0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2714ab5c-74fb-4bbc-ad78-b6bb40cfaf06")
		)
		(fp_line
			(start -0.8 1.45)
			(end -0.8 -1.05)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "92395e29-cac6-4fd4-91ec-e9958a3fa4f0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "b91bde7d-f5ba-4766-89fb-2c930a4800f3")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "25096cae-1926-4fda-aa64-91089bdcbb3b")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U1-SW)")
			(pinfunction "SW")
			(pintype "output")
			(uuid "f9bc7a30-f768-4b45-b1b1-43613f136688")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "Net-(U1-VIN)")
			(pinfunction "VIN")
			(pintype "power_in")
			(uuid "68608058-8360-4f86-93bf-1f8d4c152fc6")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "Net-(U1-VFB)")
			(pinfunction "VFB")
			(pintype "input")
			(uuid "75b46e46-0234-41f1-bc78-94854b883b0b")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "Net-(U1-EN)")
			(pinfunction "EN")
			(pintype "input")
			(uuid "6d20c996-e9cb-40ec-a2c2-fece5f60970b")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U1-VBST)")
			(pinfunction "VBST")
			(pintype "passive")
			(uuid "97626861-deb4-47ea-89f4-de908d5e7fca")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "b6fdda1e-e622-452c-99a0-5f848eec4c7e")
		(at 59.2 113.6375 90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "inductor handsolder")
		(property "Reference" "L9"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(uuid "49c01759-6137-4cf3-a08a-4aeb89db86fa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7uH"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "86750663-2fb0-42ae-8632-c9378dee9e7e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "03bcc9f4-9db5-48f1-addc-e3e69b62f267")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8b153fdf-47a7-4303-899b-48532a223624")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/d029387f-dccc-47a2-9396-d08ec1dc8924")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.71)
			(end 0.261252 -0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c880a530-29e2-48be-afb1-4e5eabf20e47")
		)
		(fp_line
			(start -0.261252 0.71)
			(end 0.261252 0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d9954672-b33b-46b9-ab3b-0b248ed65562")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f72d0291-222a-4c2b-9b3b-fb1f6d576732")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a4de9fef-dc5a-46eb-b0c0-1edbdf82b343")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dbeadc58-07f4-496b-8c3f-2cf428e7400f")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ce58513d-7c0a-4e74-aad4-26193583a6a2")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ab9b912-5bff-4361-80bd-9cb341e306fd")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c3b551c9-081a-4053-8919-e56177b0da4f")
		)
		(fp_line
			(start 1 0.6)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "40688cc2-e728-4bf4-8394-ed95dc9f1c44")
		)
		(fp_line
			(start -1 0.6)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ea96b859-f24d-4932-84af-d4057945a3fc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "624cd364-157a-44e7-8b62-cb8a04bfd240")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0 90)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 3 "VDD_NRF")
			(pinfunction "1")
			(pintype "passive")
			(uuid "4d61bff1-112c-494c-8d35-819f38cd6f54")
		)
		(pad "2" smd roundrect
			(at 1.025 0 90)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 53 "Net-(U3-L)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "98ba6168-2fc7-465d-8d33-0ded0c695ad9")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "b851f59e-e671-412f-9a04-e9e1aba51fd5")
		(at 190.2125 103.94)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R24"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "e60836ec-145e-4270-8a7e-596c81169da8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "6248de76-3416-4552-9685-cd16c9a5b614")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "94dda4c5-7415-4c5a-9041-ce426eef6c44")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8ab9ac66-f0cf-4500-8b51-396397781978")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/33a0d09e-9c82-4b62-a61b-c4004b740d49")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f82bfbb6-00d0-42b5-95d1-92187c8428b8")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac0d9d75-d969-4563-8f19-dbd0f7293c1e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6a7bab53-778e-46c4-ab63-98038950e3a1")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a0e382d7-8be2-41fc-bd56-2b8fe88acde6")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "de7676b8-c04f-4f0e-9e6c-108869b6674c")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "40afe0e8-1dbc-424a-ac98-d8c231522622")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5b36a1bd-e5e4-44ca-850f-e7a9369c2872")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1d2b0350-277e-4774-9279-2ebce2b25c18")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "02258cea-6b27-475c-bf09-4b38d9547985")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b7400f66-8d27-4eae-8c4f-12216e8c30f8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "adbb7a20-ed08-46a7-8d98-adbc381b2d7a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "b57fddaf-d69f-4960-b80a-4771332efc58")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "USR_BUTTON")
			(pintype "passive")
			(uuid "bf48bc71-df26-4c36-8699-17f5bb596381")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "b8d5291c-13ea-4099-9f9d-a1d46da38681")
		(at 47.4 108.8875 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(uuid "5d77ddff-8e9e-46eb-b19c-63618f5139cc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "7c810a97-f180-4e46-85ba-dc21a328dc4c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "be36a027-9d9f-48b3-a4f5-2fe0ab2078a8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7ab9bc5f-7ac0-4485-a832-0d630d936f1f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4d9d01dc-76fe-458e-90f2-e0d9973b73cf")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cac1f09b-baeb-4298-918c-67d1b2ce64a7")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "78f63fa8-c40e-4aab-a984-dd40548791e0")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc9a2cec-d50f-4de6-ae94-f9fe99412fea")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1d70ccb0-86bc-469d-aae7-2eb9900ea05e")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8d646a10-4ff8-4997-93c8-625271f2a45b")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f96a0219-24e3-41ea-857d-4a37e06ab9aa")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc1fc25a-cf32-4cf5-a0e3-2f5021dfee14")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "50b4a820-4bd4-4bc8-9ff5-20aebe0c4c43")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b0437a78-3cc5-44fd-96e5-88da20ad140d")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "42712ce0-b11f-42a8-b2f8-d095ee9664f5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "524ea902-2b1d-40ed-8399-7ee288de4926")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "90a3a49f-5870-46e5-83e6-7792020fa89f")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 58 "Net-(IC1-VBUS)")
			(pintype "passive")
			(uuid "20050e67-c692-4377-91b3-fc381be6885a")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic:WioWM1110"
		(layer "F.Cu")
		(uuid "bc852194-ea21-49c2-aed9-8f6844b32fb7")
		(at 168 117.5 -135)
		(descr "Wio-WM1110-1")
		(tags "Integrated Circuit")
		(property "Reference" "IC5"
			(at 0 0 45)
			(layer "F.SilkS")
			(uuid "caf654fe-fd2c-446c-a0f2-b42c04a21f4f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Wio-WM1110"
			(at 0 0 45)
			(layer "F.SilkS")
			(hide yes)
			(uuid "b956f41a-e773-4b2b-a2bc-95d3dd4ce39b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" "https://files.seeedstudio.com/products/SenseCAP/Wio-WM1110/Wio-WM1110_Module_Datasheet_V1.3.pdf"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "6f1e9748-adc9-4771-88f7-8a0a62a06672")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "LoRa Wireless Module - Powered by Semtech"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "b6e871db-6993-4294-a3eb-f48d35435205")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "2.3"
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d9399825-9552-4d5a-8088-425bb54725f4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "Seeed Studio"
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3d9620a4-3a3d-4a8c-95d7-8aff1d968b7f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "Wio-WM1110"
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9efa7240-8cac-40a1-8968-c9257db6f287")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7305d712-4004-41cd-9601-eb74f37f06ad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8571806e-7c1d-4708-b0d6-4b7cee2b2e50")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Part Number" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b6af8c23-c1e7-4842-90e9-372bb3005dd8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "98ab9940-5301-4683-8e42-4af13750deec")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/59f65753-6df6-4309-bfb5-4e74afe50ff5")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -10.5 -7.65)
			(end -10.5 -7.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f2a3bfde-2b3f-454d-83a6-f67ddea8a696")
		)
		(fp_line
			(start -10.6 -7.65)
			(end -10.6 -7.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "963dad85-3fe5-4c10-a8ed-405a90588a5e")
		)
		(fp_arc
			(start -10.5 -7.65)
			(mid -10.55 -7.599999)
			(end -10.6 -7.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ff8d895b-399d-43fa-a062-73cf4f7a8e95")
		)
		(fp_arc
			(start -10.6 -7.65)
			(mid -10.55 -7.7)
			(end -10.5 -7.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "babf7594-50d0-404b-8a72-11a1a02b7082")
		)
		(fp_line
			(start 11 11)
			(end -11 11)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9bc2299b-1d77-423e-b79c-1a6fce18c617")
		)
		(fp_line
			(start -11 11)
			(end -11 -11)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ce0c7059-acc1-489e-a409-1a941fc33af1")
		)
		(fp_line
			(start 11 -11)
			(end 11 11)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c90cf587-1f93-49ea-bc29-bd120daf727c")
		)
		(fp_line
			(start -11 -11)
			(end 11 -11)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3a525ad2-dfeb-4d80-b357-ff4ad4db3b69")
		)
		(fp_line
			(start 10 10)
			(end -10 10)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c9d58f5-55d8-4602-8c2a-d1087a0a96c8")
		)
		(fp_line
			(start -10 10)
			(end -10 -10)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "55dd6963-e5ad-4c31-ae18-d3adc07b1e01")
		)
		(fp_line
			(start 10 -10)
			(end 10 10)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6807aa1-c8c3-48a2-9623-5183e6a2a170")
		)
		(fp_line
			(start -10 -10)
			(end 10 -10)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e78b2666-089b-4f5e-8726-b645c956898a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "861e5c56-d362-4222-98f8-d6d9213d2d44")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -9.25 -7.65 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_1")
			(pintype "passive")
			(uuid "c51f611f-8802-445e-812a-2cc9b642e15f")
		)
		(pad "2" smd rect
			(at -9.25 -6.75 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_2")
			(pintype "passive")
			(uuid "c70b8e16-32aa-4429-8578-dd81a8361fd5")
		)
		(pad "3" smd rect
			(at -9.25 -5.85 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_3")
			(pintype "passive")
			(uuid "bd186b33-dae6-46a2-bfff-ff89b44c15fe")
		)
		(pad "4" smd rect
			(at -9.25 -4.95 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_4")
			(pintype "passive")
			(uuid "b3f3eff6-2360-4a82-9a84-f2d92bf84fdc")
		)
		(pad "5" smd rect
			(at -9.25 -4.05 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_5")
			(pintype "passive")
			(uuid "8b8a39be-aa44-4e1a-9c35-ff74b2483f49")
		)
		(pad "6" smd rect
			(at -9.25 -3.15 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_6")
			(pintype "passive")
			(uuid "b20b1f3a-b01f-4148-9731-80005f4cd9f9")
		)
		(pad "7" smd rect
			(at -9.25 -2.25 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_7")
			(pintype "passive")
			(uuid "dab00000-4b6c-470e-90f9-29a28cdc9bb0")
		)
		(pad "8" smd rect
			(at -9.25 -1.35 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_8")
			(pintype "passive")
			(uuid "4aae6da9-d83a-40b5-9890-21c37ab10fe5")
		)
		(pad "9" smd rect
			(at -9.25 -0.45 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 118 "unconnected-(IC5-P0.29-Pad9)")
			(pinfunction "P0.29")
			(pintype "passive+no_connect")
			(uuid "fe0e6d09-a220-4a09-9795-1908784ab73b")
		)
		(pad "10" smd rect
			(at -9.25 0.45 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 110 "unconnected-(IC5-P0.31-Pad10)")
			(pinfunction "P0.31")
			(pintype "passive+no_connect")
			(uuid "9902d8a6-c9bf-44dc-920e-36a7dba36b2e")
		)
		(pad "11" smd rect
			(at -9.25 1.35 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 108 "unconnected-(IC5-LR_DIO9-Pad11)")
			(pinfunction "LR_DIO9")
			(pintype "passive+no_connect")
			(uuid "8d6aa432-9061-4442-a081-5e9efc09519c")
		)
		(pad "12" smd rect
			(at -9.25 2.25 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 103 "unconnected-(IC5-P0.02-Pad12)")
			(pinfunction "P0.02")
			(pintype "passive+no_connect")
			(uuid "754068a6-0946-4e9e-bcaa-cb8941bbbf6f")
		)
		(pad "13" smd rect
			(at -9.25 3.15 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "Net-(IC5-P0.03)")
			(pinfunction "P0.03")
			(pintype "passive")
			(uuid "d1573d6b-d78a-421b-bd20-86bb9a4d7a34")
		)
		(pad "14" smd rect
			(at -9.25 4.05 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "unconnected-(IC5-P0.28-Pad14)")
			(pinfunction "P0.28")
			(pintype "passive+no_connect")
			(uuid "c3c51cc7-59f3-47fc-abab-cd8e7c30f544")
		)
		(pad "15" smd rect
			(at -9.25 4.95 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "unconnected-(IC5-P0.30-Pad15)")
			(pinfunction "P0.30")
			(pintype "passive+no_connect")
			(uuid "0c1e8609-1904-4af7-a385-0f7b0cfeb0d1")
		)
		(pad "16" smd rect
			(at -9.25 5.85 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "unconnected-(IC5-P0.27-Pad16)")
			(pinfunction "P0.27")
			(pintype "passive+no_connect")
			(uuid "4a80c12e-aa68-477f-bcb9-399aa59b70d7")
		)
		(pad "17" smd rect
			(at -9.25 6.75 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "unconnected-(IC5-P0.05-Pad17)")
			(pinfunction "P0.05")
			(pintype "passive+no_connect")
			(uuid "923547c6-edf5-4d71-984a-e2909392f921")
		)
		(pad "18" smd rect
			(at -9.25 7.65 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "unconnected-(IC5-P0.26-Pad18)")
			(pinfunction "P0.26")
			(pintype "passive+no_connect")
			(uuid "79a38bb7-1b1e-4525-b596-c4cce0042b15")
		)
		(pad "19" smd rect
			(at -7.65 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 117 "unconnected-(IC5-P0.07-Pad19)")
			(pinfunction "P0.07")
			(pintype "passive+no_connect")
			(uuid "f96aa818-f7b0-425a-92d3-7982633bc334")
		)
		(pad "20" smd rect
			(at -6.75 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "unconnected-(IC5-P1.08-Pad20)")
			(pinfunction "P1.08")
			(pintype "passive+no_connect")
			(uuid "52150786-b7cc-4d02-bdec-c4610f22c4e3")
		)
		(pad "21" smd rect
			(at -5.85 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "VDD_LR_1")
			(pintype "passive")
			(uuid "b101e96f-da8a-4512-80a5-ea70dfee362a")
		)
		(pad "22" smd rect
			(at -4.95 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "VDD_LR_2")
			(pintype "passive")
			(uuid "38aade9d-08b2-4584-a1a1-4655ed70e7d0")
		)
		(pad "23" smd rect
			(at -4.05 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 106 "unconnected-(IC5-LR_DIO8-Pad23)")
			(pinfunction "LR_DIO8")
			(pintype "passive+no_connect")
			(uuid "7b832ad3-4e8a-42ed-bb8c-dc11c384acf6")
		)
		(pad "24" smd rect
			(at -3.15 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "unconnected-(IC5-LR_DIO7-Pad24)")
			(pinfunction "LR_DIO7")
			(pintype "passive+no_connect")
			(uuid "17d2ac97-5e48-472e-823c-8d2a8b57643d")
		)
		(pad "25" smd rect
			(at -2.25 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "unconnected-(IC5-P0.11-Pad25)")
			(pinfunction "P0.11")
			(pintype "passive+no_connect")
			(uuid "10d4cc8b-0ca4-422d-89c1-fb52384b8200")
		)
		(pad "26" smd rect
			(at -1.35 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "unconnected-(IC5-P0.16-Pad26)")
			(pinfunction "P0.16")
			(pintype "passive+no_connect")
			(uuid "0cc84f70-9a31-4622-adea-1d78863454be")
		)
		(pad "27" smd rect
			(at -0.45 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "VDD_NRF_1")
			(pintype "passive")
			(uuid "5ca81d42-7916-4594-9598-25b662e88f23")
		)
		(pad "28" smd rect
			(at 0.45 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "VDD_NRF_2")
			(pintype "passive")
			(uuid "4ea2a9ac-1526-4a49-a369-6cb7f18b8ce6")
		)
		(pad "29" smd rect
			(at 1.35 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "unconnected-(IC5-P0.00-Pad29)")
			(pinfunction "P0.00")
			(pintype "passive+no_connect")
			(uuid "223803a5-0bec-4201-81d7-cda242039033")
		)
		(pad "30" smd rect
			(at 2.25 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "unconnected-(IC5-P0.01-Pad30)")
			(pinfunction "P0.01")
			(pintype "passive+no_connect")
			(uuid "62d6a7da-85ed-4b8a-aea0-7d411970b449")
		)
		(pad "31" smd rect
			(at 3.15 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "unconnected-(IC5-P0.04-Pad31)")
			(pinfunction "P0.04")
			(pintype "passive+no_connect")
			(uuid "4d1445c6-f1e1-4cbe-a817-62b871a8dfd3")
		)
		(pad "32" smd rect
			(at 4.05 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "unconnected-(IC5-P0.06-Pad32)")
			(pinfunction "P0.06")
			(pintype "passive+no_connect")
			(uuid "1ec29639-d8e7-4b7d-87be-b28e532df4ea")
		)
		(pad "33" smd rect
			(at 4.95 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "unconnected-(IC5-P0.08-Pad33)")
			(pinfunction "P0.08")
			(pintype "passive+no_connect")
			(uuid "4a0c8616-006b-4650-af8b-932768b9cfe1")
		)
		(pad "34" smd rect
			(at 5.85 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 90 "unconnected-(IC5-P1.09-Pad34)")
			(pinfunction "P1.09")
			(pintype "passive+no_connect")
			(uuid "256951e5-388f-49e4-8e73-e9d3ee1af3c8")
		)
		(pad "35" smd rect
			(at 6.75 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 115 "unconnected-(IC5-P0.12-Pad35)")
			(pinfunction "P0.12")
			(pintype "passive+no_connect")
			(uuid "c94352e7-12a7-421c-b103-f97fe1021bc9")
		)
		(pad "36" smd rect
			(at 7.65 9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 114 "unconnected-(IC5-P0.18-Pad36)")
			(pinfunction "P0.18")
			(pintype "passive+no_connect")
			(uuid "c86119b2-7614-4ff8-9a7e-2c47080aa213")
		)
		(pad "37" smd rect
			(at 9.25 7.65 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "+5V")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "4f4f537a-155d-47b1-91c6-cf6cb7620046")
		)
		(pad "38" smd rect
			(at 9.25 6.75 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "unconnected-(IC5-P0.14-Pad38)")
			(pinfunction "P0.14")
			(pintype "passive+no_connect")
			(uuid "6db15384-36bf-4942-bf69-93ea6b799c0f")
		)
		(pad "39" smd rect
			(at 9.25 5.85 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 99 "unconnected-(IC5-P0.13-Pad39)")
			(pinfunction "P0.13")
			(pintype "passive+no_connect")
			(uuid "679c3adb-3f25-4f59-ac9b-4e799c962856")
		)
		(pad "40" smd rect
			(at 9.25 4.95 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "D-")
			(pinfunction "DN")
			(pintype "passive")
			(uuid "74cbf7c3-9531-4b98-b6d1-b727350bcdc2")
		)
		(pad "41" smd rect
			(at 9.25 4.05 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "D+")
			(pinfunction "DP")
			(pintype "passive")
			(uuid "b1beab55-37fc-4710-9402-253605634c74")
		)
		(pad "42" smd rect
			(at 9.25 3.15 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "unconnected-(IC5-P0.15-Pad42)")
			(pinfunction "P0.15")
			(pintype "passive+no_connect")
			(uuid "454f1ce7-2c76-4e41-8c4b-1cab043108c0")
		)
		(pad "43" smd rect
			(at 9.25 2.25 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 91 "unconnected-(IC5-P0.17-Pad43)")
			(pinfunction "P0.17")
			(pintype "passive+no_connect")
			(uuid "3e9a2af7-7b73-4697-a449-c6d45c0044d5")
		)
		(pad "44" smd rect
			(at 9.25 1.35 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_9")
			(pintype "passive")
			(uuid "e29c6210-948a-4ce2-b24a-fb9d9ae1604a")
		)
		(pad "45" smd rect
			(at 9.25 0.45 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "GPS_RX")
			(pinfunction "P0.20")
			(pintype "passive")
			(uuid "f5df97ee-339d-464d-a1a4-bd445f26cf7b")
		)
		(pad "46" smd rect
			(at 9.25 -0.45 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "GPS_TX")
			(pinfunction "P0.22")
			(pintype "passive")
			(uuid "b07da5a4-ed58-4082-85e2-00559d3a6cd5")
		)
		(pad "47" smd rect
			(at 9.25 -1.35 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "GPS_EN")
			(pinfunction "P0.24")
			(pintype "passive")
			(uuid "28aba1f0-8bd4-4970-9a7d-1e1ed0bbb74d")
		)
		(pad "48" smd rect
			(at 9.25 -2.25 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "USR_BUTTON")
			(pinfunction "P1.00")
			(pintype "passive")
			(uuid "e9d8ca27-b9dd-4b87-89ea-44f8a7bce09e")
		)
		(pad "49" smd rect
			(at 9.25 -3.15 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 116 "unconnected-(IC5-P0.21-Pad49)")
			(pinfunction "P0.21")
			(pintype "passive+no_connect")
			(uuid "ee60db10-cbbe-4a43-87cc-5c0c26050ca7")
		)
		(pad "50" smd rect
			(at 9.25 -4.05 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "SWDIO")
			(pinfunction "SWDIO")
			(pintype "passive")
			(uuid "87a3cb95-599c-4b84-a2a2-8f3e014a51a2")
		)
		(pad "51" smd rect
			(at 9.25 -4.95 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "SWDCLK")
			(pinfunction "SWDCLK")
			(pintype "passive")
			(uuid "7f6961d1-1224-4bd0-aee4-66b6114ee3c8")
		)
		(pad "52" smd rect
			(at 9.25 -5.85 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 111 "unconnected-(IC5-P0.25-Pad52)")
			(pinfunction "P0.25")
			(pintype "passive+no_connect")
			(uuid "b0bf2ebd-86fb-4318-8c27-6d70a72cda0d")
		)
		(pad "53" smd rect
			(at 9.25 -6.75 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "unconnected-(IC5-P0.23-Pad53)")
			(pinfunction "P0.23")
			(pintype "passive+no_connect")
			(uuid "7abb1373-84df-4d1e-9432-1c933992644f")
		)
		(pad "54" smd rect
			(at 9.25 -7.65 315)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "RADIO TX{slash}RX")
			(pinfunction "P1.01")
			(pintype "passive")
			(uuid "bf1784de-a226-4dff-a5fb-499b207dc5ea")
		)
		(pad "55" smd rect
			(at 7.65 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "unconnected-(IC5-P1.02-Pad55)")
			(pinfunction "P1.02")
			(pintype "passive+no_connect")
			(uuid "7010b8f4-ee12-4c0e-9d0e-57ac15f73409")
		)
		(pad "56" smd rect
			(at 6.75 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "unconnected-(IC5-P1.03-Pad56)")
			(pinfunction "P1.03")
			(pintype "passive+no_connect")
			(uuid "4babcd29-2007-4b41-9836-f3a7c29720b7")
		)
		(pad "57" smd rect
			(at 5.85 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "I2C SCL")
			(pinfunction "P1.05")
			(pintype "passive")
			(uuid "7d4534ce-6a97-461b-a87c-6989813abee5")
		)
		(pad "58" smd rect
			(at 4.95 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "I2C SDA")
			(pinfunction "P1.04")
			(pintype "passive")
			(uuid "9dd7ae9d-586d-49cc-b876-6a3ed7d51995")
		)
		(pad "59" smd rect
			(at 4.05 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "unconnected-(IC5-P0.09-Pad59)")
			(pinfunction "P0.09")
			(pintype "passive+no_connect")
			(uuid "1a5f2d1b-e9a3-46c9-9908-c95337feafb6")
		)
		(pad "60" smd rect
			(at 3.15 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 107 "unconnected-(IC5-P0.10-Pad60)")
			(pinfunction "P0.10")
			(pintype "passive+no_connect")
			(uuid "8151d4bb-9b0b-407b-95c4-722faa677c92")
		)
		(pad "61" smd rect
			(at 2.25 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 112 "unconnected-(IC5-P0.19-Pad61)")
			(pinfunction "P0.19")
			(pintype "passive+no_connect")
			(uuid "ba0ec350-c3ad-42ab-bbbc-2cb89ec99f22")
		)
		(pad "62" smd rect
			(at 1.35 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_10")
			(pintype "passive")
			(uuid "bf91786a-8944-4d73-8beb-9bf20d6b69d0")
		)
		(pad "63" smd rect
			(at 0.45 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "RF_WIFI_BT")
			(pinfunction "ANT_NRF")
			(pintype "passive")
			(uuid "ac83d642-6f85-4abd-914c-efbddb7b8573")
		)
		(pad "64" smd rect
			(at -0.45 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_11")
			(pintype "passive")
			(uuid "96444730-e8fc-409b-aa36-c7577f2642bf")
		)
		(pad "65" smd rect
			(at -1.35 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "unconnected-(IC5-ANT_WIFI-Pad65)")
			(pinfunction "ANT_WIFI")
			(pintype "passive+no_connect")
			(uuid "1c874e0d-4a31-4772-bfb4-a003adf4deb2")
		)
		(pad "66" smd rect
			(at -2.25 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_12")
			(pintype "passive")
			(uuid "98c5522a-229c-428d-8b9f-2a145b1a65ab")
		)
		(pad "67" smd rect
			(at -3.15 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "unconnected-(IC5-ANT_GNSS-Pad67)")
			(pinfunction "ANT_GNSS")
			(pintype "passive+no_connect")
			(uuid "6fa7a332-522f-4030-9af4-11b33f646dc9")
		)
		(pad "68" smd rect
			(at -4.05 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_13")
			(pintype "passive")
			(uuid "a6619be7-c7e4-4d57-b73a-8fe394bf23ff")
		)
		(pad "69" smd rect
			(at -4.95 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_14")
			(pintype "passive")
			(uuid "c68bde7d-2c57-4849-aa33-414301e89313")
		)
		(pad "70" smd rect
			(at -5.85 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_15")
			(pintype "passive")
			(uuid "4bc75a54-a445-4cd0-bfd9-f33f9aa97e69")
		)
		(pad "71" smd rect
			(at -6.75 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_16")
			(pintype "passive")
			(uuid "aad444e8-a35d-4857-960c-caaf7d73ea56")
		)
		(pad "72" smd rect
			(at -7.65 -9.25 225)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "RF_LORA")
			(pinfunction "ANT_LORA")
			(pintype "passive")
			(uuid "64465169-8bbb-4202-9fc8-07d3d9905b3c")
		)
		(pad "73" smd rect
			(at -9.25 -9.25 315)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_17")
			(pintype "passive")
			(uuid "4cf0074d-98d1-4db4-b764-cdf490dca207")
		)
		(pad "74" smd rect
			(at -9.25 9.25 315)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_18")
			(pintype "passive")
			(uuid "2fb39f51-e3a6-4f82-8793-b0623e64ff78")
		)
		(pad "75" smd rect
			(at 9.25 9.25 315)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_19")
			(pintype "passive")
			(uuid "6279544f-c5d5-42cd-90f5-154e0ffd09c5")
		)
		(pad "76" smd rect
			(at 9.25 -9.25 315)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_20")
			(pintype "passive")
			(uuid "790f242e-8d50-46ff-86b1-78140348760d")
		)
		(pad "77" smd rect
			(at -4.235 -6.94 315)
			(size 2.3 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_21")
			(pintype "passive")
			(uuid "dab47eb1-6785-4abc-b3b0-d89863a2037a")
		)
		(pad "78" smd rect
			(at -4.235 1.95 315)
			(size 2.3 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_22")
			(pintype "passive")
			(uuid "6a4cf9a0-1804-41eb-be76-40a639dbe635")
		)
		(pad "79" smd rect
			(at 4.235 1.95 315)
			(size 2.3 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_23")
			(pintype "passive")
			(uuid "9502492a-aecb-4a08-affc-d1a601c4fd0a")
		)
		(pad "80" smd rect
			(at 4.235 -6.94 315)
			(size 2.3 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_24")
			(pintype "passive")
			(uuid "89d1d0f6-9f38-46ab-b4f6-a14929b3f9ed")
		)
		(embedded_fonts no)
		(model "Wio-WM1110.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_C_Receptacle_G-Switch_GT-USB-7010ASV"
		(layer "F.Cu")
		(uuid "bde9163f-6e91-465f-a0da-8620191628e8")
		(at 139.75 144.725)
		(descr "USB Type C, right-angle, SMT, https://datasheet.lcsc.com/lcsc/2204071530_G-Switch-GT-USB-7010ASV_C2988369.pdf")
		(tags "USB C Type-C Receptacle SMD")
		(property "Reference" "J1"
			(at 0 -5.5 0)
			(layer "F.SilkS")
			(uuid "8bbd701d-c20c-41bd-8117-22d1a595f94f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "USB_C_Receptacle_USB2.0"
			(at 0 5 0)
			(layer "F.Fab")
			(uuid "ad73d41f-facc-40c0-8762-29b597c5dde9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d4c1e9f4-5220-4d98-a7c0-280c19f6f3e7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2ab91758-984b-4457-bafa-c4631ecf786a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(path "/853cd093-ee5d-412d-acaf-339a7c25043c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.58 -1.85)
			(end -4.58 0.07)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2979d594-85b3-41e5-b5fc-148fb561afff")
		)
		(fp_line
			(start -4.58 3.785)
			(end -4.58 2.08)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b80ccf22-49f8-448d-9de1-a2dd7d627e0c")
		)
		(fp_line
			(start 4.58 0.07)
			(end 4.58 -1.85)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ecb4c1ca-e9a0-4752-b866-330a2ee0f264")
		)
		(fp_line
			(start 4.58 2.08)
			(end 4.58 3.785)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22d9e2db-27f3-4557-9cbc-79eb499aa91f")
		)
		(fp_line
			(start 4.58 3.785)
			(end -4.58 3.785)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f8f385c4-eed2-4763-b208-0b69c89bcb3a")
		)
		(fp_line
			(start -5.32 -4.85)
			(end 5.32 -4.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "373f450f-d026-4436-b135-1ce5893c3234")
		)
		(fp_line
			(start -5.32 4.18)
			(end -5.32 -4.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c4c3eea5-1fcc-4476-aa63-ab3ad68ecd41")
		)
		(fp_line
			(start 5.32 -4.85)
			(end 5.32 4.18)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "51df08dd-cae5-4469-acb3-7c223f2fa0cb")
		)
		(fp_line
			(start 5.32 4.18)
			(end -5.32 4.18)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d9757ddd-20ae-478f-b1d9-bc21cc362616")
		)
		(fp_line
			(start -4.47 -3.675)
			(end -4.47 3.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cd96950d-150d-43e7-b757-283af5587bf7")
		)
		(fp_line
			(start -4.47 -3.675)
			(end 4.47 -3.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7e773700-178a-4446-88a4-e8c8ae44b5aa")
		)
		(fp_line
			(start -4.47 3.675)
			(end 4.47 3.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b42f50ee-1837-4dcb-b7f9-e3f1687b576f")
		)
		(fp_line
			(start 4.47 3.675)
			(end 4.47 -3.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c3865e5b-fd5a-4f3b-92d1-0da4a03bf0fc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "cfba840a-ad4d-4f7c-bbe2-c1b084a126c7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -2.89 -2.605)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(uuid "4f2d51b4-be6a-4cc6-9d17-feb9a5d25b39")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -2.605)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(uuid "43786c0d-c32a-4097-b01c-46ae4caa36d9")
		)
		(pad "A1" smd rect
			(at -3.2 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "a9857e17-d266-4fea-b059-55acf10c3202")
		)
		(pad "A4" smd rect
			(at -2.4 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "63be8e29-08c0-4430-9004-bee27f30e0b3")
		)
		(pad "A5" smd rect
			(at -1.25 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "CC1")
			(pinfunction "CC1")
			(pintype "bidirectional")
			(uuid "26fc30d4-feea-4cb1-9615-b1e033b1300b")
		)
		(pad "A6" smd rect
			(at -0.25 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 119 "Net-(J1-D+-PadA6)")
			(pinfunction "D+")
			(pintype "bidirectional")
			(uuid "15d7558d-dc92-4609-93b9-7089873a564b")
		)
		(pad "A7" smd rect
			(at 0.25 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 120 "Net-(J1-D--PadA7)")
			(pinfunction "D-")
			(pintype "bidirectional")
			(uuid "d4acb950-b49a-4fcb-89e4-fa197499942b")
		)
		(pad "A8" smd rect
			(at 1.25 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "unconnected-(J1-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
			(uuid "07093f92-7569-4825-8dfe-286d8216df90")
		)
		(pad "A9" smd rect
			(at 2.4 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "642ea092-5527-4778-84d8-0639d21d18c0")
		)
		(pad "A12" smd rect
			(at 3.2 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "bd04ade7-8865-41b4-bdb7-976b790e5996")
		)
		(pad "B1" smd rect
			(at 3.2 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "d8da3db0-dcb8-4c23-ad30-d58372496c23")
		)
		(pad "B4" smd rect
			(at 2.4 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "f0963a34-c6b3-4429-8ff4-475bc9678776")
		)
		(pad "B5" smd rect
			(at 1.75 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "CC2")
			(pinfunction "CC2")
			(pintype "bidirectional")
			(uuid "480bd928-51b8-4e3a-9474-42aeb0e75823")
		)
		(pad "B6" smd rect
			(at 0.75 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 119 "Net-(J1-D+-PadA6)")
			(pinfunction "D+")
			(pintype "bidirectional")
			(uuid "030b64bb-cd8e-4e2d-9b31-b974e5d97bb1")
		)
		(pad "B7" smd rect
			(at -0.75 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 120 "Net-(J1-D--PadA7)")
			(pinfunction "D-")
			(pintype "bidirectional")
			(uuid "7eb83fc0-f6e9-4b21-a066-33f9b0e32435")
		)
		(pad "B8" smd rect
			(at -1.75 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "unconnected-(J1-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
			(uuid "4a789334-e538-40a6-9d24-1005bc703373")
		)
		(pad "B9" smd rect
			(at -2.4 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "22f29a87-1108-4c48-aa18-9acb1e35deb1")
		)
		(pad "B12" smd rect
			(at -3.2 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "dc1bb228-36c6-4b74-ba9e-8b0867bd2f80")
		)
		(pad "S1" thru_hole oval
			(at -4.32 -3.125)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "be985af3-9508-43ed-906d-e87d17f83553")
		)
		(pad "S1" thru_hole oval
			(at -4.32 1.075)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "f2c05585-e918-437a-901f-51b7273d8868")
		)
		(pad "S1" thru_hole oval
			(at 4.32 -3.125)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "2e325794-6a81-4fca-904c-36a3b1834bf7")
		)
		(pad "S1" thru_hole oval
			(at 4.32 1.075)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "77b0c35a-3285-4431-a042-bc959fb8f409")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_G-Switch_GT-USB-7010ASV.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "c13ea29e-b177-4c7e-9c21-e35eb9e1e87a")
		(at 68.5 128.0375 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C19"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "1889add8-b5d3-4abd-8666-71020028f449")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "46a27c42-db42-480d-b59f-3a07519371f1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ec9903db-feaf-46a0-b41b-fac5f291618a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "184b4670-bfbe-433d-8cf3-d0ef9a04e164")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/7b6c0af1-17dc-471c-9e5e-a88867fa8c1e")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "18a78634-9127-431b-a509-a8147382833b")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7883e9dc-64be-4248-901b-bbf8da64fb52")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "694112b0-c503-4341-b47b-71200c5a7278")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4e39e368-684a-470e-b3cc-c753028f0f90")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "480dbee3-194b-431d-a9c1-1120bfcd5741")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "17ed6a2c-300b-496a-8472-66f1dffee1ce")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a3df2ae-0665-4d8c-90f9-cc5b031ba9d6")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9333f036-dd0b-4a78-8652-26518c22c9b7")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fe354dcf-b1a1-4634-91db-85b21545ce9e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ead8d689-dd69-4595-8aca-955eab5f7ea4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "5eef83c3-516b-41f5-9824-4c7960be2168")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 14 "+5V")
			(pintype "passive")
			(uuid "a60d7338-47a7-48f6-9e73-ceb39c57faca")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "4cb87839-f737-4a0e-9ca7-1a76bb9c84ad")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "c1b281e0-2c37-424a-9944-5ede500dff78")
		(at 197.6275 110.83)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "inductor handsolder")
		(property "Reference" "L6"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "c89a4b06-c562-4263-aa50-5ba2bd1ceb50")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "3.9nH"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "94f16ed3-46de-4523-9093-337e371bcc13")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "219c7a87-bf19-4ff7-8371-54cdcacc1c28")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "876acf89-d181-4492-8f5a-c5e43ac5fef1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/6cfd3b13-916d-4154-b740-1be7e55c640d")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.71)
			(end 0.261252 -0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e0e817b4-e21f-433f-b089-890408eb2a23")
		)
		(fp_line
			(start -0.261252 0.71)
			(end 0.261252 0.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "666c183a-df3e-4a4c-b7a7-1136315b6dfc")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7b272428-fb79-441a-a2b0-d08014d5b859")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "37a9aae7-493d-4273-a88e-b5997180016a")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "281759db-2733-4c1b-aaef-c0dd1b36d3f2")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7a399797-a031-4563-a675-849583b16d28")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d571b7be-9252-4ed1-9345-24d95108e92f")
		)
		(fp_line
			(start -1 0.6)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "28b045fe-5f5b-41fa-b6f6-a4e3179ccfbc")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "423413a3-dbcf-483b-9faf-34452f5238e5")
		)
		(fp_line
			(start 1 0.6)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "39d03087-74f2-4456-910b-cffa765a65fd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c09273d1-7657-4d78-ac4a-7726b4c9407d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 52 "RF_WIFI_BT")
			(pinfunction "1")
			(pintype "passive")
			(uuid "1758ea1e-e9d0-41a0-a1ab-c982fe64cc9e")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 10 "Net-(C31-Pad1)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "5c181442-f298-4161-ad68-0094b012f679")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "c6fcf7fb-9bda-475c-8839-4c0a633b24ad")
		(at 171.0375 90.57)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "57d2ad80-9c0b-460a-b22d-a2ac714f1461")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "dc654f8f-e399-4dd2-8b38-c493980e3c10")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "de44cbf1-c84b-4254-8ddc-687f5382292e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0197ee3c-00d8-4113-aa68-d96458561ce4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/965795cb-9784-4a8d-9ea2-e2e6ba1e88d3")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "31583bf4-05c0-46fa-97ff-b26b92a75e48")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cf5da59d-a526-4d55-94ff-315c6bcb40ed")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b2cbad21-164d-4e55-bce9-1c5f13fbef05")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "083f22c2-0cdc-49f3-8c86-034dadab2a2c")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fb4cc7f0-9cea-42b1-a94f-5ea4f58bf10c")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "05b5b7b4-31dd-4ba8-aece-dc764994b7ff")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a8c4c22c-bec4-4604-a4b2-66f1ad30c1d5")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ab9d828-dcab-447e-9b66-71d5a7fc2fcf")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "07dd266b-badb-4087-9016-99dcde0e3093")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "294e87cd-f813-4f76-ab27-18064e744101")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b1747ec4-40fc-49d0-a4ea-1b93ec059556")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "ee4f1f19-2b71-4a7f-9e1d-0b62d31c3d13")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "987ece0a-84b9-4482-beb1-5e41578f7527")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "c738c225-a4b3-4411-bcdd-dccef08b3e43")
		(at 47.43 128.0375 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "c75032b9-4dad-4283-9e0c-997c0d4fb250")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "2a50567f-f78e-4ff6-b81c-3cebff365062")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b8a70ff8-6a89-414d-a9c7-7466ba164702")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1a820a2f-a74f-4b4e-8225-f55806634032")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/23dcf4dd-d4ca-4f8a-a243-8a31a23acd6e")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0f2740a0-a4fa-4e73-889f-e330128abfc2")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7851754d-f7b0-4e75-9d47-58d295349a56")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "37482d4e-d76d-40f8-a96b-9e2cfa2db778")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3cee6d76-83af-4906-a09b-e17a22a37c2d")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9611a761-75ba-4d9f-8fb1-cfd9afb83ac0")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dbc8f016-e19b-4a9e-b605-a64db86edfb0")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "23fd6c7c-24a7-4b5c-8a83-ab6fb306c569")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "db0f77ff-3bc4-42c5-906d-a83ad9ff9a3f")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0d67e323-3e71-4482-aadb-6eca9bd230d1")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2707a4c4-6ce4-4988-b5bd-c1dcd23d478e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "529e383f-b536-492c-95bb-f251d7a00248")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 77 "Net-(U1-VIN)")
			(pintype "passive")
			(uuid "0958de80-1957-409a-b6a4-a2f3c4abd371")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "9b580830-6eef-476d-93c4-34633ac06743")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "c8af4613-c737-40bf-b32e-8afdf6c3e445")
		(at 185.4625 103.94)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R16"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "1fb2506d-8009-4205-a327-e7655a1ab64f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "5f474e9f-53d0-4085-aed0-a3c213e951b3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d9267a37-48cf-4eef-bb0d-4aecd21e7351")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0e60b757-dc51-44fb-b904-3a2bab214ad5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/154c0391-b6ce-4973-9abc-0a85f91031d0")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91a0c545-ddd4-4996-a663-b52bb06636e4")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2297b18b-b248-488e-9d77-9c166a315bac")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e036df0-5383-4c8f-b6fa-424663430738")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e613b077-c1f2-4124-8fbc-e4f6dc27ea2e")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a0b1d692-f85e-499a-ada1-6d245b0bfe9f")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "60daf839-bb08-4c89-828e-14df5b468b14")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1107abf8-c6d3-44e2-8ee2-c8ea2f960d30")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f540a384-86b4-46a7-885a-4e6cf5d9754b")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2966e289-377c-4a48-97e6-1bbde85a12de")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "25a37c20-6daa-4e8e-a075-e86056747008")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "df52fc01-f6ab-4f73-808c-163ab182cbd3")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 64 "I2C SDA")
			(pintype "passive")
			(uuid "4dff7a5b-e305-4f60-8e3a-23c542e4c861")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "c88e8658-a258-4f7d-8603-3f85f5bb06a6")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "cbf9616e-1210-4223-becd-e6f61f54382e")
		(at 127.25 117.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R38"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "acd68bfc-7888-4549-a9dc-f6148c613525")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "237e2d6d-6007-41ec-8c31-395d4678d5c2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6caddaaa-f7e9-4a42-a1a6-c0f4e5418bd2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "65e22087-aa92-4a01-b370-9c3bffbf6ca7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/0499b774-d170-4317-8a35-62c4212ef7ba")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8c459b66-0ae4-402c-99c7-8e6f6441534d")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cccd7400-9503-438a-ac8f-3a0a62b43728")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6bdc8f2a-2070-4f6f-9590-97326a323949")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "62e7ebd0-3cc0-40b7-a5c4-be8bbde1dc47")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4c93f29d-0016-4948-bed4-a46ff41c5a83")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8e2c7ad4-df7d-44cf-bb6f-43b0a343fb02")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7073c215-91af-412a-ac7c-9ee6a40ef0e1")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7546e4ca-66a7-4e7a-95b6-f7b5bdedca63")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa1d6ee2-7a1e-48a4-92bf-900958485eb9")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c7c701b-201d-4382-802d-4dc74e50f023")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2d493928-02c8-45cf-85ef-4328e8712d0c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 5 "Sys Load")
			(pintype "passive")
			(uuid "9ac52aa5-4666-4e54-b244-74e1769232c1")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 5 "Sys Load")
			(pintype "passive")
			(uuid "04b474ac-8613-4e1d-b47c-599ab71673a5")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "ce117634-ce1b-4c5c-96ec-22157288e1f0")
		(at 65.49 128.0375 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C18"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "fb59c1ef-25fa-4ec2-89b3-02b42cef47c9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "4e7f4503-7780-442f-8d9f-c91d9b418a01")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b7050323-fea0-449d-b319-17fd906ec5bd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "875a800c-1c7a-4073-8d35-5c72fa090b3f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a93ded5b-6273-4ee1-8bd1-5085b3c0a712")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c3ebc507-dfa5-4734-b0b8-f86ea399bdfe")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a5a241b4-0558-4dcc-91cb-53449ecbf586")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d4bb0909-a17a-40b5-ad08-ef18d7180ff3")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "45783706-8ea8-4738-abd5-44231fa06be0")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6af1b456-4c1d-4f0f-8b6d-3677174966a6")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "23b500cd-7391-4b63-a208-143f747e99df")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "91b83c59-390e-4b3e-a4e9-652dbf0c687b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "41832d81-54f8-4e26-8375-e2bba62222ba")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "35de0306-ba0e-4927-8582-13a1bc0b824f")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e6dc8ec6-a6a4-4dfe-99dc-114f82f35f1d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "7478b10a-cb21-4fd3-8c62-e40a003e9a1a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "11476be4-6b90-40e3-9996-28b1acbf639d")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "7847dedb-45db-41eb-9134-1c6feb47c90e")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "cecad789-a76d-46af-8263-1ac7eaa09657")
		(at 62.48 118.4175 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C39"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "f986afd1-36b6-48da-bfdb-456c2ffdf0bd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "ce5d5995-f5b9-406e-92a7-660e7cec934e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b0a812c4-8cc0-40c4-ad12-9c70f7b51c3b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4d6522c7-41e1-4aaf-b2aa-566401d8b7b7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a9b40957-bb73-46ad-8d77-e7851f163459")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aaf39ff0-e03a-48e9-bfc3-f851f8ffe3c7")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c44f11da-7260-44ec-a726-b6399cddcb34")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b8afe449-36a5-4e9c-ab7e-b3b537570aa6")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "335d5b44-5323-4a0c-9ce8-95d9475cffa1")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "14c949c0-a2d2-4530-a2ca-980c40fef0ab")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50afb692-c7dc-4471-9ef1-00d3774ef3f6")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b6bd964b-271e-49c0-a192-67844abc5f8c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3a3c3f63-5936-4294-832c-261541e3a75d")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f7ef6eb5-066b-4d5c-9408-3e7d831f47e6")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9d599b1d-f58c-4f93-b60c-2a7ef1cfd3d7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "682b8958-6cf1-49a7-8c2e-f1253011effc")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 14 "+5V")
			(pintype "passive")
			(uuid "1a52e513-1af5-4a4c-9128-36175ad54d70")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "af35366d-27be-4ba3-ba11-c1c355ea7b77")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "cf423af5-e52c-480a-a481-d6d6a90e8638")
		(at 188.0375 123.02)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C29"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "c72cf4d1-c55e-4f6d-b016-7ce868853290")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470pF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "7ee6a161-d8a0-40e8-9267-53465d12049a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a6a0c98f-8f8e-4b0e-bee4-fc0375dd8934")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d7c253c9-e55c-4631-8bc3-cec5bb51e815")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/e6238dc2-1497-4aa0-b345-6fd9f1f027b3")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3c5b936b-0b8d-4b0e-a33e-87400be52692")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dee32b58-ed06-4f0c-965f-ae798fa68736")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fc08e9a2-d64a-4f55-8ee8-a6eeca35dc9e")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "79de36d7-3aff-49d8-9b8b-8b8a4973ee8d")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2ccf2dde-1190-490d-aff8-37c5f6eb6cda")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0077f9dd-0077-4ef2-8f9f-154b9ac12bcb")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "56d6063d-ee91-4653-bce3-05f46312f22e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c161a498-af59-447f-ac8b-7f3c1ce9e169")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "99066928-27a0-4a77-8acb-48083db1bb51")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "72157a1f-a52b-4dd2-8697-ba1792e17b21")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6eaa0968-5050-4cac-acff-04bab9190c29")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "6fee300a-322b-4dd6-aa36-06faef1d5091")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "92de7b17-b853-4918-bc17-842e98b36e6f")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "d01861e2-f32e-4a47-987e-0667c43bf9e3")
		(at 201.5 122)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R19"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "e2ddf251-9fd3-4870-98d4-330f1b8619b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "ac234717-78b5-443f-8878-18b5e6410a4b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4c7abbd6-839e-4812-849f-783038957b57")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ecbbf3b6-2832-4f35-a0dc-bb24425c4e55")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/0a7f186c-c5d1-43dc-8b61-ead9cb92ffad")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f62337cb-d1e8-40d2-8625-a4a7b0262ca8")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "44c73b53-53f1-4bc6-aca1-769796d5e290")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f389802f-070f-4b44-978f-5ef3821c86ab")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "776ddae6-e530-49db-9370-aef107d9c67b")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b03d9318-22ff-4169-81be-0e032558b4ca")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d8e39e0e-68f0-4885-8d3a-314604531cde")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b80516c-eba1-465d-a351-caa9051e7e1a")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6df0576-4a3b-40b1-8d53-52286d84d9f2")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "303f6a33-3565-471d-a642-4f0add9de7f2")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7afda6ac-657e-49b7-a0e8-a03837f21219")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "da092562-005e-48cf-afe4-3cc3412ad2be")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "393a3bd3-02c3-4808-999d-dc924f866c03")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 66 "USE_ANT_2")
			(pintype "passive")
			(uuid "89311539-8ce8-42cd-95c5-ea37603f445c")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "F.Cu")
		(uuid "d05b256d-6be4-4d6e-8633-daf89a757208")
		(at 135.1545 125.11)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q2"
			(at 0 -2.75 0)
			(layer "F.SilkS")
			(uuid "49bdd294-1361-44e9-a0d8-5fa0a0c7a49d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PMOS"
			(at 0 2.5 0)
			(layer "F.Fab")
			(uuid "cc2fedd4-a3a6-4f4e-ab5e-9affa477f52c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_MOSFETs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e3e174d4-c06b-42b0-82ee-9d644ecd5ded")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "P-MOSFET transistor, drain/source/gate"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "06b94f1f-f2dc-4509-b86d-e08d9c894b7b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "PMOS"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "551aea96-55c3-4228-9021-d491511aa5e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Type" "VDMOS"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b8df333a-7c54-4c24-b684-d8aa4761f7ad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=D 2=G 3=S"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2824c6c5-6cbf-407d-8019-dcaa37cca66d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/16f6fc64-eb5f-4533-a552-1f541d148eb3")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.04 -1.58)
			(end -0.84 -1.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "11ad0c91-42e4-4f7e-a5b5-729d69802736")
		)
		(fp_line
			(start -0.04 -1.58)
			(end 0.76 -1.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "14b81fb5-7f23-4aca-84f8-d037cec1f66e")
		)
		(fp_line
			(start 0.76 -1.58)
			(end 0.76 -0.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "955e992b-443b-423f-a0ff-00f01380543e")
		)
		(fp_line
			(start 0.76 1.58)
			(end -0.7 1.58)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "de369089-c82f-4ab4-b45f-4bbccfd1e260")
		)
		(fp_line
			(start 0.76 1.58)
			(end 0.76 0.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "98405243-2140-44ce-855f-68c3a313b8bd")
		)
		(fp_poly
			(pts
				(xy -1.34 -1.61) (xy -1.58 -1.94) (xy -1.1 -1.94) (xy -1.34 -1.61)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "d30392c1-9a10-496a-b714-7ef9ab522bd5")
		)
		(fp_line
			(start -2.7 -1.75)
			(end 2.7 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5441515d-8669-4681-add6-3a5bf01bcf1f")
		)
		(fp_line
			(start -2.7 1.75)
			(end -2.7 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5eb1991f-5367-4748-b939-e7e1840e4a52")
		)
		(fp_line
			(start 2.7 -1.75)
			(end 2.7 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5b1aa87b-a5e8-40e7-aceb-c2b4b43699b0")
		)
		(fp_line
			(start 2.7 1.75)
			(end -2.7 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5870f5dd-adb4-4258-bf0b-8e6b0d80e8dc")
		)
		(fp_line
			(start -0.7 -0.95)
			(end -0.7 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2bb76fc9-370b-4e41-a01f-669384d22d12")
		)
		(fp_line
			(start -0.7 -0.95)
			(end -0.15 -1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9ac74dd-e5cf-46bf-b6af-6c8642413dea")
		)
		(fp_line
			(start -0.7 1.52)
			(end 0.7 1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f7c2ea05-b5b1-449a-9469-a6a97db87713")
		)
		(fp_line
			(start -0.15 -1.52)
			(end 0.7 -1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8edce869-8c5e-4665-b9c8-6944aa8cdd26")
		)
		(fp_line
			(start 0.7 -1.52)
			(end 0.7 1.52)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c9f8a40-e066-494a-8b47-17848f975710")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "c46ed128-c0c3-4160-9458-4582a1607d16")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.075)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.5 -0.95)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Charger Load")
			(pinfunction "D")
			(pintype "passive")
			(uuid "32d66cfa-4326-4dee-b7be-e2ca11dcd39b")
		)
		(pad "2" smd roundrect
			(at -1.5 0.95)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Net-(IC2-VG)")
			(pinfunction "G")
			(pintype "input")
			(uuid "b8649d5e-9ccc-4def-91f5-2f896231241b")
		)
		(pad "3" smd roundrect
			(at 1.5 0)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "Net-(IC2-VCC)")
			(pinfunction "S")
			(pintype "passive")
			(uuid "9d7356ec-b395-47fd-836b-f4a10f972be7")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "d11684f6-5a4a-4071-9946-ff452a2ae4a6")
		(at 50.44 128.0375 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C11"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "d9cf5aae-2015-4e5d-9196-5ddfd969fe14")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "f3c4da62-4bef-4a91-8569-169002dcedbb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c4be6ff7-16dd-42b8-9e94-3da21d430e1d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fa17de3a-9847-4a57-898c-3d8d2568e806")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/2aee7a45-9f20-4a9d-9840-e7711dd4db71")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f7737188-1889-4410-98e9-1315912177c5")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "df6a1521-bf2e-46e0-817e-c51553978b8f")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a489acee-1b6e-42df-945c-5004944b033c")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "93f7e7ff-5cc9-4aff-8a5e-8d8fcf16381d")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "420d57e9-3fd0-48e7-9879-762e57c9c151")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3d3aef70-ade4-4b50-a756-cacaf92af78e")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ad6a00ab-501d-4951-ba73-3b3a6556608c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "74c9c61c-eeec-499e-b128-a57f40414080")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ebf1335c-af65-4583-9078-3fc5ed840fb2")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d5b87440-01ce-4e2f-ae1b-e73c11159829")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "e5aac1ca-aa94-4229-ae93-46f18f9e59fb")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 77 "Net-(U1-VIN)")
			(pintype "passive")
			(uuid "f1fd833b-6196-4b49-a1f2-0fc5dff94e23")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "cd492c51-65f8-472e-8e7c-964bf59e0218")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:CP_Elec_4x5.4"
		(layer "F.Cu")
		(uuid "d3716ff9-6e83-43fe-ac6f-4c14f1432e5f")
		(at 94.313 118.56)
		(descr "SMD capacitor, aluminum electrolytic, Panasonic A5 / Nichicon, 4.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C24"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(uuid "609cad01-84aa-4869-bd1f-9a81b4c55570")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 3.2 0)
			(layer "F.Fab")
			(uuid "9db29e06-5a1d-4dec-b22e-e0a99d1212fb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f294f7e0-dd6a-47ab-91ff-beb5c31e7ca5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b8282756-f057-4202-a044-8d6400882e5c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "CP_*")
		(path "/d30c7ca6-b507-41b1-bc16-e705b5af3ff1")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -3 -1.56)
			(end -2.5 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6188bf6b-8cd7-4292-b729-4f8e1311f380")
		)
		(fp_line
			(start -2.75 -1.81)
			(end -2.75 -1.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b55af39c-36d0-44fb-9a4a-3a6752247de2")
		)
		(fp_line
			(start -2.26 -1.195563)
			(end -2.26 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "285d3122-1726-4c05-843b-35669d5ad8a1")
		)
		(fp_line
			(start -2.26 -1.195563)
			(end -1.195563 -2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "df9012c8-720b-4f96-8f41-62f24b1b9d25")
		)
		(fp_line
			(start -2.26 1.195563)
			(end -2.26 1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2201a8ba-9af4-4ffd-af91-d43b27b0e77d")
		)
		(fp_line
			(start -2.26 1.195563)
			(end -1.195563 2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "38928a51-5d09-48be-aadc-800a7c422093")
		)
		(fp_line
			(start -1.195563 -2.26)
			(end 2.26 -2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "900bd985-8249-449f-8ba8-6f8d3d4dbc61")
		)
		(fp_line
			(start -1.195563 2.26)
			(end 2.26 2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3ec95ed0-3fda-4cdb-ad45-71591a2341ca")
		)
		(fp_line
			(start 2.26 -2.26)
			(end 2.26 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "726f59bd-3f28-4b44-9b34-9a75aa7e8201")
		)
		(fp_line
			(start 2.26 2.26)
			(end 2.26 1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7dcdb639-6df3-483e-918a-08f496b2d8a2")
		)
		(fp_line
			(start -3.35 -1.05)
			(end -3.35 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "01f84332-a49d-4cf1-99b5-55eb8720fe86")
		)
		(fp_line
			(start -3.35 1.05)
			(end -2.4 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c404ca29-77ee-4166-91e9-d4ca0ca944a7")
		)
		(fp_line
			(start -2.4 -1.25)
			(end -2.4 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3dea8a82-6226-46f1-9e29-5e451bdb295e")
		)
		(fp_line
			(start -2.4 -1.25)
			(end -1.25 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "26a3c696-3a27-4c8b-a5ee-23e7e6ad8793")
		)
		(fp_line
			(start -2.4 -1.05)
			(end -3.35 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "66da8eac-83c9-44e3-b464-bbca00fb5f23")
		)
		(fp_line
			(start -2.4 1.05)
			(end -2.4 1.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d28733b6-c792-4fd7-9620-520da70fe1b0")
		)
		(fp_line
			(start -2.4 1.25)
			(end -1.25 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bddeabc1-4d20-49d3-955c-c94559a29519")
		)
		(fp_line
			(start -1.25 -2.4)
			(end 2.4 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "59ea2418-ffa3-4284-8b21-52018a34bb82")
		)
		(fp_line
			(start -1.25 2.4)
			(end 2.4 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a4a86f50-ce61-4a9a-bec0-03fc32101491")
		)
		(fp_line
			(start 2.4 -2.4)
			(end 2.4 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9c418922-637e-4b79-993d-9b1c84726a84")
		)
		(fp_line
			(start 2.4 -1.05)
			(end 3.35 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0215b8b8-61a8-4edb-8daa-e7b97fa6bc96")
		)
		(fp_line
			(start 2.4 1.05)
			(end 2.4 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a04a4049-91c9-4696-8d8d-e8c33ec232f3")
		)
		(fp_line
			(start 3.35 -1.05)
			(end 3.35 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c449813-6e21-4151-b752-e0dc8746fb75")
		)
		(fp_line
			(start 3.35 1.05)
			(end 2.4 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bbc85715-3722-4783-9871-a0eadd6317bb")
		)
		(fp_line
			(start -2.15 -1.15)
			(end -2.15 1.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f760747-47d5-4f59-954c-c1ac951919fb")
		)
		(fp_line
			(start -2.15 -1.15)
			(end -1.15 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7dbe43c-297d-4a64-9fec-8c3e025bf3ff")
		)
		(fp_line
			(start -2.15 1.15)
			(end -1.15 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca3db510-3d7b-475b-a162-d99b23b291c7")
		)
		(fp_line
			(start -1.574773 -1)
			(end -1.174773 -1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "97d52a36-11e9-419a-b424-424bf435c1d1")
		)
		(fp_line
			(start -1.374773 -1.2)
			(end -1.374773 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2d78fda8-2b11-4389-b4b7-e7ca7c788d8b")
		)
		(fp_line
			(start -1.15 -2.15)
			(end 2.15 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b2ceafc-8653-4866-9271-3b391d74dfa2")
		)
		(fp_line
			(start -1.15 2.15)
			(end 2.15 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c15d2117-23fb-49ec-8dd3-3bae0ad27565")
		)
		(fp_line
			(start 2.15 -2.15)
			(end 2.15 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cd1e846f-2e05-4400-bb5f-afcedd90854b")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "fb89a288-141e-4f12-a78e-cc7015851ca9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9f626e53-5fe7-41f3-b681-2f52219922ed")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.8 0)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 55 "Net-(IC2-VCC)")
			(pintype "passive")
			(uuid "6ba6803d-385e-49f8-97bc-a73cfcc0833a")
		)
		(pad "2" smd roundrect
			(at 1.8 0)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 56 "Net-(IC2-VG)")
			(pintype "passive")
			(uuid "e259f2d0-de00-4a74-8ae2-35a3e9f3cb19")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_4x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic:SKY6531321"
		(layer "F.Cu")
		(uuid "d51b1641-a103-4ee3-af10-7b1a4240db60")
		(at 193.999 116.998 180)
		(descr "SKY65313-21-5")
		(tags "Integrated Circuit")
		(property "Reference" "IC3"
			(at -0.3 0 0)
			(layer "F.SilkS")
			(uuid "1737eb9b-fa37-43b9-b32a-e4b19bba927e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "SKY65313-21"
			(at -0.3 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "3d42ca00-a9e4-4866-9616-37587085ae79")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/1/SKY65313-21.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d48aca96-8854-4353-b7f8-eab0781e06ce")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "RF Front End 900MHz TX/RX FEM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9555d629-c750-4b2a-92ef-d2ba24857bd2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "0.9"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "164d2b28-ff91-466e-be22-311c0ed9c3f0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "Skyworks"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "435296c3-ae2f-4f26-a32a-60fe3f022e02")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "SKY65313-21"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "416da953-cab8-4c19-88d0-5a928be587ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" "873-SKY65313-21"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "85a6baf2-dbcc-476a-8990-7686fe616b11")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Skyworks-Solutions-Inc/SKY65313-21?qs=VxEzYtM1ylfKtczVdpm%252B%252BA%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f2532860-3f59-429f-8bdf-cc602163b597")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d5a0be4a-5ebf-4023-8ff1-9b5202220064")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9462c4fd-b059-4774-b4d5-d2f055342988")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C5144140"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2252dcfb-d06c-4a36-8d85-38370ed3406f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/d5ea5d59-56b0-43bd-8397-a41f8049e541")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.65 -2.6)
			(end -3.65 -2.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8fb4d642-8c13-413f-952e-a56116ae7402")
		)
		(fp_line
			(start -3.65 -2.8)
			(end -3.65 -2.8)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7af4c2d2-9bcb-4fe1-9ece-0bb1b9ce64a6")
		)
		(fp_arc
			(start -3.65 -2.6)
			(mid -3.75 -2.7)
			(end -3.65 -2.8)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "51361af3-aba3-4a0d-8545-401ed54874a5")
		)
		(fp_arc
			(start -3.65 -2.8)
			(mid -3.55 -2.7)
			(end -3.65 -2.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cfe918fe-c2f9-4b4b-9286-d87df9db6067")
		)
		(fp_line
			(start 3.65 3.65)
			(end -4.25 3.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e73f86b2-b1d8-4ee2-b480-bb00288b75aa")
		)
		(fp_line
			(start 3.65 -3.65)
			(end 3.65 3.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "41145c2d-59b8-4e6b-aff6-1e69ba457092")
		)
		(fp_line
			(start -4.25 3.65)
			(end -4.25 -3.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "55989f86-7556-4b28-bb3b-9f2ff488cbba")
		)
		(fp_line
			(start -4.25 -3.65)
			(end 3.65 -3.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c82aa179-245e-4ca4-a9e5-45a5a66ebbc7")
		)
		(fp_line
			(start 3 3)
			(end -3 3)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8004f41-97ce-4678-bc98-1ebf6e3345a5")
		)
		(fp_line
			(start 3 -3)
			(end 3 3)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9c260654-7361-4d3e-aa1c-3682f41b3f90")
		)
		(fp_line
			(start -3 3)
			(end -3 -3)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9400cf8e-76c2-4940-b877-3e7123c0aaa0")
		)
		(fp_line
			(start -3 -3)
			(end 3 -3)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eaa3f5c7-ba02-49df-a54c-35728bea1c07")
		)
		(fp_text user "${REFERENCE}"
			(at -0.3 0 0)
			(layer "F.Fab")
			(uuid "bbab7821-5360-42eb-835a-4b0b0811f256")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -2.75 -2.775 270)
			(size 0.75 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_1")
			(pintype "passive")
			(uuid "d7d4bbab-6c8f-4f9a-a80b-4d78fd3113d3")
		)
		(pad "2" smd rect
			(at -2.75 -1.813 270)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "RADIO TX{slash}RX")
			(pinfunction "CTL1")
			(pintype "passive")
			(uuid "6425c261-b785-44bf-941f-8bf830fdba26")
		)
		(pad "3" smd rect
			(at -2.75 -1.088 270)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "CTL2")
			(pintype "passive")
			(uuid "3845450b-2c47-4a94-8039-0e106c4eace1")
		)
		(pad "4" smd rect
			(at -2.75 -0.363 270)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "CTL3")
			(pintype "passive")
			(uuid "22870fb2-6ccc-41ca-ba86-2e1f53fc6d3e")
		)
		(pad "5" smd rect
			(at -2.75 0.362 270)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "VPC")
			(pintype "passive")
			(uuid "d99195b8-feee-4351-a2f3-b059b90006c7")
		)
		(pad "6" smd rect
			(at -2.75 1.088 270)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_2")
			(pintype "passive")
			(uuid "d7806ec7-ea58-45fb-9c8d-057e0c77900d")
		)
		(pad "7" smd rect
			(at -2.75 1.813 270)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(IC3-ANT)")
			(pinfunction "ANT")
			(pintype "passive")
			(uuid "b87f16c7-a7c3-48c6-99eb-3887a7d0b81a")
		)
		(pad "8" smd rect
			(at -2.75 2.775 270)
			(size 0.75 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_3")
			(pintype "passive")
			(uuid "a68049f2-4932-4db3-8311-54c3ac3e88b6")
		)
		(pad "9" smd rect
			(at -1.813 2.75 180)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_4")
			(pintype "passive")
			(uuid "687f0b4a-6e47-48e1-b9bd-9544603bbc5f")
		)
		(pad "10" smd rect
			(at -1.088 2.75 180)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "Net-(IC3-RX1)")
			(pinfunction "RX1")
			(pintype "passive")
			(uuid "54af7ad6-0629-4679-b6aa-6008c082ec94")
		)
		(pad "11" smd rect
			(at -0.363 2.75 180)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_5")
			(pintype "passive")
			(uuid "bd585144-d98f-469f-9819-1982ec0d0932")
		)
		(pad "12" smd rect
			(at 0.363 2.75 180)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_6")
			(pintype "passive")
			(uuid "b7c4bf74-42b4-48be-b042-0d0847b6debf")
		)
		(pad "13" smd rect
			(at 1.088 2.75 180)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "Net-(IC3-RX1)")
			(pinfunction "RX2")
			(pintype "passive")
			(uuid "50c2dc22-2527-4773-b2da-a4d3686885d8")
		)
		(pad "14" smd rect
			(at 1.812 2.75 180)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_7")
			(pintype "passive")
			(uuid "c2148f27-86da-469d-b5c3-7f4906df62be")
		)
		(pad "15" smd rect
			(at 2.75 2.775 270)
			(size 0.75 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_8")
			(pintype "passive")
			(uuid "b4ffd62b-30e9-4101-90df-3680a4704fad")
		)
		(pad "16" smd rect
			(at 2.75 1.813 270)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "VDD1")
			(pintype "passive")
			(uuid "73f0ae27-a2b0-45b8-b674-5a1abed73db6")
		)
		(pad "17" smd rect
			(at 2.75 1.088 270)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "VCC_RX")
			(pintype "passive")
			(uuid "559580be-d0e4-49e3-a350-b4d280132947")
		)
		(pad "18" smd rect
			(at 2.75 0.362 270)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "Net-(IC3-RX3)")
			(pinfunction "RX3")
			(pintype "passive")
			(uuid "b955313d-8fb7-4512-b13a-5a00e11ccf24")
		)
		(pad "19" smd rect
			(at 2.75 -0.363 270)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_9")
			(pintype "passive")
			(uuid "55ea0af8-3853-426b-a4e2-2954f71c6199")
		)
		(pad "20" smd rect
			(at 2.75 -1.088 270)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "Net-(IC3-RX3)")
			(pinfunction "TX")
			(pintype "passive")
			(uuid "44b45349-c592-4822-bba6-e2e0add4bd2c")
		)
		(pad "21" smd rect
			(at 2.75 -1.813 270)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_10")
			(pintype "passive")
			(uuid "e9e98ad2-e21d-452d-a41e-92db6f7ae739")
		)
		(pad "22" smd rect
			(at 2.75 -2.775 270)
			(size 0.75 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_11")
			(pintype "passive")
			(uuid "0a55c277-a1b7-4ad3-9dfb-1bd85f75ae94")
		)
		(pad "23" smd rect
			(at 1.812 -2.75 180)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "+4V")
			(pinfunction "VDD2")
			(pintype "passive")
			(uuid "e92971fd-0f22-41fe-b49d-7e4fb8b5a983")
		)
		(pad "24" smd rect
			(at 1.088 -2.75 180)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "+4V")
			(pinfunction "VCC_TX1")
			(pintype "passive")
			(uuid "4038d24c-f7c5-42d3-94a7-15c5e11012a4")
		)
		(pad "25" smd rect
			(at 0.363 -2.75 180)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "+4V")
			(pinfunction "VCC_TX2")
			(pintype "passive")
			(uuid "6ce9b064-e277-41dc-8876-a9d37eb1bb7c")
		)
		(pad "26" smd rect
			(at -0.363 -2.75 180)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "+4V")
			(pinfunction "VCC_TX3")
			(pintype "passive")
			(uuid "44e1af12-54e0-49a5-8d10-176a9bff6613")
		)
		(pad "27" smd rect
			(at -1.088 -2.75 180)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_12")
			(pintype "passive")
			(uuid "0ea26dcb-0247-4cfb-b39d-e1fdf00a0400")
		)
		(pad "28" smd rect
			(at -1.813 -2.75 180)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_13")
			(pintype "passive")
			(uuid "e7af7b8d-f943-4525-9a35-999eaa39621f")
		)
		(pad "29" smd rect
			(at -1.502 -1.502 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_14")
			(pintype "passive")
			(uuid "c3fddcae-3a6c-4062-9935-0dd5aac40215")
		)
		(pad "30" smd rect
			(at -1.502 -0.501 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_15")
			(pintype "passive")
			(uuid "bf7f4370-85e4-40cd-974d-937cf581edb3")
		)
		(pad "31" smd rect
			(at -1.502 0.501 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_16")
			(pintype "passive")
			(uuid "67810388-1b73-4348-b847-b4b4c5fd5797")
		)
		(pad "32" smd rect
			(at -1.502 1.502 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_17")
			(pintype "passive")
			(uuid "3b431cbd-f727-4f2f-beb2-1c6e3cf4fc53")
		)
		(pad "33" smd rect
			(at -0.501 1.502 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_18")
			(pintype "passive")
			(uuid "6de7afd0-6ac0-4cbe-8545-b5c1f84c3606")
		)
		(pad "34" smd rect
			(at 0.501 1.502 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_19")
			(pintype "passive")
			(uuid "66a153da-d0cb-4520-9d6b-c9fd5a53cd09")
		)
		(pad "35" smd rect
			(at 1.501 1.502 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_20")
			(pintype "passive")
			(uuid "470f0e27-ea7c-4d5c-9f28-2f78129b138b")
		)
		(pad "36" smd rect
			(at 1.501 0.501 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_21")
			(pintype "passive")
			(uuid "023e175a-46f4-4494-9e32-fa09470bc556")
		)
		(pad "37" smd rect
			(at 1.501 -0.501 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_22")
			(pintype "passive")
			(uuid "b4ef1ef0-1fc9-42c1-b079-010fe16b10f8")
		)
		(pad "38" smd rect
			(at 1.501 -1.502 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_23")
			(pintype "passive")
			(uuid "1862f04b-ca8b-47e4-a592-514a6d590bc5")
		)
		(pad "39" smd rect
			(at 0.501 -1.502 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_24")
			(pintype "passive")
			(uuid "d895f67d-034c-4468-9830-3d79a40422d8")
		)
		(pad "40" smd rect
			(at -0.501 -1.502 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_25")
			(pintype "passive")
			(uuid "bed68414-bf64-4332-a412-26e3efa75f33")
		)
		(pad "41" smd rect
			(at -0.501 -0.501 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_26")
			(pintype "passive")
			(uuid "f514f02d-503d-4470-840e-e6efd0dfbbe4")
		)
		(pad "42" smd rect
			(at -0.501 0.502 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_27")
			(pintype "passive")
			(uuid "458e8a7b-5677-482e-9f2e-ba8c0546b463")
		)
		(pad "43" smd rect
			(at 0.501 0.501 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_28")
			(pintype "passive")
			(uuid "4350cd47-881a-4031-8577-6994744ee156")
		)
		(pad "44" smd rect
			(at 0.501 -0.501 270)
			(size 0.625 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_29")
			(pintype "passive")
			(uuid "c1865d9d-486e-48eb-87bd-ad437dbb5cfd")
		)
		(embedded_fonts no)
		(model "SKY65313-21.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "d5aa95d6-0925-4bb5-a9d0-5fe68fce9d77")
		(at 50.35 108.8875 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(uuid "41744341-879d-4479-a24a-2c9528264cfa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "383c2043-a504-4c87-8aba-c56f7ae82c42")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "213f8a14-1d91-434b-8126-8c14747dabb2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5f34ec08-663d-4f01-bbc0-013ffd3bf8f6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/3a29d0ac-1a2f-4f2e-aa6a-e2c8eea20ac5")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2facdf7-920d-4ba9-b619-17ed844d5219")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c840e72b-a2b8-4679-a083-b7229cc98582")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aabb5ac7-c750-4ee2-8703-3e735cd23ede")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2555140b-f63a-4f1c-bffd-934ed07c38ae")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f81a7d3b-da33-4df8-89ca-598ec0ff6533")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "61c603ba-d48c-4d60-9f84-bd167f20ed70")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b14bd6a7-823d-473a-a49f-dd7db9ebe8ae")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6a1232a3-b232-4aa9-b2c3-9c9852c0a031")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "33768798-9df0-4f2e-bd8c-ba3a95eb293c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aedbd23f-3a97-45b1-8d11-23a30fc05edb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "fedd064c-2722-437e-ab9c-fd12d1263c6a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 59 "Net-(U1-EN)")
			(pintype "passive")
			(uuid "a05dd52a-f9e4-416c-8407-80f8b8eb338e")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 77 "Net-(U1-VIN)")
			(pintype "passive")
			(uuid "edffb35a-6875-4552-98ea-7a48749de0ce")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "d89df673-feec-44c7-9e05-ee01bfc18596")
		(at 177.5 106.51)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "9cf8822f-d3ed-4559-946f-e26d1bdb2f34")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "4b9a0824-6b97-46af-a0ea-9839e658dfdf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c464d266-222a-4ab4-84d6-ba6304453c59")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1c841b36-83ea-4eaf-bb24-470e14eb7ed4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/2aff84df-f517-4280-a422-3aee2ba91baa")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed7e36d8-e55e-420c-9d1e-4714fa568e3a")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5280775b-37cc-499c-8ee2-d8f507e64215")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bc9741ad-adbf-484b-9013-6a283e039e5e")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d1092c3b-73ac-4b0d-a553-bf5191ed646f")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "69eb089c-7cf3-4f97-8c26-7ff23f4a3e8a")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "73b75ea1-e7ec-42e3-ad82-32789d4e1a67")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2292440f-4c21-4ff2-b6d8-ca64aaef1e9b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b8277391-4120-42b2-836c-ef55cf77b224")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "036c1adb-1af9-4a22-8d5e-144bdc537b0c")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d3a1318b-68aa-4fc8-8105-ad27badd3dfe")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "debceda8-1a6f-4455-8337-f4e9087687b3")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "8ec014e0-0d31-4ec0-9f0f-5134431ebe4e")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "a20a715d-ec93-4402-b754-f78117efeb58")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "da762b3d-d523-4458-829b-fc07903c99fa")
		(at 177.5 97.48)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "2e32d65e-3e58-4954-a579-0e99015745d1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "1c47868a-a4ee-46a4-b190-71d6d6f437cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "404f25db-e8c2-4800-bb98-9d6a1cedbc5a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "50bdf25c-a894-4781-8c09-473629bd9cfa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/2aba3709-1593-4aeb-b114-e94971cd0b98")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f0753f58-467d-45ab-9e73-3072b78b7b14")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fcc898d1-698f-4dec-b192-832c2d5287dd")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "938bdabd-9b83-46fa-a919-07d0c0b88214")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "170c34c3-f2e9-4193-b9bb-ee36c00aad07")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4032d46a-5539-4707-9c55-770f330ae3b4")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "47c199b4-978b-4692-bb96-e6e78cd22396")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3ceae2c1-231e-489e-a937-f452cb36764e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a6d8c27f-eaaf-4c11-a9a7-3e0da19920b6")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "89aa3a0c-d761-4f6f-8d2c-3a79d6652ae0")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "45e56d88-6b26-4b9d-81de-4186b975df33")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bde320df-83c2-400a-9789-f6e463b20783")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "537e611d-f731-4db0-bd39-75640c37f251")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "6343aa9f-1a2f-40ee-b2dd-83bc9b6015f9")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "dd3fbada-79b2-46c5-8180-ee29faa308a1")
		(at 127.25 114.55)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R37"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "23810ac7-c96d-4ff2-be83-701b730f577e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "ec18dfe7-8ba8-4cab-bec3-f9fc640ffa63")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "de106169-4033-4291-a968-9ea953bb3bf0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "42a14d19-3451-4c2f-8c63-fcd85db7cbc7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/ee484925-4472-4702-ae2c-7f9ee40d3d71")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d868f5e-4b53-45e5-9441-441a8863016e")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0717e276-d5ec-4db5-a4f0-267c839d9142")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cfd386eb-995a-4dda-b5a6-c10c7c6d6c1b")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "44a14846-fa11-4599-890f-03cd7bedc728")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "822b4653-b289-4a5f-a9bd-a68cc23b2e29")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "43a159cd-1270-429a-a63d-04e6db567980")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9ca209c9-a98f-4665-8009-0cb1bf377e3e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ec2c8401-d7ed-4151-b350-c99ac645099e")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ef39456a-1f30-4430-91a0-43f2b2a4bb72")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a67580fa-93d5-4597-9cb5-aff18a6e3bd1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "cee9a1a3-816d-4743-bb1a-ec325f723b74")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 35 "Sol Shunt 1")
			(pintype "passive")
			(uuid "0ee67f6e-dd03-4763-aa03-081660a5b9e7")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 35 "Sol Shunt 1")
			(pintype "passive")
			(uuid "830c3a80-3d4f-4a09-83db-165dd5267430")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(uuid "de01f564-ad09-4436-ab4c-d69457550aab")
		(at 149 100.4 90)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 -1.998 90)
			(layer "F.SilkS")
			(uuid "24245e46-a11c-4fe2-a18e-0c7340aa281a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 2.05 90)
			(layer "F.Fab")
			(uuid "1ff97129-0ef1-4bd4-8122-bda0c0ef2aa3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "874ed733-cd65-4f6d-8d6a-d2ba2803d96a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "60b4ce37-7da1-4980-b4c8-8d81ef8801b5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/860b2ab8-d4dd-4880-bdeb-4b0f18cdab93")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_circle
			(center 0 0)
			(end 0 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "e58cb978-52a8-4898-a6e2-3bcf66a64e77")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "67dcb134-4603-474e-8c9d-0dd94247a17b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
			(uuid "1629a55f-f3c7-42a1-9fcb-366604caefc3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 70 "RADIO TX{slash}RX")
			(pinfunction "1")
			(pintype "passive")
			(uuid "0e9a7db3-ca3e-4d9c-b50c-99c61cb90137")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "df3d7e36-ed9c-4d3b-8e5b-db0d83779e81")
		(at 56.46 128.0375 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C13"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "41b60878-6d00-4c8e-a394-71d88fafc4ea")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "b4902b55-c234-4aa5-bac2-7f25ccd65428")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ebb703fa-43de-4994-b004-4d395386b90c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "67646660-b367-4b4f-831b-3814ae363d22")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5386a405-ca64-4db7-9b58-2b01b62dfa51")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a511fe33-7cfa-4f6d-92ee-781f80e01898")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e0ebe98-e875-4c2e-93eb-6660c8aa40a6")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ef351019-af51-43e3-9be5-10fdd34e48e6")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "92f63f26-84a9-4bcc-a5db-ceecd7c9cfeb")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "090d5d4d-4547-4477-bcfa-44dfd5824d8b")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6981afb8-6707-4a4a-ab07-43e65cd66013")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "251c302e-f19f-4a39-9035-a0caedd67602")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6058b699-5e7b-49a2-8c50-3827c38d6dfe")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "05f09231-eb2e-4599-af58-15e9889d001b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c3fd870-0601-483d-939c-ef74643d6927")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "f0a40215-238e-49c2-a850-f070aac50161")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "705e329f-b0e9-4382-a11f-5ef47f6f76c0")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "1871887f-5fc6-4dd8-8c65-3fdb671dee0a")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "e0e4279a-0b02-4767-820f-4c75656423a1")
		(at 62.15 113.6375 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(uuid "54b17896-0fcc-44b2-bbbe-5511534c26d5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "6.8k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "93f8ba87-b036-414d-80dc-e1b5b8cb4b94")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e35743a8-fa78-4d89-8750-13fb7904958d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ef1f2df2-3df6-4c55-8cc5-09197dedd894")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/2894f8eb-bc78-4349-846b-395a7a6f5b80")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84b1451c-fcd1-424f-932b-b82b45906389")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8cbacf92-86eb-4cc0-88cb-d182ba656d42")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b4d679b9-2e0d-4b7f-898b-2f435a5c249c")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "64752108-38cb-4dad-a6f9-b36c0b8a6397")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b8efb819-3a76-48e9-a204-07270fff7c87")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f7647991-a358-497e-ba99-7ddee2382e90")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c603caf-8b0c-4256-999d-a6faba0f7828")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "88db9a65-a398-48c5-8335-15ac39b80fff")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "733c870c-ccd4-4d4f-b361-33720b95e681")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "28a0c85f-8316-4d83-9adc-0e98abbdd8d4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "ec0032aa-cb48-4b39-88a8-ff520f790061")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 57 "Net-(IC1-CFG1)")
			(pintype "passive")
			(uuid "861c97ec-94d7-4e5e-940c-e3d15c599326")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
			(uuid "f12d3e71-fe6b-4174-b522-08d93a9d4409")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "e3283b6d-0454-45a0-8ec0-fb3ae1897f69")
		(at 62.48 101 90)
		(descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "fuse handsolder")
		(property "Reference" "F1"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(uuid "c233ce87-9fb6-4194-b012-55c79a8a6658")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Fuse (3A)"
			(at 0 1.43 90)
			(layer "F.Fab")
			(uuid "143e136b-8b86-4087-a0fb-9c96b974052d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "eabd8951-0361-4a75-b368-47276f339c42")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Fuse"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "61cd8e55-b8dd-4df7-abde-7b2fcfc50674")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*Fuse*")
		(path "/15872d8b-470a-4104-924e-cd63363d4b9f")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.171267 -0.51)
			(end 0.171267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e9d191d6-9fbe-4a94-b294-2ed4277cfefc")
		)
		(fp_line
			(start -0.171267 0.51)
			(end 0.171267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d2dc18e9-5839-4031-a20d-3095e117fade")
		)
		(fp_line
			(start 1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1667d613-90f6-4dd2-8409-07d85cb34e7f")
		)
		(fp_line
			(start -1.65 -0.73)
			(end 1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a156f7cf-9a49-4e37-9aff-9077acb52f7e")
		)
		(fp_line
			(start 1.65 0.73)
			(end -1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ddb8d4d9-4a91-4733-a6b9-937c1bd52dcd")
		)
		(fp_line
			(start -1.65 0.73)
			(end -1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7963abe4-c1dd-44a9-a021-2033a50cf2d7")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7356b608-0aa9-441f-8669-4fcd966073cf")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "75b35144-3411-4b54-a03d-83600369a0d9")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2bc85513-2f1d-4e88-8531-e22bc85e778d")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77d95b28-285f-4cfe-82ea-7916b6ee19f8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "079c1175-1b12-4e5d-aecb-17255d4504f8")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.875 0 90)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Sys Load")
			(pintype "passive")
			(uuid "e1fd37bc-472a-4b48-97bb-b1efc1d2a56e")
		)
		(pad "2" smd roundrect
			(at 0.875 0 90)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "Net-(U1-VIN)")
			(pintype "passive")
			(uuid "6e0b0206-8397-4557-93ee-90d466dc2d88")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "e669f132-2d32-4314-882e-6ec6bda5cf1d")
		(at 47.4 99.3875 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R21"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(uuid "74285715-6fd2-4395-b451-f3ae697c36e3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "700k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "75163310-0781-4bbe-ad0e-a35d90ebff40")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2605a959-f6c2-4e11-8f41-a2c28dc8d856")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "139657d9-9831-44a4-83dd-a326b8fd4da3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/3685251d-c1a7-4ba5-96e8-2fa61160a79c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "33c6df42-0030-41b2-a401-b3af3cc1f458")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c53c6ed3-a552-4268-8e32-5f14df68ca87")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c986e192-fda3-4964-bb13-c9fafaa78410")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e9ffdd67-0562-453b-b4e1-ea21a255c60d")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7947e752-fa44-4a99-9685-326c62303ceb")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "36603a61-7acd-4dbd-ab33-2f87346254a0")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8cb4fba1-cf12-4a96-8a94-5a6d351bd2bb")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0e3b13f3-a149-4659-b610-b89fc170ca4a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b424cc12-05ff-4ddd-967b-a661f8816bf8")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eea91f39-e310-4952-9838-96f05de6f451")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "6c9053ec-543a-4e30-87a2-63eb9a7f52f3")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 14 "+5V")
			(pintype "passive")
			(uuid "c5fb3005-c041-4743-97bc-7606a979eb5e")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 67 "Net-(U3-FB)")
			(pintype "passive")
			(uuid "6972b6ba-dede-4e33-9379-9a96c18f223e")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "e6a6e133-efbf-46dd-9936-b73a1227b887")
		(at 117.3125 126.41)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C20"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "d7478e95-4af3-4c5e-b4fa-87cad6370345")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "220nF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "259bbc0b-8cc5-430a-8881-c4020da6b251")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ec05f09b-0193-4c08-87e0-a4f83a543b98")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f3670a9e-abfd-4229-ac11-37d33ee7a354")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/38788ddc-4ba6-4b44-a7a2-2d76cb4fe9f9")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9075f22f-9904-4bc3-bd8e-4b0efea89303")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a10e0dbf-94ca-462f-a410-83a1aa6173cb")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "59a59672-00d0-494e-8439-fd23dde099f7")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e4d4c1f1-49af-4351-987e-5293a67d4cec")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c4fe8d93-fecd-4f31-a4d1-493ea79977fc")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d26bd8d0-82df-4bac-8741-d729c1d2333a")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0dd09b59-e17e-4c54-8f40-2279d9711001")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c50e50f6-3dcb-4728-a4ac-7a1b566807d0")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "82e6d547-d3cb-419b-ba79-a06f4eb9c09f")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b9811b63-6ca6-412e-83b8-fbb7cc2e645a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "574921c9-5f4c-4eda-85ba-7aba5599b3e6")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "2fbb67e9-8cef-4936-a4bf-60c9abb27e38")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 8 "Net-(C20-Pad2)")
			(pintype "passive")
			(uuid "5cb08552-27b4-4b28-a094-4735c834663c")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "ebb7f557-88d8-4239-bd24-a19850540afd")
		(at 191 99)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C23"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "cee1e522-84d3-4adf-ad5a-9429845ef3be")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "2a4d7f0e-db5d-4106-b1a6-1fb0f3f99ee0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3ea8a6e1-6f98-4e9d-b8a5-a691005085d8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "950fcbc0-b117-4303-840a-e21311ad80b1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/dd80ffef-09ba-48db-8d24-fb4fc1723e22")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3425f733-2418-40a7-9992-eed9495d2585")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e4e18141-895c-407d-a253-9d1f759cb698")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5e8ea67-d38f-4e00-9f1b-384d1ae16f74")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c713f67f-bd1a-437b-b11e-2537a98cfb5c")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "308a4729-5dd2-4768-b4eb-b1b5b07bab71")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9467df28-64cb-4557-874c-0db308e7dc26")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7607b9c8-675c-48bf-9d99-8b192cbd28fd")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "647330b1-821f-4cb8-93f2-2bd135c73efd")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "91c03043-9779-4207-bd4a-c22547e9968b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ba7aa4fd-c63f-4bf7-a1e9-0b4e834918ee")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "cb84ad27-7192-4312-911b-178b26e2e3e3")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "6beeac27-24c5-466e-8749-0031f0d2d8c6")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "5c2f668d-861f-4271-89a1-30a6d6a2a0f2")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "ec11765d-8cc2-44ce-b610-5116d79052de")
		(at 188.0375 113.99)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C26"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "9a99b9aa-e386-4e06-b00e-e4f1bb454e90")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "470pF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "44a5e158-cfe6-4d88-b272-496a7955756c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e8e8f0d7-2fb0-4ee5-8df7-f4c498fa432e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cf831c19-defe-4b76-b0e4-9b47bf1c5c55")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/65b26f36-1540-4bd2-8746-120d2100802c")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b1e2adc7-45bb-4796-bbb9-649a157f9d65")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3038523-ae47-4e4e-bd1d-f682e04ad590")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c38102dd-e1df-4b1e-9b41-98918613ccf4")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8eeed2fb-2d81-4dd8-a112-3aaefbfb5ee6")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bbd8a74e-596b-464f-a170-f057a420791e")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eec8723e-8892-459f-8d94-2722246ca831")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f073f12c-52db-40b8-8a1f-67c109dcf166")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e513d36d-bdbb-4cb5-bc25-c451ec3c4d7b")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c9a50bca-968f-4011-bd94-164a084958b8")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "53b7bf97-4c04-4ade-8969-8f4fe13b0b9a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bf90f026-8fc8-4d68-adb1-1d350f189bb7")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 9 "+4V")
			(pintype "passive")
			(uuid "0d7b329d-8e2d-460b-8aee-dd6a92716eb2")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "ba6e9191-4501-4597-ba8c-2994dab44459")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "ed7239b3-1c38-4695-a11b-23246050be57")
		(at 117.75 114.55)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R18"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "6296ee1b-75f1-46f0-9722-ad795cad7ecc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "2eed6010-41b7-43b3-9608-ef86ec1426fd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3fa63596-05fa-43fb-8b5e-911a556ece7f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f769ad90-8d4c-4bf7-aa22-31504220edb5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/f9f9b350-ceb2-4685-abe3-a2b246ef02bb")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3d813631-f9ba-44c8-92e0-43663ec9f048")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fd490937-0de2-4b5d-997b-5626c9d91d94")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bcaf6b04-400d-46d4-8c7b-54d43407b21b")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "309cc3ce-49e5-4223-a420-c8f8263f8cad")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e889cedd-1b1e-4e6e-8bc2-38bcb76d90c2")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0326acab-fa13-44e1-9df8-ff45cffc7a1a")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "13eeda9e-e4d2-4b6c-8827-14303cb46c24")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80813ee4-d39d-4d94-b6a8-295d19d4c18c")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "076c253b-395b-458b-a747-282796cc2a80")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "66da291e-1243-4dcb-91d3-8e4d8bf5d282")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1cb78e10-50d7-4c0e-9245-9b10debfcb22")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 56 "Net-(IC2-VG)")
			(pintype "passive")
			(uuid "a36de695-70ec-41f4-99c7-e3c36c94e0e8")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 55 "Net-(IC2-VCC)")
			(pintype "passive")
			(uuid "f4dd0eee-aaf4-45c3-9fe6-82a4d096a7f0")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "ee36d78e-ab81-4ad5-b23f-d2183a2c4457")
		(at 122.5 117.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R27"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "813f4323-14b8-4208-9091-6fd78f208686")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "23.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "88ca6c6f-9f91-4540-bccb-37ea6d7df327")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2e0669de-9aa1-4781-8d82-ae04c6c44246")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c3d7cbdb-5178-401e-8afb-18e5f4656eb6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/ec5b8e2a-c0a4-4c3a-8f84-ad1f8af688f8")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0f110f30-5279-4217-b2e9-ac79f572ecc5")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb1c8d5c-b4da-47fa-ae57-2ea0139c3693")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "902f70b0-aa90-4a8e-8b57-e8e6ba1e3f75")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "301a5ff3-1ade-499b-a6be-c2a32a77b75b")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "82b42843-9876-4084-9e83-1ad929519b8a")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf16b841-6156-4853-ac3b-a89097d07c08")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f8f084e9-2880-4f77-ba5a-4266956fa50d")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d38e2ab0-4e04-4861-a172-c3e8bb1a31a7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b8e7c1cc-8882-4950-80ba-f8522899647f")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0330a6bb-d9ec-4c77-9ea4-baa5e5f2a08d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "439a6b2e-9604-48d6-8d47-8af261e920fe")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 40 "Bat Shunt 1")
			(pintype "passive")
			(uuid "3ae5bff4-8051-4ee0-99d0-f3c74ca37d98")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 37 "Net-(IC7-OV2)")
			(pintype "passive")
			(uuid "b1a89321-b1cf-4690-956a-1fe8290ecf4b")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic:SOP100P600X175-10N"
		(layer "F.Cu")
		(uuid "f1503c32-bd22-4475-a0a5-a4587010b400")
		(at 89.138 125.41)
		(descr "CN3791")
		(tags "Integrated Circuit")
		(property "Reference" "IC2"
			(at 0 0 0)
			(layer "F.SilkS")
			(uuid "3c5bb2b8-427d-47c1-b912-5c14308904a1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "CN3791"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "b307858e-0afe-44d9-a7bb-23f4a6e25cb1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" "http://www.consonance-elec.com/pdf/datasheet/DSE-CN3791.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "27f382d8-95c7-4df6-9e65-74d94f5669ad")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "ic"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "56a76d19-3c9d-4aa9-a656-1acddda28c3e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "1.75"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0276554-d744-4cf4-835b-8ba86f11ed86")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "Consonance"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e63de228-0922-4c31-a5f2-01d13ece6f4f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "CN3791"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bd5e29cf-d970-43a3-b232-a0fb99adfeb5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "35d22861-5f86-4af5-a801-5944a6cc426b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1543022b-8d35-4001-b7fe-9589623812ea")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cdf416b3-53df-45c2-9a8d-c4e70fff9fea")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5fc81db7-5f98-4bdf-a985-fc832dcaaf45")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C154992"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9231ef61-3a0f-4940-a53c-6401468c9399")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/714c827e-f961-4794-94bb-bb28cdcf6f2e")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.475 -2.675)
			(end -1.95 -2.675)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6808f8ce-95a8-4baa-bd69-f0be0a46a6de")
		)
		(fp_line
			(start -1.6 -2.45)
			(end 1.6 -2.45)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "56e490c1-761f-496a-a01d-6a6dbaaf9a37")
		)
		(fp_line
			(start -1.6 2.45)
			(end -1.6 -2.45)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb8e5ca4-8d73-4835-9863-6c8ecc3bdfa7")
		)
		(fp_line
			(start 1.6 -2.45)
			(end 1.6 2.45)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a0f97160-53c1-4d61-84af-9386a47b2480")
		)
		(fp_line
			(start 1.6 2.45)
			(end -1.6 2.45)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a59597d6-bacf-45a7-b103-3c88d662c02e")
		)
		(fp_line
			(start -3.725 -2.8)
			(end 3.725 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dd9638f8-a620-4709-a801-38c6811d6a2f")
		)
		(fp_line
			(start -3.725 2.8)
			(end -3.725 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c7b2f001-3407-4007-b6ad-724aabcfa2d0")
		)
		(fp_line
			(start 3.725 -2.8)
			(end 3.725 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5fb0c79d-df96-4e1e-b9ec-88e5f30f8e1f")
		)
		(fp_line
			(start 3.725 2.8)
			(end -3.725 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4067d1fc-7368-4d4b-a00a-f93d9f7e826a")
		)
		(fp_line
			(start -1.95 -2.45)
			(end 1.95 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "513d8756-c90c-4519-96f6-dd3501004510")
		)
		(fp_line
			(start -1.95 -1.45)
			(end -0.95 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2092405f-1ded-4f88-87c5-3d1a3e0bbf62")
		)
		(fp_line
			(start -1.95 2.45)
			(end -1.95 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ef5cbae7-f455-47b4-9f31-d6ab249ca419")
		)
		(fp_line
			(start 1.95 -2.45)
			(end 1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b09a8ee-6539-4ee1-a703-d446c06ec2eb")
		)
		(fp_line
			(start 1.95 2.45)
			(end -1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8be3d7f7-fc37-49b1-ac78-746a890cb20e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "86659340-2e04-43c2-bcb0-8df23b5e59ec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -2.712 -2 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "Net-(IC2-VG)")
			(pinfunction "VG")
			(pintype "passive")
			(uuid "7078609f-ac6b-4849-8d3e-add802b72762")
		)
		(pad "2" smd rect
			(at -2.712 -1 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "9d5cd3ed-7047-4cb1-b169-072750b1a6e1")
		)
		(pad "3" smd rect
			(at -2.712 0 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(D3-K)")
			(pinfunction "~{CHRG}")
			(pintype "passive")
			(uuid "bcd2e505-b6dd-4e9c-9d5e-9e5a6a060236")
		)
		(pad "4" smd rect
			(at -2.712 1 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(D5-K)")
			(pinfunction "~{DONE}")
			(pintype "passive")
			(uuid "e4188923-358f-4771-9d52-af996618b7fb")
		)
		(pad "5" smd rect
			(at -2.712 2 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "Net-(IC2-COM)")
			(pinfunction "COM")
			(pintype "passive")
			(uuid "3ae011f8-2f1e-4a9f-855c-dfd005d06816")
		)
		(pad "6" smd rect
			(at 2.712 2 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "Net-(IC2-MPPT)")
			(pinfunction "MPPT")
			(pintype "passive")
			(uuid "381fe988-9343-4621-a38b-e916bf64a93f")
		)
		(pad "7" smd rect
			(at 2.712 1 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "Bat Shunt 1")
			(pinfunction "BAT")
			(pintype "passive")
			(uuid "02bf658f-bcf8-4147-b5e8-31fa8072c08f")
		)
		(pad "8" smd rect
			(at 2.712 0 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "Net-(IC2-CSP)")
			(pinfunction "CSP")
			(pintype "passive")
			(uuid "13ad4e6c-7828-41f4-8172-a5505e604980")
		)
		(pad "9" smd rect
			(at 2.712 -1 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "Net-(IC2-VCC)")
			(pinfunction "VCC")
			(pintype "passive")
			(uuid "ca1f9dbf-4988-4bcb-b8e1-8014ec2ced49")
		)
		(pad "10" smd rect
			(at 2.712 -2 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "Net-(IC2-DRV)")
			(pinfunction "DRV")
			(pintype "passive")
			(uuid "3223e698-3334-46a3-aa43-e2f21d84e38d")
		)
		(embedded_fonts no)
		(model "CN3791.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic:SOP100P600X180-11N"
		(layer "F.Cu")
		(uuid "f1fa73d4-1ece-4ae9-9ee9-44b7fd5778ab")
		(at 127 139.25 90)
		(descr "ESSOP10 (5*3.9mm)")
		(tags "Integrated Circuit")
		(property "Reference" "IC1"
			(at 0 0 90)
			(layer "F.SilkS")
			(uuid "da742b2d-7f95-49d3-a901-d8b5eab2810f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "CH224K"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "a2a2c862-921b-4db6-b069-b694e7fe9687")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2204251615_WCH-Jiangsu-Qin-Heng-CH224K_C970725.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "4d28e701-c890-4a69-8c57-51bd63ac33a0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "ESSOP-10 USB ICs ROHS"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "708b18ef-1019-41c1-bd78-7023acbaeed3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "1.8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "07b68039-0c82-424a-9b11-2a2fb410dda1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "WCH"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ba9966fe-a128-4e60-8c9c-8009ab3764ef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "CH224K"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "26be2c1a-3729-4577-a1fd-33966973c768")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "87d937b3-93dc-4429-9866-f9aa424f0354")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3952bb5b-d5f0-434b-9877-717b2fcba49f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cd88002a-5444-47b0-805f-9ad54d3e4696")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0c2017a7-11cf-4c46-8b00-43abe10de4e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C970725"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1f439f1f-85e7-40be-ab42-f731c17e0a7c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/e54b9406-6388-4ea0-9a3c-ff1d4e346d52")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.45 -2.7)
			(end -2.05 -2.7)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "38a89cbf-639d-41f8-9235-3de0ea055051")
		)
		(fp_line
			(start 3.7 -2.75)
			(end 3.7 2.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "818f179e-d3d9-4e0d-a75e-a4ec1120afab")
		)
		(fp_line
			(start -3.7 -2.75)
			(end 3.7 -2.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5cb470ef-42c2-44a8-956e-8085dd4600b8")
		)
		(fp_line
			(start 3.7 2.75)
			(end -3.7 2.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f698a251-c581-4226-8d77-37903339df9c")
		)
		(fp_line
			(start -3.7 2.75)
			(end -3.7 -2.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "55333010-2f47-4180-b7aa-62ebad5d11ec")
		)
		(fp_line
			(start 1.95 -2.5)
			(end 1.95 2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc87121a-0df8-47ac-b50f-e12a47c32284")
		)
		(fp_line
			(start -1.95 -2.5)
			(end 1.95 -2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7315d653-645a-4c2a-a690-5ef866b593aa")
		)
		(fp_line
			(start -1.95 -1.5)
			(end -0.95 -2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "357e4166-5528-41cf-9f58-8f5ee9fc6b96")
		)
		(fp_line
			(start 1.95 2.5)
			(end -1.95 2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1ea1f640-f472-4e1e-99f6-5bcbb0bc3d34")
		)
		(fp_line
			(start -1.95 2.5)
			(end -1.95 -2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e28ce972-72a8-482c-8cab-2b1e365facf0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "f1514472-850d-4abf-8401-f5a04c308f04")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -2.75 -2 180)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(IC1-VDD)")
			(pinfunction "VDD")
			(pintype "passive")
			(uuid "f7c8bca1-1f00-4bc8-b9be-cd8942860d00")
		)
		(pad "2" smd rect
			(at -2.75 -1 180)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "unconnected-(IC1-CFG2-Pad2)")
			(pinfunction "CFG2")
			(pintype "passive+no_connect")
			(uuid "0521abe1-b5bd-469d-8f88-2712c8344c21")
		)
		(pad "3" smd rect
			(at -2.75 0 180)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "unconnected-(IC1-CFG3-Pad3)")
			(pinfunction "CFG3")
			(pintype "passive+no_connect")
			(uuid "e08db625-c40e-433f-a6f7-eff6a7dab0f8")
		)
		(pad "4" smd rect
			(at -2.75 1 180)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "D+")
			(pinfunction "DP")
			(pintype "passive")
			(uuid "d10c07f2-0618-435b-9edf-d317b9c48aea")
		)
		(pad "5" smd rect
			(at -2.75 2 180)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "D-")
			(pinfunction "DM")
			(pintype "passive")
			(uuid "e20b732f-2a39-4256-a0eb-6f173b1ae061")
		)
		(pad "6" smd rect
			(at 2.75 2 180)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "CC2")
			(pinfunction "CC2")
			(pintype "passive")
			(uuid "02564af1-b1f9-49e5-b097-f501846c3fe3")
		)
		(pad "7" smd rect
			(at 2.75 1 180)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "CC1")
			(pinfunction "CC1")
			(pintype "passive")
			(uuid "63ce785c-831d-429d-a6e9-8be47bfee509")
		)
		(pad "8" smd rect
			(at 2.75 0 180)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "Net-(IC1-VBUS)")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "feaff177-ea34-4666-b0a5-82b1c076a6bc")
		)
		(pad "9" smd rect
			(at 2.75 -1 180)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "Net-(IC1-CFG1)")
			(pinfunction "CFG1")
			(pintype "passive")
			(uuid "444ae261-be9f-4e6d-9b1f-8222239889f9")
		)
		(pad "10" smd rect
			(at 2.75 -2 180)
			(size 0.7 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(D1-K)")
			(pinfunction "PG")
			(pintype "passive")
			(uuid "7c334be5-76ab-4479-8cc5-1e992e988bc9")
		)
		(pad "11" smd rect
			(at 0 0 90)
			(size 2.3 3.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "2039ada4-7587-4451-bb33-5b6e83066342")
		)
		(embedded_fonts no)
		(model "CH224K.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "f316b5e5-37ed-444a-b8c5-ab48a1a66448")
		(at 113 111.6)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "b6cd3f5b-c47f-4846-9957-2d0b8b626f5b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "4c982388-33cd-4ddf-9624-d91854e16c45")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "288037a0-b9d0-4d99-b8fe-1b4ea14e6861")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b4b5b699-c549-437e-92c5-76311e35160e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/348368da-ad5e-4fbe-ac3c-75c0da2d5fb5")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b9042c10-45cf-4efa-b9da-9842ff8d50ff")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6c70e2bd-0cfc-4e70-aa36-ee1049131154")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0be2828f-31cd-4f03-9999-ad90c5d30ee3")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3cf55256-df80-4886-b833-d4415c3923fa")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ee2240d3-e788-4ec1-8ee1-67deaf46db43")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f2b4dc3b-0dd8-43df-b1b0-c1ac8e7281a9")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b7f0e59-caa2-4bf7-9f22-f39ac9d4f42e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0e9acdb9-1e61-4e87-aefe-c036720164d6")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc074140-ba8a-409f-af59-a32a54413885")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ea42c11d-94bf-4bf9-9ffb-ccb640dca06d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "00ea16c4-e472-4bed-ada4-602886f3ac0d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 40 "Bat Shunt 1")
			(pintype "passive")
			(uuid "241ef98f-f4e7-46fd-827f-baf3d0b1be7d")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 40 "Bat Shunt 1")
			(pintype "passive")
			(uuid "0319209f-c82f-4ddc-bf77-8cb29364a45c")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_EH_S2B-EH_1x02_P2.50mm_Horizontal"
		(layer "F.Cu")
		(uuid "f4cbd09f-c07b-4acd-b33f-3658054dce78")
		(at 150.45 92)
		(descr "JST EH series connector, S2B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH horizontal")
		(property "Reference" "J4"
			(at 1.25 -7.9 0)
			(layer "F.SilkS")
			(uuid "274a0893-4bfc-4980-a2d3-9ffbf6770a20")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "02375bd1-53d6-494d-96de-0499b0c45e38")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "19a31b72-cb44-4d42-b5e6-c8fd843b722a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8e1fd052-096c-4f2b-b68c-6eda33178c44")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/296868c1-3d5c-484c-b414-2dd158a853f3")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.61 -6.81)
			(end 5.11 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a4cdddd3-3619-48e5-9827-d87058502285")
		)
		(fp_line
			(start -2.61 -5.59)
			(end -1.39 -5.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ea9e2c7d-6d25-40ff-9400-84b9a98edb7e")
		)
		(fp_line
			(start -2.61 1.61)
			(end -2.61 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "63274bab-9463-49de-a17d-50cda3ec006c")
		)
		(fp_line
			(start -1.39 -5.59)
			(end -1.39 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "201e8ea0-e116-4a96-9cd6-9b94878e5689")
		)
		(fp_line
			(start -1.39 -1.59)
			(end 3.89 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a8e53064-c2ac-4dc8-98f1-566856203aab")
		)
		(fp_line
			(start -1.39 -0.59)
			(end -2.61 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "302207f4-968e-4ce8-b368-fdcda41d3beb")
		)
		(fp_line
			(start -1.39 -0.59)
			(end -1.39 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6b923c08-75b7-42f8-9037-f4935a4c25d9")
		)
		(fp_line
			(start -1.39 1.61)
			(end -2.61 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e338c447-3cad-4fe4-9394-235e60ab2a50")
		)
		(fp_line
			(start -0.32 -5.01)
			(end 0 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c5e02709-7dee-4d3c-9c13-d83d097e40dd")
		)
		(fp_line
			(start -0.32 -1.59)
			(end -0.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "72f04b48-8024-46d9-80e6-349f492e5a65")
		)
		(fp_line
			(start -0.3 2.1)
			(end 0.3 2.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b248fa9d-8fbb-4774-b11b-69992a82df21")
		)
		(fp_line
			(start 0 -5.09)
			(end 0.32 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "35ab41bd-ff3c-47bf-92ad-c5762eb0c6a0")
		)
		(fp_line
			(start 0 -1.59)
			(end -0.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d2085e34-cfea-4519-960c-9f481d3a3c3f")
		)
		(fp_line
			(start 0 1.5)
			(end -0.3 2.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "df42761c-a828-434d-906b-62d049a0692f")
		)
		(fp_line
			(start 0.3 2.1)
			(end 0 1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1909b930-b7c8-4a31-8c84-242cf5aa2a6d")
		)
		(fp_line
			(start 0.32 -5.01)
			(end 0.32 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b8a0bc7d-43b2-4314-83b3-acf51e753b08")
		)
		(fp_line
			(start 0.32 -1.59)
			(end 0 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "340661c6-05e4-4bd6-ae41-861ef9b38cd8")
		)
		(fp_line
			(start 1.17 -0.59)
			(end 1.33 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a1f0b3a-d5d9-4396-8f0c-35692237a07f")
		)
		(fp_line
			(start 2.18 -5.01)
			(end 2.5 -5.09)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "839ab2ae-e350-4554-9550-ccd0a474225c")
		)
		(fp_line
			(start 2.18 -1.59)
			(end 2.18 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3a35c5b3-24e0-4ef5-a038-e52d7011d76f")
		)
		(fp_line
			(start 2.5 -5.09)
			(end 2.82 -5.01)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6dc0b325-b1e3-4cc2-99f7-202db1194bc0")
		)
		(fp_line
			(start 2.5 -1.59)
			(end 2.18 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bace69ff-d6bd-4014-8458-6af090d465d6")
		)
		(fp_line
			(start 2.82 -5.01)
			(end 2.82 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e51f6615-7bfd-427c-9c59-825b9b9b322d")
		)
		(fp_line
			(start 2.82 -1.59)
			(end 2.5 -1.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f73de616-24e3-4d32-98cd-690a283345cf")
		)
		(fp_line
			(start 3.89 -5.59)
			(end 3.89 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4f4d449e-7734-47ea-8a0c-b4863ae8f177")
		)
		(fp_line
			(start 3.89 -0.59)
			(end 5.11 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ee825601-3003-42a5-8d3b-5baf17734114")
		)
		(fp_line
			(start 3.89 1.61)
			(end 3.89 -0.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ddbe3abd-13d5-4da9-b781-3c1f53061403")
		)
		(fp_line
			(start 5.11 -6.81)
			(end 5.11 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ca7a2af3-3e55-4a31-ba29-d6cbb556d7e4")
		)
		(fp_line
			(start 5.11 -5.59)
			(end 3.89 -5.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5932fb8b-729f-40fb-9a44-60fd605a8e75")
		)
		(fp_line
			(start 5.11 1.61)
			(end 3.89 1.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1e42c22e-7b38-4a2d-b935-248443570324")
		)
		(fp_line
			(start -3 -7.2)
			(end -3 2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9400b476-b2b0-42bb-a704-73399dd5d3b8")
		)
		(fp_line
			(start -3 2)
			(end 5.5 2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d8218ab4-3846-4f46-b5f4-0aab6b7e8f1f")
		)
		(fp_line
			(start 5.5 -7.2)
			(end -3 -7.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "193b76eb-410e-4e25-9481-d7cdb65ea664")
		)
		(fp_line
			(start 5.5 2)
			(end 5.5 -7.2)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ac355b19-43de-436c-933e-aeea12aab831")
		)
		(fp_line
			(start -2.5 -6.7)
			(end 5 -6.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ffe23eff-71ce-4f10-ae4e-4eb0b7e56e84")
		)
		(fp_line
			(start -2.5 1.5)
			(end -2.5 -6.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b3c9d5e8-e059-4b97-bb95-2e6fc1deaa2e")
		)
		(fp_line
			(start -1.5 -0.7)
			(end -1.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f135176-61c5-4475-89a3-9c30073e78b8")
		)
		(fp_line
			(start -1.5 1.5)
			(end -2.5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8bce553e-b34a-4566-be23-7e8bc9f11845")
		)
		(fp_line
			(start -0.5 -0.7)
			(end 0 -1.407107)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e4c703a-8453-402e-b189-ed1b01d9cc53")
		)
		(fp_line
			(start 0 -1.407107)
			(end 0.5 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d4b5c737-942c-4b3c-b808-1bc972b0e319")
		)
		(fp_line
			(start 4 -0.7)
			(end -1.5 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "55eb5114-4825-45b1-8843-cca03a52d8fa")
		)
		(fp_line
			(start 4 1.5)
			(end 4 -0.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1ab27096-bdea-4eea-bd22-e4857692fdf5")
		)
		(fp_line
			(start 5 -6.7)
			(end 5 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "726a4e57-ef45-4dd1-a63a-8f04d826e063")
		)
		(fp_line
			(start 5 1.5)
			(end 4 1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "193e47a5-5d3a-4e3e-9b53-3930010722fb")
		)
		(fp_text user "${REFERENCE}"
			(at 1.25 -2.6 0)
			(layer "F.Fab")
			(uuid "f90a2cf7-8d68-4a7b-a9ef-b44782248c9c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 40 "Bat Shunt 1")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "2367da7f-3598-44b7-9e2c-de78b6fe28ef")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "edabc9f1-5876-4c4b-a313-682764779498")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_S2B-EH_1x02_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "f7073d94-e130-4e81-a67f-b17392571436")
		(at 71.51 132.8475 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "fbae190f-05a9-4a54-b834-e7fb3ce5b6e9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "5d51f218-b2ac-4965-9661-497760a976e4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3e6e92cf-45db-44b7-aea9-772554e73ab7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d3ce9ba7-6a74-454c-a67b-6150e9806dcb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/b50c11c9-1724-4da1-8c0e-a2025eb4ca55")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4efe28e0-18d5-48ea-8875-20ee17248479")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "082fa8b1-c72a-4b2d-84b8-8858be386c9b")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0a8eb077-8c6f-4274-8139-6dded9cc51e0")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "937c15b1-bd2f-456b-ba60-6577983e691e")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4da814ce-91bd-464d-8733-6e2a3960513c")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bbabbed3-a7cd-4404-a4a9-162dd9f84ba0")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aed8ed7f-f9b5-49f4-954d-fa230d9dd1d5")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ac34e279-f391-4c89-a74c-4aedb0e471ca")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "255033aa-9433-49d4-81cc-16e2de8ba8ca")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bcd84ff2-ce69-498f-a57b-aa4f1470c5ad")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "92c8ec85-f76b-4fd0-a695-b264ec3327f2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "Net-(IC1-VDD)")
			(pintype "passive")
			(uuid "e9fa886b-d532-4036-97b7-23dcaf1637f7")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "c743ef2d-d32a-4e2c-a70f-ab97e7866bba")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPS:TPS2121RUXT"
		(layer "F.Cu")
		(uuid "f820a95a-cd65-4a56-b163-c013f94814fc")
		(at 116.4395 133.765)
		(descr "RUX0012A")
		(tags "Integrated Circuit")
		(property "Reference" "IC7"
			(at 0 0 0)
			(layer "F.SilkS")
			(uuid "5a7e0096-74f7-45ac-ab2c-82d1f4fd8b25")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "TPS2121RUXT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "fc72b89b-ee75-41fb-a8fd-0c3e043bc0dd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" "https://www.arrow.com/en/products/tps2121ruxt/texas-instruments"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e8b735d6-4cf0-4d6c-b3d0-24c11deeca19")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Power Switch ICs - Power Distribution 2.7-22V, 56mG , 4.5A, Priority Power MUX with Seamless Switchover 12-VQFN-HR -40 to 125"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8a0c61b8-c603-4220-9de4-240b413bd066")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5ac4833c-f8cd-4268-844c-2f34696235ef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8bb96b2b-baf3-4c8d-9a47-3cb1ab784c77")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "TPS2121RUXT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cff90eae-efbd-42c3-9cbd-d690aa465ef2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" "595-TPS2121RUXT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1dce4954-390b-4330-9492-d8800b1544b9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/TPS2121RUXT?qs=l7cgNqFNU1i6abJCbO5ulQ%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "467ad415-1ad9-4b4e-84d0-71641dd12b9a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Part Number" "TPS2121RUXT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "580a3388-13e0-4440-b63c-5abe5250393e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/tps2121ruxt/texas-instruments?utm_currency=USD&region=nac"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6f320414-ae99-4265-a464-6764dadfa4c7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C2156025"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fce4c1c4-61e1-401e-84e2-d8b60a094a7e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/57364ad1-cd13-46df-8637-cc8856f8d3ce")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.6 -0.4)
			(end -1.6 -0.4)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ef24a7f7-7194-44ef-8c2a-6c42474d8693")
		)
		(fp_line
			(start -1.5 -0.4)
			(end -1.5 -0.4)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c1cfbf24-64ea-4ce1-b4a9-fd866b3a8a4c")
		)
		(fp_arc
			(start -1.6 -0.4)
			(mid -1.55 -0.45)
			(end -1.5 -0.4)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b2fcff79-bcd2-4e95-ba3e-fdc6bdaa3d30")
		)
		(fp_arc
			(start -1.5 -0.4)
			(mid -1.55 -0.35)
			(end -1.6 -0.4)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "44e5a7e9-26b0-4bdb-b7b9-964ef80175a9")
		)
		(fp_line
			(start -1.9 -2.15)
			(end 1.9 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ce22a66-b738-4864-8d64-9839595fe892")
		)
		(fp_line
			(start -1.9 2.15)
			(end -1.9 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f9083d8-7da9-4915-a348-e16a831c0424")
		)
		(fp_line
			(start 1.9 -2.15)
			(end 1.9 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc4a644f-1fe5-4abf-bb9e-8506fefe6dc0")
		)
		(fp_line
			(start 1.9 2.15)
			(end -1.9 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8bf610d9-2f38-4478-ba0a-d98d06cf55ec")
		)
		(fp_line
			(start -1 -1.25)
			(end 1 -1.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2f73533-e62a-41ab-a639-57fbb32662c0")
		)
		(fp_line
			(start -1 1.25)
			(end -1 -1.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e4cbadf-f52a-4358-a073-610f2ec4fa65")
		)
		(fp_line
			(start 1 -1.25)
			(end 1 1.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6570b674-29ba-4a09-abe4-d8ed4d9c041c")
		)
		(fp_line
			(start 1 1.25)
			(end -1 1.25)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c4a75780-e15a-4730-b5d7-f0e61c15c94a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5ff9b283-4349-44c4-ac20-1403d5253603")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -0.675 -0.35 90)
			(size 0.4 1.05)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Sys Load")
			(pinfunction "OUT_1")
			(pintype "passive")
			(uuid "a02a0b1c-976b-402c-a554-4d27e7789f7e")
		)
		(pad "2" smd rect
			(at -0.675 0.35 90)
			(size 0.4 1.05)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "Bat Shunt 1")
			(pinfunction "IN2")
			(pintype "passive")
			(uuid "e2fdb4dd-d18e-4667-baad-6969c0bc9037")
		)
		(pad "3" smd rect
			(at -0.75 1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "unconnected-(IC7-CP2-Pad3)")
			(pinfunction "CP2")
			(pintype "passive")
			(uuid "acdf7919-e78f-4254-ad70-f2bc0b514ee3")
		)
		(pad "4" smd rect
			(at -0.25 1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "Net-(IC7-OV2)")
			(pinfunction "OV2")
			(pintype "passive")
			(uuid "7fb139bf-2adf-436f-8236-72542197820c")
		)
		(pad "5" smd rect
			(at 0.25 1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "Net-(IC7-OV1)")
			(pinfunction "OV1")
			(pintype "passive")
			(uuid "786a6a94-c897-4c49-a8eb-c550eacdd67d")
		)
		(pad "6" smd rect
			(at 0.75 1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "PR1")
			(pintype "passive")
			(uuid "a67ee2a9-d315-4bb6-8032-656688e9dad6")
		)
		(pad "7" smd rect
			(at 0.675 0.35 90)
			(size 0.4 1.05)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "VBUS")
			(pinfunction "IN1")
			(pintype "passive")
			(uuid "3890df50-5adf-4ab1-9b96-241984fc0413")
		)
		(pad "8" smd rect
			(at 0.675 -0.35 90)
			(size 0.4 1.05)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Sys Load")
			(pinfunction "OUT_2")
			(pintype "passive")
			(uuid "f85abed3-1ff8-4707-a4a9-1c05e5a17b11")
		)
		(pad "9" smd rect
			(at 0.75 -1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "ST")
			(pintype "passive")
			(uuid "7e72b340-dca2-4f8f-b73a-979bf8f435fc")
		)
		(pad "10" smd rect
			(at 0.25 -1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "Net-(IC7-ILIM)")
			(pinfunction "ILIM")
			(pintype "passive")
			(uuid "d4c512a9-e6f0-4c39-894f-1e06d6faaeb9")
		)
		(pad "11" smd rect
			(at -0.25 -1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(IC7-SS)")
			(pinfunction "SS")
			(pintype "passive")
			(uuid "d388eaed-5d06-4610-b25f-15024abd26bc")
		)
		(pad "12" smd rect
			(at -0.75 -1.15)
			(size 0.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "9e021aaf-360b-4292-915d-3b0ff7a15932")
		)
		(embedded_fonts no)
		(model "TPS2121RUXT.stp"
			(offset
				(xyz 0 0 0.999999985)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "fab7c077-ea14-4ef7-97ca-49bea80922c8")
		(at 68.05 113.6375 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(uuid "738c7bdc-08b3-498b-b374-fb803a75bd3c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "4e30d669-a082-41ca-99d2-b16fc5f2270f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e3b8da03-414d-4117-9f25-9fe3a249bb5d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8de2a07c-fd18-487a-966c-b8236af09332")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/a4f26091-217a-4fcb-9585-739b8cb48c50")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f77d054e-3e55-40a4-9c85-cf4753e391b2")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "56b6f427-9ea1-48b4-ac95-bdc51fc88043")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e9b85db1-d53f-447f-92bf-8c52145387d5")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f6698652-6e17-499b-b8ba-ae91c600c9ca")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fd268ca0-88c9-4a8c-aa92-bfc3f15c7fab")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3bc040b-4b7a-44e6-a409-0dc02a02c004")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00bf20b1-df74-4fb8-b0d7-70f30a53f554")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c4c4205-b5b1-4f35-a538-695ff1d4b97e")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a6d07ed2-67b7-4a9e-8329-221fb3d81d68")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f71320d-f0bd-466d-8252-a205c1de875b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "6863b845-3c93-4702-aa3b-578e53ed8746")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 4 "Net-(IC1-VDD)")
			(pintype "passive")
			(uuid "e11de2a9-c201-4e06-b817-4531c2334127")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 16 "Net-(D1-A)")
			(pintype "passive")
			(uuid "367d6eb6-b1b5-4fca-a36c-e1235661abcb")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "fb2a10ab-ff15-49e7-aaa5-d9cbaf56e579")
		(at 122.5 120.45)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R28"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "5e7f805e-cc7b-4a04-b1b2-869a4c602bbd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "23.7k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "59df8b75-01d7-4358-8040-491b9e0c2dce")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1648407e-efbb-4ac8-b751-c4510f739f86")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "97a50fd1-4274-44e7-863b-b00111356c53")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/9101b906-2ec4-4e50-9448-21fcf78df54d")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c4eb4e3d-88fe-409b-bfb4-714d2eb7b121")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a0410f13-146b-4d66-9dd2-8e574e3f96a2")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6770586d-58aa-4403-b1ff-245e04e6e350")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "95230e03-a34f-4a15-ad2c-906746f1ecd7")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d897f97d-d133-48cf-b810-61af0cb6e7e4")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6c691af5-b6cb-4d8a-9310-0a39e0fa5dd9")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3bb11c52-6187-4bff-84ff-00e76cde819c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9383e2ae-54be-40f5-b088-1a2ae90bc12e")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e535614c-3687-497e-99ca-b27f4f1a9bfa")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ce438fe-d7bb-4e74-912a-b5b677f25e99")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "269b39bd-5dd7-44a4-a236-695354d63704")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 34 "VBUS")
			(pintype "passive")
			(uuid "80b4dc77-908d-45ff-96f0-ffa4891b1b83")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 29 "Net-(IC4-OV1)")
			(pintype "passive")
			(uuid "2e0ef2b8-2fa9-48c7-9087-dc52722bdb3d")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "fdcb9837-b868-4412-b25c-a800f9ca0aa0")
		(at 177.5 103.5)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "3f2f9294-8e29-4173-b6f0-09020d52ef61")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "4fbc5aad-832d-4fa0-a8c1-ed76e0273e8e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0b5870b6-a6d3-4e5c-a61f-87fa10751a92")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "47feb04c-9da7-4060-b2c1-2ba0b83d605a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/fcf0e2d3-1699-4445-9fcb-6107a28dfda8")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9069914c-aa8c-484a-9e7a-8b9f1646d7ce")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4296f291-ade9-49c2-b3c5-28b4826e6f8b")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "85e95235-f913-474f-9d7b-33daa1b7dc1c")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "18807903-b610-44f8-b8d5-55467f8c239b")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3c4a99ff-35f1-4f72-82ad-27524f8201d5")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f2fa5f33-96f5-4c88-b964-e798551f0fc5")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7cf665c9-e2d9-45bb-b08d-f0df50c056d6")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "31c8384a-9723-47f3-b245-f53915197970")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b82ba588-3324-4dbd-96f9-9405042a3c1e")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a6931d92-171e-46ab-87a3-5be945689d51")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d6f2e120-e30d-4153-b06d-95f1070c78d7")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "VDD_NRF")
			(pintype "passive")
			(uuid "327ea53e-ef9e-4225-95e1-0ce8e6dc03ed")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(uuid "f8f0d728-8ca7-4033-80a7-bdab97daa827")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_LGA:Bosch_LGA-8_2.5x2.5mm_P0.65mm_ClockwisePinNumbering"
		(layer "F.Cu")
		(uuid "fed93031-67b0-4478-88d3-ae1da63e4eca")
		(at 178.975 91.005)
		(descr "LGA-8")
		(tags "lga land grid array")
		(property "Reference" "U4"
			(at 0.015 -2.465 0)
			(layer "F.SilkS")
			(uuid "405ce4ab-904e-4a79-ae54-59e0a867bc96")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BME280"
			(at 0.015 2.535 0)
			(layer "F.Fab")
			(uuid "1ecfa703-02c7-4369-9bc8-f155d2153bf0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.bosch-sensortec.com/media/boschsensortec/downloads/datasheets/bst-bme280-ds002.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "150694a5-91d0-4e32-81f8-7361f66f6031")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "3-in-1 sensor, humidity, pressure, temperature, I2C and SPI interface, 1.71-3.6V, LGA-8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "416d04f1-c1df-4bc7-be21-95015e84a5d5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C92489"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ff77c7e3-1165-4628-8012-6f92db51645a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*LGA*2.5x2.5mm*P0.65mm*Clockwise*")
		(path "/4e4c8d6c-4ffb-4887-974e-d494aba72112")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.35 1.35)
			(end -1.35 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b59dfc21-7b87-48f2-a81a-0a3b98a4deef")
		)
		(fp_line
			(start -1.35 1.36)
			(end -1.2 1.36)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "953f1c5d-ce5e-472e-a8fa-dfb5b153e229")
		)
		(fp_line
			(start 1.2 -1.35)
			(end 1.35 -1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e117091f-8d6d-4735-807e-a4b74e64fff3")
		)
		(fp_line
			(start 1.35 -1.35)
			(end 1.35 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d45d182e-f985-47ec-a9a6-d04f46fdccc4")
		)
		(fp_line
			(start 1.35 1.35)
			(end 1.2 1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "268ea325-fc58-44b7-9c01-7d3ff5d107f0")
		)
		(fp_line
			(start 1.35 1.35)
			(end 1.35 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fe6aa4c3-73e7-4d2a-8dec-9c3a5ed6389c")
		)
		(fp_poly
			(pts
				(xy -1.35 -1.35) (xy -1.71 -1.35) (xy -1.35 -1.71) (xy -1.35 -1.35)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "9d2d58af-9384-4279-a444-3ea8f345585a")
		)
		(fp_line
			(start -1.41 -1.54)
			(end 1.41 -1.54)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d0e58d1d-c6a9-4856-ae2e-0b625867338a")
		)
		(fp_line
			(start -1.41 1.54)
			(end -1.41 -1.54)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "23bff4fc-2763-4779-bf0e-7f32b54c04e2")
		)
		(fp_line
			(start 1.41 -1.54)
			(end 1.41 1.54)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "993545b4-216e-45d3-8390-3454b5a18b58")
		)
		(fp_line
			(start 1.41 1.54)
			(end -1.41 1.54)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "51f5542d-b6fc-4776-84c4-8f1fff737953")
		)
		(fp_line
			(start -1.25 -0.5)
			(end -0.5 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8fa17c25-1af6-4444-8e2f-b16aab514b0b")
		)
		(fp_line
			(start -1.25 1.25)
			(end -1.25 -0.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "763d1cb5-26e2-44af-a620-3307a44b47b0")
		)
		(fp_line
			(start -0.5 -1.25)
			(end 1.25 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a31bd974-17bb-4f64-ac68-a630aa8d417f")
		)
		(fp_line
			(start 1.25 -1.25)
			(end 1.25 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "25841be5-f66e-450d-b257-9af4b122c9e4")
		)
		(fp_line
			(start 1.25 1.25)
			(end -1.25 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "863312ee-bd40-479b-bdc9-6f8ca2483f25")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "f69c3b76-fd92-47b9-8624-b3a2e83ec164")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.075)
				)
			)
		)
		(pad "1" smd rect
			(at -0.975 -1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "42e32984-5cac-48e5-ba25-5fce342c6bdc")
		)
		(pad "2" smd rect
			(at -0.325 -1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "CSB")
			(pintype "input")
			(uuid "e9913d5b-5e87-4715-ab39-aefefa1899ad")
		)
		(pad "3" smd rect
			(at 0.325 -1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "I2C SDA")
			(pinfunction "SDI")
			(pintype "bidirectional")
			(uuid "41ca9d9f-ae6e-4ec8-a0a8-90d7b4cb36ad")
		)
		(pad "4" smd rect
			(at 0.975 -1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "I2C SCL")
			(pinfunction "SCK")
			(pintype "input")
			(uuid "08023ec3-31c1-4427-9be3-c5b69f842544")
		)
		(pad "5" smd rect
			(at 0.975 1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "SDO")
			(pintype "bidirectional")
			(uuid "b7a0ad92-4cb3-45d9-b28c-b10b7006d0d8")
		)
		(pad "6" smd rect
			(at 0.325 1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "VDDIO")
			(pintype "power_in")
			(uuid "8b9ce0e4-aaff-4d56-9fdd-9de932b55c64")
		)
		(pad "7" smd rect
			(at -0.325 1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "56d83438-6101-4902-9fcc-7a4b7a73198d")
		)
		(pad "8" smd rect
			(at -0.975 1.025 90)
			(size 0.5 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VDD_NRF")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "8be032bf-cc31-4e5b-981c-b3471d0a76b6")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_LGA.3dshapes/Bosch_LGA-8_2.5x2.5mm_P0.65mm_ClockwisePinNumbering.wrl"
			(offset
				(xyz 0.01500000025 -0.03500000059 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "meshtastic:SOT95P280X145-6N"
		(layer "F.Cu")
		(uuid "ffdc7de0-20bf-4ce1-be35-e199faab247b")
		(at 187 117 180)
		(descr "HMC433ETR")
		(tags "Switch")
		(property "Reference" "S1"
			(at 0 2.715 0)
			(layer "F.SilkS")
			(uuid "f646208a-df4a-4f29-bd82-8895334fd861")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "HMC544AETR"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "144e47f7-4159-41fa-b0c5-21794a71c6ea")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" "https://ms.componentsearchengine.com/Datasheets/2/HMC544AETR.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "34c91955-3aa8-4100-927c-d3fab87e81dd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "ANALOG DEVICES - HMC544AETR - RF Switch IC, Positive Control T/R Switch, DC to 4 GHz, +3 V & +5 V, SOT-26-6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a597d6da-ceae-40c1-9494-69353789ed7b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "1.45"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e391ae2c-45f8-435e-806e-54dbf00e124f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "Analog Devices"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "974f3e93-1ce2-4b62-b753-04c1eea9c0d2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "HMC544AETR"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4802b752-725c-4fc5-80cf-ff3abc8e1744")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" "584-HMC544AETR"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9974d1d0-c10d-4604-b95d-743abdc2ab00")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Analog-Devices/HMC544AETR?qs=UfUFg%2FkmHHF3BoWJNAxnfw%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bafd65a5-6b09-4296-bc15-083a6e44c4c6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Part Number" "HMC544AETR"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8df2efd5-dbc4-4a0c-96cd-e4aa56c71c0e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/hmc544aetr/analog-devices?region=nac"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "10cba12e-e4d2-443b-8dc3-4d0f5a10ede8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C579555"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8d60cafd-7a8c-4dd7-bacf-f240c3962989")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/325fb2e6-61ac-4610-8147-1bda06132cef")
		(sheetname "/")
		(sheetfile "meshtastic-node.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.3 1.45)
			(end -0.3 1.45)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7f39c8c9-136c-4c3f-bc63-bcaac916ef52")
		)
		(fp_line
			(start 0.3 -1.45)
			(end 0.3 1.45)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "254e29a1-26d0-4701-9d3f-0521deb1c496")
		)
		(fp_line
			(start -0.3 1.45)
			(end -0.3 -1.45)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84449b78-ba11-424e-865c-5ac43cae5537")
		)
		(fp_line
			(start -0.3 -1.45)
			(end 0.3 -1.45)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5a0a070e-573a-4f1d-a2e2-0636415aab88")
		)
		(fp_line
			(start -1.85 -1.6)
			(end -0.65 -1.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68fe20eb-34d4-4d98-b9f9-52afdff5a672")
		)
		(fp_line
			(start 2.1 1.75)
			(end -2.1 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a645d7bc-e69d-4d89-ab45-8536a1956fd3")
		)
		(fp_line
			(start 2.1 -1.75)
			(end 2.1 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0ab1fc1e-32c1-4a0c-8802-bf3271f571ab")
		)
		(fp_line
			(start -2.1 1.75)
			(end -2.1 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "143dcbbd-449f-4b62-ae97-5e4894748fc7")
		)
		(fp_line
			(start -2.1 -1.75)
			(end 2.1 -1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d1a72cab-ccc3-4516-b206-a1d9899d96a6")
		)
		(fp_line
			(start 0.8 1.45)
			(end -0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0ec875e3-89fc-4edf-a07e-737e7748d8a8")
		)
		(fp_line
			(start 0.8 -1.45)
			(end 0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51ce4f64-459c-4d4a-9dac-e4620f02c37b")
		)
		(fp_line
			(start -0.8 1.45)
			(end -0.8 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "662f307e-5402-41ac-be02-06293fa04497")
		)
		(fp_line
			(start -0.8 -0.5)
			(end 0.15 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b4257113-cbad-4b4c-9164-cb93e67dc24e")
		)
		(fp_line
			(start -0.8 -1.45)
			(end 0.8 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0b8d03ae-44e1-4da3-a015-8eae2970d3a0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.715 0)
			(layer "F.Fab")
			(uuid "2fac1f4e-e101-4120-9453-1f637e848c23")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at -1.25 -0.95 270)
			(size 0.6 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 121 "Net-(AE1-A)")
			(pinfunction "RF2")
			(pintype "passive")
			(uuid "41f3c3c1-b3ab-4987-82bb-d0841dd5c882")
		)
		(pad "2" smd rect
			(at -1.25 0 270)
			(size 0.6 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "5694a513-ffcc-4212-89a2-d6d9c200b37f")
		)
		(pad "3" smd rect
			(at -1.25 0.95 270)
			(size 0.6 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "Net-(IC3-RX3)")
			(pinfunction "RF1")
			(pintype "passive")
			(uuid "ffe520e1-0bc8-418c-9c2e-fadc4961911a")
		)
		(pad "4" smd rect
			(at 1.25 0.95 270)
			(size 0.6 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "USE_ANT_2")
			(pinfunction "B")
			(pintype "passive")
			(uuid "380af2b9-9606-4dd8-bdfb-057b3d8c35cd")
		)
		(pad "5" smd rect
			(at 1.25 0 270)
			(size 0.6 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(S1-RFC)")
			(pinfunction "RFC")
			(pintype "passive")
			(uuid "80a71f1e-7f24-4431-9c0b-bf74282d59ec")
		)
		(pad "6" smd rect
			(at 1.25 -0.95 270)
			(size 0.6 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "USE_ANT_1")
			(pinfunction "A")
			(pintype "passive")
			(uuid "8783a8ac-7183-4957-8cde-aecdb9b2bd9c")
		)
		(embedded_fonts no)
		(model "HMC544AETR.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(embedded_fonts no)
)
