(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+3V3")
	(net 2 "GND")
	(net 3 "+1V1")
	(net 4 "Net-(U2-VREG_AVDD)")
	(net 5 "Net-(U2-XIN)")
	(net 6 "Net-(C5-Pad1)")
	(net 7 "Net-(Q1-C)")
	(net 8 "Net-(Q3-C)")
	(net 9 "+12V")
	(net 10 "+5V")
	(net 11 "Net-(D3-A)")
	(net 12 "Net-(D4-A)")
	(net 13 "Net-(J7-Pin_1)")
	(net 14 "Net-(J7-Pin_2)")
	(net 15 "Net-(J8-Pin_1)")
	(net 16 "Net-(J8-Pin_2)")
	(net 17 "Net-(D1-A)")
	(net 18 "VBUS")
	(net 19 "KEYPAD_ROW_0")
	(net 20 "Net-(D5-A)")
	(net 21 "Net-(D6-A)")
	(net 22 "KEYPAD_ROW_1")
	(net 23 "KEYPAD_ROW_2")
	(net 24 "Net-(D7-A)")
	(net 25 "Net-(D8-A)")
	(net 26 "KEYPAD_ROW_3")
	(net 27 "Net-(D9-A)")
	(net 28 "Net-(D10-A)")
	(net 29 "Net-(D11-A)")
	(net 30 "Net-(D12-A)")
	(net 31 "Net-(D13-A)")
	(net 32 "Net-(D14-A)")
	(net 33 "Net-(D15-A)")
	(net 34 "Net-(D16-A)")
	(net 35 "Net-(D17-A)")
	(net 36 "Net-(D18-A)")
	(net 37 "Net-(D19-A)")
	(net 38 "Net-(D20-A)")
	(net 39 "Net-(J3-Pin_1)")
	(net 40 "USR_PWM_0_AUX")
	(net 41 "Net-(J2-Pin_2)")
	(net 42 "Net-(J3-Pin_2)")
	(net 43 "RESET")
	(net 44 "unconnected-(J4-TDI-Pad9)")
	(net 45 "unconnected-(J4-TDO-Pad3)")
	(net 46 "SWCLK")
	(net 47 "unconnected-(J4-~{TRST}-Pad8)")
	(net 48 "SWIO")
	(net 49 "Net-(J5-Pin_2)")
	(net 50 "USR_PWM_1_AUX")
	(net 51 "DISPLAY_RST")
	(net 52 "DISPLAY_BL")
	(net 53 "DISPLAY_SPI_SCK")
	(net 54 "DISPLAY_SPI_CS")
	(net 55 "DISPLAY_SPI_MOSI")
	(net 56 "DISPLAY_SPI_DS")
	(net 57 "unconnected-(J9-SHIELD-Pad9)")
	(net 58 "unconnected-(J9-DAT1-Pad8)")
	(net 59 "SPI_MISO")
	(net 60 "SPI_SCK")
	(net 61 "SPI_MOSI")
	(net 62 "SPI_SD_CS")
	(net 63 "unconnected-(J9-DAT2-Pad1)")
	(net 64 "Net-(U2-VREG_LX)")
	(net 65 "Net-(P1-CC)")
	(net 66 "unconnected-(P1-VCONN-PadB5)")
	(net 67 "D+")
	(net 68 "D-")
	(net 69 "Net-(Q1-B)")
	(net 70 "Net-(Q2-B)")
	(net 71 "Net-(Q3-B)")
	(net 72 "Net-(Q4-B)")
	(net 73 "USR_PWM_0")
	(net 74 "Net-(R3-Pad2)")
	(net 75 "QSPI_SS")
	(net 76 "Net-(R5-Pad2)")
	(net 77 "Net-(U2-XOUT)")
	(net 78 "USR_PWM_1")
	(net 79 "Net-(U2-USB_DP)")
	(net 80 "Net-(U2-USB_DM)")
	(net 81 "Net-(U2-GPIO25)")
	(net 82 "KEYPAD_COL_0")
	(net 83 "KEYPAD_COL_1")
	(net 84 "KEYPAD_COL_2")
	(net 85 "KEYPAD_COL_3")
	(net 86 "QSPI_SDCLK")
	(net 87 "QSPI_SD2")
	(net 88 "QSPI_SD1")
	(net 89 "QSPI_SD3")
	(net 90 "QSPI_SD0")
	(net 91 "unconnected-(U2-GPIO28_ADC2-Pad42)")
	(net 92 "SPI_THERMAL_2_CS")
	(net 93 "SSR_SWITCH")
	(net 94 "unconnected-(U2-GPIO29_ADC3-Pad43)")
	(net 95 "unconnected-(U2-GPIO27_ADC1-Pad41)")
	(net 96 "unconnected-(U2-GPIO26_ADC0-Pad40)")
	(net 97 "SPI_THERMAL_1_CS")
	(net 98 "SPI_THERMAL_MISO")
	(net 99 "unconnected-(U5-NC-Pad8)")
	(net 100 "SPI_THERMAL_SCK")
	(net 101 "unconnected-(U6-NC-Pad8)")
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "0e3a84d7-32bd-421d-9897-83a5f795a774")
		(at 134.647265 75.732387 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "0000234f-a5fc-43d8-9e86-b9018fc8a09b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7uF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "c3ae6b21-781d-4daf-97a8-c9b77948dc52")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "475d52f7-9961-4a9a-862b-92604b097e96")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "35bae20d-d7ea-41dc-8247-c22eb18f39aa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/f26c3e70-59f5-4c1d-ba96-67a4d35a5f42")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9b4739a8-9721-468a-9cfc-962789796f38")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "feba6f5b-48a5-4810-9299-51afe78f459c")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2f98e24c-3882-4777-ad4b-2d30db27c712")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5e900de8-3de2-4ee1-89f5-32442e159ac4")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "477c8cfa-1175-46f2-8fa4-3fe926846279")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b47de47b-454a-4b89-8c38-85949948a326")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "53517486-91cd-4626-a2c6-5c519a82efec")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f74c81f5-ec43-4194-a029-178dcd9612b0")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "68c10a1e-e318-4123-a17e-cfd459cc6e5f")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b18d0325-fe94-4bb6-bd96-2ff225c7cf00")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "c9b9f06c-8e13-455c-b37e-4dcc0bc98c5d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "ea667109-cfef-43ee-9b47-6229e479659c")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "fea9357e-f5ed-4d22-9905-c23d69c57383")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "10fa3a1d-e751-4661-8ec0-0711b83336ee")
		(at 77.75 82.85 -135)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C16"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "15861efb-5376-4242-8836-38eb1313aeb2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "95bbc650-603e-488c-99eb-b42ada3c8f73")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "573acc79-4f8e-4b1e-ad6e-db0cab66b0ae")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "ad17a41e-17a8-4865-a648-64f93af3d161")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/3f457cd6-e0e7-4646-9186-45798b91af73")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "82466ccc-1bf3-43d6-888c-3563f8f6fe7a")
		)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "971d4a4e-9bb5-406e-a6e1-7d767497cd61")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7a159006-3ea5-4a63-be1b-98425b3e50a0")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf1add3f-1102-4cbf-a794-33854dcff20f")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d07bdc91-312e-4a88-b55d-9ae12cd3fc99")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3b182c07-6047-43c0-8d34-8dfa7c66e7f0")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f8a982b5-1a52-4d4f-a841-03a9cd463543")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "867c8f12-fb62-45dd-adaf-cc1649359f20")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "36a41fa3-3a2a-4cb3-8213-f1e67b64588f")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "efb1313e-7261-435f-97ff-cfebd18688df")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "e59adcf1-6f9c-473a-9c03-a11f08026656")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 225)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "c87200de-d428-4cd8-993a-02bc92817bb2")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 225)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "1e7ab38d-0d49-4747-a0f0-180b846765a3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "11a006a8-ffae-4dd0-be4e-879651b12233")
		(at 61.5 86.5625 90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 0 -2.4 90)
			(layer "F.SilkS")
			(uuid "478654ea-9f4f-480e-873e-219f55783337")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PNP"
			(at 0 2.4 90)
			(layer "F.Fab")
			(uuid "7ed937fa-ae19-4213-bc2b-c2fa934c8050")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "389fdf64-898c-4f84-91df-de855007e6b6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "1c02896c-3a01-452f-bc41-10dafa884adb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "400d86d6-9fe2-4e0f-be2d-ac474d78f50d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d41d4ed2-ea16-4202-bb37-c58dc6710085")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f1d8df64-ebec-4341-bc4d-4638bab0eefe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/12c3fccb-b9ab-40f2-a98a-9836bf5dbb1e")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8743ffb9-c005-4677-a8a4-c0f351f0cf7c")
		)
		(fp_line
			(start 0 -1.56)
			(end -0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "96646bd8-0ba6-4d2e-9dec-4a09c47efe4d")
		)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "05ca07b4-4b5f-443d-8bf0-ef19230dff7d")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a644dda-b871-42e5-8182-754b74f893df")
		)
		(fp_poly
			(pts
				(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.84)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "83f8fe7b-f2c6-4e67-bc72-0e5a5d77965f")
		)
		(fp_rect
			(start -1.92 -1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "c8d6caa8-ba80-4445-9858-73012f4015e1")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f0e5dd14-21dc-4501-95a3-3876ea6513ca")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3cf52940-d2ef-41a4-963f-26b03372c159")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c1500779-32a8-4328-8dd3-4d44b9d08fe6")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "88955dc4-9f7a-498f-bd8c-7a8ca3419169")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a4bcdcbe-c715-4029-b45d-0f26f5bb4ee6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "0b160e42-44e9-488b-ac56-404ab64383a8")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "Net-(J2-Pin_2)")
			(pinfunction "C")
			(pintype "open_collector")
			(uuid "36e73a7a-a1b4-4a87-8ff8-d95bc0350155")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "Net-(Q2-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "ef62f350-853f-48d0-831d-c9d3bea3cb9d")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+12V")
			(pinfunction "E")
			(pintype "open_emitter")
			(uuid "8896afb2-2836-4260-8626-30cc8910b6a2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "15631f63-e295-4080-8a54-28baf8f28783")
		(at 64.2325 111.4125)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "213b5a9e-ac5a-4040-8f08-0f401269320d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "2800bda8-db81-4032-b271-2d13c04a6a25")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2de324b4-2644-4006-87a3-d201131f354a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bb928587-91cb-4cc4-b518-1a96d4ceeb6b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/9a4b48b7-7d9e-4752-bada-99536762c978")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "950358eb-71ad-441f-83e5-cd997c9fe85a")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d89bbc34-121d-415b-8a9c-28133aa1b3d8")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2d9d23cf-7c9b-4894-a5e9-c24d2d8b8a7e")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cb4e7a03-d712-4c7e-816f-62fb164422ab")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb0fdc66-cef6-403f-98b9-7a3132adc117")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c8a15523-c7b5-49c8-be87-4fbae0e727d0")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "670f7ec3-e784-4f3b-ac6d-639af7b5b5d0")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2d68a876-c76e-4b42-a0c7-bfd4f0751371")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "738ec1da-2b19-4039-8486-946d29432afc")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2fa992f2-23b4-4ed0-9fd8-22cde07ce5ce")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "6baa31e8-c59f-489a-924a-cd6dbe3df342")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 72 "Net-(Q4-B)")
			(pintype "passive")
			(uuid "97a8dbec-f4b8-4998-99ce-bf6d7854ed4c")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 8 "Net-(Q3-C)")
			(pintype "passive")
			(uuid "f9d636cf-d0ec-4ffb-9183-dc5a6d0b4407")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "1804f102-f29a-4851-a9b4-f799b9ad8282")
		(at 155.27 111)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "216e465b-55bb-4584-844e-90165213e138")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "33"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "03699e4d-7ac7-464e-a942-03e2474bf523")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "becb50bb-3cc1-46f9-96b5-809c18415efb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2e3ec89b-5613-433e-af29-e7e6221588f5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1382886b-9b3d-488a-b2ce-c032df8c6a14")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dcaaf604-81a8-419d-b5d9-4e11632b0e6e")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "60c632e3-73f9-436d-8b6b-bb919e684716")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c4b0b2e-f1a8-4790-a7f9-ef67c3238609")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "83ba2cc0-8abd-45ad-bcda-3231f961608f")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f9b790aa-9dec-4edc-bd20-38978e6c993c")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3432ecee-fcdc-4992-bab0-638395233315")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f0b785a-2d23-45ed-922d-34162a33cfa8")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "92375bce-deea-48c2-91db-ce991ab8c093")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51dee041-d6c6-4635-a721-85ce69283889")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9d41f24b-06f3-4972-865d-b4a0a43fd22f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "dfa8dbdf-c551-4c19-935a-64ece2427b8c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 4 "Net-(U2-VREG_AVDD)")
			(pintype "passive")
			(uuid "bb0654c9-fa7e-4e1b-9878-a4a5f2edba57")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "429849e2-a300-4335-beaf-1051aeaf1781")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "1947799f-8f79-4bab-a738-a1f2297c8050")
		(at 87.4 74.05 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C13"
			(at 3.358757 0.035355 45)
			(layer "F.SilkS")
			(uuid "808e2876-6979-4088-a47b-686c1fa5b0cb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "0b3fe555-374e-4fa7-8ec6-ac801052c500")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "e577d522-a961-44fe-a92d-081599edf204")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "4c6edd63-d3d1-4313-b220-1e368e359954")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/b582eea0-0b50-4a0a-b4c4-27082592dc53")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8ff1350b-8547-4fae-ae93-9e48df5c34c0")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1791e945-aad3-46eb-a872-af912f7f34da")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c169bcd7-73ab-492c-94f5-41a976495afd")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6574adf-e3b8-4dc4-b1be-2e459cc15775")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6efd2654-fe04-4ce9-90fb-074a4844f86f")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bed808ff-c3bc-411e-bbc5-b4a9a83bc4ea")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1d91188b-b438-4e4e-ba09-f14b5dd57c60")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a3f101ea-5f96-449c-b741-47c94fa591ef")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e6ce950-29e8-4033-af2d-b48d3c7d7866")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a9a49b81-0dc6-4689-b96e-3c89c46e3b99")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "e6ec80e7-8277-4c39-afa4-fb15ccf0c839")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "c2a55aa5-bc23-4388-82b1-8c7528798770")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "2f811711-842a-41e5-a62d-a53b39a8778f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "196054ba-05a8-4292-ab63-472a53387e53")
		(at 140.17684 74.459594 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "a01a4236-d6ab-4dc0-b937-3c68afeb96e1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "3cba7cbb-0ec4-4386-aae5-8ed3e6961e1f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "adc92787-6861-457a-b7d0-3cbf07c5a5cc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "025f980c-9b2a-4832-b43b-cb1be7725a43")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a23c640b-8e2c-46b7-abf8-88e1e86ba38f")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "95b2e8bb-65f2-4db9-a97f-ddf2feb1615a")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fe5fce5e-44c7-4650-aa9b-f5e212413b66")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8bcfa054-0f33-47b6-a5f1-e1de30094c3d")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a968c217-6c47-4ee0-8c4b-f250e4c9cd10")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3830222a-1dc6-4afd-9215-3a445e0cb4bb")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "08c7ccbd-042d-4ee5-914b-e82a8d2a421c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6b9d38bd-7eb2-4759-819e-994762b78b38")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb4d1f43-6d53-4962-9ab3-79fe0f9ed226")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d87f18a2-e0f3-489e-8bad-b55cde65ddb7")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f007b2b0-4c7c-4724-a8f3-4b4ba11bc696")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "590bb1ab-1064-4d95-90a8-3f4645badadc")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "+1V1")
			(pintype "passive")
			(uuid "9d23716f-de63-4f71-933d-8437ce5a89f5")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "73fa12b5-ec57-42b6-ba3f-06a357b8c974")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "23ad9857-60cf-4f4b-9e6f-70956ac748c6")
		(at 56.75 147.4575)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW5"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "23fc6d52-5375-4b04-849d-331e4e220e7f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "e36355bb-ea62-4f75-aaff-573459b0e5f9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e62e656b-ae1e-4019-bb80-4a8e6a053418")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c4873666-5376-48e7-9999-7d71b000359f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/e7a23208-6339-44b5-a5e0-f589766a7aaf")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7a669139-02b0-4176-8764-787103661c6d")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd9d8e31-e9b1-462d-b16d-d31ff50132dc")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "07a2073e-28a9-4126-900f-599893095e6a")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a205ebce-a876-4c44-9992-2a7f1b19c3c0")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "827a0743-ce4b-4e15-af95-0251df749bc4")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "06a65b06-b5c4-4993-af20-d64cfae9b777")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "e9243ab8-0a18-4959-bac8-616ca86e505e")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "9a54ceeb-467e-4e75-8432-99fc6bfc8d27")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d6ad5f2f-2c4d-4190-b3f2-c3b3d2ca96d1")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4b0e97db-b27b-4a55-aafb-d6aaf8b2cabd")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bdd0d299-7b74-42fc-8e30-9238023948f7")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c63af1b-c3f3-4866-bbd6-387c4303fbd4")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2181e738-9df6-4115-bb69-d6bd5d2e19c5")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e6c40978-ec2f-488e-8dbc-f5f411d7a6ef")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0590e9bb-4530-44e7-8f3b-44bce0f3f924")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bfed2671-14a1-407b-8c20-323f14db4dc1")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "7ef0efa1-e4cb-47d2-83c8-0a3d2178525c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "3970d0df-a42e-421b-9ee8-ec8a35b99b7e")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "18da5dfb-ec54-476e-92a7-3685d5731f2a")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "e63ab760-e7fc-4272-9823-254141bf4360")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "KEYPAD_COL_0")
			(pinfunction "1")
			(pintype "passive")
			(uuid "c582dd80-a1b2-46ef-a8d6-fa000120bf0b")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(D7-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "d2a91e49-d680-49a9-85eb-44936908ec7a")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "2752c331-2c51-4821-a5b6-4e9f2d9b792b")
		(at 95.11 147.4075)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW13"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "1c56ba69-9a22-45c4-bf12-dfba4d17541b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "a497ba45-c129-4c39-80e5-cf7e45274281")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6598e08c-f546-422b-8c3e-d12015fa47af")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cd5467a4-3266-4de9-8b0c-65db6e8c7edc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/ed067864-4173-40b8-b9b6-1511ecd3f4de")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "33438751-e12d-45c1-86a6-15557dc131f4")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5196aabb-ee66-48ab-ac04-5b13217b4c37")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ce982f45-9936-41e9-9adf-41ca718d7f58")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4da61e11-8074-4ec1-b267-8181f2b01005")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "145a2b91-4b04-448e-a53d-8458c3a92777")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "cd00b391-1b5e-4b34-99cb-7c68124ecbf7")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "3fc3b2fb-912e-48e0-a923-b75e354b63e0")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "2fc70619-7e6c-4756-a42d-7bab6064ca55")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fbc48933-d44a-4fd7-bd4b-03174c20e5cd")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "452b925b-f5d1-4e59-b5df-43187b4b8c44")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f2e5c206-645b-46ea-b1ee-6d74da3f84a5")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5576710-6d89-42e1-aacd-70952b7b7bdb")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15c66a1e-b909-4f3e-ba25-55e787e16294")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c3fa0c99-42d8-43ef-8f34-343f976ba34c")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d7121a0-d0bd-49ab-9547-0f1bbe4e003f")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6579eaeb-54cf-48bf-a40e-37510b6cc994")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "aac1cb6f-8fb9-4bd3-a3f9-b04a297d9baf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "5f85abd6-699f-4666-ae89-c8403331dcf3")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "e96479a9-7be1-45a2-bae2-517cafcac5dd")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "f2a0722e-7fff-4967-ad76-0b5de4d22d66")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "KEYPAD_COL_2")
			(pinfunction "1")
			(pintype "passive")
			(uuid "c7f1b35c-8fde-4a66-a9fb-0a02780ed008")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(D15-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "f74ce187-806b-469b-90e6-03dcaa90d8aa")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "285212b1-0367-44ba-8530-10bc80f80f58")
		(at 147.417613 88.502735 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "ea522d0c-c548-42e8-a89f-6048c08a69d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "4412963a-9d82-425c-beda-52d487e08568")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "754e4c08-527a-4984-aa6e-56eac8e58bf7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "e6e6728c-bc00-49b4-b8f7-24c5f183d2ad")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/4e09b638-9256-4823-9912-1d75ac4609a0")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "398e2671-c9fa-4b2b-b0bb-f26efee8d1a1")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9ef10d86-6117-4940-945f-ad71e311d4fd")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5a306284-4247-4092-9fa6-d818e0201a90")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "41bf92a7-7912-45c1-b9a4-59d4bec45a80")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "54d9c17b-45a6-4695-9a46-0b5067a9b085")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "283f30c7-a8f5-44e0-b2fe-4d8cd8d286b5")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cbe51fe8-f944-4778-a42e-6f9563d12ced")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1d77b3fc-7607-46ed-a43c-5af4dbc81313")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3010db9e-a786-42ba-886f-0cf3a9aa6d53")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a511255b-aae4-45dd-99e1-83c6956a0817")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "ba97644b-d6ae-4092-809a-36a4ce3f12d7")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "+1V1")
			(pintype "passive")
			(uuid "caa99124-75f1-4344-b85b-ec749834fa30")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "93300497-6160-4449-8e21-17c37650cd9b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "2919b863-47b9-4c59-8c8e-72381bd006b4")
		(at 160.02 113.95)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "14645686-a793-4588-a43a-3b397c24a338")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "27"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "e0ce81a9-96c6-44bb-bf78-f9f05f1972a8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3420baad-027c-4b89-bf4c-156e53887660")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e9b62684-3249-4f28-80b3-5d213c1230cb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/45e08493-3d7c-48a3-ba55-d6667c94776f")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2254c53-5385-4666-aa8e-d089c03f4fec")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6439a737-eef5-433a-8d60-73292ad8189f")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf169ffc-f7aa-4685-a410-dbe249c307ae")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3833b297-318b-48ff-8a2f-9eab7130e36e")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1c972388-2a54-4f64-a880-799133f5e370")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2dd6e39c-0408-426a-b457-475dbe02a9f8")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f41f1585-f4a2-43b2-99de-8d14441c374a")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "430a0f27-22e7-48da-86e4-ea63a3463363")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "60fa27ee-1f38-4ab0-b465-d77537ec0bce")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb8d5f5c-b56f-4a53-a5b2-0ba83261546b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "fe3ee2bc-b290-4d73-bee3-5770f1f42d63")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 80 "Net-(U2-USB_DM)")
			(pintype "passive")
			(uuid "309e4ebd-bca5-4189-b416-3881e3593760")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 68 "D-")
			(pintype "passive")
			(uuid "dad2d20a-74e0-4d4c-9b46-30a41a14b02a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "2a811098-6c39-448f-a4ff-340c1a334a58")
		(at 114.31 147.4075)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW17"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "174d9115-d44d-4ab6-91ab-11abcd840d7a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "140c0134-2692-45e6-9789-7cf1b786f517")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "eaec7de3-dcbd-4758-81b4-59f0d943b540")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "782aff56-31cf-4d84-b958-358fa79c84a6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/003b19c6-1ae5-4a0c-82e4-f7bbf830186d")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "acf897d1-5df1-4d5a-a717-a5292da7b39a")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "60469db9-3a02-430c-9c66-cf73923bf69a")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "da9d29d9-a003-4a9e-a969-4ff36c453f16")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "27d754c1-cd08-4c78-920c-c139e3ef3b9a")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "7b30ebfe-cbea-439b-a7d4-3a77a4aefd7e")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "8a1a375a-5fe1-4af1-8f67-08c18117d850")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "debb582a-46d6-4940-b5f2-058c301804a9")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "581b51fe-fa77-40a1-a8d7-44ab3a3b6116")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0b54926d-2ab9-418f-aaad-d405b8fa2e16")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "435ba197-5ceb-4c2b-9d93-688964915a3a")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "67e04fdd-2f9d-4931-8740-11d3460f50a7")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "60925314-edac-456a-8e69-ca63a91cf1c3")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d736b5c-d886-475d-8b61-b1cac5fcf187")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fe4855f8-2db5-4abd-aaf0-871fba61e473")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "52c72bee-e230-4bc5-a838-7cb379badb5e")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "402fe7ae-a9d8-427e-8441-f62d92c4b31c")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "796aba13-12c9-4154-9647-a526db94da2a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "83ae28a6-4b35-4f10-a491-0817f17cfc90")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "a4426016-b5d4-4262-bff5-5b74d1b3c1cd")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "37f3ec07-6092-4693-853e-7b1a6f6c49cc")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "KEYPAD_COL_3")
			(pinfunction "1")
			(pintype "passive")
			(uuid "ff7bcac2-9461-48e8-abed-3de0cb25a079")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(D19-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "15b64459-da13-4913-b1e7-93489ee8ae86")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Diode_SMD:D_2010_5025Metric"
		(layer "F.Cu")
		(uuid "2d5c5002-45d5-40d7-92a5-1ea52edbc5a8")
		(at 95.75 54.6 180)
		(descr "Diode SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D3"
			(at 0 -2.28 0)
			(layer "F.SilkS")
			(uuid "b0dad9da-68a9-47f7-8da7-f419ceb1b926")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "D"
			(at 0 2.28 0)
			(layer "F.Fab")
			(uuid "736375c4-91a7-48e5-87eb-7bef1ad2d28e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "76bdc134-52f6-44a0-a872-c4c17748f884")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9fee2903-2443-4e8a-8b77-cf454811ff1d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3f828c36-1d35-4503-ba70-2bc3c30fdc7c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b265c189-906b-4f5c-93a0-b7f1090be377")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6a3e78b6-f8e7-4fbe-ba64-17d17427f6aa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4249ae27-c307-44b2-8a53-41a7986c1aaf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/610f7f02-3d6d-410f-bf77-9974a049998a")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start 2.5 -1.585)
			(end -3.185 -1.585)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bbe45993-fbb4-4875-a7ed-1f8453f2662b")
		)
		(fp_line
			(start -3.185 1.585)
			(end 2.5 1.585)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cdbdf51b-ae52-436d-9b82-84da47dbd504")
		)
		(fp_line
			(start -3.185 -1.585)
			(end -3.185 1.585)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed83ba42-dc69-41d6-99cb-b417ec1f9f76")
		)
		(fp_line
			(start 3.18 1.58)
			(end -3.18 1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "007a30fb-b62e-42f4-a430-c240ccb2b443")
		)
		(fp_line
			(start 3.18 -1.58)
			(end 3.18 1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e9dfdc42-0cab-4230-9f24-eb1239b7cb50")
		)
		(fp_line
			(start -3.18 1.58)
			(end -3.18 -1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d17782cb-dc86-476b-ae6e-8bdc15b45a1d")
		)
		(fp_line
			(start -3.18 -1.58)
			(end 3.18 -1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1ebf619f-0bfb-46e8-ab26-50dbc92e54da")
		)
		(fp_line
			(start 2.5 1.25)
			(end 2.5 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "71787ac4-e8e3-41cb-8275-a48b75747fc1")
		)
		(fp_line
			(start 2.5 -1.25)
			(end -1.875 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e95da8e9-334e-4fc7-824e-b1d89ad5e8e4")
		)
		(fp_line
			(start -1.875 -1.25)
			(end -2.5 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "466367ea-5cc0-46d4-9eb7-49177558587c")
		)
		(fp_line
			(start -2.5 1.25)
			(end 2.5 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "994968d7-8555-4933-9a6c-13f67e0ba4e9")
		)
		(fp_line
			(start -2.5 -0.625)
			(end -2.5 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "64eaf8fb-4976-473b-b8e9-cdc7d2168bbf")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c3703e58-892a-485a-b11b-364c9c437852")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.25 0 180)
			(size 1.35 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.185185)
			(net 10 "+5V")
			(pinfunction "K")
			(pintype "passive")
			(uuid "1384b498-c426-45fd-a52b-8935370e5892")
		)
		(pad "2" smd roundrect
			(at 2.25 0 180)
			(size 1.35 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.185185)
			(net 11 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "64858302-d989-4e3e-aa5f-37c37f64963e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_2010_5025Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "2dbb78a6-e9f5-4655-9f8f-ee41436fe25e")
		(at 114.31 128.2575)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW16"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "333d41d9-52ae-4736-9e21-cb5d831bc2df")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "033b6b14-4f9b-4fbf-b94a-edc73ee48fce")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "789cd972-8fe9-4fbb-96d8-957388526c52")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1300382b-4ee4-4ad5-b54f-0174502d3dfc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/12ec19c6-8238-4a8d-b694-8136d6023786")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d6e8160a-c890-44a2-991b-c2da2e21d35a")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7b9d5a2f-4a63-468d-8dd4-b1893743cf0c")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e753898-ae08-4d6f-85ba-4664f63a0f0f")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d62eeb2-fe32-4e13-9d3a-d3c5c2cb261d")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "56b324a6-f00f-4f0d-8e23-47f0b2f1f39a")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "7bb0d73c-954e-4f1e-bf46-d91896040ad4")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "16ed8a5d-21ba-46cc-92cc-79e8e9533d6f")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "97f921b3-d349-41b5-9f01-2ec3144f40f3")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e7e33d44-1939-4ad8-b98d-70943cb109d4")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a83d02f7-9d7f-478d-8ccc-73c4afef8bac")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a0ea3b05-d4fa-4316-b709-f2a1c31c48bf")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f298d429-7b43-4408-b96a-87140d71bcb1")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ab91060-8f09-42a3-89cd-fef71edd65dd")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b388ecf-39ab-4c25-abf4-c5b002975370")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "85ebc4fa-a687-457b-b853-8b468a01343f")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37659789-927c-4cd6-b404-45268e24c634")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "09a1dfd7-eacc-46a7-a6c5-88db6a70e6c8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "14812386-a40d-47ce-a583-2c990464fafa")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "98c28797-bc35-434c-98d9-6c2c0eea0675")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "1fc5ecf1-a3b5-435b-ad35-2755390ab2b7")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "KEYPAD_COL_3")
			(pinfunction "1")
			(pintype "passive")
			(uuid "5a40ee01-161b-4f97-9132-4e194956bd56")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(D18-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "339ef4bd-3171-4bc2-911a-72b69b496e08")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "33b3c78b-9a2a-424b-b109-eea6fb4e4986")
		(at 75.91 109.0875)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW7"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "1c444ab2-85ca-4c47-91a4-a00a364add7b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "c615bebc-5466-44e4-9e04-3d74dd08eea0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8a146b18-755a-428d-bb63-12dcf1462ca1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "aa55d3ac-d06d-48c6-aa4e-4250575e8217")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/02762e2c-6dfd-415e-b65e-0a3f2f1e64a5")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9e1744d3-ba5b-4620-a109-4ef7fd8603fb")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1e4becf1-4fb2-4d72-b709-c7d4ed6c9427")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "066fd8ce-e17b-4396-afc2-5e0a98df154a")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "67d180e5-6143-4a4c-9c72-b231b58b7696")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "0a64655e-6390-4007-add9-2e0b71839d64")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "423e758f-ae56-4abc-9404-6b71b708c876")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "8f3b0f23-3f8f-45ec-bdab-7779d94e3d0e")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "66433a9f-3f7c-4e0f-bf53-e0af3b44269a")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c9095b17-96bb-4c56-8cd6-48160746ae8d")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c0e068a0-ed5b-4ee3-998b-0d9336fc49c5")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e8a1e50d-91f7-4a62-92fd-7179619c2c54")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "674b5ea1-326e-4050-a9a4-59e992660be0")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c30da0a-3f58-4f7a-99d2-fdfeddd6bcef")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ef7d25dc-21f2-44c3-85af-e9ef1cb8884c")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32abfd50-2027-4532-9f65-98899681a639")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "774d7c92-26ba-4d53-8114-5a3bca69f0ec")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "c7ae079c-69db-4be0-b61d-2023f0d22d7b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "923d85fb-f979-4439-b4eb-ea2af5a1ee6d")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "65369c15-7faf-45bd-8a76-c9cc1498b1bb")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "026a0c2b-2400-4ac6-a61f-914057040577")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "KEYPAD_COL_1")
			(pinfunction "1")
			(pintype "passive")
			(uuid "61fdf4fb-a435-44c9-a463-4e3c7166ae2d")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(D9-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "4c3f697b-3066-46c1-8aa2-3ee10a38b942")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "34e76a0c-60a0-4665-a4ea-c354c35f8366")
		(at 56.75 166.6575)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW6"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "2c5f74e3-61eb-4b3a-b4b0-d8d797b7c590")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "5ee4ed2a-838e-4991-b26f-11bf88f0f18a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b5b47f80-225d-41ec-a97a-32fe76376d72")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f351c1ee-2e14-456e-931e-e3f37b5c0b2c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/d7d9eb16-2e83-4b05-85d1-506f574a4eb2")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0ba7552c-dcd0-4eef-83d0-c633aed56bae")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4e692afa-5d3d-4125-ba64-b0ec19119b31")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "efb24f84-87ef-40ae-871e-d22abc6700ac")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f922e2ab-29e3-48c0-81f0-c8a0534719ad")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "b11fa579-f763-47af-a66e-71f1a4c50d69")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "f3cbea9f-6edd-4d40-98a7-e8a25e2afb0e")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "6a7b5ba8-c5d0-4056-a891-cccd70d9274b")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "65549ba3-7817-49ad-974e-8d74c5c055c6")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "97058f2d-ea20-49cd-b19a-23148d294a2b")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4eafba5b-2ee9-4e65-b131-06093e2f5a17")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b49cbff6-056b-4ed6-82a0-91fafcf5e72c")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4e9c3d72-38a6-4060-b0a0-aeb5fb8bcf3e")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "875a1742-662a-431c-8a6c-357e4daac49c")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4fa053b8-07d2-44dc-86cd-6f0faa4d226b")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9876d0a2-624a-41c1-839c-1569bda310d8")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "abe57aa3-4e78-4b49-9bbc-37b86b641daf")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "e68192ad-7f3a-4fa9-822f-9d829aac2e3c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "42af2a89-7950-45f8-8d54-f81243deeb7d")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "3bc33853-fa0a-40a0-804e-62acf4e97ead")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "2f5d6a4e-1f62-4304-994f-c841ae8dd86d")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "KEYPAD_COL_0")
			(pinfunction "1")
			(pintype "passive")
			(uuid "ddce6842-2aac-490f-b4a2-b3e9e12ee3c9")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(D8-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "2fde1d2d-1d7c-4479-9319-0e381210eaaf")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "373aa0b6-33ec-4b5c-a2c3-94e063fc3ec9")
		(at 75.91 147.4375)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW9"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "3069b090-90fb-449a-822f-5bdbdbc0ce28")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "9d41b78f-24b4-4407-ada9-d8e6c731a60c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "32e70039-64d7-4eb9-800b-a0563e576de9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "45c4ae0e-61a3-4cd6-a998-af24383b86b9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/045c1bf7-a59a-48d8-a17a-b0852d45461c")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e948bf9e-7455-4144-a52f-7197a0b1b73a")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84d8df84-361f-4f31-b90c-112da2a92a33")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e1d5c964-5ac7-4951-8fdb-2ec457587c95")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0cec1558-d751-40f6-9f13-27e3d941b19b")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "1b1b7155-0334-4bca-8698-5ee491addd23")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "0817482f-b6f4-4fde-a704-563d5db62ed5")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "0bb9bafa-8888-4905-8a10-41e3390cda9a")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "08dc44e5-7117-42ed-9fbd-a7023947bd24")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0f499465-5484-4e6a-a43d-0c1cfd5d39e2")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12524cce-043c-472b-a7c4-dc9994ca321e")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07061477-2bf1-49fe-829d-336c3afe1a79")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b4f14698-9c52-484d-ba74-369fb5ae25c1")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7376a1b1-e359-4559-bb3b-63438e4d5bb6")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "994f36ee-4c89-420a-ab70-366a7052d03e")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c4b165b0-6338-4a12-8131-7c54e56fb632")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "44ac0bfb-40ac-4b17-9528-bc55635ba89c")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "3f6024b0-dd37-4cd5-8001-5b06fb8dfae5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "176452c3-f155-4179-834e-89d87eefb11e")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "7dabdc0c-82e2-4cf1-a811-b5ba706014aa")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "22785bd9-87e0-47cb-a51f-9ab465b12755")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "KEYPAD_COL_1")
			(pinfunction "1")
			(pintype "passive")
			(uuid "6dcbd722-d95b-4518-ae6e-06db8392fe0f")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(D11-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "f3d67898-b04e-4e2b-99f2-7670fb1ec051")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "3b6badcb-cc14-44a2-a5c7-d6b8a5e73dd5")
		(at 64.2325 99.6125)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "f71940b3-51eb-4cc7-85a6-40e767cb19ee")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "a1062677-6fe7-4349-9404-745715f4e22c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "89be11ce-d1cc-4959-a95f-2757b9996df1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b50467a4-f2a3-4e7d-a462-b7f7c96f7acf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/6f8686e3-f64f-4e49-9c1a-fa3722a58bb9")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4e6f92cb-a24d-4e96-ade5-e16d0cee5c59")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "411d87cd-b903-4105-9ee7-cad064c655e6")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12e9f481-32f4-48ed-9f08-cd070ff859ba")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6d138673-ad22-41b8-8982-1a5b39e1fbd7")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a86bce6d-0963-4e04-b426-050b615e9a50")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2ca1b70a-83fc-474d-9f19-5811ec10ff32")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f37e3146-223d-4acf-a832-16a6e2ea2c76")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb67f21e-2cec-4ca2-a33c-798bac38bd71")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b484206-f30f-4637-9206-8021cc3e07b8")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "798dd1e7-91bf-42e7-a2ff-6f26e9c461fc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d4e14d50-ef8a-49be-9190-12ee19459f66")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 78 "USR_PWM_1")
			(pintype "passive")
			(uuid "fd78683b-3656-4fd6-ac57-e80ac36c213a")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 71 "Net-(Q3-B)")
			(pintype "passive")
			(uuid "125a684b-db3d-4437-9f82-9f3a76b84102")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_2010_5025Metric"
		(layer "F.Cu")
		(uuid "40c3ce8f-92db-45cc-b46a-584f09958e7d")
		(at 93.25 89.7)
		(descr "Diode SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D4"
			(at 0 -2.28 0)
			(layer "F.SilkS")
			(uuid "a9c3f76d-3be0-4280-8ea0-c2ea477c48c9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "D"
			(at 0 2.28 0)
			(layer "F.Fab")
			(uuid "fd9009cf-5721-40ec-a2f2-2e303f5cd562")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "62b6e69a-365a-454b-85bd-3fbc0db1a4e3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "de6cb728-123f-4d6d-8cb7-3133bbcd93f0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0a516b9d-9339-4e85-b7bd-b9af5121b031")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2349b668-a9cc-4703-a536-0676b114e52d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "14359add-1b5a-4756-b554-6240f1c6aa67")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "84f7bcb5-d1eb-4d8e-b55a-bcaaba574d18")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/4a4747bc-b6b6-44ee-8bed-d81eb9a8e7eb")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.185 -1.585)
			(end -3.185 1.585)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d8b6eae-7d3d-4f05-b179-7cbeff75924b")
		)
		(fp_line
			(start -3.185 1.585)
			(end 2.5 1.585)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7b8c6e43-3bad-4cef-b997-1e12d31e3dfe")
		)
		(fp_line
			(start 2.5 -1.585)
			(end -3.185 -1.585)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4f357f17-6434-4554-866b-5bd6e4d0deca")
		)
		(fp_line
			(start -3.18 -1.58)
			(end 3.18 -1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "15a54f1b-abe3-4d3c-8280-f5b0b18c58d5")
		)
		(fp_line
			(start -3.18 1.58)
			(end -3.18 -1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0f2cddb9-1be6-49cc-8f1b-34a53a6995aa")
		)
		(fp_line
			(start 3.18 -1.58)
			(end 3.18 1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1005aafa-98d9-4b07-83fc-a736df49edc0")
		)
		(fp_line
			(start 3.18 1.58)
			(end -3.18 1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1fe9350e-39cd-41c1-9136-3e5c3183feef")
		)
		(fp_line
			(start -2.5 -0.625)
			(end -2.5 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca452d8c-3177-4048-93ba-4ad5461ec5a6")
		)
		(fp_line
			(start -2.5 1.25)
			(end 2.5 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca0e775a-ccab-4777-82ec-8dc79182db01")
		)
		(fp_line
			(start -1.875 -1.25)
			(end -2.5 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8da967f8-497e-4fbc-8dd3-3868548833ee")
		)
		(fp_line
			(start 2.5 -1.25)
			(end -1.875 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15b95e6e-590b-4021-94aa-25f10c32d7b3")
		)
		(fp_line
			(start 2.5 1.25)
			(end 2.5 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2e01018c-bd36-4c98-bc6d-9db783a2ed49")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "afe6961e-f511-4a65-a88e-40f49c3dbb09")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.25 0)
			(size 1.35 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.185185)
			(net 1 "+3V3")
			(pinfunction "K")
			(pintype "passive")
			(uuid "db0443b7-cf6b-42b0-958f-f5e88edfe591")
		)
		(pad "2" smd roundrect
			(at 2.25 0)
			(size 1.35 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.185185)
			(net 12 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "9f51bdfb-2c44-40ee-aa01-b7960b218eb6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_2010_5025Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "429bc2fe-8903-4c3e-96bc-f0103f8e40f2")
		(at 56.71 109.0975)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW3"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "558fd007-f104-42e0-82e7-ce71af2f68dc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "94b56c32-1fa7-4511-b11d-d30bcc8ebfb4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "15decdd4-64f2-4e5e-8fe0-955fefd0e953")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "14f193ca-371e-4f94-a6f7-a1afd29a8428")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/d780a094-f79a-444b-8ee4-6ceade4c0e77")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "557171ae-6d94-4dcd-839a-288f3c3bbde6")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "431360cb-bd84-4147-8126-3461c03ee7cc")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "217e2b76-5a63-446a-a9a1-fbdf5cb92960")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "205c3436-4851-4193-907d-cbded569cf7d")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "3972c4cd-8391-43c5-8054-4efad34c3080")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "9b991231-93a0-4b9e-ac67-14f3a78a5f7d")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "910d6144-cb62-4965-93de-7f2402636efe")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "9bc080c8-2459-4e03-84d0-730c78a7c1a9")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "edfcfc6d-d586-479e-ab99-53ec0b5b88a7")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "76918c1c-4cc2-4443-89e4-cc0a9045058a")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0c0c6d4b-fc6a-4efe-b93c-3d0197f4e2c7")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5458536d-8d20-4c88-b9b9-da9d580e1e19")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f971e4c6-7242-4a34-b140-41017ba65e18")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3289ce66-cf45-4502-9e66-acefb1e5e213")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c9968b5-f355-4f98-ba10-932a6eef2cd2")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2b59f03c-206e-46e0-b16f-360a10069222")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "bbeb80b0-b43d-4877-9738-74ebf3aacaf2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "405e612c-a26f-4180-ac66-196fe115dbd9")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "f717ab35-048e-48b9-8a1a-c37a36e07dfb")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "0d8af5ee-6ce6-41a6-9d56-b453d6c74309")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "KEYPAD_COL_0")
			(pinfunction "1")
			(pintype "passive")
			(uuid "d247b087-c453-4c99-adad-ed14b4f7df79")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(D5-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "bc3ad8ca-516a-487c-aced-6b7137f06a39")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "453fb44f-5ee2-4302-8714-ac08535e4288")
		(at 146.775 127.35)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor handsolder")
		(property "Reference" "L1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "83323d9c-301d-4880-89c3-5a937bb9d015")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "3.3uH"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "663e1b3f-b829-4de4-80a6-c22ca053d9f3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bc212abb-b223-4f85-8ad6-5a147ce3cf3b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "894571c2-db7b-48fb-85f1-50de4c2ce919")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/b370158b-3186-483c-80a3-3a0c953e6aaa")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.171267 -0.51)
			(end 0.171267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cceb2884-b7e4-45c3-af89-dd6f6948a212")
		)
		(fp_line
			(start -0.171267 0.51)
			(end 0.171267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cf534cc7-4ac4-486b-935b-f84e4dd6e31f")
		)
		(fp_line
			(start -1.65 -0.73)
			(end 1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "289e497e-c729-4990-9ccf-5156a126639d")
		)
		(fp_line
			(start -1.65 0.73)
			(end -1.65 -0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "80480da2-607a-4caa-a084-8ba9778c04cd")
		)
		(fp_line
			(start 1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e085de1c-6ae4-4394-bb7d-9c5d44fda336")
		)
		(fp_line
			(start 1.65 0.73)
			(end -1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f8fe567c-df87-4862-ae53-8e1fcf288d61")
		)
		(fp_line
			(start -0.8 -0.4)
			(end 0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8eb8bcfb-9c9b-4543-b082-d4c6e5f3a995")
		)
		(fp_line
			(start -0.8 0.4)
			(end -0.8 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2e1c473e-2858-40af-afb3-706adbe19a92")
		)
		(fp_line
			(start 0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "61640f2a-b139-442e-be71-a38c55952abc")
		)
		(fp_line
			(start 0.8 0.4)
			(end -0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cdf913b2-fb87-4d04-afe3-6bc815171d2c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d15de8bd-db49-4c2d-8616-400e47e0af83")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.875 0)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+1V1")
			(pinfunction "1")
			(pintype "passive")
			(uuid "9d74d030-44b2-4bf3-a157-f565efdce35e")
		)
		(pad "2" smd roundrect
			(at 0.875 0)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "Net-(U2-VREG_LX)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "fc584daf-37f2-4c24-8ecf-b68c5d473807")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "457ced74-4f6f-4678-8295-17ef4d6aa2e5")
		(at 56.72 128.2575)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW4"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "1896fef1-5fb7-46a7-a641-31fb22bfc3bc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "22a0780f-e8d8-4fd3-8c3f-6abf9cd2f66b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "97666a17-6d98-4bac-8f85-4efe1a6dfb21")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b3e5eb01-ce57-46e4-ad92-d24eab27691d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/c493d526-6676-4509-bba0-3f2ba2caa6fe")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5a7c04fc-21f3-4f22-9183-5d7ead0160f1")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eed9be05-8d6e-4cab-990f-92760492f6c8")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9309c278-ed9a-47e0-bd4b-3c6141e37be1")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73e481e0-89de-4915-94a8-cfd4f6bcdd77")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "a9c31631-e976-48ee-a64d-d7d68a26c30e")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "4f92438b-30c6-41b0-87b7-ad238e3651b9")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "a42d6302-7a26-41f5-af4b-9d5f8fcaa2f0")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "03afe4aa-65c5-4678-8f54-d3e18d39b8a1")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "20fa1b65-8ca1-4ece-a8c8-f17cbaedf650")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c7122e0e-d84c-4f62-85e8-70f7ac54f947")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9327d23a-a9b7-4034-85a9-0713ac342982")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f9110b40-8d3f-4fa6-ae64-2b32f540b86e")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eccda702-59f0-4fdf-892d-526d64d82296")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6fbfc8e8-3332-4208-857b-b8c7d47c1350")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c181c526-14ea-4981-8201-c146eea8ca7c")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "db10190d-64f6-4984-9374-52b9cf9e1cb3")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "ce99f5fd-cc14-44fe-82de-409366acda9e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "9b4fc9dd-bd3a-45af-a1b1-7669b2dea3b8")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "769e279b-b1b9-4a67-b366-ab8793f1ab7f")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "adfaf38c-5434-4687-ab52-e38d4a7560b9")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "KEYPAD_COL_0")
			(pinfunction "1")
			(pintype "passive")
			(uuid "765e7e12-d64e-4471-97c7-058015cabe7e")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(D6-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "eed00bb8-34cb-4c4c-bb0d-89259c39e25c")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical"
		(layer "F.Cu")
		(uuid "4c16b89d-f66c-44e2-a504-92750300c255")
		(at 82.07 63.27 90)
		(descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
		(tags "Through hole pin header THT 2x05 1.27mm double row")
		(property "Reference" "J4"
			(at 0.635 -1.745 90)
			(layer "F.SilkS")
			(uuid "51c910ab-0f21-4d56-9404-2154e1fd554f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "AVR-JTAG-10"
			(at 0.635 6.825 90)
			(layer "F.Fab")
			(uuid "d9a98a25-92ba-4d8e-92ab-7d65222e5c83")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "194205a6-758e-4d30-88b0-bbfe3895afdc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Atmel 10-pin JTAG connector"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "76557ca7-f2f7-46bb-9528-150532316feb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "IDC?Header*2x05* Pin?Header*2x05*")
		(path "/57514800-ac8f-4238-ae93-771131c4b7df")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.18 -0.81)
			(end 0 -0.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e1731a57-d83a-4c0a-b6fa-a586d4363204")
		)
		(fp_line
			(start 2.45 -0.745)
			(end 2.45 5.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3e33c84d-1aaa-400c-b973-644d482e51c4")
		)
		(fp_line
			(start 1.587923 -0.745)
			(end 2.45 -0.745)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49eba6fa-a72a-49ab-93a4-9a68e878c865")
		)
		(fp_line
			(start -1.18 0)
			(end -1.18 -0.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2593ce6a-0519-44d4-a0d9-54974d16753c")
		)
		(fp_line
			(start -1.18 0.81)
			(end -0.666708 0.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d2a4e905-f21b-4ff0-912e-d06e27bba3b3")
		)
		(fp_line
			(start -1.18 0.81)
			(end -1.18 5.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5caa9c9d-b034-4909-a7e3-195256ec1af6")
		)
		(fp_line
			(start 1.587923 5.825)
			(end 2.45 5.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c4b8cc4b-5077-4e48-9ec8-a86553a92f6c")
		)
		(fp_line
			(start 0.317923 5.825)
			(end 0.952077 5.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2c0127fa-2743-450d-a255-54e04e2ae79e")
		)
		(fp_line
			(start -1.18 5.825)
			(end -0.317923 5.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1e980a15-7b35-4616-b8cb-bbff3a33468a")
		)
		(fp_line
			(start 2.84 -1.14)
			(end -1.57 -1.14)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e91d376c-d45e-4ed6-8a6e-1ca0ba5cd64d")
		)
		(fp_line
			(start -1.57 -1.14)
			(end -1.57 6.22)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf90a9b4-7759-403c-b10e-93fe2ab02702")
		)
		(fp_line
			(start 2.84 6.22)
			(end 2.84 -1.14)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1f92cd58-dd0d-401f-9b7b-42db9d5823b7")
		)
		(fp_line
			(start -1.57 6.22)
			(end 2.84 6.22)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f43773ae-4035-47f1-a9cd-dfe4ffaede78")
		)
		(fp_line
			(start 2.34 -0.635)
			(end 2.34 5.715)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9541e1aa-bdd6-4ccd-840f-7a28bcbdbaf1")
		)
		(fp_line
			(start -0.2175 -0.635)
			(end 2.34 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ac2a7423-52e8-420b-8616-a2bd38702f81")
		)
		(fp_line
			(start -1.07 0.2175)
			(end -0.2175 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0f893851-bdf8-4699-a3bc-e607f978b3fa")
		)
		(fp_line
			(start 2.34 5.715)
			(end -1.07 5.715)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c082b39-390e-4eb0-9f4d-83c843bcf15d")
		)
		(fp_line
			(start -1.07 5.715)
			(end -1.07 0.2175)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ebe5a8f-542e-4411-b93f-113528c4bf9c")
		)
		(fp_text user "${REFERENCE}"
			(at 0.635 2.54 0)
			(layer "F.Fab")
			(uuid "c0305597-a871-4c91-a266-d3cb644668f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "SWCLK")
			(pinfunction "TCK")
			(pintype "passive")
			(uuid "49768a9d-5475-458e-946d-865c82346119")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 90)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "8c2564ba-a03b-400c-8da1-459a9d4e5267")
		)
		(pad "3" thru_hole circle
			(at 0 1.27 90)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(J4-TDO-Pad3)")
			(pinfunction "TDO")
			(pintype "passive+no_connect")
			(uuid "2f8862c2-bbab-48e8-98eb-2059374e2438")
		)
		(pad "4" thru_hole circle
			(at 1.27 1.27 90)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "VBUS")
			(pinfunction "VREF")
			(pintype "passive")
			(uuid "d8f79772-96c3-48c2-8c38-0974c762119f")
		)
		(pad "5" thru_hole circle
			(at 0 2.54 90)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "SWIO")
			(pinfunction "TMS")
			(pintype "passive")
			(uuid "e65bfaed-632c-4ce9-b44f-b8f01cd9ca02")
		)
		(pad "6" thru_hole circle
			(at 1.27 2.54 90)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "RESET")
			(pinfunction "~{SRST}")
			(pintype "passive")
			(uuid "270d8411-650b-4a55-b9a8-9634481f1eb0")
		)
		(pad "7" thru_hole circle
			(at 0 3.81 90)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "VBUS")
			(pinfunction "VCC")
			(pintype "passive")
			(uuid "f7836cc5-3e2e-4665-bfb4-8c1e085a062a")
		)
		(pad "8" thru_hole circle
			(at 1.27 3.81 90)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "unconnected-(J4-~{TRST}-Pad8)")
			(pinfunction "~{TRST}")
			(pintype "passive+no_connect")
			(uuid "c138ce9b-fb29-4417-95c1-16c5ff5085c5")
		)
		(pad "9" thru_hole circle
			(at 0 5.08 90)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(J4-TDI-Pad9)")
			(pinfunction "TDI")
			(pintype "passive+no_connect")
			(uuid "2770ddf0-96db-4243-9cb9-ee9fc0d54aed")
		)
		(pad "10" thru_hole circle
			(at 1.27 5.08 90)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "c567083c-e315-4f14-a8e0-7f5304a68a59")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "4c4023f7-bc7f-4d23-a4ca-6bc5dee32ecd")
		(at 65.3 90.4125)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 2.85 -1.25 0)
			(layer "F.SilkS")
			(uuid "b839d5ea-907d-4585-b341-365af77872b3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "NPN"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "2e5324bb-e94f-45b8-8d00-41af53da1ac8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "401dd4b2-ef46-4a9b-b44c-f6358e23774d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f6552edf-3e48-42d5-85ae-12434f8ab281")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "NPN"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ba5473d2-510c-4563-866b-cd8f06e026f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "70e7ee2a-0acb-4f42-a495-ebf0d492efc7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6d7337c9-5f1a-4245-b336-8d54b781af4f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/43a3c124-dd3a-4a8e-b9ad-89e57f70a6a2")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b481c1ab-3446-469d-be57-8d36d3dbd0a5")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "01e6e84f-07fa-445b-9a35-0e7998d480dd")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "30467ccc-29b8-462d-8bf1-f0e984dd1b4f")
		)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e1c111b8-0532-4700-8df9-11bb0675ce95")
		)
		(fp_poly
			(pts
				(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.84)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "3201a445-35fb-4300-846c-c4117d50d391")
		)
		(fp_rect
			(start -1.92 -1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "b5cef274-0e79-4fda-bcd0-d3081b13e1f2")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a82eb32-01bc-43d2-b5f7-3538df1f3315")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bc75ac88-ec78-4e74-8f6a-2e9950d102a2")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5d5a93d2-b7c4-4407-a773-f3f21ab94f8d")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3a36c863-fa16-475b-95ed-690bf8781072")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9d904794-f6ee-4e09-8c45-441fb73825fd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ff8c5833-f7cf-4250-92ab-1994e5aa7ad0")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(Q1-C)")
			(pinfunction "C")
			(pintype "open_collector")
			(uuid "e77c1865-9bf2-4cfa-ae1e-275b8776c6fb")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "8116fdec-5a42-425d-ab6a-909f1d2af7ae")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "E")
			(pintype "open_emitter")
			(uuid "9611593e-1594-4e04-b5d8-2df6ba2df1ec")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "4c5c7732-0d3a-40b6-a70d-bea5e095c7ec")
		(at 75.91 128.2375)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW8"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "83ab438f-3184-40d5-aca0-e2e1b1dd6cbf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "45d74f73-99aa-4d0c-aecc-06490faa8f1f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b5dc535d-5e16-462b-8b9f-e115cf29e1dc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7d0459fb-321b-4171-9277-367af36df83f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/ff690b5a-7854-45b7-ba54-cef96740420b")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f185d6bb-6e13-48da-a5c7-bf611a7cc866")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c8063d7c-4af4-4151-802e-ded8d0f56f8a")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "15d62925-c40d-44b5-bdb1-95f01c141542")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d6355364-0646-41c2-b793-b896de6ee5f8")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "be8b8c9a-3011-46a7-9a89-e6d861fd665c")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "ea90b198-6eb1-4509-be27-c84e8e03ad1e")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "100106ed-15b2-4b4c-84ce-aff7fca81503")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "cf5572ec-ec6e-4d25-8699-d3f97da1cb7f")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72ca3cf6-a734-45fa-86d1-727d988e5438")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ae7275dd-3fa9-47ea-9139-896a69f47d18")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "13dfd370-94b8-4deb-93ab-08d3e7bd6b3b")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a1b430e2-98ca-4f17-a7b3-13643eefacb0")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a2104787-6e05-4a7e-97c7-cb3fe89273ed")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0b409845-aee0-4ed9-93e4-867a02d9d920")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "70733a6a-18a9-45b5-b05e-c74f10211fdc")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9ab4e0d0-270d-45a5-97b0-2065637e57b0")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "3ccec369-17ce-4d9e-b67a-dfab3b002125")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "84263749-d3ca-49ea-b22b-7aa230044783")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "8745da86-49fc-4ed8-8476-e5efc2712168")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "bb8926c4-fdb8-495f-8ed4-a9124f816392")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "KEYPAD_COL_1")
			(pinfunction "1")
			(pintype "passive")
			(uuid "0861336e-e4c2-410b-aa1b-d3eb131f63f0")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(D10-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "8d7c721f-7086-4f59-8f26-425f56a211de")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "523fe645-848d-495f-821b-be1d5a212a57")
		(at 152.091589 79.571976 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C23"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "bc9d252a-3617-4c83-8c65-5a5df8957c7f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "4cb6b95c-87f4-4bfc-9587-def53e315e06")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "9defab4d-f6e4-45a3-8127-abe4ad4255de")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "ca70a303-446e-4d76-8a2e-645ce9e83c37")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/fbf0b643-688a-437c-a7d2-a58ab0f72acd")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0f362134-5b83-4aad-a071-55476e6011ca")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9adec02c-5e86-4290-b4d3-ee26734000e5")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "67ffc2c9-6132-4472-8db1-518724aa2050")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "47232274-7412-4f84-a164-766511ee78bf")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b891b26f-35ea-4fe2-a128-74a9d2adb17e")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ac1c47c6-628c-478c-a2a7-d63f80cb1a20")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "94c0a57c-d73d-4415-a1e3-1e4c0be76058")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f240877-172f-4ad4-8296-b1a59d9f24f8")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1d7bea04-7d90-438e-ae69-a4188fed3e62")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9feebba9-2f52-451c-9253-203a61800fef")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "79a6b6a2-2b92-4761-80a3-f1d2702ba392")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "4f31965f-10b7-419e-a097-f0781b885874")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "3d880192-6d3c-4c02-935c-62ec87240b54")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(uuid "5292e833-f338-405b-8e5e-2060485feaf2")
		(at 93.45 48.45 -90)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U3"
			(at 0 -4.5 90)
			(layer "F.SilkS")
			(uuid "8c89b1bf-f910-4ea1-8322-5604b7bd2640")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "AMS1117"
			(at 0 4.5 90)
			(layer "F.Fab")
			(uuid "b16f9195-e312-4900-9a5d-0435147f7147")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ed53e381-b702-4ade-bf0a-36bd3199f1f0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "1A Low Dropout regulator, positive, adjustable output, SOT-223"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f13304a8-9433-40db-a743-25451d7fe0c3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?223*TabPin2*")
		(path "/821c3552-d9c9-43ff-a940-b960ed9a52d5")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.85 3.41)
			(end 1.91 3.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f791bb25-c99b-4b3e-87ac-87bcacaf7b16")
		)
		(fp_line
			(start 1.91 3.41)
			(end 1.91 2.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b048b0d6-4659-40c4-8103-5ddbecf0e03e")
		)
		(fp_line
			(start -1.85 -3.41)
			(end 1.91 -3.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c6613016-bd31-4567-a554-5fbf7e433dfd")
		)
		(fp_line
			(start 1.91 -3.41)
			(end 1.91 -2.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5b0fff59-09fe-4f67-b464-d0fe28f65fab")
		)
		(fp_poly
			(pts
				(xy -3.13 -3.31) (xy -3.37 -3.64) (xy -2.89 -3.64) (xy -3.13 -3.31)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "d94e8a5a-8faa-4293-8ed8-4fbb95e8f586")
		)
		(fp_line
			(start -4.4 3.6)
			(end 4.4 3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a20a9f6d-56f9-4a5f-bba1-781f4f67f591")
		)
		(fp_line
			(start 4.4 3.6)
			(end 4.4 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d5800b71-4342-4ade-b204-7d4f4a2fa734")
		)
		(fp_line
			(start -4.4 -3.6)
			(end -4.4 3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0be5a33d-94e6-4254-82cc-4d6ff02c085e")
		)
		(fp_line
			(start 4.4 -3.6)
			(end -4.4 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "224d1af1-ec22-4793-8811-c915d90d210b")
		)
		(fp_line
			(start -1.85 3.35)
			(end 1.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "09f64a91-ffc9-4d9b-a7f5-00f5d026dfd8")
		)
		(fp_line
			(start -1.85 -2.35)
			(end -1.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "403f0ac3-860e-4b8d-aed7-2d839592b070")
		)
		(fp_line
			(start -1.85 -2.35)
			(end -0.85 -3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9c25c47a-1b06-4a3e-b885-c5aad356e2b9")
		)
		(fp_line
			(start -0.85 -3.35)
			(end 1.85 -3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "49e60f69-9673-4d48-9909-2c2828eb98e0")
		)
		(fp_line
			(start 1.85 -3.35)
			(end 1.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "368b8e53-c55a-437d-a851-3c8ed83c484d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ac68997d-bd84-4271-99d3-8eec3ab96393")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -3.15 -2.3 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "ADJ")
			(pintype "input")
			(uuid "1259b14a-cf05-42e1-a33e-01b5bf55ccf1")
		)
		(pad "2" smd roundrect
			(at -3.15 0 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(D3-A)")
			(pinfunction "VO")
			(pintype "power_out")
			(uuid "b37b122c-3af3-46c4-bcd2-45e76361ccf0")
		)
		(pad "2" smd roundrect
			(at 3.15 0 270)
			(size 2 3.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(D3-A)")
			(pinfunction "VO")
			(pintype "power_out")
			(uuid "fee2131f-03b4-4738-ac0d-965168cb5a3e")
		)
		(pad "3" smd roundrect
			(at -3.15 2.3 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+12V")
			(pinfunction "VI")
			(pintype "power_in")
			(uuid "410bc4dc-4ed8-40ed-86ee-9845250c6fda")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "567630ae-692a-4d52-a9ca-bed76cfb8dd0")
		(at 61.45 70.9175 180)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U5"
			(at 0 -3.4 0)
			(layer "F.SilkS")
			(uuid "47d4992f-5906-464d-8815-c1ecf37b5dc4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MAX31855KASA"
			(at 0 3.4 0)
			(layer "F.Fab")
			(uuid "a5ff536a-726f-4519-9e64-9d41f7d862f7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX31855.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5742a6e1-becf-48f5-a931-2965c73ccf49")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Cold Junction K-type Thermocouple Interface, SPI, SOIC-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "816d218b-cc20-4821-9388-1b128e22b633")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm*")
		(path "/84c51924-c7e3-451f-8657-4959215501c8")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 2.56)
			(end 1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "38b39fd1-071d-4403-914c-c47b6b167b7d")
		)
		(fp_line
			(start 0 2.56)
			(end -1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c5f755a6-29ae-40e3-82c5-c65162176392")
		)
		(fp_line
			(start 0 -2.56)
			(end 1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9025bdf1-a1a6-405c-91ee-a623f2a65d9f")
		)
		(fp_line
			(start 0 -2.56)
			(end -1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3095cc0c-7131-43ab-8168-5a615244af91")
		)
		(fp_poly
			(pts
				(xy -2.7 -2.465) (xy -2.94 -2.795) (xy -2.46 -2.795)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "c44686fc-7c54-4fd1-b51c-588b2d545d5b")
		)
		(fp_rect
			(start -3.7 -2.7)
			(end 3.7 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "8a85c1ff-dbe5-48ca-abd5-4adf4144f728")
		)
		(fp_line
			(start 1.95 2.45)
			(end -1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87f54555-5e9f-4989-92a9-de3c5d6a95e7")
		)
		(fp_line
			(start 1.95 -2.45)
			(end 1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "35ca4c28-cb42-4b44-a09f-53aa77e7d567")
		)
		(fp_line
			(start -0.975 -2.45)
			(end 1.95 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "26951220-b2ea-49cc-99a7-4beb00e582d9")
		)
		(fp_line
			(start -1.95 2.45)
			(end -1.95 -1.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "30a1e061-2ad4-45a7-b866-4e8dbc77487c")
		)
		(fp_line
			(start -1.95 -1.475)
			(end -0.975 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "050e7f3b-4fb0-4aaa-85ca-9b7b628a9856")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "dde8ea97-b54e-47dd-b83e-df0811a5e388")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "43793bff-bb8e-4db2-8512-a5963eb37d70")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(J7-Pin_1)")
			(pinfunction "T-")
			(pintype "passive")
			(uuid "e27b97b3-0a4d-4a6f-b2a6-6f4c37a6fda0")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(J7-Pin_2)")
			(pinfunction "T+")
			(pintype "passive")
			(uuid "d7545c27-a997-415d-b9d5-88f5e96261b5")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+3V3")
			(pinfunction "V_{CC}")
			(pintype "power_in")
			(uuid "6298d903-c73f-4b86-b634-080ce3d52df1")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "SPI_THERMAL_SCK")
			(pinfunction "SCK")
			(pintype "input")
			(uuid "e016ab10-328b-4331-9053-27cc0ae46d67")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "SPI_THERMAL_1_CS")
			(pinfunction "~{CS}")
			(pintype "input")
			(uuid "339c311b-35b5-49c7-9d4f-f18b8d209710")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "SPI_THERMAL_MISO")
			(pinfunction "SO")
			(pintype "tri_state")
			(uuid "09c91f0b-e1cc-4b5e-baa1-2de8bae50c0c")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "unconnected-(U5-NC-Pad8)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "22708fb2-99e6-4ff0-bf45-643ee7751e94")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "5f41951f-9c0f-4b77-88af-c43386324617")
		(at 145.289222 86.374344 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "88bb2299-d637-4537-b1cd-d02668a21746")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7uF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "be65f916-89d7-4253-9c06-b34716b4300e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "9bb2f894-4e76-44a6-98ef-2ec869a97adf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "4398be2b-27ef-42fc-b479-ebbc951a4acf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/579b78cb-274d-4bbb-94d0-ed4012bfe2e8")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "504a0209-4f81-4ca5-874a-0452ab3f6c43")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eed0ebfc-e975-452e-8612-fa26904be1eb")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8260448d-31b5-4e0c-8ee0-b29d7051a192")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f788102a-33bb-4b46-b971-66eb984cea0b")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d50609a7-85b1-48ac-8b1a-97cdc26ffbd6")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6f4faaba-0206-41e7-af05-c4d82577129d")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c8a2b5b-49ca-4af7-b304-c149b3768e33")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "efc9d42e-33c3-44aa-a27c-b726b3663725")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f993676f-0927-42a7-8127-3e0bb6b7b8b5")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "85010769-6b5b-4a07-8e71-734c459c3417")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "3a2f383c-7b80-4074-8f60-49e035755117")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "+1V1")
			(pintype "passive")
			(uuid "bbb8d1c5-1b58-4fe5-93ef-f2925e15007b")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "dbc67387-0ba3-4d2d-9f68-c20a9b97f510")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "62945ffe-4cdc-4ba1-a2c3-fbb91559df24")
		(at 72.1 75.95 135)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C17"
			(at 0 -1.679999 135)
			(layer "F.SilkS")
			(uuid "dd5f0215-c9c7-4968-a67a-2abbd777ebdb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.679999 135)
			(layer "F.Fab")
			(uuid "e88092fb-58be-4b6f-a057-98368a7a73da")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
			(uuid "b1d814eb-22e3-4627-9839-fe402bb097f6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
			(uuid "7b61d28f-9cf0-46ca-9407-a059b13fa970")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/36bc5bdf-6338-4633-8cce-f2df366b86e8")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cdc94033-a453-45da-8b50-f31df9886239")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b4046921-3852-4642-94c8-e041f5b3aadb")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1300fb47-db22-4f74-b26a-ea2501ff3afa")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "749a1de2-f836-4d83-8b41-0c0e3ff82371")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8880c362-d3db-4d01-a768-aded4b77f87b")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8e3cbe5f-e02b-4ad3-8389-c8f731281947")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc5dde04-4998-4d3d-82f0-739161e76ee9")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c1f50c6-13f5-45df-906c-555400564d22")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "035845ba-5c44-407e-b9d2-098fd81da5cd")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "358398ae-fe24-4e4f-a1b3-34a2bbb9c8d8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
			(uuid "98a9fea1-5816-4a7f-bf8a-94f14433908c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 135)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "19616502-d760-4373-b9dd-835df3abb44d")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 135)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "660b3940-9d0f-4f29-9ffe-f10900f46eb6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_Push_1P1T_XKB_TS-1187A"
		(layer "F.Cu")
		(uuid "629e7d9a-791d-4623-8884-10b198b55f19")
		(at 119.05 66.9175)
		(descr "SMD Tactile Switch, http://www.helloxkb.com/public/images/pdf/TS-1187A-X-X-X.pdf")
		(tags "SPST Tactile Switch")
		(property "Reference" "SW1"
			(at 0 -3.75 0)
			(layer "F.SilkS")
			(uuid "02ce76d0-4bee-4c8e-b460-ad904c43a156")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at 0 3.75 0)
			(layer "F.Fab")
			(uuid "02bdc295-f7ef-4309-b77b-8dc1d16ad51b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ca8ff494-f37d-4afc-8181-16d915141b27")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5125cf98-90cc-4a73-89ea-3085cd11c2f9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "73b2af31-ec1d-4fa3-8f96-a32b439fa837")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "08830c63-f359-4c6c-b2fc-f9d3081dd45e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/d636d96e-3565-423e-8659-abd4f8db5838")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.75 -1)
			(end -2.75 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7e7f648-8a41-43ef-a963-fe00dbb2d82d")
		)
		(fp_line
			(start -1.75 -2.3)
			(end -1.3 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d7a3d32a-1c9e-41e2-94bc-14dac07a1466")
		)
		(fp_line
			(start -1.75 2.3)
			(end -1.3 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f8468201-0928-47d5-996e-92e1aa3f7149")
		)
		(fp_line
			(start -1.3 -2.75)
			(end 1.3 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "df14b8a0-21ba-46f9-bb51-e0bd8e0c6f94")
		)
		(fp_line
			(start -1.3 2.75)
			(end 1.3 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "451a39f3-2265-4a4f-abdf-dd3cde931d17")
		)
		(fp_line
			(start 1.75 -2.3)
			(end 1.3 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bb47e481-4d9d-45fe-a52d-c15df47a70bd")
		)
		(fp_line
			(start 1.75 2.3)
			(end 1.3 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "15e70241-e647-4fc3-9b3d-4edc5e8eae6e")
		)
		(fp_line
			(start 2.75 -1)
			(end 2.75 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f2a4d0c7-ec48-40c3-b319-f7255ba8f4a9")
		)
		(fp_line
			(start -3.75 -2.8)
			(end 3.75 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0710d069-fe56-46d3-99d7-d56d3d960589")
		)
		(fp_line
			(start -3.75 2.8)
			(end -3.75 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "28c6421c-0c2c-4d82-ab0e-7953387ffc29")
		)
		(fp_line
			(start 3.75 -2.8)
			(end 3.75 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8a3ad5be-8717-45eb-884f-66a4750a7df4")
		)
		(fp_line
			(start 3.75 2.8)
			(end -3.75 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aa74b647-d929-4d1f-9e3b-e741fed7e936")
		)
		(fp_line
			(start -2.9 -2.1)
			(end -2.9 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "772f7a64-9d2d-44a5-b882-68fea1161a19")
		)
		(fp_line
			(start -2.9 2.1)
			(end -2.9 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "52e239ed-6b75-4c5c-9508-72bf2e74dafd")
		)
		(fp_line
			(start -2.4 -1.4)
			(end -1.4 -2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fa06eabb-2f70-480f-8370-5bc35d7ea797")
		)
		(fp_line
			(start -2.4 -1.25)
			(end -2.4 -1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "68cdf718-0f66-4be3-a7e2-361cc50185ce")
		)
		(fp_line
			(start -2.4 1.4)
			(end -2.4 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0fbc446c-8dd3-4408-9756-f56043d870b3")
		)
		(fp_line
			(start -1.4 -2.4)
			(end -1.25 -2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0e444fec-c4d4-4ca8-b42b-2c35a87b65fd")
		)
		(fp_line
			(start -1.4 2.4)
			(end -2.4 1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "076c9bc9-ec99-408a-a351-01ff503544fb")
		)
		(fp_line
			(start -1.25 2.4)
			(end -1.4 2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87477997-8690-49c2-9293-722898e40ada")
		)
		(fp_line
			(start 1.25 -2.4)
			(end 1.4 -2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c5f69e62-b7e3-470f-9367-29c52340c4f4")
		)
		(fp_line
			(start 1.4 -2.4)
			(end 2.4 -1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9701df2b-6d7e-4f10-af22-f2c7ade543e5")
		)
		(fp_line
			(start 1.4 2.4)
			(end 1.25 2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc0645e1-f782-42f3-a780-3b16b5862d50")
		)
		(fp_line
			(start 2.4 -1.4)
			(end 2.4 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ed9dd618-3ade-4e49-975b-563ae436b306")
		)
		(fp_line
			(start 2.4 1.25)
			(end 2.4 1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c66506e3-ff83-4ed7-86cd-391251af81f6")
		)
		(fp_line
			(start 2.4 1.4)
			(end 1.4 2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "caef5a2a-8c01-4ffe-8204-f743610d3d9d")
		)
		(fp_line
			(start 2.9 -2.1)
			(end 2.9 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2c83e0d5-ba90-475c-b0bf-f587888a2e53")
		)
		(fp_line
			(start 2.9 2.1)
			(end 2.9 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9175e950-c4de-403e-8139-41cb1ae7a426")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "086b27db-5b97-4e7a-b949-248c15e96207")
		)
		(fp_poly
			(pts
				(xy -1.7 -2.1) (xy -2.2 -1.6) (xy -3.25 -1.6) (xy -3.25 -2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "ba5cf76a-f41e-47d3-8c92-8b868eaa1e0d")
		)
		(fp_poly
			(pts
				(xy -1.7 2.1) (xy -2.2 1.6) (xy -3.25 1.6) (xy -3.25 2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "675c5d9c-63c1-418e-b5f8-15216d6086cc")
		)
		(fp_poly
			(pts
				(xy 1.7 -2.1) (xy 2.2 -1.6) (xy 3.25 -1.6) (xy 3.25 -2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "9d48498d-3674-4db0-a4de-d4e81740ac23")
		)
		(fp_poly
			(pts
				(xy 1.7 2.1) (xy 2.2 1.6) (xy 3.25 1.6) (xy 3.25 2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "dff27279-c5ee-4859-aaf6-9cf2f77f5922")
		)
		(fp_poly
			(pts
				(xy 0.85 -1.85) (xy 1.85 -0.85) (xy 1.85 0.85) (xy 0.85 1.85) (xy -0.85 1.85) (xy -1.85 0.85) (xy -1.85 -0.85)
				(xy -0.85 -1.85)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "6140b883-8d5f-4156-93ea-2e3d33dd879b")
		)
		(fp_poly
			(pts
				(xy -1.25 -2.55) (xy 1.25 -2.55) (xy 1.25 -1.975) (xy 1.575 -1.975) (xy 1.975 -1.575) (xy 1.975 -1.25)
				(xy 2.55 -1.25) (xy 2.55 1.25) (xy 1.975 1.25) (xy 1.975 1.575) (xy 1.575 1.975) (xy 1.25 1.975)
				(xy 1.25 2.55) (xy -1.25 2.55) (xy -1.25 1.975) (xy -1.575 1.975) (xy -1.975 1.575) (xy -1.975 1.25)
				(xy -2.55 1.25) (xy -2.55 -1.25) (xy -1.975 -1.25) (xy -1.975 -1.575) (xy -1.575 -1.975) (xy -1.25 -1.975)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "b22dc6e1-936b-453b-afb6-ed69cd29b061")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -3.75 0)
			(layer "F.Fab")
			(uuid "b5993853-db20-4fdb-ae44-efc12e0922ec")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -3 -1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(uuid "8821bd41-30f5-4534-8419-39e47e6a3a80")
		)
		(pad "1" smd rect
			(at 3 -1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(uuid "8821bd41-30f5-4534-8419-39e47e6a3a80")
		)
		(pad "2" smd rect
			(at -3 1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "Net-(R3-Pad2)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "b9b7086a-7dff-47d6-b464-990ac5b345d1")
		)
		(pad "2" smd rect
			(at 3 1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "Net-(R3-Pad2)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "b9b7086a-7dff-47d6-b464-990ac5b345d1")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_XKB_TS-1187A.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "648c038e-1c5e-4541-8b7a-0c8d8ab3d051")
		(at 73.55 74.5 135)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C18"
			(at 3.394113 0 135)
			(layer "F.SilkS")
			(uuid "907f34ca-9679-4359-886b-416ea2678559")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.679999 135)
			(layer "F.Fab")
			(uuid "6620058e-27e8-4614-a57d-3430c9b8012d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
			(uuid "2d267f5b-b610-40db-ad7d-16bbac362927")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
			(uuid "1570d5fd-c3a1-48bf-9382-ed501e6f338e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/80b46181-cd0f-4f33-a704-861c4d4e9496")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6cc2346c-cc3c-41da-b4d3-082cf89807ee")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f91357ea-ddd5-4706-9e1e-b9c8eb3d450e")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e81836c9-b4be-4990-99d7-e4783e4826c3")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "19d85623-393f-4d77-9eb3-771af126b499")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "92abde0f-0bb8-433b-a967-2d36121f41eb")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d380e040-d5aa-4fb1-ae36-cb967a8a803a")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc9ac8dd-174a-4b34-9837-bb63870252ef")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d754f44b-bfad-438d-abb4-0517487e992c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "df157b02-0cca-4731-ac56-675924714754")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5dc61949-3091-4038-8d51-ab54250896eb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
			(uuid "6728b9da-8bc6-4ea6-9fdc-96a2b1c6ee32")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 135)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "b0f81c1f-6316-4aa0-beae-495298d5bea1")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 135)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "dacfbb94-faf1-43a0-b739-a30f8cf985e9")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "64fd73cc-4e7c-4d9f-b041-233d76c37528")
		(at 95.11 128.2875)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW12"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "15f64f69-f56f-489b-9f9b-c05f15d00afd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "a1b4a003-62ed-4e8d-a393-d9a450d992a0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5586927e-0514-4d5a-95a9-95de7856ebbd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f99932d1-b54f-437a-adc3-8e44df9796a6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/f6f7e7d5-d005-40a2-abc7-755543dcea0d")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "adbfa793-3f02-4031-a261-2aadd4fa547e")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73ce767b-da88-4865-94bb-82da3ff9bf49")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c5e272f1-9dfb-49ac-8240-99f736503898")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0d618c47-9178-4c7f-9667-3a178722a7c9")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "f3048489-6759-4ffe-a589-c0f9e8630d4f")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "ecd9aca4-74a6-412b-9063-a0a7c6b29440")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "a6d45d9f-1637-418f-b3dd-e9b4461439ab")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "2a3696e4-3d8a-46dd-87dd-0c413e832aa6")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7fe11da2-ba3f-4571-9001-fdefef42b8ea")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f41d64df-8fde-411c-95ee-6624b2ae53d3")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7992e516-c56a-453c-ad71-6df157a2d9d2")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "891ede49-18cb-4978-9b05-62113e4dabb1")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "420a0acb-a3a1-4fc9-9fb4-670040021fd8")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a4e91e4f-f031-42b9-9923-7101e313f340")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "589434b1-a62c-4be7-bcda-348d11244596")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b5e5f78-dade-4d98-b6aa-69e06972eb42")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "00ac1112-2908-49df-8978-7bc53e607ed1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "73f5d7d1-b4d9-46b1-b6a0-f57b25be942b")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "29fa417b-3fd3-458d-a9b5-a0fed51e2553")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "a7c94f27-9188-4400-87b3-c66a64af7cc5")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "KEYPAD_COL_2")
			(pinfunction "1")
			(pintype "passive")
			(uuid "ec723b95-5ee1-48c8-a3cb-80d1d2e78f5f")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(D14-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "8b578a3b-4623-4fd5-b22b-c33a4dc27e5d")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Capacitor_SMD:CP_Elec_5x4.4"
		(layer "F.Cu")
		(uuid "685898ae-4385-447d-b1a4-8bd2c5f78ae1")
		(at 93.5 40.7)
		(descr "SMD capacitor, aluminum electrolytic, Panasonic B45, 5.0x4.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C19"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(uuid "ba7e60bf-f69a-47a7-846e-159ee1939c97")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 3.7 0)
			(layer "F.Fab")
			(uuid "3120a9f2-757b-4827-aadc-1d0cf5baadca")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3f97cd3d-80a5-4bbe-bdd2-5c369ba0f083")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "74bc25bd-dd8d-40fd-8299-a5a53655ec21")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "CP_*")
		(path "/482c0595-73fe-432b-a6d5-4d43655ec591")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.625 -1.685)
			(end -3 -1.685)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "997db276-aa2a-4f56-96bd-e0031a5de86d")
		)
		(fp_line
			(start -3.3125 -1.9975)
			(end -3.3125 -1.3725)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a0b44b52-56ba-4a6e-8bd5-1471f7dd0c2b")
		)
		(fp_line
			(start -2.76 -1.695563)
			(end -2.76 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fae083be-4e78-445a-a81c-c3334b6bf906")
		)
		(fp_line
			(start -2.76 -1.695563)
			(end -1.695563 -2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "047c0724-028c-4a4c-9818-7216dfabaec2")
		)
		(fp_line
			(start -2.76 1.695563)
			(end -2.76 1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b4393be-a8c1-42ee-8f3a-4634348ccc30")
		)
		(fp_line
			(start -2.76 1.695563)
			(end -1.695563 2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3c6e7a2-6c48-4499-9e2d-bfc6aec30f6b")
		)
		(fp_line
			(start -1.695563 -2.76)
			(end 2.76 -2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fe91b4a8-ee54-41fc-aea4-38863625cfc8")
		)
		(fp_line
			(start -1.695563 2.76)
			(end 2.76 2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "551e3eef-c9c4-47bd-b86d-8897e2e1705e")
		)
		(fp_line
			(start 2.76 -2.76)
			(end 2.76 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c51cbf8b-fee0-4a0b-8a8b-f67648997729")
		)
		(fp_line
			(start 2.76 2.76)
			(end 2.76 1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5fd766e2-5452-4923-ac9b-8da4a9897bd9")
		)
		(fp_line
			(start -3.95 -1.05)
			(end -3.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f2b1631-ecde-4e7a-9f04-02eca7ee4dd4")
		)
		(fp_line
			(start -3.95 1.05)
			(end -2.9 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "557da90b-fdfb-4474-a4b8-d4b49f0b7a44")
		)
		(fp_line
			(start -2.9 -1.75)
			(end -2.9 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e7725d96-b534-47d1-babb-64dd323f5fad")
		)
		(fp_line
			(start -2.9 -1.75)
			(end -1.75 -2.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b5f0c6da-0bf4-4c44-bae6-960621b6d833")
		)
		(fp_line
			(start -2.9 -1.05)
			(end -3.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c73d791d-c881-423e-b48f-a51d892b2188")
		)
		(fp_line
			(start -2.9 1.05)
			(end -2.9 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d1fbe683-6079-4f98-a46b-e5410beedbea")
		)
		(fp_line
			(start -2.9 1.75)
			(end -1.75 2.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f8243afd-7758-4f75-ae23-1b1fcba15136")
		)
		(fp_line
			(start -1.75 -2.9)
			(end 2.9 -2.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "755db7a9-b1c1-4ee1-8e41-5e060f66bfbb")
		)
		(fp_line
			(start -1.75 2.9)
			(end 2.9 2.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0278bb71-59b7-4283-a7c4-2d9333986e09")
		)
		(fp_line
			(start 2.9 -2.9)
			(end 2.9 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "56cb8ec8-61ba-4765-ba9d-73b38c920655")
		)
		(fp_line
			(start 2.9 -1.05)
			(end 3.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8d2d435f-21d6-438c-a1e6-abe6c28b824e")
		)
		(fp_line
			(start 2.9 1.05)
			(end 2.9 2.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7966bbbb-b308-493c-806a-6bc20bdfca0d")
		)
		(fp_line
			(start 3.95 -1.05)
			(end 3.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d8c72eb0-0819-4d46-afb0-8aac75b06268")
		)
		(fp_line
			(start 3.95 1.05)
			(end 2.9 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ad43fb17-5527-46a8-a0ba-c9357ffd9626")
		)
		(fp_line
			(start -2.65 -1.65)
			(end -2.65 1.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "961398d4-83cc-4ae0-8c62-7f0ec14cd9f0")
		)
		(fp_line
			(start -2.65 -1.65)
			(end -1.65 -2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5532c472-469e-4659-b612-064b8fcdf5a2")
		)
		(fp_line
			(start -2.65 1.65)
			(end -1.65 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "def96eb7-5cd5-4265-a58f-f18c703d2c84")
		)
		(fp_line
			(start -2.033956 -1.2)
			(end -1.533956 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3e444afa-66cf-4235-8d6b-2307df69f008")
		)
		(fp_line
			(start -1.783956 -1.45)
			(end -1.783956 -0.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "210cf6c7-8c47-45dd-867e-603cff19e97c")
		)
		(fp_line
			(start -1.65 -2.65)
			(end 2.65 -2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8428e734-3c4f-435b-be89-a4b39d0c21e2")
		)
		(fp_line
			(start -1.65 2.65)
			(end 2.65 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6b5bf1c-ea6b-4711-b112-85bd0f074fd3")
		)
		(fp_line
			(start 2.65 -2.65)
			(end 2.65 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ff39fc8-5947-4ba3-a027-525c19e43872")
		)
		(fp_circle
			(center 0 0)
			(end 2.5 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "2bf3a334-5bc9-4c34-8b14-44431f8bd5e3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "be93fa3f-8d44-410f-87ce-e56822e5add3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.2 0)
			(size 3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 9 "+12V")
			(pintype "passive")
			(uuid "b12ee8cc-aa4d-48b2-9e0c-36ccd7db60b5")
		)
		(pad "2" smd roundrect
			(at 2.2 0)
			(size 3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
			(uuid "b3ce3ae1-41ec-4d1a-84eb-89908320f133")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_5x4.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "6e079b12-bc3c-4338-8fec-c437bb228601")
		(at 144.850816 65.528836 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C25"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "5a4692d9-ce8f-4992-8901-a9c5fdc4a86e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "f42abf7c-4df8-4513-b53b-05ebffdb3cd7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "180ddba1-7dba-4031-9f42-dc22361d885b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "9c6eac46-a2c1-4931-a171-1ceeb4369f30")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/e9b0b88b-2e4a-47ff-a6bb-4c9174f7dd45")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84deabda-ba37-4a62-97a4-1d54a09a5c43")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e6b60a17-48dc-4701-8565-faae0ed6fad5")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6fb5cf43-cf45-42e6-b8e3-b65789a36891")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a52dcafd-898c-4e18-8464-582942817d1c")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "809da82f-b833-4329-9b44-024250382502")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7eecbf2b-2015-4558-90d4-b5a05fa29a69")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a71eb9ef-2de0-4592-9bb1-2244de0f8999")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d65646d5-be8a-4276-a9ec-8c2647f467d7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "72b7f1c9-e84c-405c-a797-06d9a10c43d9")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e883a4ab-87f8-4e1a-9d72-7c1a684a3da2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "76c867b3-60a4-40b2-8813-878b859ce97c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 14 "Net-(J7-Pin_2)")
			(pintype "passive")
			(uuid "c11e8872-8154-4ce4-bc88-9f844d7fc8a1")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 13 "Net-(J7-Pin_1)")
			(pintype "passive")
			(uuid "09f78989-0c05-4dd7-930c-e9942d3fd34d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(uuid "71429b36-905f-4013-b646-a23f8f5cee6e")
		(at 95.55 95.9 90)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U4"
			(at 0 -4.5 90)
			(layer "F.SilkS")
			(uuid "84f90305-5777-4376-a19f-d7e61c45aeef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "NCP1117-3.3_SOT223"
			(at -5.7 0.05 0)
			(layer "B.Fab")
			(uuid "57c92e63-9da2-4401-afc7-6b800a58c8ad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c229f309-c73d-49b8-8378-c95ec4381909")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 3.3V, SOT-223"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a4f446a3-8c2e-454d-b711-5a35278aac52")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4838faba-abbd-4f22-aabc-e98af796c732")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5d7d451a-ea93-49fd-a604-6cb2a02c4b96")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC" "C26537"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "18544621-c34c-46b1-9190-be94a940cf13")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field8" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4b101cd5-3085-4855-9b96-9c8905d7c795")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?223*TabPin2*")
		(path "/a7ad4c26-dac9-476d-84e6-cd965e968d8d")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start 1.91 -3.41)
			(end 1.91 -2.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0d0f48b7-f34f-4559-8a06-ab22d5549f2c")
		)
		(fp_line
			(start -1.85 -3.41)
			(end 1.91 -3.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa6491df-d3b0-4987-9d72-87ce8679eef3")
		)
		(fp_line
			(start 1.91 3.41)
			(end 1.91 2.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d982ea2b-fd5e-4ef1-addd-06f13634cbeb")
		)
		(fp_line
			(start -1.85 3.41)
			(end 1.91 3.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5228459e-6b56-4a4d-b60c-c33f2d866f6f")
		)
		(fp_poly
			(pts
				(xy -3.13 -3.31) (xy -3.37 -3.64) (xy -2.89 -3.64) (xy -3.13 -3.31)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "67c01c49-e974-4077-a9f3-d969948c7149")
		)
		(fp_line
			(start 4.4 -3.6)
			(end -4.4 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cca7ae0b-5671-4c0a-9fbf-1eb04982ac71")
		)
		(fp_line
			(start -4.4 -3.6)
			(end -4.4 3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a13e6d0c-d11e-433b-a229-85f50b322784")
		)
		(fp_line
			(start 4.4 3.6)
			(end 4.4 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e3377b1a-932d-48f6-8315-8f05263980ff")
		)
		(fp_line
			(start -4.4 3.6)
			(end 4.4 3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12fc2612-a099-432d-9f1a-fddc7e3fad69")
		)
		(fp_line
			(start 1.85 -3.35)
			(end 1.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb669acd-529c-4c1a-87d5-7957f870c4e5")
		)
		(fp_line
			(start -0.85 -3.35)
			(end 1.85 -3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f332bab1-6d09-4097-8725-2538e8423ebc")
		)
		(fp_line
			(start -1.85 -2.35)
			(end -0.85 -3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "11eb1e5e-8ed8-4544-b63f-55f9af397a4e")
		)
		(fp_line
			(start -1.85 -2.35)
			(end -1.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2a85a68-fa66-47a6-90e6-a407d28e713b")
		)
		(fp_line
			(start -1.85 3.35)
			(end 1.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f5316b74-db93-436b-8de9-f4092dbfddd2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ed59b9b9-b8f1-4b10-87ac-8d3b1328103a")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -3.15 -2.3 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "c68c92f4-8c2f-4791-9226-048606d4ec97")
		)
		(pad "2" smd roundrect
			(at -3.15 0 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(D4-A)")
			(pinfunction "VO")
			(pintype "power_out")
			(uuid "fc425c4b-650c-4f99-87cc-1fe1d587a5d5")
		)
		(pad "2" smd roundrect
			(at 3.15 0 90)
			(size 2 3.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(D4-A)")
			(pinfunction "VO")
			(pintype "power_out")
			(uuid "9de24520-2260-4050-bf07-09f615744a02")
		)
		(pad "3" smd roundrect
			(at -3.15 2.3 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pinfunction "VI")
			(pintype "power_in")
			(uuid "6240c28c-4a04-426c-99f5-2057cb03354c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "74ca5edf-0b7f-4d9b-ba4a-79e8c40b69ec")
		(at 59.4775 104.6725)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C15"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "4305d0a1-0e73-4570-a64d-fe38c9a7b5b0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "d02015f7-18e1-4d28-bb8c-fd3f32d8e7a1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bdc2d8b3-4eef-4d44-8126-d031b3916272")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1fb168db-5703-470f-b71d-877cc3cba0be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/09abb068-a1d0-480d-b171-237ade00429e")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "05aced45-676b-48f9-821e-f52d3c23748e")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "debd5ff3-b330-4f17-9341-cc7578decdb4")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4539acd8-bb93-4180-a936-741d1ea67bb8")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c69816b8-26e0-41dc-9be2-dff427167f5c")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4434804f-27f2-4814-b1e8-2468dfda4f1d")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6ee25553-e56d-498d-a9a5-3d1740760a4d")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a8a7afe9-69e2-49c0-88df-22f3962425d5")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "02f36b78-c7be-4dad-862b-2f258111bfbd")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb66e017-1a3b-450b-b218-c07e4e346879")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e6b094bf-d84d-46f8-b5d8-82978690dcb7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1c25332a-de02-4bba-86d0-12242028eed1")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 8 "Net-(Q3-C)")
			(pintype "passive")
			(uuid "0f54f2f6-ed93-4be3-867d-a456bf6cc7a1")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "64e7605e-2a3d-43ad-9698-1e23c82847fa")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "79745408-38eb-4e56-8730-d40494ee583e")
		(at 65.35 93.2125 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "69a25a49-779a-4e88-8a59-2ac2d3a5f321")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "717d7e1a-00f0-4522-b9f8-74626f7c4bf6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8b6b10ad-e8b5-4efa-abea-c4fdad9b4390")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b46df00f-ab10-43b7-bda7-7c970263d5bf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/49d66afd-9d01-4343-9913-bfa89ed3b506")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "55082415-1502-4a7b-ab1e-6d6e93842613")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "088aa13a-37f7-4d31-a27a-5deaaa1532ff")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8964db27-25fa-4cdb-9247-23a50743d294")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "de699922-59de-4c3f-8781-7621abbfda54")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "61ed6304-d3d5-41c8-8043-cfeebff98e08")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f4b732ca-f29f-442c-905a-ffa191f3b518")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3becf363-6386-4e5b-829c-86e7731d1fc4")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d942c9b-13f8-4fd1-86cb-551398724984")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f2ad5f5-4011-4d8b-80b4-5075ec69fbf9")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2e36d564-758f-4d2e-b0b0-59d4091eae7d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d7b00914-9381-4db2-82de-24afda831a7b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 73 "USR_PWM_0")
			(pintype "passive")
			(uuid "dd3f29ab-6182-4a32-b5ee-9d99d6cfa222")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 69 "Net-(Q1-B)")
			(pintype "passive")
			(uuid "8f77670c-1acb-454e-b013-1403fff97ec2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "7cd0a4de-de4e-4781-9130-69e2115c19c6")
		(at 155.27 119.85)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "cbce8924-2258-453d-afab-df1d0212459e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "f15d8d63-6c9f-4c55-b2d8-c863fb8a308d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "edce09f8-ea56-42a2-8f98-4124cf05183a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f002c2ad-74b6-4ca4-b613-17702aee5817")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/749df753-a271-4533-a555-f594b89b0be9")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3c0d1c11-e475-48e0-befb-4eb795d25c42")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ebcdb422-9a08-4e96-b9c1-801c75f2188f")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1338a90e-cbab-4bd5-b67f-b0dc3dad6afb")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dabcafb2-3331-4d68-8271-784e88c2482e")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9a24f2dd-49ba-4246-a8b7-acd3e089fa4c")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "93ce2c8e-cea7-4d6b-8a48-3c0a238acced")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0682d236-9395-4ffb-9e61-8efaf5e90e2b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8d7d02a-7e4c-4429-a549-97410c7444b0")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "366dd8f2-bc8c-4e2e-b48f-add6f20863e0")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e23f6222-78b5-43d1-9f4d-f67ecbd0523a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e8d03afb-2b1b-4d45-9054-3b165d2dc113")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 43 "RESET")
			(pintype "passive")
			(uuid "b2c47127-cf0f-49a2-88ec-6993b4d6250f")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 76 "Net-(R5-Pad2)")
			(pintype "passive")
			(uuid "fce32a70-2b07-4892-b952-2cff21678b64")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "7df10751-79db-45e1-857c-bbc7333168d7")
		(at 61.4 89.7125)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at -0.1 2 0)
			(layer "F.SilkS")
			(uuid "f9f7f9d6-9c9d-462e-bd06-24f3a44f500a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "510cbadf-5368-4116-abcf-8fa4b32d2d27")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "fd714ec1-a4e0-429e-a058-94a7fa2fed02")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6b2fefe2-c253-4706-9f0e-f396f67b01ed")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5dc7c975-5d56-467a-8655-18ff4b892811")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1b5a57eb-6c71-4213-96d4-9fdf8d3ce2db")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "305d0d88-b7e5-4860-9d40-378dfac856a1")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8c73692e-404f-4402-9767-4e85ab509dfb")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "80ba71d3-7de1-4eef-841f-768dcf370648")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e44a4d67-4c5e-44b1-a3b2-12d2f1d3506b")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0f66d6bf-8924-46b7-97cf-27227e5eeb80")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "040bd873-c391-4af9-827f-f607199fe348")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e0824b2a-f7fb-4f3d-98db-a61b20ee0a70")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "56b9180c-51dd-4a92-9a37-f43a7af1962e")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "38e3c7c0-cbc5-463d-8cf9-cba50a564dda")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "611de543-c800-4761-b9b5-c779d79cee6a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 70 "Net-(Q2-B)")
			(pintype "passive")
			(uuid "fb9e5bb5-76ba-4815-8f24-fc8ab07fd2f9")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 7 "Net-(Q1-C)")
			(pintype "passive")
			(uuid "fc4ccdef-2c72-4359-96c6-9ffa7672c14b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "815d5868-02e5-46c7-a446-e129a87fd082")
		(at 138.904048 79.989169 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "9e114716-612b-4a56-b08e-7ab2ac8d9116")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7uF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "eb3ba189-cce8-423e-84e8-a1038aedeced")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "a9ebfd3c-0c0f-4db0-90ff-7fc3c4aa8391")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "f8310270-3000-4a82-8f17-3c71d2c9bc3d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/3f4c1fa7-fe6d-492b-92df-aeeef29650aa")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7e4c3722-9c58-4c7d-ab0b-04debc5aa101")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5c069b6c-4314-4b39-9f3f-27879770604b")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d0615f0a-76ae-46c0-ada2-b43ac05c4b15")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8de3c402-9f9c-47eb-95ef-04e323c4a031")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2b5f4019-48e4-4960-b573-c0fe4f4b8c8e")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "64d493ab-b11d-4823-9397-cfd5dd12c816")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e32fdfe5-5c68-4695-ba7d-f11c46b33303")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "95e02a8a-c856-4169-829e-a8c289121166")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63546c12-d2e1-4d78-b909-25f7ca1d0614")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3e9878bf-3ede-4758-b8e5-4a0ae7dc9a4d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "f806b55c-aec8-4323-84d0-bbfd2e358574")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "Net-(U2-VREG_AVDD)")
			(pintype "passive")
			(uuid "6174f73e-0e9b-4873-b728-92e9af463243")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "bacdba5b-d160-44be-96be-02f3a0046e57")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "832de2f3-93ce-47b7-aa27-a33be69d0231")
		(at 114.28 109.1075)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW15"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "345c07c2-2cad-4fc5-9b2f-e9708b73e9cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "b8914b83-2c36-4ad8-a05c-48e13129b904")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e9ce9e8a-5427-4d79-87fe-25342e15af68")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "59a467a3-c848-4a60-a0d6-e57cae8c5da7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/d1b5c031-ee6e-44a0-bf7b-e764eb00d0c8")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0434b3c6-4f5c-4c63-b7dd-fcbfc4fa3612")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "915938f5-3e71-4546-bbac-4b08cfc4efc5")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cae52252-a03f-4b09-afaf-8d988b9a7c60")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c764cdcc-9a4b-4583-909c-c60a52e1ec36")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "13a99c61-20ae-457e-8e3d-bf22b31c6c88")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "c7d18b35-1185-4c80-aad5-3e2115c50a60")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "abd2763e-dc09-43b5-84c7-419b5259fd39")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "70f1595e-83db-449b-a387-d3997d65f196")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "11cb4132-5647-4f61-a6fb-1dd09ed86b04")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "59ee96f3-4509-4224-b23b-c3f9921fd1f8")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "664bcce6-a8c7-4b57-9e1f-ec0ca23656b4")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f84c3c8f-31c2-4d30-a15d-1af066988f1f")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dd18c9e6-2e0a-4a51-b914-57fb910206a4")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c60d5223-f286-4a2d-a50b-4222f620ca8c")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "82b3960e-2727-4d8c-9e3a-b04d630e289d")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "73f2dcfc-a3f0-4342-a0f2-28e8ea351e4a")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "c5e7c344-116a-4261-bdec-fcf94af93aeb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "88565ccf-f2ee-432c-9f95-23c207a004e5")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "5bdda2c4-e1c3-4496-a08c-043d5d232b44")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "445ed124-a248-47e7-8afa-b87427ff3e8c")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "KEYPAD_COL_3")
			(pinfunction "1")
			(pintype "passive")
			(uuid "411b82d6-3734-47bf-b704-d2b15f77dd38")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(D17-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "4df920a9-d7f6-4bfb-a651-3264815a0524")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "8587c1f5-a014-4a7b-8f9d-0d644e7751e2")
		(at 84.25 82.3 -45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C11"
			(at 3.464823 0 135)
			(layer "F.SilkS")
			(uuid "c6870bea-d761-482e-a71f-4904c52e337d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.679999 135)
			(layer "F.Fab")
			(uuid "0c47d0fc-6f7c-4e3c-91c1-92412f2d3c6e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
			(uuid "553d0ce1-fae2-493f-b466-ea9047ecd047")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
			(uuid "91763ac8-5267-4e86-be4a-d62ee98a1fe8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/cb86643f-f6f8-4d47-8d0c-d787a0bac2ac")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "02c1e879-c2af-4711-a7d4-c3f287516b7a")
		)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8347b484-58ff-457e-98c5-1c8ff9dafc5f")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a6e33afa-e6b2-4fdb-9d34-55bd7e091a02")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b49135c3-ccdc-4116-81b9-a877950a96bf")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a688a5d6-8c28-4fda-86d1-54f447a0b14f")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "74ef315e-1891-44f4-a033-b54ec78c9bb9")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4048396-6e32-45f4-a0e5-12243199f75c")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "efb7f7ce-f929-4bfa-b431-bf0db9aa977a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0fb34de9-8a89-42f0-a6a9-164cb029bd25")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1ed0c8be-c5a1-4557-b6e7-cda514504bdd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
			(uuid "3d03ba7e-9c10-45d0-bf9f-0402a45e1d3b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 315)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "0f97b81a-07f3-4346-8ece-3a2f7339ec16")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 315)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "7a0f5b3d-d87e-4077-a16e-8b2cf2abd6eb")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "8ada16b6-c314-4035-bf37-1b6244405b6d")
		(at 75.91 166.5975)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW10"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "d39ea378-719b-4255-8b65-7d1f7db8e55b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "9b0f9c4b-f8d5-4123-9566-56b0c98d4f63")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a3976051-4ca6-4666-8934-316667bd1251")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "61a122b2-d28e-4085-9c93-1cf59a163d31")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/9d199b29-5242-460d-bf54-990dc5d61eb3")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "31d8786b-6ac3-45c8-a5ce-ed2b8238f912")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5037a8a4-074c-44fc-a134-8b84d83ce5cd")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3eaea952-2093-41ee-8725-7e3413f94870")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "24ea43cc-76a3-4aca-81f5-265bdaa423dc")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "c2b53e1f-a902-468a-8fca-751a308bf3cb")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "3a739817-1acf-4b03-ac6f-45a02197233e")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "126f3e53-b242-42f7-bcfe-668da352c840")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "2a50c0b2-21b3-4700-a455-4a92a2f488d8")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7b169137-43fa-4736-a54e-50b8b467179e")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4bcaeee8-ba77-49f6-bd82-de1076dc20c3")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f57ada1c-6082-45b2-ba02-acef80e7819a")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "34c0c172-8677-4191-a801-4dfe4b78bd69")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d05dcea9-3952-4e26-82ea-6fa03b902581")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4f11e233-bb5e-4a9e-b3f3-837a42aeb10c")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "98aa2c8f-0e2e-474b-bc67-0d245bb6d555")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3ddad57d-ce82-4698-bede-1495f1b350cd")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "4ce63ec1-77d7-48f3-b6fa-bb10b5a5bd71")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "72d393a9-9219-46b8-8bd0-c7c0ca66d867")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "c7ddbd96-336a-4fea-9f73-921b91d9f4e7")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "380822b2-ba00-4134-a7c6-4c868a956520")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "KEYPAD_COL_1")
			(pinfunction "1")
			(pintype "passive")
			(uuid "ffa6cac3-cb88-4795-8f00-4867a9530c46")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(D12-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "d7048f12-483e-4322-bc55-f4b8b8e59b78")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "8d6bd961-ed1b-485a-a6bc-a01795808276")
		(at 155.27 122.8)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "ad522a9d-b3ba-4285-a0e5-34702916c8de")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "b0ad2455-b18f-4e5e-8625-08f491e7c935")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b9101756-f9b4-42b6-8ae1-621baa5a8e39")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "737d5207-751e-452d-af7a-0eec95337df5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/58d0915a-c74b-4514-97c6-feffde3098e8")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "66109a8d-b3d4-459b-a10c-291c0d05c589")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "def434be-b07f-4c7e-8053-a990f5fbc69e")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7afad1cd-f732-422d-b759-6c5b25480c26")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c77c60a1-0778-41ed-92b6-7c1ecb8be16c")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3c84507b-80cd-4809-b8d8-e35c2526bcdb")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dd92332b-a7ae-4a7b-b15c-8a6e0e46e2cd")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "046ceca5-66bf-44b7-ba2e-6d80f94d6f81")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f5c1fb41-5500-437f-aa39-faec4ce3ae60")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c8678e0-0230-44eb-8449-572e293b64e8")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6cd6f493-36b6-4bd7-9906-409c956e894e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "011594c8-d7ff-440d-ad9f-7d43f5de8e62")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 6 "Net-(C5-Pad1)")
			(pintype "passive")
			(uuid "6496975f-3383-40e5-848b-8b464a4b8224")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 77 "Net-(U2-XOUT)")
			(pintype "passive")
			(uuid "817ff4a9-cc6d-4a77-88d5-ce5dafe69020")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "94ea722b-28b2-4911-86d8-fc715437b67f")
		(at 160.02 111)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "578fc7c4-761b-4e8d-aaa3-41cb48938c2b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "27"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "f2562daf-51b8-417c-a0a7-870747178034")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0917b333-36f9-4dc9-9b7d-0fa6c175c1f6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f932d1c8-bc07-463a-84c1-2534d066f7a3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/704b62fc-baf0-436f-b763-9f5f05e4e9db")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8c3e79b7-eec2-448c-b9c8-5928bdf964b6")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6a652ed2-b95a-4cb8-8b08-657f21a56161")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4ae7ebef-52d8-42ec-b5d3-120a34b03907")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ecbb66ea-f956-44da-a695-eedf1dcccb56")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d4c340b9-ccb2-4e0c-a8d1-14fb4d2a4cbb")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "51c054f1-b3a7-4915-b463-0837ba5ad1d9")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1856c9e-99da-4eda-a983-4a1985977a3b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0da965ee-1a03-4e3d-9d4f-22f86980999a")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e33c192-56a1-4fa8-a1e9-6c73572abc25")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5770256b-2496-40bf-9c37-91ee19786b3b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4ff85bd1-444b-496d-98ee-6cbffacc6017")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 67 "D+")
			(pintype "passive")
			(uuid "867b2e6c-b2eb-46fd-a6f1-fd7e3a175c69")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 79 "Net-(U2-USB_DP)")
			(pintype "passive")
			(uuid "3a09c128-ae8a-402d-bbb9-10e61ac89069")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "97b21d8d-3eed-4847-b01e-a3bf4f6750cd")
		(at 146.979207 67.657227 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C26"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "6a65896c-d347-49f3-8305-a4be0b0a0985")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0.1uF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "4f68b248-dd0d-4130-b7c6-f5bc8087d06a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "21113c64-25c5-41c9-a194-ec151147ecc7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "419f7814-6315-48db-8bf9-0f807e55cc03")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/6c7e0eb9-7fad-4aef-99de-25c2ddbb2efc")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "abe60d4b-041b-4c79-b858-02b2f28206cb")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "52754fde-25f3-4b1d-a13a-db1b8c42e0e0")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5bd0642f-f94f-4846-8aa4-b64aae223894")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1d5340d3-7aac-4a94-9fa7-fd71e61066e0")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0b3e12ca-bf38-435f-809c-649b4fa2603a")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "15d8689f-f494-4d84-bb15-a02e3a2695b5")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "93e524b5-8e45-4871-b999-f80e11509c41")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1e9592b-ec34-4781-b963-6587155e5c58")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c449a07d-e5b1-4e94-b716-c3d8a5062da1")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0673721a-ce84-4ccd-8433-810c5679ad8f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "c0723381-ce62-4dd4-8845-fc33ddca734b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 16 "Net-(J8-Pin_2)")
			(pintype "passive")
			(uuid "f7fd524e-3cc1-46f7-b895-7dc7ef31e027")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 15 "Net-(J8-Pin_1)")
			(pintype "passive")
			(uuid "22731aa7-eb09-495c-b9b8-2e2e52074b01")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "9974cf75-fbdf-4a71-aebb-11d32bfe7c3f")
		(at 149.107599 69.785619 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C27"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "8a1461c5-32ce-4065-98ca-a6d2cb4262ee")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "b68ea67d-3541-42e1-8bd9-58b3c6394465")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "3abbb9be-4e34-4984-b909-1d06bc106922")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "37c72759-3994-4b4a-bc2b-a2cacb0b6539")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/e7845e5d-cac0-4d77-9847-4f3a52546e82")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4283d193-e53e-4da9-b535-042efbf23e17")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "529443a7-445c-4b12-b428-5c79785384ab")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8e56592f-ef6c-4900-955a-eb23765557e4")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9174423a-5b60-4992-a47a-913aad3bcecc")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "55039055-5f2c-43a3-9f9e-cc663e029e80")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2c81aee0-3698-4362-8f99-a16cd6a8f688")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3a21626b-579d-40ef-8ed3-fa75204df186")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3f574813-9d7d-456e-980c-6c09a248e828")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "27e3edb0-e1c8-48b7-8f91-444f7c2539ea")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b656d6fa-d4db-4d6c-8a6e-ee50b070ad52")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "9aa590cc-9b5b-48c1-90b7-ad8c736284d9")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "b52cf5eb-6509-4e03-a0e8-a0fbcd0e56f2")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "578982f4-c7e1-4cc2-9823-5fd0b9c08d78")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "9f55339b-0549-4d79-b2e9-583f8e9bd38a")
		(at 64.3375 103.25)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q3"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "a865b4d0-19b3-4da3-83f5-5405374689f4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "NPN"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "344e7a9a-23c6-4b89-91a2-1ccb35b34939")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9e5ebff0-6a85-4009-9a69-103cf84438fc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2b241946-46ef-44d2-b82b-57f3f3b0e5b1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "NPN"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "61d7546b-a975-44ae-8f0a-c90c146cb14c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e59d52a1-ee57-4152-9aba-3e21a58d3a37")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4ab0dfef-dd32-457c-b1fe-d2e084dafcbf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/8690a23f-72dc-4bf0-9b56-bda5ed7fe277")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "18aadc13-437b-4378-8388-8ffc8aa92441")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cfde28a4-1d13-4232-8f0a-0debbb70a0e8")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "234842c7-2393-47ad-baef-705d2516581e")
		)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "032ab18f-9cff-40cb-a30c-dbf29afafc2b")
		)
		(fp_poly
			(pts
				(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.84)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "7bbaa5ee-0bea-4f9d-8697-28f9ace193f5")
		)
		(fp_rect
			(start -1.92 -1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "03c7f4b5-517e-469f-bd44-145156213574")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da1ed29e-92ef-402b-ae21-5f1a8f3ead58")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "72e3edad-c6fd-403f-be4e-6dc10f5534cf")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "913581ac-3587-488b-8a56-528cb98dcf30")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c1375092-7269-479f-94d0-2aa3e3cf3b31")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6e288531-1287-4a61-94bf-44060098eaf2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "fc6e1d64-cde3-4627-8ca3-df2c0f4a9cf1")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(Q3-C)")
			(pinfunction "C")
			(pintype "open_collector")
			(uuid "3a35024c-ed7b-4e71-899f-eb2ca8bd7d13")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "Net-(Q3-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "407aaf5b-b5c7-46ad-879c-2e96675cadd4")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "E")
			(pintype "open_emitter")
			(uuid "da6b1c7b-d785-4a06-94cc-aa983d15ca52")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "a1e691ed-8e6d-4c30-8ab9-3661be8a59c5")
		(at 145.706415 73.186802 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C20"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "3c52e76a-7707-4f88-a45a-8d36ded6eabe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "ea6255ac-9e27-4c96-a864-48743f3bfe49")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "a71f055b-09f6-407f-8fff-3c41ce3a08b1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "8bab4566-4a9d-4831-89b6-cb4898a39629")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/79f22a62-7637-4fc5-b90d-a31072eba47f")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cfe73403-d166-4db3-93c3-10c401056dd4")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9423f7c6-d2b2-4721-ad66-f78905821352")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1641e816-be5e-42db-8899-8b8cbed30425")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8dae7a9f-94fb-45e6-b16a-362dfa32ac42")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b32b00e2-6d85-495c-b71e-7844c77af724")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9a0afd00-ccc1-4dad-9f95-73591460fd4e")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b81fc33e-4f26-4090-a6e0-d77596a2688e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1f29f60c-dc35-4c1c-8def-3476d1f3368b")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ff327982-fbd8-48d9-97c4-3e2109c478d3")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3447371f-d10a-4612-a1dd-206ce2413ad5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "a89e0b72-6da6-45e5-8ba4-f28a5a856b99")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 10 "+5V")
			(pintype "passive")
			(uuid "b798b55c-d3bc-4991-9f2b-3a1472bfa8b0")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "8cea7d35-b46e-4da8-846d-59e7c1728cab")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "a3a5572f-7876-4cca-9b9d-c3988cdc62e0")
		(at 147.834806 75.315194 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C21"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "a330b910-2706-45b5-a54e-e2755af0b856")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22uF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "1a9dcd00-917a-4ba5-8060-d4c60eb95cd6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "67bb1ce4-b26e-455f-92ae-55e38a5b431a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "db4bf94d-923b-4f17-866b-801b7f63076e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/832585a8-c3a7-42a4-9f95-ade33277a552")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8115434e-d43b-4531-ae19-19e5f4b58336")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c781555e-0e23-42c9-8aa8-ddb65d1ad2d4")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7db6c90b-49b8-45e5-958e-5d25c4abfba2")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6c417cdb-7076-4ae2-a030-6fd61caae84e")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3ad09366-4060-4a3d-b3f9-acb6d058f18c")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "988c1c75-c9ae-465b-ad69-d5d06680b842")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f9c2a34b-77a1-4314-ae57-c6fd240574e6")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "118e3412-cd1f-4d31-9367-9bd940cfdd12")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2c734188-d0b9-43f1-92d3-d54cd8cae745")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1dea61c-b69a-4b1f-98f6-530d454ac1ed")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "0c302a67-0b19-4509-9062-759cd7c130ef")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 11 "Net-(D3-A)")
			(pintype "passive")
			(uuid "291f3289-98f3-4dc2-a81c-3ecf720afb39")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "01f860cb-1735-4a9c-8a75-600b95810fd0")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "a5550f22-c56b-4409-81fb-420f88ec9431")
		(at 95.11 109.0975)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW11"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "f31e33e2-a170-4ec0-9b6e-a58ad47665ee")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "ee6cb2e1-8d0b-44aa-b7b7-0565571b359a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "97fbd093-ba64-4b6f-bfc9-f79eb5e364e0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5ac9b822-b79c-43c8-b30b-f33fe687b12a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/7453af6f-bb08-4af9-96e2-241e703d468a")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7c298b45-32c4-4097-8c15-dadaa2ef0291")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d9d9313-27b3-421f-81e6-4206ada30013")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1e97a773-e344-4a29-98a8-68b6c57ee909")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "be660e48-7f11-4cf7-af0c-1a7fd15c4d3b")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "c7f1364f-50be-455b-ad73-d4a1565ee034")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "e19be87c-7526-45af-988d-1b8043eb1030")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "dc35c145-3220-4e1a-8d67-333b0b29e5b0")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "75e10afc-9a7d-4497-8b8a-cb9961a5256a")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9ac32eb9-a8b1-4c1e-b16c-e2f48967b620")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5e3e8965-1cc1-4311-9195-761495dbdfef")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "591e58b0-27a9-483a-85c8-006dda3a1df5")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e3921207-49da-48a3-a1b7-a35a96d0bf04")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "45933b07-3a66-420a-b436-4889e79bf86b")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1a002d7f-7ed4-4135-9a3b-c3fa52154f8b")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "71dde296-14b0-40d4-bd18-1ab37452c90b")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9ada0719-2145-42e9-ad84-6b0e73811dc5")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "0e7104b2-776a-421d-aaa1-b7bc21c47121")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "7c845750-b041-476a-bcb3-8dbf341667a8")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "322801b6-6ca0-4bad-aef4-b42f6bdb1adc")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "cbee4da7-861a-4dce-ba6b-53e26c553c29")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "KEYPAD_COL_2")
			(pinfunction "1")
			(pintype "passive")
			(uuid "e6103901-68d8-4f8c-8a1b-cdc44e79d377")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(D13-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "e8ed4ddd-3d9f-4c55-a089-b9535b087823")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "a5f005cd-36ef-431f-93b6-14bf41718c67")
		(at 84.45 71.1 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C14"
			(at 3.288047 -0.106066 45)
			(layer "F.SilkS")
			(uuid "4f21b535-c580-41e6-b226-fd91f00a71ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "457ce185-1c9a-4174-b715-0c24b4635924")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "23399cdc-2aeb-4d63-b552-03c5cc972f83")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "5d694c52-f73b-4750-ab7a-5df0328aaef0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a6268d8b-3917-4159-9564-bfe21cf75fba")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8a3e8e39-3d73-46ca-b606-7c0edb3701b4")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b6159666-5e93-4cd5-92d9-5834c4b7f14b")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7a1155e7-5fe2-4b44-a030-35e7efd74ce7")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a7b15140-9bc2-4784-b29b-160ad4b2e1ce")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "70099490-22c1-44fb-a60b-8afb003d6e23")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7525a1dc-08f4-4582-9e9f-c5b2a75a580d")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a5ea7ae3-756f-4eab-ae5d-29b0fbc9d90d")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "58d22286-191b-44d8-992d-b7353c187739")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5346f44f-5755-4f6a-9879-34983d1c7b99")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "564813d4-d03c-4cb0-8c27-6612726f2a36")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "02954d50-5a14-4852-a080-1e03a7566432")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "253f3d3c-c4dc-46e8-a0fa-2aa75ce8edb4")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "9fd34539-8409-4a0b-833f-df6624d34c0d")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "a86bc49d-578e-4731-bbde-a32f642645a2")
		(at 141.032439 82.117561 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "05d6dcba-d0de-46d2-b7b7-f9b479269d1d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "15pF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "3767b831-4c9b-482c-bcf6-b7fe9d7a65fe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "0ba066b2-c85b-4b44-884f-02eb46287167")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "e3fb5a77-5134-4c10-88d3-2d12ea615ce6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/b8a4673e-8bc2-46a0-b74f-a1f6ffe742ad")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73717b7f-e1c3-44cf-81d5-11866d4abd5f")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7a06aa20-47b0-4c83-add7-b3d628887a20")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "53dd1f47-d46c-4475-a27c-c105cf1dff61")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9d271fbe-a881-4a0f-8118-e5b2be14e983")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "534cc631-eb99-4ab9-9f94-ffdd9f615a03")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bc41d48e-ad7c-4940-a529-394468ca761f")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "98941cd7-14b7-4517-a786-faf0f98d5b05")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c89d34a9-0131-4a17-aaf7-e871116e1e98")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b083f9aa-f2d6-4c0d-a2fe-1b90a0476016")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9de0a601-2124-4458-826e-84ad939b9fac")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "16b6154c-9b40-4e38-b91c-cc8e8a4bfcef")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "fe0e2731-cb7d-4c4b-9b89-07d7e1c1bc5b")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "Net-(U2-XIN)")
			(pintype "passive")
			(uuid "1c28734a-357c-466b-b65f-0b8ac638555b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "a9812f16-3254-4e67-8691-e25f81f21f35")
		(at 85.7 80.85 -45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C12"
			(at 0 -1.679999 135)
			(layer "F.SilkS")
			(uuid "79046386-bf89-4aa1-92b0-65df71a9c6cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.679999 135)
			(layer "F.Fab")
			(uuid "2ec76279-cce7-4452-97e3-ff00cfb8bda5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
			(uuid "25bf1cbd-477a-48e3-acaa-425d241fcd25")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
			(uuid "8059b246-e0d2-4063-a385-cbde98daf985")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a4bf6afd-38cf-4c51-a630-fb9386e04866")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cf0f3c93-182f-488d-95cb-30bbd96b8988")
		)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0de723d0-bcf0-4edf-81f6-0d8a749c308d")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dd6e527c-85a5-4a09-89ba-daffd10f0f84")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "661cf680-7d25-4501-bcb5-fb23df4f1a71")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb9b8046-6ef5-452b-b463-71181c0c3742")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dde2b16e-af7b-4da5-8700-b849fc11ab33")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "df259b91-2ba5-48cc-a933-cf03cf209002")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f02ca67-f4c0-411b-b8b8-9375c70b6325")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ee9d8258-eaaf-4617-b511-e51cbb9cc711")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a43040c2-de6b-4da7-bd0f-9cdbb1333681")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
			(uuid "51b7054b-e4cb-4bd2-a86c-24ea653400fb")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 315)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "65b114bc-c8f3-45b8-9945-20e4a0319baf")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 315)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "a1b99f99-c6e7-4eb5-83ee-25b92484e7c4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "a9892559-8839-409d-a758-16f9fc59da9e")
		(at 149.963198 77.443585 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C22"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "a5d8d0b9-8c89-49c2-9b71-3f61379d6dd3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "da0e44a2-65be-41b4-b9e5-ea137659696d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "0ddc51a6-b174-4fb8-b3d0-b0910fbb1a89")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "5f88cf52-4dcc-4063-8196-784a9dd41d17")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/14e80746-68ba-4a2f-9c07-bd95a11b7a1f")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "23325229-7d67-4812-bb1d-4d5f5e52c2cc")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "102afdd5-0b33-46a6-bd4e-8109113c1a37")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "00bec143-ccd7-4d41-a470-ed0103bff2eb")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5480df59-f250-4382-8868-7cee561935d5")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07868227-759b-45f7-b8d2-32f56d0bf27b")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4f1c6b54-4bcf-4a83-9cde-d1d5b3b83956")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9a830d26-b01d-4301-8ee1-364d826260cb")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "365fe30b-4650-4dd4-abe7-b820e20e77d7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "22f442c1-181d-451f-90a6-0247d6e48c15")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "729cf264-1f52-4bc9-bdc2-0583c0908e60")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "c86c238c-14ea-4f3c-ba79-2a07a19b2b6d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 12 "Net-(D4-A)")
			(pintype "passive")
			(uuid "ff0f62d9-ee82-445b-9f90-f170231fbe65")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "3d48ef66-9d2e-4701-b8ea-9debc293ab93")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "ab107845-b1b7-4499-9c2f-49830c7946e5")
		(at 164.77 116.9)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R16"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "248a6e58-1736-4b27-a39a-13adb5db5a6e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "275d8743-03a4-4099-ac1c-958928782d99")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "dabc5c88-b66d-4d39-b42f-0cb64ba360b6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2fff9caa-abaf-465f-914b-cd56ee67c119")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/9d064fc4-b2b9-431e-b621-90c3f092bb46")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8654cbea-5b2e-44a5-9ae9-6161cb8f546b")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ff65b36e-f3a3-4558-92ad-7b8deea77109")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "47ac4b37-67b2-4a7e-bb86-946c38631f47")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6e3c2a36-26ec-4898-84e8-4b44e9e7c457")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "11d32586-d9c7-415d-b07e-a5d0c2a6f432")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "671aba99-262e-49c1-a108-1566d9b6b4a1")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "36dc1423-f121-45f9-9818-8d04ff59e608")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e200a11b-adf6-4984-8cfc-29019ff5aadc")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d98c8f3e-813a-4e0a-8b5b-f022c199529d")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c1ae3f02-9fa5-4c51-bcbf-69598b931585")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4df1527b-8650-4410-939b-772d087f77d5")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 65 "Net-(P1-CC)")
			(pintype "passive")
			(uuid "451f6ec0-a9a9-4b17-83b7-3155c5fb9049")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 18 "VBUS")
			(pintype "passive")
			(uuid "cbef3da2-9061-47c2-af66-d02487dab2d2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "acc3ef9a-24f0-40f9-bd76-2e602fc1664d")
		(at 160.02 122.8)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "a3835af3-3ca3-4554-b308-627a442a7b72")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "a011b47a-4516-4c8e-8cc6-cda1a5826c44")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bbe5fe7c-7af5-40c0-8adf-0f404e43bf27")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "69282ef7-ca83-4e06-8a3e-7824d9e987c5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/fea2aeeb-b62d-480a-81bd-6553581948f0")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7a3c8a4c-b856-45c3-8d11-3f4dae1d94e1")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "786af99e-fc62-4928-8d32-742cf30b3861")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "effc7984-1961-4887-9170-aa0c6219d79a")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c5a6d5b4-d4fb-4f08-84bb-d05af1a641c8")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0aa725e8-102a-4ffa-8e08-820f5afae306")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "55409444-d6e9-4de6-bcb7-85fc49d9f83d")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6762eaf9-d20e-4971-bdee-ccc70344c8d1")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a8c50191-9f64-4db7-be70-89ca833bb7c0")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "293404e3-bd7b-4cd4-a815-a03fe3404123")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cf27b27a-23f1-4b23-a6a9-dc3abc5892ed")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "39654352-1320-4e11-8857-fde6ed4b91e4")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 62 "SPI_SD_CS")
			(pintype "passive")
			(uuid "3107fdf3-00b4-49ff-86d1-774f23c5529c")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "62d14689-bcbf-486e-821f-25d09a5bebef")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "b725ebaa-b833-49a9-a9f8-c5e6e87a6aaf")
		(at 164.77 113.95)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R15"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "82cbe428-28cb-4673-9982-34935f71f852")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "2d29c0c8-562b-4377-af98-73bef3a29030")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d174cc3d-21b6-4520-9941-1c0cf0c02d90")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "72b9c9e0-bb51-4953-ab4a-e35320a8360a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/188fc517-4dcc-4b4c-b8ca-d623c4c0c6c0")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "63e66b57-bda4-4fab-9b92-dbcdd21d99bb")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "56067ed6-ac95-4210-b42a-a4576b32e1fd")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6fcc8d48-809b-43be-ac1e-b86f5566646d")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f56d75b6-8e7f-453d-9829-7d45145bed6e")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bf7b50a1-5cbd-4d80-98dc-bb132fdbacaf")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b0f879cc-bec8-47c7-8134-429c6ce59155")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f243364-a717-4c30-80ce-3c3d411d77b1")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "044b8a16-f029-4bac-b144-9052c9484ce2")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9dc54bfb-16ef-4a47-b63e-e5956733a437")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8bb865af-f371-4882-bdef-a3c31909a578")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "521f5eae-a072-43a7-b0d4-da710b2e51eb")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 59 "SPI_MISO")
			(pintype "passive")
			(uuid "5a05ce68-767d-464e-bd5d-c6479fde0aea")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "77fb4ac7-b6d4-4f0a-a632-12a574986a0b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "b942ff3f-d44a-4542-a1ac-041efe1d8ef6")
		(at 138.048449 72.331203 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "24254d06-6f29-49fd-bb62-e7a869b077c9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "4d2e6fac-733e-4536-993a-26ee0d8725ec")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "cb83de31-1111-4489-8cc4-929c18291865")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "7be60c12-0fe5-4f6c-8e9a-d564957251c7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/ddb78eb8-58c3-4b7e-afc2-40ec57d4cd67")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4044d68e-cce2-49d3-aa87-8b430bd8870c")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "60073732-2e29-465c-9275-50f5de57700f")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9c059f83-944e-483a-9194-d2b2ce05310b")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "05a9a518-3a60-4c92-b03f-076ad9da2489")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c5392037-7952-424f-8a3e-f52d02152176")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c50b7f2b-5a34-44cc-83ce-752e31cff16f")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bc3d192b-5016-4fac-9c39-eda00e37036a")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c5cf1db-0036-4952-b47f-e19090fe3cb5")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e53378bb-675b-4bdf-90b9-72c36b4c1256")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "520902b6-4442-4fe8-85bb-2d6511c958ec")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "4ab80910-4735-413d-9e42-f4192e97eb7c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "95df5bf1-0e53-4718-aa01-f2d9150a762b")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "6bd15f11-787c-4e1e-a35d-b786ff65516f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "bb307c33-4d89-4172-96f9-4e3e2f1a4a82")
		(at 61.45 64.3375 180)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U6"
			(at 0 -3.4 0)
			(layer "F.SilkS")
			(uuid "d5a4d203-b81d-4183-9ab6-f2b7eced1c14")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MAX31855KASA"
			(at 0 3.4 0)
			(layer "F.Fab")
			(uuid "6711ec8d-d2f5-4781-88ca-efbf4105ab92")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX31855.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a59fc46b-26c8-40ac-a13f-6a5d40de18b8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Cold Junction K-type Thermocouple Interface, SPI, SOIC-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6ff9cc70-fdf9-41c4-90c1-5456d0dbbf32")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm*")
		(path "/884d7df7-a31d-462d-909c-1917c119e6ae")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 2.56)
			(end 1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e5e72290-1030-4b7a-a8ad-97bfe9c249b2")
		)
		(fp_line
			(start 0 2.56)
			(end -1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "47e50cf6-ad10-46e4-be05-6482357b9b2b")
		)
		(fp_line
			(start 0 -2.56)
			(end 1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "37f46f9b-eaab-4e35-aa90-a26b84d24626")
		)
		(fp_line
			(start 0 -2.56)
			(end -1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "618fd374-f5b7-48f8-bd3f-95eca2dedfdf")
		)
		(fp_poly
			(pts
				(xy -2.7 -2.465) (xy -2.94 -2.795) (xy -2.46 -2.795)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "89b58b07-fe6e-41ad-ab6d-329b12462028")
		)
		(fp_rect
			(start -3.7 -2.7)
			(end 3.7 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "a577ab5e-7103-4f97-8388-efd58b9d42d0")
		)
		(fp_line
			(start 1.95 2.45)
			(end -1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab8a2e1b-3a84-4c4d-b3af-67f52df60d83")
		)
		(fp_line
			(start 1.95 -2.45)
			(end 1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e237301-3591-41e8-a02d-f0c30876906f")
		)
		(fp_line
			(start -0.975 -2.45)
			(end 1.95 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a141316f-8fc1-42ab-a390-083cf9cafe99")
		)
		(fp_line
			(start -1.95 2.45)
			(end -1.95 -1.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "adef47bf-cdff-451b-bf08-2a387073e6d0")
		)
		(fp_line
			(start -1.95 -1.475)
			(end -0.975 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ec62f3fc-839d-4290-89f4-02a88ca14262")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8255b25a-de33-4670-bc94-3115e33671f1")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "6627d25f-951e-4e30-8444-45dd62e5f173")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(J8-Pin_1)")
			(pinfunction "T-")
			(pintype "passive")
			(uuid "49ebb7f6-33d0-4c74-869a-1b3574701bf3")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(J8-Pin_2)")
			(pinfunction "T+")
			(pintype "passive")
			(uuid "3d7c56fe-f6e7-46c5-95bb-32da9c80e384")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+3V3")
			(pinfunction "V_{CC}")
			(pintype "power_in")
			(uuid "2a7dfad6-0aa7-4eb1-bcd9-51d774824af9")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "SPI_THERMAL_SCK")
			(pinfunction "SCK")
			(pintype "input")
			(uuid "f90a36fd-3da5-4d66-b4c3-185d14fb262b")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "SPI_THERMAL_2_CS")
			(pinfunction "~{CS}")
			(pintype "input")
			(uuid "5dcefe06-3f94-4307-ae0a-355a4383503f")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "SPI_THERMAL_MISO")
			(pinfunction "SO")
			(pintype "tri_state")
			(uuid "cd047695-6717-4c1a-ae6b-7f0e59ea89c2")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "unconnected-(U6-NC-Pad8)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "0173c147-7cb5-4f01-9b1d-02e5fee477fa")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "bda82df6-4313-4d21-a951-a8a85b04e14c")
		(at 64.3375 107.875)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q4"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "d1a7f566-f92e-495d-ad7a-4842adf7e4b0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PNP"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "b84393b4-60bd-4f10-86de-92c1586f9e1c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "dd8a959c-8f48-4110-8fed-4f7909d8a006")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ceb69f46-c31e-44f3-a922-de41e5b9e5c5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d3cccdfd-9e48-45f8-8248-3a53d5125966")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7cab7f3e-2d8a-4930-be03-b696cd1e56c4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "28353271-11a7-446e-b532-5a35e7399e77")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/bcf95ff2-1fe2-4c84-bf12-63478c889d09")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ec5479e6-b944-4cff-bb64-5334e41640c5")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fbeb17fc-05b5-49d0-a309-da8287d003c2")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4f4ae3b7-1e53-4981-8c03-4bb0d114ef08")
		)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8b402ab9-3377-4938-8e1a-1a4d41d0033d")
		)
		(fp_poly
			(pts
				(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.84)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "f9b00fb7-87ab-4361-b0cc-3c9884d955bb")
		)
		(fp_rect
			(start -1.92 -1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "52500f34-354b-4361-80b5-2672632e8ef8")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51fe9295-96cc-4728-8383-bbb012ef621d")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "971d222e-58c9-40ca-ad49-47d1c6a08354")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b4969d52-7a5a-4a50-b984-b8f9a2c6b163")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "92b9c0ac-3b45-4dcb-aa05-14e7d1732279")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b082980d-16c5-458d-93b1-177f9651db6b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5669d7f0-8c66-428e-bb82-dfd47b66efb2")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "Net-(J5-Pin_2)")
			(pinfunction "C")
			(pintype "open_collector")
			(uuid "46048297-53e5-4fec-8ef3-5521c4133f55")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "Net-(Q4-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "b7cc1f32-9dc1-4d4f-a155-7c600be344a0")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+12V")
			(pinfunction "E")
			(pintype "open_emitter")
			(uuid "bfe1d45d-2c2f-477a-97b5-83fdf15632da")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "c56fd8d9-fed1-43ab-aa67-f66f5c77778b")
		(at 164.77 111)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R14"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "ca46af52-a058-491b-bcf2-90dbfa7ee04f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "d653ee28-2946-41f9-abdd-dddf434aa47e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "afcac37d-dfbe-4015-bb1a-06d26184ac0a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8403cdab-e488-4c69-b01e-67bbfff42ce9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1a78330a-c635-4ba6-b23b-8a4fd9b6a143")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e9396bb2-80fe-46e1-bb77-f8d425ee93f1")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b8c0d7f-fe40-46fd-b8e9-f5a829b5d69d")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "30439d09-f468-45a9-92ba-cf62019e6765")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ba83a7b9-b064-44d4-bd35-22b8047a38ad")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "947d4420-d880-44af-bf23-1ff83fd8e4f2")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d077bd26-76c2-4485-9fd2-4659e016f9ed")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b90aa4b5-13ac-4ed8-848e-23aea1f59585")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c9d5f1be-e09b-4ca3-9b86-d66474b697d6")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d48fdc4f-a9fe-45fa-abdc-dd80e67ddeed")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e35e2920-c07c-4240-8422-f501148f6746")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "7498ad8b-697f-4ceb-88f3-5a3d131ba1af")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 60 "SPI_SCK")
			(pintype "passive")
			(uuid "6eccd06c-87a7-47cb-9c8f-888de7faa482")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "532eeac4-1fb8-406c-953b-3321b9b4f02f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_S8B-PH-K_1x08_P2.00mm_Horizontal"
		(layer "F.Cu")
		(uuid "c99597b2-8b58-4bec-a7ea-893b87ac08f8")
		(at 70.8 93.45)
		(descr "JST PH series connector, S8B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH horizontal")
		(property "Reference" "J6"
			(at 7 -2.55 0)
			(layer "F.SilkS")
			(uuid "ac827bec-79d2-4333-bb3a-fb267bc3d38b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Conn_01x08_Socket"
			(at 7 7.45 0)
			(layer "F.Fab")
			(uuid "ea9de23a-a93d-4a65-ae8c-92962b5573d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a92440c6-2c71-4f88-a105-d45560882685")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "70dee2f8-1fa9-43d9-a352-547d854e745e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/b11a1b5e-479e-4ce4-9c91-84d9a867e922")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.06 -1.46)
			(end -2.06 6.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b72dbcc8-3719-40dc-b80a-a2d917183505")
		)
		(fp_line
			(start -2.06 0.14)
			(end -1.14 0.14)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a0103311-bc62-4d36-bc86-a03815706b74")
		)
		(fp_line
			(start -2.06 6.36)
			(end 16.06 6.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "31eee998-da7d-4b04-b6c0-57850de573fe")
		)
		(fp_line
			(start -1.3 2.5)
			(end -1.3 4.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "420bab52-5ca1-45d4-9fba-9800d623d16b")
		)
		(fp_line
			(start -1.3 4.1)
			(end -0.3 4.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "874a1cea-6837-474e-a08e-25a762736795")
		)
		(fp_line
			(start -1.14 -1.46)
			(end -2.06 -1.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9851f6c9-1b34-4e5d-b000-e24e03f0d28c")
		)
		(fp_line
			(start -1.14 0.14)
			(end -1.14 -1.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9a86981a-9f40-4b31-b4c7-6f56100b9331")
		)
		(fp_line
			(start -0.86 0.14)
			(end -1.14 0.14)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "07f4c270-b23e-4053-9a53-daf99691dde6")
		)
		(fp_line
			(start -0.86 0.14)
			(end -0.86 -1.075)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0efc8604-e409-4abc-9ae0-c3d90d5cabf1")
		)
		(fp_line
			(start -0.8 4.1)
			(end -0.8 6.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a30f0f2c-c4db-48e0-bfa4-8b1e6443e0af")
		)
		(fp_line
			(start -0.3 2.5)
			(end -1.3 2.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e9a279c4-c01b-4ab0-8b65-b734fcc03271")
		)
		(fp_line
			(start -0.3 4.1)
			(end -0.3 2.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bb8693da-d678-4050-b277-fd13ee0f8448")
		)
		(fp_line
			(start -0.3 4.1)
			(end -0.3 6.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "51b13832-8673-4737-b1ee-1fec74e92648")
		)
		(fp_line
			(start 0.5 2)
			(end 13.5 2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "626f5bc3-0b4f-4abf-8467-0c069d63cbef")
		)
		(fp_line
			(start 0.5 6.36)
			(end 0.5 2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7e770d00-61f8-43da-bcec-25b02d2c2640")
		)
		(fp_line
			(start 13.5 2)
			(end 13.5 6.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "884a79d1-9288-4708-b2c7-7d7b242f97cb")
		)
		(fp_line
			(start 14.3 2.5)
			(end 15.3 2.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ccad46cd-b2a6-4dc7-b6ab-4a299cc54fc9")
		)
		(fp_line
			(start 14.3 4.1)
			(end 14.3 2.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b0863d18-ea55-49b8-a208-ac951fb980ed")
		)
		(fp_line
			(start 15.14 -1.46)
			(end 15.14 0.14)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d0eacb09-db18-41d8-84b9-fe0284465bcd")
		)
		(fp_line
			(start 15.14 0.14)
			(end 14.86 0.14)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8182d2e9-1258-4880-b886-82e8b7adb823")
		)
		(fp_line
			(start 15.3 2.5)
			(end 15.3 4.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a769860-7b0a-42e1-85fd-e6fb34e4db0e")
		)
		(fp_line
			(start 15.3 4.1)
			(end 14.3 4.1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "81633273-a571-4d4d-881d-d265ff84ed77")
		)
		(fp_line
			(start 16.06 -1.46)
			(end 15.14 -1.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "af066227-16ed-4641-8478-3a0c4617d5b9")
		)
		(fp_line
			(start 16.06 0.14)
			(end 15.14 0.14)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "098a4cc5-9e3f-41c8-a945-c01e439d46aa")
		)
		(fp_line
			(start 16.06 6.36)
			(end 16.06 -1.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3fffa586-ba1c-4eb7-a9fb-ecbc373d8aac")
		)
		(fp_line
			(start -2.45 -1.85)
			(end -2.45 6.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3280ce0f-9f0c-48e6-9694-83a743618cfa")
		)
		(fp_line
			(start -2.45 6.75)
			(end 16.45 6.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ae97342d-5e05-40e7-9610-5ed0f2310c3d")
		)
		(fp_line
			(start 16.45 -1.85)
			(end -2.45 -1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3f57a4db-f7e4-446a-9e11-809aa448d18a")
		)
		(fp_line
			(start 16.45 6.75)
			(end 16.45 -1.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6b081ea9-85f5-425c-ad60-95624809598b")
		)
		(fp_line
			(start -1.95 -1.35)
			(end -1.95 6.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c5dfb55-04f9-4186-ab66-379deadbb65c")
		)
		(fp_line
			(start -1.95 6.25)
			(end 15.95 6.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "73f58fee-676c-4b15-ac59-5bdf2e8fec6d")
		)
		(fp_line
			(start -1.25 -1.35)
			(end -1.95 -1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6d1c6c4c-ba08-449d-9bf0-75e755d2b730")
		)
		(fp_line
			(start -1.25 0.25)
			(end -1.25 -1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be9ea350-7d62-451a-acb1-69158f959b2b")
		)
		(fp_line
			(start -0.5 1.375)
			(end 0.5 1.375)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54ad8d63-c568-4caf-8840-7dbf553c5a8c")
		)
		(fp_line
			(start 0 0.875)
			(end -0.5 1.375)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "02a04a8f-7965-4e56-a743-c41f7f628dac")
		)
		(fp_line
			(start 0.5 1.375)
			(end 0 0.875)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7def15b7-aa88-487b-b075-84b4c059584a")
		)
		(fp_line
			(start 15.25 -1.35)
			(end 15.25 0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "62e68931-8ce0-48e5-8add-2c126520fc6c")
		)
		(fp_line
			(start 15.25 0.25)
			(end -1.25 0.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8abb6fe0-53d1-43ec-b622-d440c40fa52b")
		)
		(fp_line
			(start 15.95 -1.35)
			(end 15.25 -1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "281e6b47-b291-4661-a37a-c4d4843af589")
		)
		(fp_line
			(start 15.95 6.25)
			(end 15.95 -1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "88a9feba-84e4-41a9-8440-e5a622f450ab")
		)
		(fp_text user "${REFERENCE}"
			(at 7 2.5 0)
			(layer "F.Fab")
			(uuid "7ec78226-4429-4d1e-a6b9-131d65b47263")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 1 "+3V3")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "305807a9-fbe0-4a84-8f3e-eda09945ff69")
		)
		(pad "2" thru_hole oval
			(at 2 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "b9f3e422-ff10-459d-9909-2a5f19e4eb85")
		)
		(pad "3" thru_hole oval
			(at 4 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "DISPLAY_SPI_MOSI")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "cd8619cc-58c6-43ce-a687-427c647a7db1")
		)
		(pad "4" thru_hole oval
			(at 6 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "DISPLAY_SPI_SCK")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "8661412d-4531-42e3-937e-c68216312e0c")
		)
		(pad "5" thru_hole oval
			(at 8 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "DISPLAY_SPI_CS")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "ba527d97-13b2-4e36-ab3c-a41e184ae638")
		)
		(pad "6" thru_hole oval
			(at 10 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "DISPLAY_SPI_DS")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "d2ce8d30-6e0a-4c64-9d3a-6ce48c782b3d")
		)
		(pad "7" thru_hole oval
			(at 12 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "DISPLAY_RST")
			(pinfunction "Pin_7")
			(pintype "passive")
			(uuid "16623f8b-0b83-4ac7-8ed5-92e441ad17f2")
		)
		(pad "8" thru_hole oval
			(at 14 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "DISPLAY_BL")
			(pinfunction "Pin_8")
			(pintype "passive")
			(uuid "80c4e2f7-0063-4ec2-bcc6-b5d33e6b5cb4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S8B-PH-K_1x08_P2.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "cd835296-e24a-4f05-aca1-50a1e35392f1")
		(at 114.32 166.6075)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW18"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "38afb6f5-b06b-447e-a734-111010e6d981")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "a3089e1b-bebf-4c2a-b7c3-135f4005571e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bfca49e8-cb62-4ada-b4ca-4d4dcc143396")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "04557031-21a5-4dbf-9b2c-55e8d82d5db4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/2e3f07a3-f917-4cdd-b082-20a785c5af0b")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "83026cdb-a682-4a6e-99c8-252c7036a135")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4fe5fe9b-bd8f-4288-bbe3-42ad226daf2f")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb318dbd-bc1e-490c-95db-c7d2e9c59ca8")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b2647407-b254-41f0-849d-544f1dcf9d64")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "ca287416-943c-4744-88e2-865264455b84")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "9cee49bc-ae11-454d-a238-c1ad4f83c4f4")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "79f3e312-bfcb-41dd-a689-fa6a8702f513")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "5e1d4029-250a-4866-9a5c-9d2aa32043bc")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "33111973-bfcf-4a4b-b776-ebe25ae3ddab")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aef93227-719b-4b21-b570-4a6348223ef0")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "528feb54-c1e9-429b-aafb-b37f81c22f9a")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4c4a6abc-1fd6-468b-9aa3-35fd293d65ed")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7206c257-e415-49bc-ab20-6dc92ce30b87")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c8ac558-84f0-4962-bc1f-44ce6ef24399")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cd2b696f-9460-4fda-8426-3dcdb90fa655")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4eac59e1-73fc-465e-ac10-162ce88ebbcb")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "ba953b6e-92c2-4f04-a62b-1f9684cc269d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "f213c11f-b209-483d-9133-be97bf47471e")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "69bb1596-89d4-4b3c-aed3-b2c9bdc8f82f")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "4fbb5c3c-df1e-481e-80f4-9b55a30bc37a")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "KEYPAD_COL_3")
			(pinfunction "1")
			(pintype "passive")
			(uuid "ca8709e4-c241-477e-b78f-a762816ac16e")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(D20-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "913cedc3-87fa-454b-a87c-ce5303850cca")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_Push_1P1T_XKB_TS-1187A"
		(layer "F.Cu")
		(uuid "ce83780a-a0f0-41a7-9baa-445d963c0766")
		(at 119.15 57.6925)
		(descr "SMD Tactile Switch, http://www.helloxkb.com/public/images/pdf/TS-1187A-X-X-X.pdf")
		(tags "SPST Tactile Switch")
		(property "Reference" "SW2"
			(at 0 -3.75 0)
			(layer "F.SilkS")
			(uuid "4588645e-4309-41d6-b104-e292581b9400")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at 0 3.75 0)
			(layer "F.Fab")
			(uuid "55685e4d-ad54-4359-8cd5-91150095d942")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fdce69cb-035b-4ac5-ade3-e49887173154")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c0f13a5c-72cf-47a0-9e70-bf4edfd09ad3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "44738418-984d-4e56-ad59-4a25e6013020")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f7b14c4d-2aa1-4b6b-aa0d-e33c7d9b0ff1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/67a27820-781a-423e-9d89-5ec4398c5cc9")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.75 -1)
			(end -2.75 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2dbdf214-1037-4257-b0e4-74be0a220962")
		)
		(fp_line
			(start -1.75 -2.3)
			(end -1.3 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1dfc3625-e180-44f0-a605-50bfc797c2d0")
		)
		(fp_line
			(start -1.75 2.3)
			(end -1.3 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "add163f3-2a82-41cf-ad64-d87ab1d47cd8")
		)
		(fp_line
			(start -1.3 -2.75)
			(end 1.3 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4c10c649-29b3-41b3-9060-92849cb79937")
		)
		(fp_line
			(start -1.3 2.75)
			(end 1.3 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cfb021e0-9150-42ac-b5e0-198f6ab208a8")
		)
		(fp_line
			(start 1.75 -2.3)
			(end 1.3 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "baffc2cc-3ae2-4d5d-890d-cb23ef93466c")
		)
		(fp_line
			(start 1.75 2.3)
			(end 1.3 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "26243c95-1c67-4fdf-917b-262d728a91c2")
		)
		(fp_line
			(start 2.75 -1)
			(end 2.75 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dbbcb1ff-6eaa-458d-952f-699cf458496e")
		)
		(fp_line
			(start -3.75 -2.8)
			(end 3.75 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "56e4f277-f8e8-42dc-a33a-14dd2801937e")
		)
		(fp_line
			(start -3.75 2.8)
			(end -3.75 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0aee0b79-b352-4dbe-9af0-d303517b1325")
		)
		(fp_line
			(start 3.75 -2.8)
			(end 3.75 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72e5784f-3c08-4e97-86ce-7733c4545677")
		)
		(fp_line
			(start 3.75 2.8)
			(end -3.75 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ee0c7410-57d6-4e9c-b567-ce3ecf8b258e")
		)
		(fp_line
			(start -2.9 -2.1)
			(end -2.9 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e86d8b23-1243-4bd1-930a-9d34ab45d639")
		)
		(fp_line
			(start -2.9 2.1)
			(end -2.9 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32bf0cb6-7b1f-4f0e-bf68-8fbc8c68fffb")
		)
		(fp_line
			(start -2.4 -1.4)
			(end -1.4 -2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb600080-507b-4bf7-a9af-b3c26a6254a0")
		)
		(fp_line
			(start -2.4 -1.25)
			(end -2.4 -1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "daec8d2c-92b8-47c2-bf83-97236be8b52d")
		)
		(fp_line
			(start -2.4 1.4)
			(end -2.4 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "056c4dc8-9828-4e0a-a77a-d516e9829002")
		)
		(fp_line
			(start -1.4 -2.4)
			(end -1.25 -2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "337e9dac-6405-42ca-b08a-7b7a26a0b2bc")
		)
		(fp_line
			(start -1.4 2.4)
			(end -2.4 1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "29f7bcc2-d95f-4598-90a3-9127cbe97758")
		)
		(fp_line
			(start -1.25 2.4)
			(end -1.4 2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5264cfb5-b2a6-4a1d-805a-8e13be93e1c4")
		)
		(fp_line
			(start 1.25 -2.4)
			(end 1.4 -2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb7be2b5-7560-4f26-bf7b-7eba1f4ae7ca")
		)
		(fp_line
			(start 1.4 -2.4)
			(end 2.4 -1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3dfbd9f7-12ad-414b-a7f1-810b67de2058")
		)
		(fp_line
			(start 1.4 2.4)
			(end 1.25 2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9fe7c1d-ada1-45eb-afc8-0e02b6547045")
		)
		(fp_line
			(start 2.4 -1.4)
			(end 2.4 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb7e2da9-f3d7-4bcd-a672-6c8568216e25")
		)
		(fp_line
			(start 2.4 1.25)
			(end 2.4 1.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b75166a1-af59-494e-907a-6b325c85ec10")
		)
		(fp_line
			(start 2.4 1.4)
			(end 1.4 2.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "66935599-f6fe-4bdd-8d2c-e616f5c8e44d")
		)
		(fp_line
			(start 2.9 -2.1)
			(end 2.9 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a7189648-6a03-4c2e-ab04-90a55d5008df")
		)
		(fp_line
			(start 2.9 2.1)
			(end 2.9 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4730ee07-2d3c-44db-a92e-e2203f56e095")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "e7ebc5cf-e245-4e80-974a-5f2635717230")
		)
		(fp_poly
			(pts
				(xy -1.7 -2.1) (xy -2.2 -1.6) (xy -3.25 -1.6) (xy -3.25 -2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "7f1de605-01c7-43c2-925f-c3f5c1e1b3a8")
		)
		(fp_poly
			(pts
				(xy -1.7 2.1) (xy -2.2 1.6) (xy -3.25 1.6) (xy -3.25 2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "65a62957-05f0-4351-8b31-686b6d12bd91")
		)
		(fp_poly
			(pts
				(xy 1.7 -2.1) (xy 2.2 -1.6) (xy 3.25 -1.6) (xy 3.25 -2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "5fa2615e-229b-4f5f-a6e8-9cc368e71181")
		)
		(fp_poly
			(pts
				(xy 1.7 2.1) (xy 2.2 1.6) (xy 3.25 1.6) (xy 3.25 2.1)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "814295c0-4692-496d-82d7-94a152ec2f46")
		)
		(fp_poly
			(pts
				(xy 0.85 -1.85) (xy 1.85 -0.85) (xy 1.85 0.85) (xy 0.85 1.85) (xy -0.85 1.85) (xy -1.85 0.85) (xy -1.85 -0.85)
				(xy -0.85 -1.85)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "171faf79-2dd3-4e54-9b68-aab9634fd0df")
		)
		(fp_poly
			(pts
				(xy -1.25 -2.55) (xy 1.25 -2.55) (xy 1.25 -1.975) (xy 1.575 -1.975) (xy 1.975 -1.575) (xy 1.975 -1.25)
				(xy 2.55 -1.25) (xy 2.55 1.25) (xy 1.975 1.25) (xy 1.975 1.575) (xy 1.575 1.975) (xy 1.25 1.975)
				(xy 1.25 2.55) (xy -1.25 2.55) (xy -1.25 1.975) (xy -1.575 1.975) (xy -1.975 1.575) (xy -1.975 1.25)
				(xy -2.55 1.25) (xy -2.55 -1.25) (xy -1.975 -1.25) (xy -1.975 -1.575) (xy -1.575 -1.975) (xy -1.25 -1.975)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "867f561e-4cfe-4b06-9e3c-5efc70e3b36d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -3.75 0)
			(layer "F.Fab")
			(uuid "69b83b08-4ee4-40da-a019-f19727eda2cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -3 -1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(uuid "1fe3e103-d44f-4da7-bf7a-5f186c5b61d9")
		)
		(pad "1" smd rect
			(at 3 -1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
			(uuid "1fe3e103-d44f-4da7-bf7a-5f186c5b61d9")
		)
		(pad "2" smd rect
			(at -3 1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "Net-(R5-Pad2)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "482edcb2-f586-4cb6-9c6c-c822c914a3bc")
		)
		(pad "2" smd rect
			(at 3 1.875)
			(size 1 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "Net-(R5-Pad2)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "482edcb2-f586-4cb6-9c6c-c822c914a3bc")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_XKB_TS-1187A.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(uuid "d6789102-a983-4dfd-b361-9e2b1a311e69")
		(at 95.12 166.6075)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW14"
			(at -2.54 -2.794 0)
			(layer "F.SilkS")
			(uuid "c0f28611-75b4-4f82-afdf-69c214074c94")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_Push"
			(at -2.54 12.954 0)
			(layer "F.Fab")
			(uuid "57c00b94-93e6-46be-92af-1bea49225286")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8a11f46a-d04f-4a9e-b759-7293fa30f88e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "38c66989-fa71-499c-bb7b-bfd786c3c12a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/c5e52d60-9701-4e1a-a393-2b2b3fd6715e")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -9.525 -1.905)
			(end 4.445 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "30cd389b-4ece-4179-82c8-6bfc6965c815")
		)
		(fp_line
			(start -9.525 12.065)
			(end -9.525 -1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d13c6125-2d2f-4319-885f-5ced63944045")
		)
		(fp_line
			(start 4.445 -1.905)
			(end 4.445 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b1177033-dccb-495f-b006-8519e92e8ca5")
		)
		(fp_line
			(start 4.445 12.065)
			(end -9.525 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "638aecb1-9249-4851-9c8e-c3c2477e2b7e")
		)
		(fp_line
			(start -12.065 -4.445)
			(end 6.985 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "05c3cb1b-64d3-4dc9-b569-382d22adf7a2")
		)
		(fp_line
			(start -12.065 14.605)
			(end -12.065 -4.445)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "728cec95-c941-43bc-a21d-1b485f8d85ce")
		)
		(fp_line
			(start 6.985 -4.445)
			(end 6.985 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "071e1859-2b3d-416b-98fc-00426e6e646c")
		)
		(fp_line
			(start 6.985 14.605)
			(end -12.065 14.605)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "4a2c90b3-3b6c-44cb-bb15-c52c8145dfef")
		)
		(fp_line
			(start -9.14 -1.52)
			(end 4.06 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d7d273ae-5421-491e-baac-9279892cce95")
		)
		(fp_line
			(start -9.14 11.68)
			(end -9.14 -1.52)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f15dc0db-8d57-42b4-95a1-d5b435ded9bc")
		)
		(fp_line
			(start 4.06 -1.52)
			(end 4.06 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f8bb8915-2496-4313-9a07-ddfe7786093c")
		)
		(fp_line
			(start 4.06 11.68)
			(end -9.14 11.68)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3cfc8e08-5ea0-4bb0-8c42-33c7b3c1794d")
		)
		(fp_line
			(start -8.89 -1.27)
			(end 3.81 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1f73e8f7-fdff-4b26-bf0a-bb1b2aa0de36")
		)
		(fp_line
			(start -8.89 11.43)
			(end -8.89 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa41ec52-3384-4851-b9d8-b075ffb656d0")
		)
		(fp_line
			(start 3.81 -1.27)
			(end 3.81 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6dae4e6-0926-458d-b9be-07307ccde41f")
		)
		(fp_line
			(start 3.81 11.43)
			(end -8.89 11.43)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c55a15de-31cf-418c-bc53-80660a70d1fa")
		)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 0)
			(layer "F.Fab")
			(uuid "040fc9ac-e2ea-4b4a-883a-3106d945e4d5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "b9102a9f-a726-4af5-bf75-7f040bc078e9")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
			(uuid "4bc6a53b-4617-49e2-a296-1a8369f6d30f")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(uuid "e6e8355c-0b61-458b-a35c-a757391d0c8a")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "KEYPAD_COL_2")
			(pinfunction "1")
			(pintype "passive")
			(uuid "e5eb0324-c315-4627-bfb6-ed1f165d9cc4")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(D16-A)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "3d7e6d1e-c29e-4010-a4b5-80e9e951941a")
		)
		(embedded_fonts no)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry mx.step"
			(offset
				(xyz -2.5 -5 5.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "/home/benk/dprog/projects/benboard/kicad/libraries/cherry_mx_r4_keycap.step"
			(offset
				(xyz -2.5 -5 11)
			)
			(scale
				(xyz 1 1 0.8)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "dc0deeca-285e-40b3-a5a9-17a8939b0f47")
		(at 155.27 113.95)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "25c1cce8-93e7-4d42-8526-d1ea59d7107a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "562e277f-c024-4a71-8cc4-81712c67e617")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "befa230f-772b-4908-a9f3-c8bf370abeab")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2941b989-87da-4bda-932f-800c75334089")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/2e51d266-9024-4454-9fa8-05b4762e1505")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5f319187-a300-4512-a307-6dd78dade19d")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1a117781-196a-452d-affa-9df4a1b8147b")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0f6a6523-7261-4e12-a49f-9f471f5fe7ff")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b4b68f04-492b-4964-b6f2-aa16cc2385b9")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "05729fce-584c-41d0-92d2-6dfda1a1d7a1")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "24cee5b2-14ef-4f33-adee-5dff8da4b509")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2e371f0b-763c-408c-b2c5-9541dba94dd8")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb7cf86a-0a3e-4998-8864-397d380fcffd")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "953020df-d569-494c-9e61-e66e8345abe9")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "70dcdb8f-1950-424a-a0b2-a70f50fc4c84")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a04c34f6-97ce-4d4b-8ec3-7f676adc162e")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 75 "QSPI_SS")
			(pintype "passive")
			(uuid "c0d8ec8b-6b00-436f-840f-1376a2a35aff")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 74 "Net-(R3-Pad2)")
			(pintype "passive")
			(uuid "48f9522c-17d5-4c36-a029-c479ec907167")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "e158a8fe-6423-4d91-a90f-80c2955cbad9")
		(at 164.77 108.05)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R13"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "be2d2abb-f0aa-4b56-8ff6-f59bc76d155e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "5ded99e3-4623-495e-bc4f-ea69c9d501e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ad4dc099-7b4a-4101-9674-03f63fd1f45d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "857b7c19-b30b-4e65-a836-dfb77573a30c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1595c8cd-1917-48dd-9d78-089ecac964b5")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7cf6bb9b-b08d-4cf5-b496-754c7de8c99e")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "17e9c6f8-93c5-4aa7-9554-998fcf1a5f21")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2334a1e2-5f2e-40a8-8b95-523f81cbf6e7")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aa1f135a-6cc7-430d-8faa-128e40a4de30")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f071b73d-62f2-4ef1-ad9b-3d1ff0adeb48")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc6a42bb-afe5-490f-858f-89681f949499")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4998079d-c1a1-4910-98b3-de95c62003f8")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "012b5827-bbc2-4502-b1f8-7fe9e1c13a68")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "72a9262f-f83d-4417-981c-b68c60c77dce")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7de69b43-8895-417d-8ec4-897379510690")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "1730d892-c5dc-41db-a870-a8e38d94969f")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 61 "SPI_MOSI")
			(pintype "passive")
			(uuid "40e8dc1a-f8bb-4684-a356-ddab7580e139")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "a4f67666-4074-4254-b06f-8176766c93fb")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
		(layer "F.Cu")
		(uuid "e249a9d8-0f7d-4a6c-a183-938a3e8ffb08")
		(at 95.1875 81.685 180)
		(descr "SOIC, 8 Pin (JEITA/EIAJ 08-001-BBA and Atmel/Microchip, 208 mils width, https://www.jeita.or.jp/japanese/standard/book/ED-7311-19/#target/page_no=21, https://ww1.microchip.com/downloads/en/DeviceDoc/20005045C.pdf#page=23, https://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf#page=162), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO P-SOP SOP SOP-8 SO SO-8 8S2 S2AE/F K04-056 CASE-751BE SO8W 8-Pin-SOIC PSA W8-2 W8-4 W8MS-1")
		(property "Reference" "U1"
			(at 0 -3.6 0)
			(layer "F.SilkS")
			(uuid "8b6475dd-b5fa-4e82-af9e-121720e2b031")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "W25Q128JVS"
			(at 0 3.6 0)
			(layer "F.Fab")
			(uuid "ef909ebe-b80d-4cea-9c70-e08e0f26a179")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/w25q128jv_dtr%20revc%2003272018%20plus.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "12031370-403f-46ea-a755-af454b6b769a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "128Mbit / 16MiB Serial Flash Memory, Standard/Dual/Quad SPI, 2.7-3.6V, SOIC-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "00fffcae-9882-42a7-87a6-34daa7611d71")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "809aac12-7ebd-44da-a744-7ca591089bed")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "862e4d43-3317-40d8-89fd-b514d62a85e4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*SOIC*5.3x5.3mm*P1.27mm*")
		(path "/17c7e4aa-16ce-4e0c-be5f-72596dfc57db")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start 2.76 2.76)
			(end 2.76 2.49)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2e92a81-7e3f-4a97-b6b4-2c3a56d87141")
		)
		(fp_line
			(start 2.76 -2.76)
			(end 2.76 -2.49)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c38bba83-b25f-4016-b283-97f62fce0108")
		)
		(fp_line
			(start 0 2.76)
			(end 2.76 2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91552237-c686-4e80-a3ea-6b44311221aa")
		)
		(fp_line
			(start 0 2.76)
			(end -2.76 2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3129cbdd-eee9-450d-a7c8-f62f8aad94b3")
		)
		(fp_line
			(start 0 -2.76)
			(end 2.76 -2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "50188907-f589-43b4-9189-14e29067ce32")
		)
		(fp_line
			(start 0 -2.76)
			(end -2.76 -2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f7e5ce3c-c2f3-48a4-97d5-d0e97da727bf")
		)
		(fp_line
			(start -2.76 2.76)
			(end -2.76 2.49)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "50d3b757-f9bb-46c8-96d6-c094d875d596")
		)
		(fp_line
			(start -2.76 -2.76)
			(end -2.76 -2.49)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f531f15b-8c7e-4ab7-b6c8-616f3555fd13")
		)
		(fp_poly
			(pts
				(xy -3.525 -2.49) (xy -3.765 -2.82) (xy -3.285 -2.82)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "48a76268-679d-4b01-851a-cd7370c96439")
		)
		(fp_rect
			(start -4.65 -2.9)
			(end 4.65 2.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "f98a1bb8-aede-4614-9f65-da4b4781b5f7")
		)
		(fp_line
			(start 2.65 2.65)
			(end -2.65 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a92575ed-27f9-4f8b-ae40-c2c0ab70287a")
		)
		(fp_line
			(start 2.65 -2.65)
			(end 2.65 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e3afb049-e321-44fa-8a19-18802299fe94")
		)
		(fp_line
			(start -1.65 -2.65)
			(end 2.65 -2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c5c50f70-6771-4e55-adfd-23d6e645766c")
		)
		(fp_line
			(start -2.65 2.65)
			(end -2.65 -1.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "94550374-01a7-4eae-94b3-a1b3932393f6")
		)
		(fp_line
			(start -2.65 -1.65)
			(end -1.65 -2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae806656-ca41-48f7-b1c7-9b8c5bf2ffc7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "940df6d3-611a-4f6a-8ae1-b7414a5d27f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -3.5875 -1.905 180)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "QSPI_SS")
			(pinfunction "~{CS}")
			(pintype "input")
			(uuid "0ef61d2d-8c59-4f34-ad81-ef491ddaef57")
		)
		(pad "2" smd roundrect
			(at -3.5875 -0.635 180)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "QSPI_SD1")
			(pinfunction "DO/IO_{1}")
			(pintype "bidirectional")
			(uuid "819017c9-2850-4cc9-b87f-2a60aa953343")
		)
		(pad "3" smd roundrect
			(at -3.5875 0.635 180)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "QSPI_SD2")
			(pinfunction "~{WP}/IO_{2}")
			(pintype "bidirectional")
			(uuid "6917992e-b809-45f5-9005-618f409cef46")
		)
		(pad "4" smd roundrect
			(at -3.5875 1.905 180)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "4788545d-8572-4f68-b53a-62e4e38594b2")
		)
		(pad "5" smd roundrect
			(at 3.5875 1.905 180)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "QSPI_SD0")
			(pinfunction "DI/IO_{0}")
			(pintype "bidirectional")
			(uuid "e9724939-16f9-49ab-9d12-19b5693f1956")
		)
		(pad "6" smd roundrect
			(at 3.5875 0.635 180)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "QSPI_SDCLK")
			(pinfunction "CLK")
			(pintype "input")
			(uuid "2210d882-7051-4496-8cad-0225cf554ead")
		)
		(pad "7" smd roundrect
			(at 3.5875 -0.635 180)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "QSPI_SD3")
			(pinfunction "~{HOLD}/~{RESET}/IO_{3}")
			(pintype "bidirectional")
			(uuid "c68f7a7d-9fcd-472b-8012-052cd8cda40b")
		)
		(pad "8" smd roundrect
			(at 3.5875 -1.905 180)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "9c3fd6f4-df26-4b8a-89e0-43493f49511c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_5.3x5.3mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "eb51be28-aedb-4cba-923e-fdf5243bcea9")
		(at 94.95 62.15)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "a96586a4-308e-4625-9ad4-cf8e902f9841")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LED"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "86afec86-467e-4df1-b19e-c9014005acf5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ce25d75d-d7cd-4a65-b868-77d1c75ae04b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "135dfd3f-1e34-4305-b02b-2a3eb9c8e0cc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2553a80e-d302-47a2-b183-44e0595439df")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/16b30f34-0e17-4551-a627-ed5abaddcf08")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5460b2d7-d62c-4916-91c8-6d2875ad066b")
		)
		(fp_line
			(start -1.86 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10b02703-c3cc-400d-8583-af3785276980")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "89c1f983-35a7-4ec0-aee7-25b79e604fd9")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bb236f99-ff7f-41b4-aa11-04ccf1cb3271")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "196466e3-eb8a-4bb3-bed3-c9a61db6d2dd")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "71cf70d8-ca31-49d2-b990-f4df6f81bb98")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7b04ab15-292a-4dd2-8de9-7a91fc25b128")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c47e9268-86cb-4ad4-b427-c031449a52e3")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6adafbef-b359-48a6-9a6c-be184690fc0a")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "67bb0386-71e8-4834-876f-6a003500ffcc")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "221c25f7-7015-4a8d-8aef-063cae4fdec2")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8e794919-fa61-4520-8833-4d70cf28aa4b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ce55b0cc-b767-4dc9-bfed-5eb198f7fa9e")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "4a4cdee8-66d3-46e8-8ae0-11e9ce65ee36")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 17 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "114461e9-e3eb-43cd-a2f9-7402f12fc066")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "eba8d8b0-e2b2-4ff3-aaec-44cc2ee796fa")
		(at 143.160831 84.245952 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "11e55bea-6fb4-412a-be45-65cc6cbb09a7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "15pF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "8840b585-c684-4d9c-9228-9d22a45634dc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "65b43143-d1e2-4ee2-ba3d-1254231a07b5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "67c0d1e9-7147-46fd-b80a-545ecca660c8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/f6f78418-a8b8-4a89-9273-4e67878abd49")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "21bd18e0-fcf0-4526-b8fa-277c440f35be")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ffcb8958-ca50-4a0c-ad52-c194b380356a")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb0f4b3c-4094-47ef-8269-dac3093a9e1f")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "766f1023-bf73-4d38-9e92-1ac8315f761b")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ab5eff22-c5d1-4d9b-a539-9aa901a761aa")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7fccdc2e-2681-4cb2-8ee8-9c7d6b3b1a3b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e67b3c1-8736-43e0-abd2-c1038ceff2fa")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ca9bb04-4807-4864-a954-d0de14b148ef")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9ad810c7-677f-4bcf-9a58-87ac0f1df73f")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f2fb2027-bb6e-4666-87f3-1532ab051eb2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "cd07603e-6245-4c60-ab4c-2727e2610b7b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 6 "Net-(C5-Pad1)")
			(pintype "passive")
			(uuid "72016c52-365d-4df4-92cf-fa7ae6908322")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "24ca0e8a-3ecc-40e4-8516-c3c18b432314")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "f035c8d7-c216-44bb-9b9d-bc8317f9b458")
		(at 160.02 116.9)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "69fc0840-6f6f-4b10-b87a-71c3def2fdc4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "150"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "f9ae6963-ec90-46b4-ad7f-2cc5a3bfa690")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "474dc554-145b-4185-abcf-7fdf218347c5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7c20d569-6cdb-4d56-b513-fd5437100b10")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/c9453c8a-4558-47f8-8696-59d90c85fcb6")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5f72bdf4-a2a7-49b5-938e-639af16346bd")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "48360b0c-e4df-442f-a6fc-01a06935a384")
		)
		(fp_line
			(start -1.85 -0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4fa1e792-ba74-4e92-991c-b5931b37d268")
		)
		(fp_line
			(start -1.85 0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7462b320-df7f-4753-bcc9-3a4a75b06a08")
		)
		(fp_line
			(start 1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "88cefbe2-88fe-49b1-963a-05540f1229ab")
		)
		(fp_line
			(start 1.85 0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5d3acfa4-4435-4c5f-809c-0f0d80d94293")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c235eaba-e94f-40f4-8d62-5dbb6c90373d")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0ba01df4-efda-44ea-a4b6-d9468fb80a1c")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "78d99384-2e0b-404a-8263-234fad24cac4")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "df8c1c7b-a548-4f97-abe6-fe18da8fc3b2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ca9721c9-15dd-4dd7-936f-0f4fa20197a8")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 81 "Net-(U2-GPIO25)")
			(pintype "passive")
			(uuid "fffe952f-4044-43c2-b6f6-418e514f404e")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 17 "Net-(D1-A)")
			(pintype "passive")
			(uuid "9afd5187-8ed3-4108-b072-be0c6e04ded1")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "f085fdbf-339e-45ec-b512-09a5020beeec")
		(at 136.775656 77.860778 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "819a1184-0fba-43e2-b783-1443eae9fbea")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7uF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "eb100ea0-be29-42fa-bf54-b4b81853b705")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "e5796254-e3df-4c75-9d35-e10798f5931c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "8ed594c4-a44f-4e81-b94b-57254ce9d956")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/be311850-fc1f-48e2-bb71-4a0eda559f4d")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e3238516-07f3-4616-bd94-f6b7f8e97b9e")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ce31a2a3-7f09-4282-8b55-3dacbfbd2b09")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "faf84d55-c9ce-4d77-a97b-98991b04d2f8")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "15000915-a46b-4582-9cb9-b89a5d8f45b5")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "508320ac-bd83-457f-a770-b0934302d391")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b367b389-8ac4-46e7-ab52-d94f917369b2")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b0ba75d-be75-42de-bf4d-c4dce336e11a")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2679e477-29fe-4dd2-b39a-1e959f2f6d47")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0182d34a-89fa-493b-aff8-c1123efa56c8")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "71a151b3-f138-42e5-b5ed-744ed88f5786")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "17039449-eb16-4bce-b941-77f8c1d7ae63")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "+1V1")
			(pintype "passive")
			(uuid "372dcd19-f00c-4ec4-9343-98a396f9f78c")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "7852f022-d44d-430e-b609-832172ba6db8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_SMD_Abracon_ABM8G-4Pin_3.2x2.5mm"
		(layer "F.Cu")
		(uuid "f5c65689-4357-4317-a653-fa2707b900eb")
		(at 75.85 69.25)
		(descr "Abracon Miniature Ceramic Smd Crystal ABM8G http://www.abracon.com/Resonators/ABM8G.pdf, 3.2x2.5mm package, generated with kicad-footprint-generator make_crystal.py")
		(tags "SMD SMT crystal")
		(property "Reference" "Y1"
			(at 0 -2.45 0)
			(layer "F.SilkS")
			(uuid "db31b64d-bb7a-4d1c-a89d-7d7e2db8855c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "12MHz"
			(at 0 2.45 0)
			(layer "F.Fab")
			(uuid "4f3447e0-3a5b-4da8-a40a-c4bb7204f59b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c7a1bfa6-f661-4f13-8195-96e7781624f9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Four pin crystal, GND on pins 2 and 4, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f0837ef4-108e-40e4-8c54-4ae4ce746283")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Crystal*")
		(path "/3e64e7e2-6bc8-44c3-9574-fd6a0ce8c4f9")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.06 -1.71)
			(end -2.06 1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "17309373-f4c5-43c6-bd1d-efc51213ce63")
		)
		(fp_line
			(start -2.06 1.71)
			(end 2.06 1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf2058be-e5ac-4b6c-bbf6-b12899431b7a")
		)
		(fp_rect
			(start -2.1 -1.75)
			(end 2.1 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "6ed96927-cbb6-4cfb-9943-82929b5fb6cf")
		)
		(fp_poly
			(pts
				(xy -1.6 -1.25) (xy -1.6 0.625) (xy -0.975 1.25) (xy 1.6 1.25) (xy 1.6 -1.25)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "bd5494f0-4e7b-4323-bbc5-0dfd45fc4566")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f91c1ec9-6091-460f-a424-46ff84afb91b")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1 0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 5 "Net-(U2-XIN)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "928a49f1-46d0-4577-aebd-ca7a65d68ff8")
		)
		(pad "2" smd roundrect
			(at 1.1 0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "GND")
			(pinfunction "2")
			(pintype "passive")
			(uuid "7a0715ed-3191-47c4-884c-7603ee68d3e2")
		)
		(pad "3" smd roundrect
			(at 1.1 -0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 6 "Net-(C5-Pad1)")
			(pinfunction "3")
			(pintype "passive")
			(uuid "c38ab40f-1e7a-40fb-9eb1-31b3dfe110e7")
		)
		(pad "4" smd roundrect
			(at -1.1 -0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "GND")
			(pinfunction "4")
			(pintype "passive")
			(uuid "c91b2a8f-6c37-458e-b829-4939ed64ee7f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_Abracon_ABM8G-4Pin_3.2x2.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "f6446fd9-172f-42a9-80a8-bc9a12b60226")
		(at 151.23599 71.91401 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C28"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "de6df64b-efe3-4083-8f34-aafe4ffa566f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "fb0e7916-c987-4075-949b-be3542583af2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "fc94a7a6-62cb-4f6c-b436-134a7b2fcbac")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "741314f9-8ef7-441d-9624-d8b3e1e52312")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/ee1ffa83-1b60-41e6-92b5-21236267f87d")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "82a1db3c-c434-42e7-a36a-02b443d0bc39")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "85e401c4-5e5a-4104-81fe-fcc2c31cf9c2")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fab60e05-d7b7-4f85-9003-9442158634f1")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f421d583-f29d-45c1-99af-44e16a87b48d")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d4046986-ea94-471e-b3a1-e00a6d2812ff")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ac58add8-6d7e-41f2-b731-8b6e502a4067")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3de98a3c-f708-4f88-bbaa-e87b2d3e074b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e0e57c99-d228-4830-8f0c-af18c40e429a")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9cf2f309-8cee-444a-a04e-0b26bdde2d8b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be5aac30-ce63-42ce-a8e5-14966b2d18ed")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "d28b0d6b-8b6a-4897-86e5-d8a648daf013")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "518ddd1f-b86e-486b-b017-4a3f0d96a268")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "e4359db6-94eb-4728-b16e-6b422916fb81")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "f997dff4-222f-4f8a-b6fa-0f86a7121029")
		(at 65.25 87.4625)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "30c0307c-17d1-4247-acbb-7b84b4396fa5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "076c3d69-738f-413b-8bfb-eab3de43b4b2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "26dd70b4-a6db-4578-83fa-1e01498516bd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "34b8c88f-58e7-468a-8c38-3aaaa29acb9e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/95962086-9e81-488c-a83b-f6e42f57cba4")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f05c7db5-f2a7-48e4-9c8b-51038515d63a")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8f9327a0-2457-4841-bef0-ba424c56b295")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9a3a1033-c515-4c80-82a8-679dbbc2158a")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b68bb7f4-8eab-4db4-b3af-bb9fffdab718")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ccb7b093-d4f5-4c95-8057-bfa35f99971a")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3cc4f25b-71d9-484c-a088-b324bcd1bec1")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f750f0c0-8bec-4099-8ff3-15a0dcd1b3cd")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "972c38e0-f302-42c1-8d8c-23fc2b38083a")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9d0ae965-7e24-49e0-81ba-29d6bdaac87e")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7ac9df1-1e4b-4281-bec1-bcf26e457b61")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d6f1fdff-892c-46d2-b274-274245fd01a8")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 7 "Net-(Q1-C)")
			(pintype "passive")
			(uuid "971edd35-cdaa-4597-811a-2db21850c178")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "9243de7b-ca34-4aeb-aaa9-ec06ba01ca2a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(uuid "fd6b83af-7e45-4def-bda7-86f19689b085")
		(at 154.219981 81.700368 45)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C24"
			(at 0 -1.679999 45)
			(layer "F.SilkS")
			(uuid "2ae1b37a-e1e3-4975-9327-ce8212dccd9f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.679999 45)
			(layer "F.Fab")
			(uuid "16424643-0863-4b51-add6-64673ec74b53")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "ef2c756d-1506-41b5-bf1c-570f24e93ff6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "1a55cced-04ca-4f98-9ded-56fc9a5c1aac")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/3d9cdfd1-725c-4595-b94e-70cdac6cc24f")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7c3fb99f-2a42-4dda-ba3f-b6f262e247e7")
		)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ce6b4626-4f3e-447e-90bf-5ee300eaf02e")
		)
		(fp_line
			(start -1.88 -0.98)
			(end 1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07afb2b0-7ceb-4b1b-955f-e375a9b40a00")
		)
		(fp_line
			(start -1.88 0.98)
			(end -1.88 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "037b2f71-3cf3-42b5-aaee-b6f2c1117563")
		)
		(fp_line
			(start 1.88 -0.98)
			(end 1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "840268e5-33c2-44dc-a4e4-2f3a1fd6021b")
		)
		(fp_line
			(start 1.88 0.98)
			(end -1.88 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6bb60d22-114a-4ac6-a02c-e76fb60a4096")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2c9a9fe0-f246-4fd5-b024-c654d9708a99")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa3c496b-85ad-4949-b0bb-21c791c60489")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c8bfcc8a-6525-4307-9047-d066d78fc884")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f687aa7-d412-41e2-88b7-ec478dad4b79")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "b54589e1-ab75-4e5c-8d0d-feaa8524741d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "+3V3")
			(pintype "passive")
			(uuid "d4992371-4786-4cda-a76d-214ec3dfd1e5")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 45)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
			(uuid "cc65ca2f-b69d-4b63-8d21-946a4dacf598")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Toaster:RP2350A_QFN-60_EP_7.75x7.75_Pitch0.4mm"
		(layer "F.Cu")
		(uuid "fef2e02e-f9aa-4b87-bc35-4a582c22f574")
		(at 80.696878 76.6 -135)
		(property "Reference" "U2"
			(at -5.340864 -5.835839 45)
			(layer "F.SilkS")
			(uuid "ac5332c8-85b2-4c80-8870-60a7182cbdc8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "RP2350A-QFN60"
			(at 0 5.550001 45)
			(layer "F.Fab")
			(uuid "c42bf74e-484f-4672-9efa-3b2abcc8051b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "68d4c0ac-1edf-4f66-bb8b-802337f57bd2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
			(uuid "7587f10c-05b5-4bd4-8852-68c0c1040716")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/2439e9bc-b652-4896-8161-ee93cbceff51")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start 4.025 4.025)
			(end 4.025 3.2)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "5831a7eb-5873-474b-acf2-fea4e017697b")
		)
		(fp_line
			(start 3.2 4.025)
			(end 4.025 4.025)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "0e529cc7-313a-469c-9e7a-530858ece936")
		)
		(fp_line
			(start -3.2 4.025)
			(end -4.025 4.025)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "2ec56531-6656-4cc4-a886-7d67a142a346")
		)
		(fp_line
			(start -4.025 4.025)
			(end -4.025 3.2)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "97792c29-3d38-4f12-abe6-9220e3125e75")
		)
		(fp_line
			(start 4.025 -4.025)
			(end 4.025 -3.2)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "641eeb62-4c70-4e1f-a87f-04ca0f2c02dd")
		)
		(fp_line
			(start 3.2 -4.025)
			(end 4.025 -4.025)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "e333dddb-2859-4f60-b3b5-2d3d01d7ab30")
		)
		(fp_circle
			(center -3.922752 -3.962399)
			(end -3.454399 -3.9624)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "0a306899-4748-49ee-9f11-9346d16e1eae")
		)
		(fp_line
			(start 4.55 4.55)
			(end -4.55 4.55)
			(stroke
				(width 0.05)
				(type default)
			)
			(layer "F.CrtYd")
			(uuid "625547c2-b219-42cc-934d-e8c00a9c221e")
		)
		(fp_line
			(start -4.55 4.55)
			(end -4.55 -4.55)
			(stroke
				(width 0.05)
				(type default)
			)
			(layer "F.CrtYd")
			(uuid "f4b7aea1-f388-446d-8019-14558037f28e")
		)
		(fp_line
			(start 4.55 -4.55)
			(end 4.55 4.55)
			(stroke
				(width 0.05)
				(type default)
			)
			(layer "F.CrtYd")
			(uuid "85e46c76-370d-490a-899f-5b74004f2937")
		)
		(fp_line
			(start -4.55 -4.55)
			(end 4.55 -4.55)
			(stroke
				(width 0.05)
				(type default)
			)
			(layer "F.CrtYd")
			(uuid "06d1a9cd-b942-4797-9dde-a8778403196d")
		)
		(fp_line
			(start 3.875 3.875)
			(end 3.875 -3.875)
			(stroke
				(width 0.15)
				(type default)
			)
			(layer "F.Fab")
			(uuid "ebb1e889-d5bd-432a-9248-7f2e05f22a2b")
		)
		(fp_line
			(start -3.875 3.875)
			(end 3.875 3.875)
			(stroke
				(width 0.15)
				(type default)
			)
			(layer "F.Fab")
			(uuid "9b5327f0-9f26-42e7-8e57-252d4ace2840")
		)
		(fp_line
			(start 3.875 -3.875)
			(end -2.875 -3.875)
			(stroke
				(width 0.15)
				(type default)
			)
			(layer "F.Fab")
			(uuid "7abaa2b6-c15b-4e50-96ff-c303473e2440")
		)
		(fp_line
			(start -3.875 -2.875)
			(end -3.875 3.875)
			(stroke
				(width 0.15)
				(type default)
			)
			(layer "F.Fab")
			(uuid "bd7fb045-d718-4585-a5a4-21452758f199")
		)
		(fp_line
			(start -2.875 -3.875)
			(end -3.875 -2.875)
			(stroke
				(width 0.15)
				(type default)
			)
			(layer "F.Fab")
			(uuid "d845369a-21f8-4b6d-acee-a9c56c5bccb4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
			(uuid "42b1b433-d6cc-4696-a7eb-454ad4041694")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" smd rect
			(at -1.275001 -0.425 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "37422606-b183-4844-8fcb-019193198894")
		)
		(pad "" smd rect
			(at -1.275001 0.425 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "0df0facc-201c-44c6-8493-d43781bd67b4")
		)
		(pad "" smd rect
			(at -1.275 -1.275 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "090753f9-b8b4-4288-ab34-2b7bcce0e47a")
		)
		(pad "" smd rect
			(at -1.275 1.275 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "f9648f42-a7a4-47d2-a945-798f73be425e")
		)
		(pad "" smd rect
			(at -0.425 -1.275001 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "1ae3b112-8bd6-451b-9868-7187e6b36d7e")
		)
		(pad "" smd rect
			(at -0.425 -0.425 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "875092ea-f581-437d-8350-693da7f82b42")
		)
		(pad "" smd rect
			(at -0.425 0.425 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "53a3ed2d-6cde-4341-8018-ccb2d974e412")
		)
		(pad "" smd rect
			(at -0.425 1.275001 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "41ca0012-ad28-4990-a93a-01ae90ce488c")
		)
		(pad "" smd rect
			(at 0.425 -1.275001 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "06476146-6f22-4f7c-a10e-759ad5f00013")
		)
		(pad "" smd rect
			(at 0.425 -0.425 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "6949f832-bf90-4457-b208-7c6f8f29467a")
		)
		(pad "" smd rect
			(at 0.425 0.425 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "e06df1d4-3187-4fdf-b4c4-ff161dbee4cd")
		)
		(pad "" smd rect
			(at 0.425 1.275001 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "4f1b2d20-2fd6-417d-a83e-0883b66c5762")
		)
		(pad "" smd rect
			(at 1.275 -1.275 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "a72881c4-3e03-46ce-9621-d0a2fa005dee")
		)
		(pad "" smd rect
			(at 1.275 1.275 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "644ca4e4-f2c8-4d9e-af03-ef55ffb044b0")
		)
		(pad "" smd rect
			(at 1.275001 -0.425 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "689916ff-4197-4f0a-8aef-d42ca283a1ef")
		)
		(pad "" smd rect
			(at 1.275001 0.425 225)
			(size 0.1 0.1)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
			(uuid "5dddcf25-a878-4e05-8d83-5f3af7b01e37")
		)
		(pad "1" smd rect
			(at -3.437501 -2.8 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "64087625-cf7a-41d3-8dac-2ea53b2e5c37")
		)
		(pad "2" smd rect
			(at -3.4375 -2.4 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "SPI_THERMAL_2_CS")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "17fc35e0-5467-4b57-9743-aa7af21eb867")
		)
		(pad "3" smd rect
			(at -3.4375 -2 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "SPI_THERMAL_1_CS")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "e196a028-ebe5-41ce-b906-93f31fd648da")
		)
		(pad "4" smd rect
			(at -3.4375 -1.6 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "SPI_SD_CS")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "bb21b792-c0c0-4241-abac-cd1252da3b29")
		)
		(pad "5" smd rect
			(at -3.4375 -1.200001 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "SPI_MISO")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "c28f01a5-0c04-45f5-996b-0799ec813388")
		)
		(pad "6" smd rect
			(at -3.4375 -0.8 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+1V1")
			(pinfunction "DVDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "fe667b91-367a-43f0-a3de-d478055a00af")
		)
		(pad "7" smd rect
			(at -3.4375 -0.4 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "SPI_MOSI")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "a31bf5ba-707c-4336-b5a7-4210d84b91e6")
		)
		(pad "8" smd rect
			(at -3.437501 0 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "SPI_SCK")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "fd2718f7-db5e-4198-aaf0-89864671413c")
		)
		(pad "9" smd rect
			(at -3.4375 0.4 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "KEYPAD_COL_0")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "05f87333-7ccf-4148-a688-cf3189ce941a")
		)
		(pad "10" smd rect
			(at -3.4375 0.8 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "KEYPAD_COL_1")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "9ec56f10-660b-4765-b487-5bda9b6bd57d")
		)
		(pad "11" smd rect
			(at -3.4375 1.200001 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "d8139d35-e22d-416f-81c2-3e9b8a5f7f76")
		)
		(pad "12" smd rect
			(at -3.4375 1.6 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "KEYPAD_COL_2")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "547d5469-bd51-4a1e-a1e3-98939f2d0072")
		)
		(pad "13" smd rect
			(at -3.4375 2 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "KEYPAD_COL_3")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "ea8e3734-3459-4057-af69-ad103bbf558d")
		)
		(pad "14" smd rect
			(at -3.4375 2.4 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "KEYPAD_ROW_0")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "07806098-8dac-45b2-b216-15470041a347")
		)
		(pad "15" smd rect
			(at -3.437501 2.8 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "KEYPAD_ROW_1")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "e5c7d8b3-53ca-4785-b14a-234bd69ce7f1")
		)
		(pad "16" smd rect
			(at -2.8 3.437501 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "KEYPAD_ROW_2")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "a584b167-474a-45c9-8f65-151194fe8f20")
		)
		(pad "17" smd rect
			(at -2.4 3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "KEYPAD_ROW_3")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "dffb5038-3f71-4db6-8ae0-9cc0f563ce17")
		)
		(pad "18" smd rect
			(at -2 3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "USR_PWM_0")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "29829719-1155-44f4-aa9f-0cf267d16f2f")
		)
		(pad "19" smd rect
			(at -1.6 3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "USR_PWM_0_AUX")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "63959240-a92c-4d2d-918e-def3468a1bda")
		)
		(pad "20" smd rect
			(at -1.200001 3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "6b494bf0-6933-4ef1-a97b-5d730f776c5e")
		)
		(pad "21" smd rect
			(at -0.8 3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(U2-XIN)")
			(pinfunction "XIN")
			(pintype "input")
			(thermal_bridge_angle 45)
			(uuid "25930d37-1efa-45cb-a42e-1d4eaa1e50e6")
		)
		(pad "22" smd rect
			(at -0.4 3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "Net-(U2-XOUT)")
			(pinfunction "XOUT")
			(pintype "output")
			(thermal_bridge_angle 45)
			(uuid "473384d4-4829-4b62-812a-27e482a90247")
		)
		(pad "23" smd rect
			(at 0 3.437501 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+1V1")
			(pinfunction "DVDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "961ff5c1-515b-4a35-acf8-40433f2d5ba6")
		)
		(pad "24" smd rect
			(at 0.4 3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "SWCLK")
			(pinfunction "SWCLK")
			(pintype "input")
			(thermal_bridge_angle 45)
			(uuid "b20c1dcd-cd2b-418d-a93c-959a67fb03d3")
		)
		(pad "25" smd rect
			(at 0.8 3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "SWIO")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "39b2fa55-2d75-4975-ae72-d24001c847a2")
		)
		(pad "26" smd rect
			(at 1.200001 3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "RESET")
			(pinfunction "RUN")
			(pintype "input")
			(thermal_bridge_angle 45)
			(uuid "d8acb26e-70b6-48bf-8d17-2c346bb585ae")
		)
		(pad "27" smd rect
			(at 1.6 3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "USR_PWM_1")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "78c38cd9-9cd8-4b43-95c6-c6a23c2d1847")
		)
		(pad "28" smd rect
			(at 2 3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "USR_PWM_1_AUX")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "cc77cc07-027c-437a-ad23-599fd667e9b2")
		)
		(pad "29" smd rect
			(at 2.4 3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "SSR_SWITCH")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "36406cf7-8b5a-42e7-89f5-f9bcb19b9872")
		)
		(pad "30" smd rect
			(at 2.8 3.437501 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "8315959a-49ed-4166-ba68-ac8d18f69ea4")
		)
		(pad "31" smd rect
			(at 3.437501 2.8 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "DISPLAY_SPI_MOSI")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "cd3b2e4a-b5c8-4095-926f-e3ae7f0d5044")
		)
		(pad "32" smd rect
			(at 3.4375 2.4 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "DISPLAY_SPI_SCK")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "069ab311-992b-42b2-9756-b91abd1dd8ec")
		)
		(pad "33" smd rect
			(at 3.4375 2 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "DISPLAY_SPI_CS")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "79820540-687c-4ba4-9ef3-d19d08d71933")
		)
		(pad "34" smd rect
			(at 3.4375 1.6 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "DISPLAY_SPI_DS")
			(pinfunction "GPIO22")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "817d6fac-8578-4ae0-bdef-7e542c40e294")
		)
		(pad "35" smd rect
			(at 3.4375 1.200001 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "DISPLAY_RST")
			(pinfunction "GPIO23")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "011458c8-2398-4765-b94c-d3740c0dd471")
		)
		(pad "36" smd rect
			(at 3.4375 0.8 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "DISPLAY_BL")
			(pinfunction "GPIO24")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "3ccaacfe-ab56-4751-9361-15cddf6c4e53")
		)
		(pad "37" smd rect
			(at 3.4375 0.4 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "Net-(U2-GPIO25)")
			(pinfunction "GPIO25")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "cff5c640-91ad-45b3-908f-6b48fecaf6d8")
		)
		(pad "38" smd rect
			(at 3.437501 0 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "10b46276-945d-4df1-9615-70e18bd9f3ae")
		)
		(pad "39" smd rect
			(at 3.4375 -0.4 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+1V1")
			(pinfunction "DVDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "87d6c018-17b8-44d6-ac7c-5a70dd82da6a")
		)
		(pad "40" smd rect
			(at 3.4375 -0.8 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "unconnected-(U2-GPIO26_ADC0-Pad40)")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional+no_connect")
			(thermal_bridge_angle 45)
			(uuid "c0a3a1a7-f746-4bb4-a0f2-65b2751e07ae")
		)
		(pad "41" smd rect
			(at 3.4375 -1.200001 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "unconnected-(U2-GPIO27_ADC1-Pad41)")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional+no_connect")
			(thermal_bridge_angle 45)
			(uuid "65cce283-99e1-42c9-ba1c-4b2557627ff3")
		)
		(pad "42" smd rect
			(at 3.4375 -1.6 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 91 "unconnected-(U2-GPIO28_ADC2-Pad42)")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional+no_connect")
			(thermal_bridge_angle 45)
			(uuid "1598824e-bfaf-4c28-bf34-c4385f3e080b")
		)
		(pad "43" smd rect
			(at 3.4375 -2 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "unconnected-(U2-GPIO29_ADC3-Pad43)")
			(pinfunction "GPIO29_ADC3")
			(pintype "bidirectional+no_connect")
			(thermal_bridge_angle 45)
			(uuid "53342a3b-a93d-405f-a1fe-af59a8976659")
		)
		(pad "44" smd rect
			(at 3.4375 -2.4 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+3V3")
			(pinfunction "ADC_AVDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "3ed5618b-a6ab-4c1b-82c5-6dc4c52e057a")
		)
		(pad "45" smd rect
			(at 3.437501 -2.8 315)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "b526b3db-616b-4f31-a7cd-d761727b40ca")
		)
		(pad "46" smd rect
			(at 2.8 -3.437501 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(U2-VREG_AVDD)")
			(pinfunction "VREG_AVDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "839a4dce-6e6b-4d79-b335-93f007cf0005")
		)
		(pad "47" smd rect
			(at 2.4 -3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VREG_PGND")
			(pintype "input")
			(thermal_bridge_angle 45)
			(uuid "711fb03e-e8a9-4c42-b9d3-6d81a2eed8be")
		)
		(pad "48" smd rect
			(at 2 -3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "Net-(U2-VREG_LX)")
			(pinfunction "VREG_LX")
			(pintype "power_out")
			(thermal_bridge_angle 45)
			(uuid "b3c44aba-6bd5-42eb-a4a2-3b9bd7771aa6")
		)
		(pad "49" smd rect
			(at 1.6 -3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+3V3")
			(pinfunction "VREG_VIN")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "4cc0dc44-d08e-4627-a760-d6284bc63d6b")
		)
		(pad "50" smd rect
			(at 1.200001 -3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+1V1")
			(pinfunction "VREG_FB")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "7c0ad443-f3b0-4f63-b8c0-1d034bf068d2")
		)
		(pad "51" smd rect
			(at 0.8 -3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "Net-(U2-USB_DM)")
			(pinfunction "USB_DM")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "37c2489e-8b92-4ece-9ca9-ebf4a9d9b723")
		)
		(pad "52" smd rect
			(at 0.4 -3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "Net-(U2-USB_DP)")
			(pinfunction "USB_DP")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "52c1599a-aede-48ea-a81a-16991987c924")
		)
		(pad "53" smd rect
			(at 0 -3.437501 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+3V3")
			(pinfunction "USB_OTP_VDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "87d8bef8-be36-4a49-9fe3-b1389688e5e6")
		)
		(pad "54" smd rect
			(at -0.4 -3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+3V3")
			(pinfunction "QSPI_IOVDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(uuid "b8dfc2ac-493c-4ceb-a237-5bdfe34770cf")
		)
		(pad "55" smd rect
			(at -0.8 -3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "QSPI_SD3")
			(pinfunction "QSPI_SD3")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "2fbeb605-e58e-48f7-bd36-7eaee3035f49")
		)
		(pad "56" smd rect
			(at -1.200001 -3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "QSPI_SDCLK")
			(pinfunction "QSPI_SCLK")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "b234b77f-b78a-4a29-a082-0da8690ae30a")
		)
		(pad "57" smd rect
			(at -1.6 -3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 90 "QSPI_SD0")
			(pinfunction "QSPI_SD0")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "8febb14e-da3a-4857-8acc-fb78001af4d8")
		)
		(pad "58" smd rect
			(at -2 -3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "QSPI_SD2")
			(pinfunction "QSPI_SD2")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "9cde47d8-3cf9-4308-bbc3-ae7b67607ca1")
		)
		(pad "59" smd rect
			(at -2.4 -3.4375 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "QSPI_SD1")
			(pinfunction "QSPI_SD1")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "d4137f7f-77cb-46d9-9103-3ad0ab33fce5")
		)
		(pad "60" smd rect
			(at -2.8 -3.437501 225)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "QSPI_SS")
			(pinfunction "QSPI_SS")
			(pintype "bidirectional")
			(thermal_bridge_angle 45)
			(uuid "bb804958-b633-4596-9fcf-bac4350de3bc")
		)
		(pad "61" thru_hole circle
			(at -0.85 -0.85 225)
			(size 0.425 0.425)
			(drill 0.2125)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "a82e01fb-0a2c-434e-882d-5ec735644e5d")
		)
		(pad "61" thru_hole circle
			(at -0.85 0 225)
			(size 0.425 0.425)
			(drill 0.2125)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "0a6b905c-0bb6-4a13-9fdf-3c0b727cce63")
		)
		(pad "61" thru_hole circle
			(at -0.85 0.85 225)
			(size 0.425 0.425)
			(drill 0.2125)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "28ef12c9-7c08-4d8a-89aa-c4bd9ea3d021")
		)
		(pad "61" thru_hole circle
			(at 0 -0.85 225)
			(size 0.425 0.425)
			(drill 0.2125)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "a20c5279-db6f-48c0-9fcb-b205ac62b3f0")
		)
		(pad "61" thru_hole circle
			(at 0 0 225)
			(size 0.425 0.425)
			(drill 0.2125)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "a18f8a2d-5fd1-4648-85a1-6142f9bd8f80")
		)
		(pad "61" smd rect
			(at 0 0 225)
			(size 3.4 3.4)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(uuid "6b2f4eb7-5518-4f2a-a045-bf6a53390fb1")
		)
		(pad "61" thru_hole circle
			(at 0 0.85 225)
			(size 0.425 0.425)
			(drill 0.2125)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "52743473-ef25-44a5-b1a8-7b739fdfe651")
		)
		(pad "61" thru_hole circle
			(at 0.85 -0.85 225)
			(size 0.425 0.425)
			(drill 0.2125)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "3dfab38d-845e-4a85-8249-9aeeee41d825")
		)
		(pad "61" thru_hole circle
			(at 0.85 0 225)
			(size 0.425 0.425)
			(drill 0.2125)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "89319845-4811-4cd2-877f-3d807d052094")
		)
		(pad "61" thru_hole circle
			(at 0.85 0.85 225)
			(size 0.425 0.425)
			(drill 0.2125)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "51a69de1-b744-48a4-858e-ea00a7136bc6")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/lib/toaster.pretty/RP2350A-QFN60.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_2010_5025Metric"
		(layer "F.Cu")
		(uuid "ff76a830-fe09-4a26-a13d-0eb4884f4964")
		(at 101.2 96.8 90)
		(descr "Diode SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D2"
			(at 0 2.5 90)
			(layer "F.SilkS")
			(uuid "9c5d20df-7938-4632-9886-2e3a78ec919f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "D"
			(at 0 2.28 90)
			(layer "F.Fab")
			(uuid "8287249c-8f90-4686-bcb8-7a80ba8eaf82")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "b6e9215e-324b-42db-b7b6-a7ccc1aa7ab1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "1a18d5e2-3183-4e34-b149-b0192bb108a7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0e3beafd-0a63-4a3d-aabc-5be5a8c2fa3f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c8533c9a-fac2-4b41-bf46-20f09d4b1922")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Vendor" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "708bf497-98b5-4c55-ba82-fbeb04c8c10b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "SKU" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fe27c0c1-14db-48e5-b5e7-fcc7122061cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/8313bf86-6181-49a1-ba06-1bedef04a3d2")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start 2.5 -1.585)
			(end -3.185 -1.585)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf542719-1901-44ef-a56c-45d8e5cc315e")
		)
		(fp_line
			(start -3.185 -1.585)
			(end -3.185 1.585)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "515efdaa-6180-4f68-9a5c-d16237bfaf60")
		)
		(fp_line
			(start -3.185 1.585)
			(end 2.5 1.585)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "53f70deb-a1ba-437b-be67-05e887c48ebc")
		)
		(fp_line
			(start 3.18 -1.58)
			(end 3.18 1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "082c70f9-1ef4-4c3d-a5cb-98f0bcda79de")
		)
		(fp_line
			(start -3.18 -1.58)
			(end 3.18 -1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "46c90801-7ca5-4080-bde4-171773c758e0")
		)
		(fp_line
			(start 3.18 1.58)
			(end -3.18 1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6acee458-8fb3-4065-b159-ed7de718f7cc")
		)
		(fp_line
			(start -3.18 1.58)
			(end -3.18 -1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "516723f3-b644-4504-b345-afe10994fc82")
		)
		(fp_line
			(start 2.5 -1.25)
			(end -1.875 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bd3c97a3-fd94-4e5f-a144-fec196b300f9")
		)
		(fp_line
			(start -1.875 -1.25)
			(end -2.5 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "62936169-b6ff-4a8e-b4cf-2c510726203b")
		)
		(fp_line
			(start -2.5 -0.625)
			(end -2.5 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "533a0ca7-22fb-470e-aa85-d266301280f1")
		)
		(fp_line
			(start 2.5 1.25)
			(end 2.5 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a69fe627-ae15-4899-ace7-9a4e549bf9d6")
		)
		(fp_line
			(start -2.5 1.25)
			(end 2.5 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63374155-56ec-49f4-af58-04e4626e82fc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "723df926-1a79-428e-b05b-d815655bb2b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.25 0 90)
			(size 1.35 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.185185)
			(net 10 "+5V")
			(pinfunction "K")
			(pintype "passive")
			(uuid "69788375-e9df-4c13-8b18-a6802e5341b8")
		)
		(pad "2" smd roundrect
			(at 2.25 0 90)
			(size 1.35 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.185185)
			(net 18 "VBUS")
			(pinfunction "A")
			(pintype "passive")
			(uuid "b395fb73-39cf-44a3-a20c-6ee62145ad65")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_2010_5025Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector:FanPinHeader_1x03_P2.54mm_Vertical"
		(layer "B.Cu")
		(uuid "01c91437-4e47-4a11-be62-35f0bdf8c133")
		(at 58 100.35 180)
		(descr "3-pin CPU fan Through hole pin header, see http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf")
		(tags "pin header 3-pin CPU fan")
		(property "Reference" "J2"
			(at 2.5 3.4 0)
			(layer "B.SilkS")
			(uuid "474031b5-dd9b-4570-a9d3-ef865c1d460f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "Conn_01x03_Socket"
			(at 2.55 -4.5 0)
			(layer "B.Fab")
			(uuid "f68949e6-27be-4192-9233-879eced77593")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "78606792-8718-4743-89c5-0f0128650056")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "2fd6945d-f86d-4950-9c2c-e5bfc2e5bb7e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/c898f037-5515-4eca-b16b-5597f2f97896")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 6.45 2.65)
			(end 6.45 -3.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "18335da3-8beb-4a1b-9425-bcad2a5761a2")
		)
		(fp_line
			(start 6.45 -3.4)
			(end -1.35 -3.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "adfd0bec-b91c-4402-8da5-0754d5f80bf6")
		)
		(fp_line
			(start 5.08 -2.29)
			(end 5.08 -3.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8b000063-ee49-4b58-82b3-6328eb744081")
		)
		(fp_line
			(start 0 -2.29)
			(end 5.08 -2.29)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b7a06e64-36b0-41d8-9619-cc18c7a4cc04")
		)
		(fp_line
			(start 0 -3.3)
			(end 0 -2.29)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "5e6a1455-400f-42ca-9195-c937bc7c51c8")
		)
		(fp_line
			(start -1.35 2.65)
			(end 6.45 2.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "56ddc205-7897-496e-9846-05cc7287f6fe")
		)
		(fp_line
			(start -1.35 -3.4)
			(end -1.35 2.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "324666fd-61dd-45a4-8040-6d36ce8d59cf")
		)
		(fp_line
			(start 6.85 3.05)
			(end 6.85 -3.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "6cc1fbf2-8266-46f6-93c1-3c425030a1c3")
		)
		(fp_line
			(start 6.85 3.05)
			(end -1.75 3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "4d7d6a28-f449-4e5d-8ddd-5cdfd4266b24")
		)
		(fp_line
			(start -1.75 -3.8)
			(end 6.85 -3.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "7fe7119d-6d49-4cc6-9084-4423c4e31927")
		)
		(fp_line
			(start -1.75 -3.8)
			(end -1.75 3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "4da98ad9-b0cf-4849-bab4-01ad5e7ad2ad")
		)
		(fp_line
			(start 6.35 2.55)
			(end 6.35 -3.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f814ac2e-f44f-4974-9030-3f2c0adc124a")
		)
		(fp_line
			(start 6.35 -3.3)
			(end -1.25 -3.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5947711b-ceff-4aa0-ba23-4edffe2cf549")
		)
		(fp_line
			(start 5.05 -2.3)
			(end 0 -2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "d577e1f0-9fe9-419e-a433-5b5a7a2ead83")
		)
		(fp_line
			(start 5.05 -3.3)
			(end 5.05 -2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "11684c00-f959-4d31-ab26-d4764185c42e")
		)
		(fp_line
			(start 0 -2.3)
			(end 0 -3.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "8aa17dab-2495-409d-bb2d-0c9b6f4d0e37")
		)
		(fp_line
			(start -1.25 2.55)
			(end 6.35 2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "e86ddc53-87f7-4af4-8fe7-e8e6568c36b3")
		)
		(fp_line
			(start -1.25 -3.3)
			(end -1.25 2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "139f0cd5-90d4-4b41-a40f-531d1d522086")
		)
		(fp_text user "${REFERENCE}"
			(at 2.45 -1.8 0)
			(layer "B.Fab")
			(uuid "5078a631-303e-406d-bfe7-c342247ada50")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.03 1.73)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "USR_PWM_0_AUX")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "24cde979-af25-46d4-be85-779190cf9389")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 2.03 1.73)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(J2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "efe57938-55c6-42cb-b8b9-6b92025eeb8f")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 2.03 1.73)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "5e63ebd0-04b2-4717-9bc7-297d2bc0d569")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector.3dshapes/FanPinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal"
		(layer "B.Cu")
		(uuid "07a2f304-bf39-4f9c-955a-730351bde44f")
		(at 51.5775 73.245 90)
		(descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
		(tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
		(property "Reference" "J8"
			(at 2.54 3.2 90)
			(layer "B.SilkS")
			(uuid "2136695c-b82f-4679-be2b-498f99c7f932")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 2.54 -11.2 90)
			(layer "B.Fab")
			(uuid "6486af6d-af1c-4dc9-87b7-c6744d5cd9a3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "8e22b0de-96e7-4566-b557-e404ef6ad01a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "766976a1-3cb1-4031-a311-c6d7f6dd7798")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/9a9fc785-bde9-4f26-a215-eafe1bd75513")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 8.73 -10.11)
			(end 8.73 2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ee1d06d3-036b-499e-a486-be9c60ea64fe")
		)
		(fp_line
			(start 6.08 -10.11)
			(end 5.83 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9b177459-3dd9-4226-8bd1-8d65d00e134b")
		)
		(fp_line
			(start 4.08 -10.11)
			(end 6.08 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a2b07a3a-779a-4919-998b-618411f45665")
		)
		(fp_line
			(start 1 -10.11)
			(end 0.75 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e9b9ac5c-214d-4774-9b07-11d33148f192")
		)
		(fp_line
			(start -1 -10.11)
			(end 1 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b0c5ded3-023b-4733-b7e0-9f14eeb6aec6")
		)
		(fp_line
			(start -3.65 -10.11)
			(end 8.73 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "391190da-8d8d-4b7a-8604-2071dd117d5e")
		)
		(fp_line
			(start 8.73 -8.61)
			(end -3.65 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "eafa7764-e948-4c0f-9172-f4d04eacb55c")
		)
		(fp_line
			(start 5.83 -8.61)
			(end 4.33 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4a444668-157d-4dc8-9d2d-668444c9012b")
		)
		(fp_line
			(start 4.33 -8.61)
			(end 4.08 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0003b53e-9d6f-4073-8c61-8c320ce04327")
		)
		(fp_line
			(start 0.75 -8.61)
			(end -0.75 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "07035b98-531b-4413-9d73-ff72dc39f6ca")
		)
		(fp_line
			(start -0.75 -8.61)
			(end -1 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "91299105-ff6b-4200-b2fa-79f0586b0f7f")
		)
		(fp_line
			(start -3.65 -8.61)
			(end -3.65 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "92f88b77-3c58-4ae8-949a-f3e9dddf6fa2")
		)
		(fp_line
			(start 8.73 -6.81)
			(end 8.73 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0ab1bbbf-6a95-4780-b821-5ace83133828")
		)
		(fp_line
			(start -3.65 -6.81)
			(end 8.73 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d5d57f69-e435-4ba0-9d25-905bf86b4288")
		)
		(fp_line
			(start 8.73 2.11)
			(end -3.65 2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e88d6c42-65a0-4821-b87e-9a6e2fbb654e")
		)
		(fp_line
			(start -3.65 2.11)
			(end -3.65 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f933937e-39ae-4d56-8582-645c8dbec6d8")
		)
		(fp_line
			(start 0 2.31)
			(end -0.3 2.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d6124a5a-c8e8-434e-9147-0fd2b54ed68a")
		)
		(fp_line
			(start 0.3 2.91)
			(end 0 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "907f030b-6b53-430d-9c12-8a77acca88bf")
		)
		(fp_line
			(start -0.3 2.91)
			(end 0.3 2.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "289590fb-b45c-4279-b2fd-a500ad9aca4d")
		)
		(fp_line
			(start 9.13 -10.5)
			(end 9.13 2.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "bb55e007-444f-45e1-9926-38593b942744")
		)
		(fp_line
			(start -4.04 -10.5)
			(end 9.13 -10.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "882240a8-4a35-458f-9649-238b4769af22")
		)
		(fp_line
			(start 9.13 2.5)
			(end -4.04 2.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "75bae5da-c5e3-4cbc-aca9-60f258cbc16b")
		)
		(fp_line
			(start -4.04 2.5)
			(end -4.04 -10.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "402a56f2-25e4-455e-ab0e-ce13f095d2a0")
		)
		(fp_line
			(start 8.62 -10)
			(end 8.62 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "72de3af6-cbe0-42a0-88ea-8c86192e9959")
		)
		(fp_line
			(start -3.54 -10)
			(end 8.62 -10)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "50cdf890-77d3-4896-951b-007d52ebd213")
		)
		(fp_line
			(start 0 0.5)
			(end -0.95 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "6eaf46dd-51fd-40f8-a3b4-760b88908ca6")
		)
		(fp_line
			(start 8.62 2)
			(end -3.54 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "81b50a75-ca64-4511-8342-cd8242487702")
		)
		(fp_line
			(start 0.95 2)
			(end 0 0.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5f6f074d-9880-4557-8d0e-988c450800ec")
		)
		(fp_line
			(start -3.54 2)
			(end -3.54 -10)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "64705be9-18e3-422c-bd4d-332f6455d2cf")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 1.3 90)
			(layer "B.Fab")
			(uuid "65461000-6a44-4a8c-982a-ae17b90fceb8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 2.08 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.120192)
			(net 15 "Net-(J8-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "f5e890b7-02a9-41d3-bf39-f3474137e89b")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 90)
			(size 2.08 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J8-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "0ea5a706-4619-4307-b1a1-2092ab32a2c6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "0b4fe290-5032-4e03-93f3-43541b6320a1")
		(at 82.69 151.7575)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D10"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "0a5b5f3a-cc23-4388-8727-fea8807d95ab")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "d70ba764-48d9-46ea-8934-b6b5490e7c1c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "3a553b0d-074b-4e9d-9991-b5ab1f9643a1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "aee02666-189e-4c95-af19-0e69a2bbf548")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "91bd6234-7a0d-4b06-9266-55236876bb36")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "135d46e1-d491-4aa3-b82a-d6b67cf02670")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/834611d7-56b1-4cc5-985d-a3465f397f16")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ac95bed8-d260-41ed-a2c8-2155c458fb8c")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "67bce2d1-cd62-46d2-b69e-8da6187a5aa6")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "586009ae-308b-4590-a94c-7f577c1097a0")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "48bc5edc-2d41-436d-936e-adf512008b7a")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "2205f921-bad4-4d69-944c-05920d40ba73")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "f4c881e0-883c-495e-a156-4c9e089d20fb")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "81d39986-23db-4485-b0a2-b9c47fe11dc1")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "ba2d63ea-0fe1-4e88-8010-a36d04d9050c")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c734a91b-c2b7-4f39-9f35-842a994ffeda")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "b59e15ff-e7c1-4197-8aa2-4febfe8b5995")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5ff64214-bf08-418d-aa2d-8dcdade0c4bc")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "b81ff111-8b29-4766-8cfa-1536045f0b28")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "d388d633-4005-4b3a-9d2b-526d5336dd7c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 22 "KEYPAD_ROW_1")
			(pinfunction "K")
			(pintype "passive")
			(uuid "a1a52c0d-9f19-4ba7-823b-5e95fba0b0c9")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 28 "Net-(D10-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "4f87c674-fa1a-4fc7-b5de-1f96fb7951b0")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "14eafd82-81f9-4c2f-bdac-710c8e582bf4")
		(at 77.895 142.6375)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D7"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "4d9c3056-c135-49d1-b9f7-beccf6277029")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "198c99f8-438e-4972-9757-4c77bfbbd831")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "1ff008ff-4a98-4de7-8b7c-d17c7e1f1d0a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "964476a1-d8c5-42d0-a237-457cf3367934")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "8c7f336d-6316-4053-afb6-cca550fcf76d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "79bf6e49-52d3-4cc0-bf03-3cafc020e086")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/34c9b0c3-620a-4a89-9ac8-c51b1ab3a7cc")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "2dd61b42-52fb-4c9e-9e79-c2c27178309e")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "99f2cf7d-e4d8-477c-9118-e588b16381fd")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ee89fc90-bc26-4d0e-ae0c-d2ca1f33e072")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e190adf0-8bf4-46d6-b1c9-081bf0722a0d")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "32856e8e-a2d1-41f6-9a05-37bd03806bf9")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "30b9fa8b-6117-4976-a547-2d377a5e9136")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "9db8d488-f948-4619-9a66-ce5c7adfad76")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "0d16327a-ae3a-4fa3-add3-41437c90edbd")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "21ae55a5-799d-418c-bb46-ca7ae9953e63")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "e1d8aaaf-8b9d-4f5d-af1c-7f03543aa4d2")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "416642d7-aeb6-430e-beb5-7ff88558ae37")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "07e0cddb-51f6-4c63-91be-df4d889d685e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "4551c888-0471-4d9b-8fc6-1db410a07e46")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 23 "KEYPAD_ROW_2")
			(pinfunction "K")
			(pintype "passive")
			(uuid "4b39dfa5-c20f-4822-a0ef-9fe0808def4b")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 24 "Net-(D7-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "ded04606-b33f-413b-9683-04d137ddc398")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "1e62bcab-9146-4f0a-a5d0-cdd9d2752064")
		(at 87.485 151.7575)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D16"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "9a15248a-9627-406f-94b2-6269dadd75ba")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "6a53148a-3e80-4798-9aab-21539d30323b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "cfd21036-6936-4134-a68c-3a7c169fc40b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "7317cfb3-fe74-4c4b-b102-f766f0b30189")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "adf7b67d-1511-490a-83c1-f13abd45e2b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "de38966c-cf6d-46f2-9624-606847932a6d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/6fb97160-7095-49fb-ad21-b9e02b34ad9c")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "3afec4c8-c429-41d3-a669-e81244792ca2")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e95fd32b-9238-4d4e-93fc-0ec7586adb6f")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "247c6ecf-e58e-4378-b878-f4624dd991bb")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b1ab394d-9cd0-46a9-acd5-8c349ae461a2")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "3bb03872-a1bd-483d-bb30-132074b5e693")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "38b9e252-0a7f-46ea-8dbe-08842d066287")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "9573ba9b-6857-4ad9-9bd7-52084c0f75b2")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "223b21da-2fa6-4061-ab03-f9710d388c30")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "83492daf-f8b5-473f-905d-2e868cab0d2a")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "831c10da-9571-4459-be55-ee2adc323852")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "289d56c6-5953-474e-bdb9-d6f158967e30")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "77699352-1b69-4023-8153-20076cc1dfc3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "a0be88c9-a555-40b9-a538-01740c77c91c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 26 "KEYPAD_ROW_3")
			(pinfunction "K")
			(pintype "passive")
			(uuid "d5e0d70b-ea6f-423b-8d47-aac9305e8739")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 34 "Net-(D16-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "45985f9f-769d-415c-afd3-106df249e068")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "21ffda83-52a9-409b-8eeb-b14b8705210d")
		(at 77.895 145.6775)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D6"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "9c7a4f64-3cb0-45a7-9e5b-5a20bfbf3d40")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "90c51c8d-f556-4eb2-9637-e87a19f1e1a2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "f4f97b9c-ebcb-4105-be26-c9c61537a9fc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "2af5aaa4-e59d-45ca-8d1f-eff7bb3a7dd8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "02b88daf-e2da-4e3e-aa85-ffff69fdf2bc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "4cdb4ea3-f892-4424-ad07-8ff53797e183")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/cc26ec7b-ac11-4902-8564-0d9c37beaff5")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "1ada8124-e8c9-4ec0-8c2f-de5658c7a628")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "7aaad712-467b-49cb-9ed7-fdf4a89283b5")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "04036d28-1138-4f33-b1a1-67b99aaf080a")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "f9b6aaab-6dc6-41f4-b91d-18c70f01a9f9")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "906cb8b2-7f18-46ad-81bc-2b7c813c4fc3")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "792253f6-7451-42c2-ad7e-162f93f2cae4")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "47dbc587-7293-4d1c-92af-c45f7b140763")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "28422839-d2da-495b-8dca-94537a159b72")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "4b490fa5-2b17-417a-b757-52eb4042c7c7")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "e2be32ae-531e-421d-b4ed-d1888f761a4d")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9740be8e-0a7e-4e08-9628-19c3ea8c997c")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "33eefdb9-9e80-4fdf-b338-b9a9e5c474bf")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "f311fd49-6e48-4d95-8406-2b5d5836fbe0")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 22 "KEYPAD_ROW_1")
			(pinfunction "K")
			(pintype "passive")
			(uuid "9d6972b2-b4d5-4d3e-b60e-74487bc6d59c")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 21 "Net-(D6-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "30e6d326-46a6-45e2-ad3f-aa7adb18151c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "2ee6e738-c44a-4bae-a47a-9f683df16d41")
		(at 68.525 108.4675)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D9"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "9af3ef80-ccfd-47c6-ae6e-05acf3670a3a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "3166c05f-3df2-46a9-8c8a-0baa8686ca42")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "281fd1b3-55f2-4baa-9f64-2d7035da7fd5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "3995406d-fc2f-46d7-b269-d51583e35c59")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "233223bc-f682-4022-85ab-4b724c5f630a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "c0c544d0-7eff-455b-b227-0a6ccdf43217")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/4f30b934-c1b5-4448-94bb-26a65b6d4c26")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f0d70f66-0186-4060-9588-624bd53c6b6f")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "43ad2c96-aae5-47ab-8e09-f8e681ca0271")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c9ae4dc9-de1b-4b42-bbf0-b6a5764b5199")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "059a95c2-75e0-404c-990e-4ce165a6a02f")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b1a3387e-72aa-4ed5-b8e1-496e57e65770")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "dce53301-a827-4d54-a269-75302e131ea9")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "69bd42cf-bfa1-4a8d-a610-e9d5455b10f0")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "06a43210-cd9c-4dc5-8e5d-5e8597e77c7c")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "70f62a99-12a9-4ea4-a75a-d837b87afddc")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "adc1cae6-cf92-4d0d-b548-4ff349cc41bd")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "e0a0f188-a12c-48de-88fb-fa21fa64c15d")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9ac067f1-e38c-4002-9bb7-77e4c82963aa")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "195138c9-38bd-4d16-a75f-4fc14a74f497")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 19 "KEYPAD_ROW_0")
			(pinfunction "K")
			(pintype "passive")
			(uuid "96b7f8bd-870c-4ced-bac9-ba2d1e02238b")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 27 "Net-(D9-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "cef14229-983f-48a2-b40b-f717db3480d6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_C_Receptacle_GCT_USB4105-xx-A_16P_TopMnt_Horizontal"
		(layer "B.Cu")
		(uuid "4c393d51-4cd7-4aa3-8a2a-20827e078623")
		(at 120.15 95.5 -90)
		(descr "USB 2.0 Type C Receptacle, GCT, 16P, top mounted, horizontal, 5A: https://gct.co/files/drawings/usb4105.pdf")
		(tags "USB C Type-C Receptacle SMD USB 2.0 16P 16C USB4105-15-A USB4105-15-A-060 USB4105-15-A-120 USB4105-GF-A USB4105-GF-A-060 USB4105-GF-A-120")
		(property "Reference" "P1"
			(at 0 5.5 90)
			(unlocked yes)
			(layer "B.SilkS")
			(uuid "1b2c9e20-be82-4849-a220-76b0f6560a57")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "USB_C_Plug_USB2.0"
			(at 0 -5 90)
			(unlocked yes)
			(layer "B.Fab")
			(uuid "882c6bd1-028a-4cca-a4c4-475e449240ca")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "e8947d9f-7f12-4e2e-aa5a-2d5081d9f841")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "USB 2.0-only Type-C Plug connector"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "eab036fb-5423-4ee0-bbad-ce43e399dbd0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Vendor" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "c0f7cb38-1d48-43f3-ab08-01d714924ea4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "SKU" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "e271c991-8b0f-4dac-bc54-1eef2796dd9e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "USB*C*Plug*")
		(path "/eef42246-033c-46a0-98a4-7291389bc9a9")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.67 0.1)
			(end -4.67 1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "36363229-07a2-4c03-ad6a-a4fa04a20bc4")
		)
		(fp_line
			(start 4.67 0.1)
			(end 4.67 1.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "22339749-3d10-4039-bfca-68555c8b5572")
		)
		(fp_line
			(start 5 -3.675)
			(end -5 -3.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "Dwgs.User")
			(uuid "7129adf1-6830-4bb7-8493-0b70ed3e81a6")
		)
		(fp_rect
			(start -5.32 4.76)
			(end 5.32 -4.18)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "B.CrtYd")
			(uuid "39b66e0a-9969-4e38-843d-af152ca520da")
		)
		(fp_rect
			(start -4.47 3.675)
			(end 4.47 -3.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "B.Fab")
			(uuid "df8506cc-5dda-499e-83b5-fcd4329e172a")
		)
		(fp_text user "PCB Edge"
			(at 0 -3.1 90)
			(unlocked yes)
			(layer "Dwgs.User")
			(uuid "a909e30f-e720-4de0-b161-51562f307cea")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(uuid "88c7ed84-36db-4816-8fdc-15b042e82bbc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "" np_thru_hole circle
			(at -2.89 2.605 270)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(uuid "930a523a-e05a-4a0c-a2fa-cdc963282392")
		)
		(pad "" np_thru_hole circle
			(at 2.89 2.605 270)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(uuid "3a99dfdb-3769-4adf-bde6-c7b3518b8b59")
		)
		(pad "A1" smd roundrect
			(at -3.2 3.68 270)
			(size 0.6 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "a2b81f94-3a47-462c-aa21-bebb1c0c5d63")
		)
		(pad "A4" smd roundrect
			(at -2.4 3.68 270)
			(size 0.6 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "7ea45634-3590-4b09-9ef4-b3df65c274f6")
		)
		(pad "A5" smd roundrect
			(at -1.25 3.68 270)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Net-(P1-CC)")
			(pinfunction "CC")
			(pintype "bidirectional")
			(uuid "1ba4be39-6d9b-4fa7-b264-67e83db2c3fb")
		)
		(pad "A6" smd roundrect
			(at -0.25 3.68 270)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 67 "D+")
			(pinfunction "D+")
			(pintype "bidirectional")
			(uuid "8883163e-a041-4a76-86d5-3dd23ae07a3b")
		)
		(pad "A7" smd roundrect
			(at 0.25 3.68 270)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 68 "D-")
			(pinfunction "D-")
			(pintype "bidirectional")
			(uuid "9a970b02-e9c3-41e1-ab81-bfe838b8d699")
		)
		(pad "A8" smd roundrect
			(at 1.25 3.68 270)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(uuid "f018b434-fa5c-4229-9f2e-b611ad3f457b")
		)
		(pad "A9" smd roundrect
			(at 2.4 3.68 270)
			(size 0.6 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "a6828b0f-11b9-4e3b-938a-cfa7733e1f90")
		)
		(pad "A12" smd roundrect
			(at 3.2 3.68 270)
			(size 0.6 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "e6074aa4-310f-47b5-89bf-be51f340770a")
		)
		(pad "B1" smd roundrect
			(at 3.2 3.68 270)
			(size 0.6 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "1c6570d0-7742-4aea-9be9-cca29fa7ed8f")
		)
		(pad "B4" smd roundrect
			(at 2.4 3.68 270)
			(size 0.6 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "cbbd92c1-a1a6-4fa7-a72e-1c8f52ee1419")
		)
		(pad "B5" smd roundrect
			(at 1.75 3.68 270)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 66 "unconnected-(P1-VCONN-PadB5)")
			(pinfunction "VCONN")
			(pintype "bidirectional+no_connect")
			(uuid "85919983-bc94-4692-b9c9-421fa2e7b59b")
		)
		(pad "B6" smd roundrect
			(at 0.75 3.68 270)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(uuid "637d7374-9359-4c53-9caf-58c939df059f")
		)
		(pad "B7" smd roundrect
			(at -0.75 3.68 270)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(uuid "4260926e-dbe3-44fb-a259-ce240dd4bc8e")
		)
		(pad "B8" smd roundrect
			(at -1.75 3.68 270)
			(size 0.3 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(uuid "1f821f42-0dd7-4819-aa74-72148ae735d5")
		)
		(pad "B9" smd roundrect
			(at -2.4 3.68 270)
			(size 0.6 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "e99dca58-a904-482d-b57f-8bc0a49c5675")
		)
		(pad "B12" smd roundrect
			(at -3.2 3.68 270)
			(size 0.6 1.15)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "1c73a341-155d-4248-9194-7403bc18cbd6")
		)
		(pad "S1" thru_hole oval
			(at -4.32 -1.075 270)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "60aeafd8-1cb6-4163-9203-27018a67ab93")
		)
		(pad "S1" thru_hole oval
			(at -4.32 3.105 270)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "a886f104-8daf-40d6-99a1-1f4d79acd79c")
		)
		(pad "S1" thru_hole oval
			(at 4.32 -1.075 270)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "798d9e08-1ff9-4092-bfe7-319ef9dcd490")
		)
		(pad "S1" thru_hole oval
			(at 4.32 3.105 270)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "8b0a9319-efdd-40f2-a07b-f4f00bfb06c3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_GCT_USB4105-xx-A_16P_TopMnt_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "5a1658e5-bc51-424f-a046-b2b7e3373f39")
		(at 82.69 139.5975)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D14"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "ec060b18-7281-4579-bdca-ff91e0d2d6f2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "52dd79e8-04a3-4371-a843-590ca79cc265")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "be5f44fc-4a1a-4b58-a78d-6b59d37eec1e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "f3964659-dc24-4002-8492-fc59a3e529b7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "00be6f65-ad8c-4b6e-ae64-dc39f62bfb91")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "c5d4d9c8-bd25-468e-8df6-9341c6843d28")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/13a6237d-d120-48cc-9dd3-d51fefffb73a")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d904affc-af6c-4144-a105-bc10634617b7")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "eed8db45-34f8-4d76-8b34-ecb22b67e058")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "265d307f-ee07-4fb1-8a32-053fa8098201")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "1c922aaa-4400-46b3-b1b6-2527eb71cf12")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "0fa36351-a4f5-4407-83b5-444f63fbd0a1")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "79d317aa-c2ba-4f08-a819-944f845b2c26")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "201c644f-82cf-49af-99df-7a163580fce7")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "88e0ef77-d281-4e08-a249-ff25cd3347c0")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a524e380-be6b-4e6c-8d54-a11c8ec764be")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "2cc80653-8e3e-4105-9506-14958344dcc4")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f1946798-a551-49d0-afae-e1f433e6ab9f")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5196bfc8-6148-4d2e-b573-6d6478139b76")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "7964f7f8-5a6a-40e7-9262-108e8e35b5e0")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 22 "KEYPAD_ROW_1")
			(pinfunction "K")
			(pintype "passive")
			(uuid "dd006a93-8f86-4f31-a828-d52eefd0a32c")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 32 "Net-(D14-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "016aa97a-0524-4322-92f9-1b4d8a4d77d8")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "6890af3c-9a74-44bf-b6c5-01e77d87ab93")
		(at 77.895 139.5975)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D8"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "04b9aab9-3dfd-4e10-b09e-69f52b36ab1b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "ebf59aff-c0c1-45eb-a9d5-656dfa810bfa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "a169d0d6-7862-4d22-af6b-3218815e714f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "5dbd33d9-4ad9-463c-9b66-b545dc819be4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "15981708-bcab-4cbd-9159-b81bce56c117")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "0ecf86b1-478d-418a-bdee-a688f3c1ca0b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/01e87de7-6842-4f4f-a1c4-83138bcdcd15")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "df627f82-2ee1-466f-bd8b-b40bae5647b4")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "01ccdc1d-3612-4437-8b9e-1fafe8656944")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "51e91df6-bcf6-4517-a673-178e7d7cf2c9")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "f37b583f-a502-4e2e-a88e-355d930b0330")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "770185f9-32c7-43b5-9555-cbc76577f04e")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "774fe6cf-6542-4751-a194-958f0e29ef79")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "edf4b67b-b78e-4389-b6e0-b5c63b5d6c9a")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "7878bbf7-e237-4ac1-9193-fe1c215f0509")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "dbc65ef1-9521-478c-b1bb-e76cbfd7390d")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c19be3c1-3050-4700-b8d4-7fd30e6249d9")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f905fa34-742e-4ef4-8b76-395eb3e0193a")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f9158173-8520-4de9-bc67-f0ca987ddc3b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "ac96b59b-1a7f-4bb1-90f3-4102d4ce4750")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 26 "KEYPAD_ROW_3")
			(pinfunction "K")
			(pintype "passive")
			(uuid "f699b55c-c253-4693-8ee8-504422137136")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 25 "Net-(D8-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "a70cac92-3b3f-4c25-a88e-d3812b035824")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "77f2ee33-7eb5-42db-94a8-649bb9f6c921")
		(at 87.485 142.6375)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D19"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "63defc83-fcca-416a-afee-714ceff0aaa0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "6e8aa179-f5e4-4afe-9ec5-c40bdd2efda7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "1b7d451b-2010-478e-913a-c2f6f130bdae")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "4b3f7abe-eb3b-4c14-a54d-047822fd5419")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "ce54527a-bfa0-47ee-96f2-b92e1875a32f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "0fdafad9-ba88-476c-9280-f5fd7eea5eab")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/51a71e74-d2cd-40f0-95c9-f4e2aa755418")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "77c047cf-af50-4141-b0f4-554e4af0643b")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0a515dd6-6ba2-4bde-9b0d-e7b5ff315455")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d49ba4a0-7ca0-4962-8d97-e79d425e02fc")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "31c5ca2d-0a63-4a8f-8a93-d9d06c18714e")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5c909b2e-6925-435a-acc3-f8217228b4a2")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "0737b76a-4c2d-45ea-b57c-75bb1afd4da3")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5244c1a6-ea71-421f-9872-812474dd99b1")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "872ecc57-3fbe-4c43-9878-8275840e5f89")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9da8ff9a-cbfb-4d92-846c-affae0dfd5d2")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "2548b1d5-93cb-42fc-8acf-e63cec72b3e1")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "296e0af3-4af0-4878-8be6-358d5ce2ed93")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5882807d-2d56-4c8c-bdbb-34ac4749434b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "df0f2199-6df4-4671-8463-a7b3e04d28df")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 23 "KEYPAD_ROW_2")
			(pinfunction "K")
			(pintype "passive")
			(uuid "db4ff1f2-3481-4055-9625-e8a34a771de9")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 37 "Net-(D19-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "da522417-b1f8-41e2-b7a6-92063c23a9a4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "875c2035-d56c-4731-ab0e-5ae48f968c20")
		(at 82.69 148.7175)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D11"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "44b7bafd-848d-4113-a886-7b4d2332316a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "916b1667-2ac2-4a74-9a85-335f26c36043")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "336295f0-0dd6-4607-8736-86388aae167b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "d10cf9c3-721d-4cd9-bf66-bf12a2c8c8f6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "730a5276-4a23-4b8f-a52b-0bcc864fcd00")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "4b9ffe1e-b83b-4c86-b2ef-4e109dd8c7ee")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/35d60591-1e7f-412f-957e-08ea8cdcf33a")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "76c61676-5009-48e6-8a84-6eb50a7c8211")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8fb61fa6-5139-4b4e-a297-db59bbd7dcf9")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d14bb578-59f4-40e0-9c5b-390bfb003605")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "cf9d71a5-7398-4308-970d-28d5c25e7789")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "4b81fe26-275f-4a09-82ae-6c5375993fbf")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "16c7710b-7d9d-4232-b50d-cb05a67e1f54")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "de661a6c-6698-4bdc-816c-e7e21bfe8e9f")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "67444812-ff4b-4587-8f4b-c6331c2b5e16")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "d6a8bb95-f690-4cea-b9ae-cbb5c4f3d854")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "0eacf150-5857-4929-a2ba-306120472ad0")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "143ec2b6-9bbc-4a1c-8c72-2d2f5c50b7dc")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "42bc0752-be84-4ab7-8a40-935b3e015d08")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "0aeff3a4-e440-4693-bc51-5b8b4c3440d5")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 23 "KEYPAD_ROW_2")
			(pinfunction "K")
			(pintype "passive")
			(uuid "e3d02e69-86d6-4726-be3d-9dbd45925b9e")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 29 "Net-(D11-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "0b726865-22f8-4a92-862b-831450b5af3b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal"
		(layer "B.Cu")
		(uuid "889d3324-3a16-4a77-b597-f3f4cb73ef32")
		(at 44.97 44.45)
		(descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
		(tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
		(property "Reference" "J3"
			(at 2.54 3.2 180)
			(layer "B.SilkS")
			(uuid "326ed8ed-d505-4bd9-baeb-410b1b073ee6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 2.54 -11.2 180)
			(layer "B.Fab")
			(uuid "b235114e-3aa6-4ecb-866c-fdd7ccc077a8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "2333cc34-b734-4f24-a0df-7ec2a2a92c39")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "d46ac18a-c672-479b-a464-8eb56d44e3e0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Vendor" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "92c904a7-7fe8-4110-a3a0-1a758fbc46e1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "SKU" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "9516ea5e-0774-40a7-be57-26a1e5f25a0a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/796baec6-cf8c-4c8d-bcb9-bceed98db20a")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -3.65 -10.11)
			(end 8.73 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "35c70712-a921-4ca0-8454-59545ba815db")
		)
		(fp_line
			(start -3.65 -8.61)
			(end -3.65 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d5cf5f8f-d007-4030-b846-71ad5dac6b41")
		)
		(fp_line
			(start -3.65 -6.81)
			(end 8.73 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "1595d416-57ef-4349-8d09-e2a26d2ba3de")
		)
		(fp_line
			(start -3.65 2.11)
			(end -3.65 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c73927fd-5f85-4fff-aa2e-abe559e6592d")
		)
		(fp_line
			(start -1 -10.11)
			(end 1 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f55f3ee6-942f-43e1-bed7-8727e11880df")
		)
		(fp_line
			(start -0.75 -8.61)
			(end -1 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "81e02682-0c50-4186-a3e9-b8d81cf8a797")
		)
		(fp_line
			(start -0.3 2.91)
			(end 0.3 2.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "bca2bb6c-9f52-49a9-b6d5-41de38e3e23f")
		)
		(fp_line
			(start 0 2.31)
			(end -0.3 2.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "af9c273c-2f8b-4c5e-9c7f-743a196dd204")
		)
		(fp_line
			(start 0.3 2.91)
			(end 0 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "3dfe604d-dc9c-46b2-a4d5-61b9e8c6b99d")
		)
		(fp_line
			(start 0.75 -8.61)
			(end -0.75 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "05a92499-d3da-4e30-8ed9-a1b2f1a8937f")
		)
		(fp_line
			(start 1 -10.11)
			(end 0.75 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8c7d4f62-fb21-44a1-9118-42c64b316531")
		)
		(fp_line
			(start 4.08 -10.11)
			(end 6.08 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e461240f-b17e-4d76-9df8-58ff462f42f1")
		)
		(fp_line
			(start 4.33 -8.61)
			(end 4.08 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "bf33c979-82be-4af7-8765-610f7fba281e")
		)
		(fp_line
			(start 5.83 -8.61)
			(end 4.33 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "1ab9509d-e077-4788-87b0-8df03587d667")
		)
		(fp_line
			(start 6.08 -10.11)
			(end 5.83 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6ab2a269-3c1c-4978-80be-bc708b2f8f13")
		)
		(fp_line
			(start 8.73 -10.11)
			(end 8.73 2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "02b0b1ee-ebea-4641-aca9-20cbbe4ce1e6")
		)
		(fp_line
			(start 8.73 -8.61)
			(end -3.65 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ad2e43c7-3539-4690-89a6-29329cb1d24f")
		)
		(fp_line
			(start 8.73 -6.81)
			(end 8.73 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "1127d0da-4cae-46b4-acd3-59eb3767a51d")
		)
		(fp_line
			(start 8.73 2.11)
			(end -3.65 2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "078957ff-b5a6-407e-bfdf-cdda2a3fae49")
		)
		(fp_line
			(start -4.04 -10.5)
			(end 9.13 -10.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "f69ea5e3-cf06-475e-9283-2989803846a4")
		)
		(fp_line
			(start -4.04 2.5)
			(end -4.04 -10.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "a3339a96-eee1-47e7-a417-e69d9b6bbe64")
		)
		(fp_line
			(start 9.13 -10.5)
			(end 9.13 2.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "8ba5692e-d8e2-4e24-a50c-b57b1160844f")
		)
		(fp_line
			(start 9.13 2.5)
			(end -4.04 2.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "80a7a12e-36c2-44b9-b8e8-dbee3ce87772")
		)
		(fp_line
			(start -3.54 -10)
			(end 8.62 -10)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "65428cf8-32bc-42e7-a879-10bb4061539d")
		)
		(fp_line
			(start -3.54 2)
			(end -3.54 -10)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9c4db1ed-144b-40b9-93e8-00f4ed78d45b")
		)
		(fp_line
			(start 0 0.5)
			(end -0.95 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "7cc0ac11-17a2-45f7-9663-c86990196591")
		)
		(fp_line
			(start 0.95 2)
			(end 0 0.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "e529c32e-68aa-4a32-a638-c6d7f5fdb7b3")
		)
		(fp_line
			(start 8.62 -10)
			(end 8.62 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "748edaf5-44a6-4954-817a-5e35b7638d7b")
		)
		(fp_line
			(start 8.62 2)
			(end -3.54 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "19730905-9a5e-49b6-bbe6-4f9c287398fa")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 1.3 180)
			(layer "B.Fab")
			(uuid "6225a907-eb3e-4bba-8977-9565a8395b5d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.08 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.120192)
			(net 39 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "1dffe2f4-c3a4-45f7-9664-073459f6d252")
		)
		(pad "2" thru_hole oval
			(at 5.08 0)
			(size 2.08 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "3e6efc79-e84f-4a05-9538-04df860c9219")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal"
		(layer "B.Cu")
		(uuid "9931443f-2ab8-4948-8f56-bfe8ddcc98ac")
		(at 51.4775 86.895 90)
		(descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
		(tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
		(property "Reference" "J7"
			(at 2.54 3.2 90)
			(layer "B.SilkS")
			(uuid "db56c4d0-3334-4c50-8714-821286b36d3e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 2.54 -11.2 90)
			(layer "B.Fab")
			(uuid "49b5785a-2ce8-4818-a5a1-db302aa9c26a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "a887eeab-75fc-457b-b9f8-212217c23b98")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "0f4336dc-7968-47ad-bad0-169daece90d1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/64a90710-11ca-4863-b975-e2a8d226ef4c")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 8.73 -10.11)
			(end 8.73 2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "85856a5c-4b77-4c66-be0c-7fe36d6e0964")
		)
		(fp_line
			(start 6.08 -10.11)
			(end 5.83 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8a1fb69b-4bd7-4300-93a0-6786f511d67d")
		)
		(fp_line
			(start 4.08 -10.11)
			(end 6.08 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ca653016-dd5c-43d6-a010-c380941bd4ba")
		)
		(fp_line
			(start 1 -10.11)
			(end 0.75 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9c3178e8-a836-4735-90bc-13ed9fec6d34")
		)
		(fp_line
			(start -1 -10.11)
			(end 1 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "030204f4-56d6-4e36-9600-5281f76a63f6")
		)
		(fp_line
			(start -3.65 -10.11)
			(end 8.73 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "152a786c-744e-427f-82ad-baddb31288ca")
		)
		(fp_line
			(start 8.73 -8.61)
			(end -3.65 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b289a958-5c92-4f32-a21a-7478c2032b6e")
		)
		(fp_line
			(start 5.83 -8.61)
			(end 4.33 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "fa70cc4c-2bc5-43af-8fa1-faa691e01b5e")
		)
		(fp_line
			(start 4.33 -8.61)
			(end 4.08 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "80485629-a7e4-4d1f-a9df-71cdfa400a2c")
		)
		(fp_line
			(start 0.75 -8.61)
			(end -0.75 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "2147b76b-3477-48c4-baed-2ca20633cb55")
		)
		(fp_line
			(start -0.75 -8.61)
			(end -1 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d19ad43f-d9fc-4fc9-bc30-476745f99197")
		)
		(fp_line
			(start -3.65 -8.61)
			(end -3.65 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e39e8fd6-1b94-4a6b-a92e-3b4893a2f50e")
		)
		(fp_line
			(start 8.73 -6.81)
			(end 8.73 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9fb59dd1-33e9-4dd2-96d9-7fbba61a45e0")
		)
		(fp_line
			(start -3.65 -6.81)
			(end 8.73 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "39a69721-91d4-4694-884f-65eb9852e2c7")
		)
		(fp_line
			(start 8.73 2.11)
			(end -3.65 2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "54018fe7-440d-49f4-8e03-2cd81f996f10")
		)
		(fp_line
			(start -3.65 2.11)
			(end -3.65 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6302ea8f-a365-4dc0-84bf-d3ed8bf8f101")
		)
		(fp_line
			(start 0 2.31)
			(end -0.3 2.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d3e7f240-68ee-4cb7-9ba6-e9bb3bc90208")
		)
		(fp_line
			(start 0.3 2.91)
			(end 0 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "49c835fa-1f1c-47a9-be96-b6ad5b9b9d2b")
		)
		(fp_line
			(start -0.3 2.91)
			(end 0.3 2.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "5bd1dbd5-1305-48bc-8832-1abec21ae68c")
		)
		(fp_line
			(start 9.13 -10.5)
			(end 9.13 2.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "29db4ee2-c8f4-4465-a784-cd9f4152f19f")
		)
		(fp_line
			(start -4.04 -10.5)
			(end 9.13 -10.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "ba1c4fd6-d064-4c84-9335-e728b072829e")
		)
		(fp_line
			(start 9.13 2.5)
			(end -4.04 2.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e3c3a80f-1d63-41c4-9976-f39880878ec8")
		)
		(fp_line
			(start -4.04 2.5)
			(end -4.04 -10.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "6b71d182-5811-4fd6-9e24-8aeec198bf0b")
		)
		(fp_line
			(start 8.62 -10)
			(end 8.62 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "eed2da8e-1c41-4e07-afce-82d7a4f8489a")
		)
		(fp_line
			(start -3.54 -10)
			(end 8.62 -10)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "7fa37caa-074d-4e5e-a9fe-1ecf1a5c8a61")
		)
		(fp_line
			(start 0 0.5)
			(end -0.95 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "66691bc5-b004-46b8-ac27-04b17f1b3aa8")
		)
		(fp_line
			(start 8.62 2)
			(end -3.54 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "cf3cfc3b-2817-4ae3-8395-f694607fde3e")
		)
		(fp_line
			(start 0.95 2)
			(end 0 0.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "29b50c4a-16cb-40fc-b2c0-bfcd8c80d6d4")
		)
		(fp_line
			(start -3.54 2)
			(end -3.54 -10)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f0e6d96b-0a7d-47d5-882e-1a312dd2823d")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 1.3 90)
			(layer "B.Fab")
			(uuid "40131998-0e92-4d31-b19d-49e4858ebabd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 2.08 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.120192)
			(net 13 "Net-(J7-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "b921c531-2038-47c6-9d02-a5b59b625f18")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 90)
			(size 2.08 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J7-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "9a59be25-992b-414f-bbec-936800392b59")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Card:microSD_HC_Hirose_DM3AT-SF-PEJM5"
		(layer "B.Cu")
		(uuid "a40c962c-16ae-4cc3-abbe-0556d3ecc141")
		(at 115.185 81.5375 -90)
		(descr "Micro SD, SMD, right-angle, push-pull (https://www.hirose.com/product/en/download_file/key_name/DM3AT-SF-PEJM5/category/Drawing%20(2D)/doc_file_id/44099/?file_category_id=6&item_id=06090031000&is_series=)")
		(tags "Micro SD")
		(property "Reference" "J9"
			(at -0.075 9.525 90)
			(layer "B.SilkS")
			(uuid "24c2225b-4774-476c-96be-8db962338f49")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "Micro_SD_Card"
			(at -0.075 -9.575 90)
			(layer "B.Fab")
			(uuid "708bff11-4108-40bd-acc7-907522436e9a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/693072010801.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "e7742168-c497-4395-86fd-bf51b156f66f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Micro SD Card Socket"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "5060fd6d-d40e-4011-a346-13ccf1ccc10c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Vendor" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "fb71210b-c903-4fbf-82c8-f0698afec590")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "SKU" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "44d89708-2bc0-44fe-a9df-f07e1e243b44")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "microSD*")
		(path "/bf5021ce-f145-41d4-a6c6-4ea07d9f9483")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -6.975 7.885)
			(end -6.975 4.275)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a11ac336-e83d-4f03-adf0-ff2ca09b78b7")
		)
		(fp_line
			(start -6.525 7.885)
			(end -6.975 7.885)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8ec6f729-76a7-43f3-b5fa-f5d7c1f779c3")
		)
		(fp_line
			(start 5.075 7.885)
			(end 6.995 7.885)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f9274813-f744-4ae3-aeb8-77913e9b575e")
		)
		(fp_line
			(start 6.995 7.885)
			(end 6.995 -6.125)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0643305d-988c-4710-bdd7-e5071d2e1d51")
		)
		(fp_line
			(start -6.975 2.575)
			(end -6.975 -2.125)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "03926b26-857c-4661-9747-1e1c2b16fbe5")
		)
		(fp_line
			(start -6.975 -3.425)
			(end -6.975 -5.225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4680d827-a4f7-4dbe-8cba-d7207cf1f0f0")
		)
		(fp_line
			(start -3.875 -8.035)
			(end 2.495 -8.035)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "197061b7-892d-4c3b-80a4-f02f1bf0d442")
		)
		(fp_line
			(start -3.875 -8.035)
			(end -3.875 -8.185)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "7e4f6832-fe70-46f3-b993-666e88d420b6")
		)
		(fp_line
			(start 5.515 -8.185)
			(end 5.775 -8.185)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "37668471-46e0-4ba1-a432-f6313c1264d2")
		)
		(fp_line
			(start -5.945 -8.385)
			(end -6.145 -8.185)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c8e6f7a4-0733-484f-8586-423e309cd2ac")
		)
		(fp_line
			(start -5.945 -8.385)
			(end -4.085 -8.385)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "15a0350a-59ff-40af-9831-cc5dc1bbc5ba")
		)
		(fp_line
			(start -4.085 -8.385)
			(end -3.875 -8.185)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "83bb948a-8ce1-40ef-b6cb-34351fe1968d")
		)
		(fp_line
			(start 3.005 -8.385)
			(end 2.495 -8.035)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ab9bef63-e66f-4714-80b2-9d6242832e56")
		)
		(fp_line
			(start 5.315 -8.385)
			(end 5.515 -8.185)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f91426ba-972b-4363-b850-cb74e1c12ca6")
		)
		(fp_line
			(start 5.315 -8.385)
			(end 3.005 -8.385)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "13bdcff4-5bde-4613-9d9b-e6d3f244409d")
		)
		(fp_line
			(start -7.82 8.82)
			(end 7.88 8.82)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "10a26d12-62e7-4b7a-a465-8738347fdc52")
		)
		(fp_line
			(start 7.88 8.82)
			(end 7.88 -8.88)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "10c62257-2719-45a1-b4fb-55f82d1e42cc")
		)
		(fp_line
			(start -7.82 -8.88)
			(end -7.82 8.82)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "fc6c14c9-ee2f-4d2b-be6d-0d41ec8f99bc")
		)
		(fp_line
			(start 7.88 -8.88)
			(end -7.82 -8.88)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b34ac656-ba73-43c9-a3cb-6cc314d9b960")
		)
		(fp_line
			(start 6.925 7.825)
			(end -6.925 7.825)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "d453788b-4387-4616-afbb-e817f3e3c799")
		)
		(fp_line
			(start 2.51 -7.975)
			(end -3.915 -7.975)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "b2fa402a-8990-48fe-b28e-51f4e01249d4")
		)
		(fp_line
			(start -6.925 -8.125)
			(end -6.925 7.825)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f698302a-fe36-4071-a1bc-0806d38bf5e7")
		)
		(fp_line
			(start -6.115 -8.125)
			(end -6.925 -8.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "db4e4478-f38f-4072-b4f8-fca857f27828")
		)
		(fp_line
			(start -3.915 -8.125)
			(end -3.915 -7.975)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "3c5be2ad-fe39-492c-8295-0dafadb95d8c")
		)
		(fp_line
			(start -3.915 -8.125)
			(end -4.115 -8.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5ae6ce55-9b9e-4534-9cf7-d33bf700316f")
		)
		(fp_line
			(start 5.485 -8.125)
			(end 6.925 -8.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "bb641cdb-5ac0-435f-89a4-d18b88f9ceb1")
		)
		(fp_line
			(start 6.925 -8.125)
			(end 6.925 7.825)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "b5aefd72-e161-44d5-a425-aa53ba2e82b9")
		)
		(fp_line
			(start -5.925 -8.325)
			(end -5.925 -13.225)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "ced13ffe-b944-4c90-b50c-ea22aa260177")
		)
		(fp_line
			(start -5.915 -8.325)
			(end -6.115 -8.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "37c5db50-cb84-4f48-80c4-b2f05cab43b0")
		)
		(fp_line
			(start -4.115 -8.325)
			(end -5.915 -8.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "bf65dee1-5538-45d9-ae67-6856798c9425")
		)
		(fp_line
			(start 3.035 -8.325)
			(end 2.51 -7.975)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "fa0922c8-870f-4a94-87fd-b93578c7eb0f")
		)
		(fp_line
			(start 5.285 -8.325)
			(end 5.485 -8.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "fd054f91-67b8-4489-8310-65b4ef4e3c81")
		)
		(fp_line
			(start 5.285 -8.325)
			(end 3.035 -8.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "dc1d4415-c90f-4cf9-b19e-8270df9a9d9a")
		)
		(fp_line
			(start -5.425 -9.725)
			(end 4.575 -9.725)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f0a25d71-88c4-4c95-bbba-cbb910433f38")
		)
		(fp_line
			(start 5.075 -13.225)
			(end 5.075 -8.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f98fe3e7-d615-4b3b-b547-23902f8b4a30")
		)
		(fp_line
			(start -5.425 -13.725)
			(end 4.575 -13.725)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "1476c49f-ab3a-4e23-b1bf-640188c195a1")
		)
		(fp_arc
			(start -5.925 -9.225)
			(mid -5.778553 -9.578553)
			(end -5.425 -9.725)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "6c549f12-be84-4714-9aa8-4b4736fda344")
		)
		(fp_arc
			(start 4.575 -9.725)
			(mid 4.928553 -9.578553)
			(end 5.075 -9.225)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "669f9330-68b7-46e3-9bcf-49b8b52d7fac")
		)
		(fp_arc
			(start -5.925 -13.225)
			(mid -5.778553 -13.578553)
			(end -5.425 -13.725)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c2d650ab-b9e9-4431-8570-1c19f6827dbe")
		)
		(fp_arc
			(start 4.575 -13.725)
			(mid 4.928553 -13.578553)
			(end 5.075 -13.225)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "61e2a82d-d6b2-4026-81c2-871886dfc9f7")
		)
		(fp_text user "KEEPOUT"
			(at -5.775 -2.375 180)
			(layer "Cmts.User")
			(uuid "08b17319-8e66-432f-9ab7-24370df0fbb7")
			(effects
				(font
					(size 0.6 0.6)
					(thickness 0.09)
				)
			)
		)
		(fp_text user "KEEPOUT"
			(at -1.075 1.925 90)
			(layer "Cmts.User")
			(uuid "100b506d-45ea-4792-895e-b385dd78e452")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(fp_text user "KEEPOUT"
			(at -6.85 3.25 180)
			(layer "Cmts.User")
			(uuid "8bef6e69-ab92-4053-818b-e40200c47be7")
			(effects
				(font
					(size 0.6 0.6)
					(thickness 0.09)
				)
			)
		)
		(fp_text user "KEEPOUT"
			(at 4.2 -7.65 90)
			(layer "Cmts.User")
			(uuid "8dc841e8-ac2c-475e-9202-8d74928824b4")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at -0.075 -0.375 90)
			(layer "B.Fab")
			(uuid "35d4e0cc-7e53-4afe-8e2d-f0e5fc23f08b")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
				(justify mirror)
			)
		)
		(pad "1" smd rect
			(at 2.775 7.725 270)
			(size 0.7 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 63 "unconnected-(J9-DAT2-Pad1)")
			(pinfunction "DAT2")
			(pintype "bidirectional+no_connect")
			(uuid "ebaf0e9c-b708-4074-b1a1-d6b63e99c660")
		)
		(pad "2" smd rect
			(at 1.675 7.725 270)
			(size 0.7 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 62 "SPI_SD_CS")
			(pinfunction "DAT3/CD")
			(pintype "bidirectional")
			(uuid "8c803caa-e138-40f3-bf4f-04d5bf16a503")
		)
		(pad "3" smd rect
			(at 0.575 7.725 270)
			(size 0.7 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 61 "SPI_MOSI")
			(pinfunction "CMD")
			(pintype "input")
			(uuid "4f9b48da-3326-465d-96f6-c8c17468f965")
		)
		(pad "4" smd rect
			(at -0.525 7.725 270)
			(size 0.7 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "4fc3dc7d-3498-4ada-83c8-7a023685e796")
		)
		(pad "5" smd rect
			(at -1.625 7.725 270)
			(size 0.7 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 60 "SPI_SCK")
			(pinfunction "CLK")
			(pintype "input")
			(uuid "4ee696eb-beb5-4590-bbcc-c4897a9df409")
		)
		(pad "6" smd rect
			(at -2.725 7.725 270)
			(size 0.7 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(uuid "37b3175a-3dc3-4d87-8cda-2ac602322e9a")
		)
		(pad "7" smd rect
			(at -3.825 7.725 270)
			(size 0.7 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 59 "SPI_MISO")
			(pinfunction "DAT0")
			(pintype "bidirectional")
			(uuid "37d4d6a3-3cd8-48b8-b618-6a2a2a01271b")
		)
		(pad "8" smd rect
			(at -4.925 7.725 270)
			(size 0.7 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 58 "unconnected-(J9-DAT1-Pad8)")
			(pinfunction "DAT1")
			(pintype "bidirectional+no_connect")
			(uuid "2c8251b4-7479-4bb2-ad2b-1bc0e05cfd15")
		)
		(pad "9" smd rect
			(at -5.875 7.725 270)
			(size 0.7 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 57 "unconnected-(J9-SHIELD-Pad9)")
			(pinfunction "SHIELD")
			(pintype "passive")
			(uuid "1b8492e0-a3f5-4743-bb3d-49869d85b077")
		)
		(pad "10" smd rect
			(at -6.825 -2.775 270)
			(size 1 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(uuid "8837cdf4-5959-408d-9f1a-8c844a212c8b")
		)
		(pad "11" smd rect
			(at -6.825 -6.925 270)
			(size 1 2.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(uuid "313bb80b-ebdf-41f9-81e2-8533a5cb532f")
		)
		(pad "11" smd rect
			(at -6.825 3.425 270)
			(size 1 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(uuid "f4445009-1848-4ab7-b9de-fa7f72e998c9")
		)
		(pad "11" smd rect
			(at 4.325 7.725 270)
			(size 1 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(uuid "47eb3fe2-6937-4300-8b4f-c66e067cdc11")
		)
		(pad "11" smd rect
			(at 6.675 -7.375 270)
			(size 1.3 1.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(uuid "de658a85-4570-4af9-b1bf-587ab8f654fe")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(uuid "04bbe0f3-5674-4dd9-b9f2-fedf6137ba5e")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 111.16 75.0625) (xy 111.16 74.3125) (xy 107.91 74.3125) (xy 107.91 75.0625)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(uuid "74d4d5eb-f590-4e71-bd66-c2fa282629a3")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 113.76 75.4125) (xy 113.76 76.1125) (xy 121.36 76.1125) (xy 121.36 75.4125)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(uuid "c90537f2-4ade-421f-bc51-f5df9d537824")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 114.06 84.8125) (xy 114.06 76.1125) (xy 112.46 76.1125) (xy 112.46 84.8125)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(uuid "a71ed464-0c0c-48b1-84c1-5ba65d392879")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 115.96 75.0625) (xy 115.96 74.3125) (xy 112.36 74.3125) (xy 112.36 75.0625)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(uuid "8328f1f9-96fc-40e8-b6e9-c4aee39185b2")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 122.16 84.4625) (xy 122.16 87.0125) (xy 123.51 87.0125) (xy 123.51 84.4625)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Card.3dshapes/microSD_HC_Hirose_DM3AT-SF-PEJM5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal"
		(layer "B.Cu")
		(uuid "adcfd51d-1c06-4e0b-9790-8459436fe6f6")
		(at 104.655 43.8275)
		(descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
		(tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
		(property "Reference" "J1"
			(at 2.54 3.2 180)
			(layer "B.SilkS")
			(uuid "423d65aa-e847-4cb8-9527-733465e97e7a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 2.54 -11.2 180)
			(layer "B.Fab")
			(uuid "ce370606-272c-452c-b198-3638ac94fc61")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "3272ec7b-dc11-4739-bf1f-873fb9650bfc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "d057f90d-818e-4569-8296-9f20317d40bc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/b2fb0e89-3acc-44df-adbb-63ddabf8adb1")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -3.65 -10.11)
			(end 8.73 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ee1fc976-bb99-470f-8f01-1631785dbf21")
		)
		(fp_line
			(start -3.65 -8.61)
			(end -3.65 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0e8c57b1-2a1e-4c3f-807a-a41566aefae8")
		)
		(fp_line
			(start -3.65 -6.81)
			(end 8.73 -6.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "bd7f792b-82b7-4325-b0ea-268705c4e936")
		)
		(fp_line
			(start -3.65 2.11)
			(end -3.65 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e6dfa1c2-7cff-418d-a3ed-24bc27b8c972")
		)
		(fp_line
			(start -1 -10.11)
			(end 1 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9eac84a5-fb38-40ff-9bb7-e79e2d9e86b4")
		)
		(fp_line
			(start -0.75 -8.61)
			(end -1 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "5ae01cbf-9ad1-41fe-ab6c-506f96da6559")
		)
		(fp_line
			(start -0.3 2.91)
			(end 0.3 2.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8cdc4258-0a9b-42b9-9fb1-709697d06093")
		)
		(fp_line
			(start 0 2.31)
			(end -0.3 2.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "431c8a74-377e-45e2-a30a-ba4485071891")
		)
		(fp_line
			(start 0.3 2.91)
			(end 0 2.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c2c9e73f-4881-4f4f-a394-aff70e8328bf")
		)
		(fp_line
			(start 0.75 -8.61)
			(end -0.75 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "09467d4a-5c91-4ab9-93ec-22f12470d334")
		)
		(fp_line
			(start 1 -10.11)
			(end 0.75 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "939028db-8056-4772-a569-316688a97c16")
		)
		(fp_line
			(start 4.08 -10.11)
			(end 6.08 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8d9d42c1-b0d7-4ba0-a02d-ab35244c67a2")
		)
		(fp_line
			(start 4.33 -8.61)
			(end 4.08 -10.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "dba27f73-a8a4-46d3-97f9-a79a5a07f72b")
		)
		(fp_line
			(start 5.83 -8.61)
			(end 4.33 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "7f9adb65-bb9c-48c6-8737-acc8c1e5655e")
		)
		(fp_line
			(start 6.08 -10.11)
			(end 5.83 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "036bf6a0-b03b-4825-b84f-365cde6f3594")
		)
		(fp_line
			(start 8.73 -10.11)
			(end 8.73 2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ce9752ef-1fe5-4eba-95f1-d907233f8df8")
		)
		(fp_line
			(start 8.73 -8.61)
			(end -3.65 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "da56ce78-3ecc-47cf-83e0-bf6e613f60a7")
		)
		(fp_line
			(start 8.73 -6.81)
			(end 8.73 -8.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9a854288-a438-4a39-9d33-3704ad11e5ed")
		)
		(fp_line
			(start 8.73 2.11)
			(end -3.65 2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "df4d9554-743f-4655-b33e-a5e29fcb5359")
		)
		(fp_line
			(start -4.04 -10.5)
			(end 9.13 -10.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "56498e32-573b-42d4-8e80-4aa3c213b406")
		)
		(fp_line
			(start -4.04 2.5)
			(end -4.04 -10.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "471b74b9-9184-4162-8ed5-285fd2756268")
		)
		(fp_line
			(start 9.13 -10.5)
			(end 9.13 2.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5966cd25-9c54-4aee-bc93-b0ca3955987a")
		)
		(fp_line
			(start 9.13 2.5)
			(end -4.04 2.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "d334e33a-cbda-4572-a965-815e736e91d8")
		)
		(fp_line
			(start -3.54 -10)
			(end 8.62 -10)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "01465e11-90b4-441c-9bae-b521198d1d36")
		)
		(fp_line
			(start -3.54 2)
			(end -3.54 -10)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "2376404d-be2c-45ca-8f18-ef9d99851151")
		)
		(fp_line
			(start 0 0.5)
			(end -0.95 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "ca7a99c3-54bf-47c3-80f2-18ae9af003c7")
		)
		(fp_line
			(start 0.95 2)
			(end 0 0.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a96d8fdf-c885-4ef2-8536-fd430f5e2ea7")
		)
		(fp_line
			(start 8.62 -10)
			(end 8.62 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c29e0ce1-98a9-4114-8cc5-535322c5540a")
		)
		(fp_line
			(start 8.62 2)
			(end -3.54 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "3f0d644c-887b-43aa-ad9c-deac21f4f5ad")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 1.3 180)
			(layer "B.Fab")
			(uuid "0f177a8f-9adf-4969-91a9-1208d9d73929")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.08 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.120192)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "b7e797fa-1030-43a3-a594-d82e644ce4f7")
		)
		(pad "2" thru_hole oval
			(at 5.08 0)
			(size 2.08 3.6)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "SSR_SWITCH")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "83fcee99-f82d-4675-97f2-771155cfe568")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector:FanPinHeader_1x03_P2.54mm_Vertical"
		(layer "B.Cu")
		(uuid "af5ea9c2-080a-4e17-bfd0-50b30d9a0659")
		(at 47.9 100.35 180)
		(descr "3-pin CPU fan Through hole pin header, see http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf")
		(tags "pin header 3-pin CPU fan")
		(property "Reference" "J5"
			(at 2.5 3.4 0)
			(layer "B.SilkS")
			(uuid "764c430d-7d46-4eb9-8a3b-fb95fceebdf9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "Conn_01x03_Socket"
			(at 2.55 -4.5 0)
			(layer "B.Fab")
			(uuid "8b862b9b-00c2-40c7-8390-e8c7e7f8f04e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "5aa51be4-0e7c-42ee-885d-3ab317bef7a0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "6bf07d77-63de-45c0-b1a8-51984376ee62")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/c2316714-3635-42d1-962b-199da05f345a")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 6.45 2.65)
			(end 6.45 -3.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b408ebf3-0d4c-4502-821e-22b03ad77ea8")
		)
		(fp_line
			(start 6.45 -3.4)
			(end -1.35 -3.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d4183267-0b3e-4827-b588-70919b7692f9")
		)
		(fp_line
			(start 5.08 -2.29)
			(end 5.08 -3.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9236781e-d7ed-43b3-9d10-420747b42f2d")
		)
		(fp_line
			(start 0 -2.29)
			(end 5.08 -2.29)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "27fa2921-37d7-48b9-a147-cf581fc227b3")
		)
		(fp_line
			(start 0 -3.3)
			(end 0 -2.29)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "479c99ec-1d63-4e82-9535-e04fd62aa2b4")
		)
		(fp_line
			(start -1.35 2.65)
			(end 6.45 2.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6972f28b-a61f-4ae0-a220-881db8edc6d9")
		)
		(fp_line
			(start -1.35 -3.4)
			(end -1.35 2.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c97e847b-6c99-4f38-b02f-3e860e2ae132")
		)
		(fp_line
			(start 6.85 3.05)
			(end 6.85 -3.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "51cd3610-3025-498a-81a4-a250a0b878d6")
		)
		(fp_line
			(start 6.85 3.05)
			(end -1.75 3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "3242dc49-b6ef-4ca5-9643-6af257cc0789")
		)
		(fp_line
			(start -1.75 -3.8)
			(end 6.85 -3.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "a68328e7-d93d-48e7-bddc-7ded9f1c0fa7")
		)
		(fp_line
			(start -1.75 -3.8)
			(end -1.75 3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "9121f16e-fa02-4feb-97fc-809f75c380df")
		)
		(fp_line
			(start 6.35 2.55)
			(end 6.35 -3.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "7be20ba6-3cfc-404b-a1e8-48cfb39ae4b4")
		)
		(fp_line
			(start 6.35 -3.3)
			(end -1.25 -3.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9bb77bd7-d36b-4937-bb55-418cc258a6cc")
		)
		(fp_line
			(start 5.05 -2.3)
			(end 0 -2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c9247101-60d4-4a5b-ab55-4f5a713ccaa0")
		)
		(fp_line
			(start 5.05 -3.3)
			(end 5.05 -2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a3611685-a20e-4b03-b112-fa37d4e07aec")
		)
		(fp_line
			(start 0 -2.3)
			(end 0 -3.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "971a4799-fec5-43da-a19c-4bcc850c05b0")
		)
		(fp_line
			(start -1.25 2.55)
			(end 6.35 2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "617cf5b5-c309-4934-89a3-9bfd16ddb625")
		)
		(fp_line
			(start -1.25 -3.3)
			(end -1.25 2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "6f6a728b-a83f-4f4d-949c-8677d9e47cc7")
		)
		(fp_text user "${REFERENCE}"
			(at 2.45 -1.8 0)
			(layer "B.Fab")
			(uuid "d99cea15-f86a-4cf2-8812-d710902012bf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.03 1.73)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "USR_PWM_1_AUX")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "40c6379d-412e-4db2-a535-0fe57bae079b")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 2.03 1.73)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(J5-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "1fc94992-6c26-4f2b-90e1-3210687aff7e")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 2.03 1.73)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "dc999089-02e7-4dd1-ba8d-3a4eed9a6fa3")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector.3dshapes/FanPinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "b45def30-dc73-4678-91a6-942a5d31f2b0")
		(at 87.485 145.6775)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D18"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "39dedb6f-b8be-48d6-8b37-1ee8627c1b1a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "b1225702-6084-49d1-827f-e8e7170d4a3f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "47b6562f-bf59-4737-8985-f02ce3e8313e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "4f190a47-1d46-433d-bb99-2fe2a8ec5136")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "5d77053d-6dfc-4784-9715-63397447f73e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "373dbe55-46e8-40d5-9edf-dd784061f123")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/6e38b205-635f-4524-89c5-bb24b23db06d")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4c9f15a7-ca50-44de-8604-caffc8581cdd")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "15283c36-fafa-4b02-86fd-021462be09f5")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "7e8f55d5-d245-4f3c-adb9-cf14ec0c265b")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b4c2abb4-7600-49fd-ab94-48bd3a5bb36f")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "1e0f05b4-9715-492e-86cc-a9553000ab28")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "affa3e76-0226-4449-9bbc-3b5c58cbac39")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "258bd79f-1e89-4a36-af39-6df54b69c9d0")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "59c2d1fc-ff9f-4dec-8a8e-0beeae36a237")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "66706bcc-729c-44b7-ac00-b3a9f0eb2da9")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "084c2de7-7afd-4540-8ad0-28f619b08dde")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9ddb923c-c8e6-40b8-b756-9002f695f57f")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "3d5e22aa-9150-4c5c-9a92-2e30526eabb3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "58f96ab9-401e-40aa-ac73-3895bc4ef9cf")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 22 "KEYPAD_ROW_1")
			(pinfunction "K")
			(pintype "passive")
			(uuid "77852ce8-bbd6-4417-b686-8479c453e223")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 36 "Net-(D18-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "6e6b4917-2a2b-4dd9-999e-b829b090f479")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Converter_ACDC:Converter_ACDC_MeanWell_IRM-02-xx_THT"
		(layer "B.Cu")
		(uuid "beead06b-ce6f-4067-9abc-8ff52ef1fd7e")
		(at 58.4 52.7825)
		(descr "ACDC-Converter, 2W, Meanwell, IRM-02, THT, https://www.meanwell.co.uk/media/productPDF/IRM-02-spec.pdf")
		(tags "ACDC-Converter 2W THT")
		(property "Reference" "PS1"
			(at -0.8 4.8 180)
			(layer "B.SilkS")
			(uuid "dd2b5678-263a-46a3-b1d1-abd9119c3698")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "IRM-02-12"
			(at 15.14 -20.15 180)
			(layer "B.Fab")
			(uuid "127eeab1-87eb-445d-9251-ea3793e24aba")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-02/IRM-02-SPEC.PDF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "6527fb26-487c-442b-9a18-ebd23e6c735a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "12V, 167mA, 2W, Isolated, AC-DC, IRM02"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "0e697828-5fe6-4225-92ce-b8bca31661e9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Converter*ACDC*MeanWell*IRM*02*THT*")
		(path "/227d057a-256e-4b1c-9a2b-3227d3c5f24b")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.97 -18.82)
			(end -2.97 3.62)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "87d23bc1-37f0-4c23-84d9-09e0221bf4d1")
		)
		(fp_line
			(start -2.97 -18.82)
			(end 30.97 -18.82)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d41cf2b1-88d3-426a-932f-bec0f42ece98")
		)
		(fp_line
			(start -2.97 3.62)
			(end 30.97 3.62)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "fa131c39-7c0b-4210-82a5-1a095a28f991")
		)
		(fp_line
			(start -2 3.95)
			(end 4 3.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "74cdc1db-7cfc-43b7-9ce2-810069bbee23")
		)
		(fp_line
			(start 30.97 3.62)
			(end 30.97 -18.82)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0dc21800-56d2-4a06-ad41-30d5cf55e659")
		)
		(fp_line
			(start -3.1 -18.95)
			(end -3.1 3.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "21853170-a632-40c9-b745-1bbd60b3b607")
		)
		(fp_line
			(start -3.1 -18.95)
			(end 31.1 -18.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "fa4bf73a-ce6e-4f99-870f-c562e1538d3b")
		)
		(fp_line
			(start -3.1 3.75)
			(end 31.1 3.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e900c9d2-8e2f-4497-8840-bef06cb4073f")
		)
		(fp_line
			(start 31.1 -18.95)
			(end 31.1 3.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "4bf397d2-7f08-4432-b409-5ea318d45402")
		)
		(fp_line
			(start -2.85 -18.7)
			(end -2.85 3.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9cccf4a4-fb50-4d24-9538-cb44b9af7716")
		)
		(fp_line
			(start -2.85 -18.7)
			(end 30.85 -18.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9eb53e78-c543-4c37-849e-5826f8fc12dc")
		)
		(fp_line
			(start -1 3.5)
			(end -2.85 3.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "04cce8e7-8aac-434b-900a-b4714abec541")
		)
		(fp_line
			(start 0 2.5)
			(end -1 3.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "3642daeb-72a2-401c-bb12-ff7994d4db8b")
		)
		(fp_line
			(start 1 3.5)
			(end 0 2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c7d3189c-0f37-400d-80bf-c614ac4927d5")
		)
		(fp_line
			(start 1 3.5)
			(end 30.85 3.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "6638369d-27eb-4203-b5b7-a4ef09199116")
		)
		(fp_line
			(start 30.85 -18.7)
			(end 30.85 3.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a07bf541-ca67-452a-b17e-5ac5e186a4bb")
		)
		(fp_text user "${REFERENCE}"
			(at 14.03 -7.47 180)
			(layer "B.Fab")
			(uuid "adc8ea3e-720f-43bc-9fad-22102fb47322")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.3 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J3-Pin_1)")
			(pinfunction "AC/N")
			(pintype "power_in")
			(uuid "85e702bb-fdcd-4eef-87fa-90617bbadc41")
		)
		(pad "2" thru_hole circle
			(at 0 -15.2)
			(size 2.3 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(J3-Pin_2)")
			(pinfunction "AC/L")
			(pintype "power_in")
			(uuid "0a06690a-f70d-468d-a056-ae8a581245e8")
		)
		(pad "3" thru_hole circle
			(at 28 0)
			(size 2.3 2.3)
			(drill 0.76)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-Vo")
			(pintype "power_out")
			(uuid "ae04e969-9f44-41ab-a4e2-507874f8b52a")
		)
		(pad "4" thru_hole circle
			(at 28 -7.6)
			(size 2.3 2.3)
			(drill 0.76)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "+12V")
			(pinfunction "+Vo")
			(pintype "power_out")
			(uuid "1dbc7b19-00df-40c8-b529-9a448ba63c66")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Converter_ACDC.3dshapes/Converter_ACDC_MeanWell_IRM-02-xx_THT.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "d04e7f23-df6d-4420-85e3-682fb637314d")
		(at 87.485 148.7175)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D17"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "4224800f-20c8-4ad2-89a5-248e0c9684d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "7a947cc6-cb54-4d40-9314-d1787c39ca51")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "d637a585-9e06-4a4a-bcda-6d42b6d8fedf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "def16a1f-f22d-48d4-bc99-c368c032b8c9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "7df310b3-2a9e-4c82-862e-cc146d6f4135")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "f31f431d-888e-491c-b8a8-8be9b7c6bb1b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/fafe3176-4338-4e1d-94fe-28fa44e16509")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4f49613d-393b-4443-8e66-9d80aaeee833")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "08090c99-1d56-4d24-b453-e3313d736284")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "aecef3ef-b994-491f-958b-458dd8d0c230")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "6854f582-7541-4974-aaf3-a3f64bdf8279")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "0c396381-e7f8-4b6d-9102-d2ee5ded316a")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b442e306-546d-4ff2-a04c-df9f6c3cddb5")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "7e2e6ebf-cc73-4cb2-97ad-eafc6992841a")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "1da7135b-cff0-4882-9b2a-41f85fd13817")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "279dcf2a-9ab8-4260-980f-3cc447802b75")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9d4afcb5-502f-4483-9338-f7b93dc3923f")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a5b6ac58-524c-4dfc-af62-b7798025dd8e")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f88c5a5d-9bc5-4ac7-9460-aefef5859b47")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "2e32e95e-c371-41f4-8ce4-1ba3616ea481")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 19 "KEYPAD_ROW_0")
			(pinfunction "K")
			(pintype "passive")
			(uuid "7f75e448-b3d6-4b4a-8b9f-ff43953ee127")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 35 "Net-(D17-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "965f7646-fa69-42bf-a6ae-01c8e2488e65")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "d143ad38-46f2-4c6d-8548-210634c18154")
		(at 82.69 136.5575)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D15"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "7d80c48e-e513-404a-852f-f7c811cd8f56")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "2111b469-d894-4bf8-8bf1-ad2c859e9944")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "9dbc202b-948f-47e4-bdda-a213139e19a6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "27c7009f-667d-4f28-ae77-43f17b00b440")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "bc6d27c0-d758-4d46-8d22-f282380318af")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "43f3ca7d-220e-4a8f-8df5-9d07e7bd7d2e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/e0bcd042-2562-499e-b716-0b0c9ebdd942")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "300e7422-e95e-4625-b405-0699336bf5a3")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8f80212d-e4a2-45a3-a711-e4b73ba5ab9e")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a0989e8d-7c1b-4df7-bafd-6027a97f1c38")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "011d2664-484b-406b-bb94-229af57c3a6e")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5542addc-7631-4bd4-b1a7-bea72f1d8478")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "d3ca4bf8-48ab-427d-8688-e0db8c40ff98")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "00e2c4fc-0f83-4570-aa7b-22f70d8498ca")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "4cc3fb28-b577-4835-ae20-72af0ad89566")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5615cea2-7f1d-4e9a-87ae-c4ce877d2984")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "03c5360c-3a16-439d-9750-8346f6cdceca")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5365ecf2-712c-48ed-906f-97bd89a63b3a")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "bccc667f-ac04-4052-9f06-103155518fa6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "89f1dffe-82db-436b-9ffa-0d50bbf2f949")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 23 "KEYPAD_ROW_2")
			(pinfunction "K")
			(pintype "passive")
			(uuid "3675b517-fd48-4d39-8744-dc6df22e0ed7")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 33 "Net-(D15-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "85ff520e-ac8e-420e-b98e-957a746fe76b")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "d662cf64-0405-45e2-be76-21a57e591fa7")
		(at 77.895 148.7175)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D5"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "e18b8c6d-1880-47ce-b51b-bb99af4bcc32")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "42d47e55-eb98-4bf5-8fd5-ddb83dee937f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "ca52611a-c407-4f87-a018-21c2769e5544")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "2b014faa-11d3-48d4-9e17-b31c244a9718")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "aaf0bac1-577a-407c-9f88-daba558a0152")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "c089d009-5928-4f37-8e73-d4631eab4f05")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/f02acbf7-ab91-4669-8a5b-cb8767ec3b92")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ec993e99-81ad-490c-85bb-346277dc207f")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0b9498b9-8441-41b8-8cdd-61a41488da8a")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b988d8c4-d4bc-45c7-881c-058b42e5b868")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "6b973668-9f88-4115-a4bf-f62427ffd14d")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "d8f1b9b2-5364-4b6a-bef0-a1a7e459639d")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "1b6d730a-9293-495b-b081-9e85b351fd2e")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e7ad1b25-bb58-4117-9ef3-68055c37a800")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "88f249ad-457f-4f85-b180-1861d4a762d8")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a719244a-2d0f-4a28-a7e9-1eb63157f62a")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "ab0011ee-c458-493a-a96f-a8e8e71e578a")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "31471f49-3a9d-42cc-9825-b1cf34e19d57")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f01c98e3-21b7-4741-a9a1-0bb6f52bdb5b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "dcc41ce3-2c60-455c-8d11-756745b4bc52")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 19 "KEYPAD_ROW_0")
			(pinfunction "K")
			(pintype "passive")
			(uuid "07565fed-4ab4-4d15-83d6-9fa32db2ac61")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 20 "Net-(D5-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "57954e56-e22d-4818-a458-26e72966efb5")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "d89acdae-15dd-4c6d-8f2e-5d73193f2f40")
		(at 82.69 142.6375)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D13"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "48c6ff41-7776-4054-bc2a-0380af381e06")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "112fe3bb-6235-4087-ac75-12ba4376f5c5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "ba554a33-11be-453a-81e4-eb286ae562d1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "ee4292fa-02a8-427c-b2d3-be67d53a9ac0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "5beff52e-dbe7-4c2c-8376-6e2f6c2ffa76")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "314a1b24-8f40-4673-a050-498af99b1bb2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/a208d8bd-214c-4389-a7ca-72ab7d76e344")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "aee3125a-df5e-4dce-8ab5-82eff5c1fd6c")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "201f1dcd-bcb0-4ce6-b1a9-739126f0b581")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "49129e41-5cae-428a-8d5c-26a3055fc196")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "49448025-0ca2-4642-9a9e-1db33ac90777")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "7e1dd845-9390-4ddf-bf4a-1128c98ed932")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e096e269-d50b-4bf9-8430-908df5a217ec")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "cd39a7a0-91b1-4470-9b27-3752b4333ae4")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5e1a3a73-b0c9-4f67-aaf6-65056c0dfb04")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "383c7514-68ff-48d2-b4cd-d40f097b1d96")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "33d3b108-e86a-42eb-b625-79a8af1a338c")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "3b407924-ab1d-4a2c-a6d3-4588d2a1eec9")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "7a6b8dfc-e62a-4c79-8f3e-e7ae14b3df87")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "38723103-e9a6-4b34-8b6b-3310927949f1")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 19 "KEYPAD_ROW_0")
			(pinfunction "K")
			(pintype "passive")
			(uuid "ae307fcb-4153-4513-b6eb-ed69e6756759")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 31 "Net-(D13-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "abcfd4c7-f105-4620-ba92-89752553668f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "dc0beb0f-0322-4004-9062-39eb94cb7954")
		(at 82.69 145.6775)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D12"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "f0c13288-4208-488b-8ab0-051d7d5243fb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "ef154728-215a-458d-aff7-0189e3cd3097")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "3e7e3c16-626d-4f3c-a213-c5ec11f0588f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "a5620519-c197-4be2-b697-939e59e2deb1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "08762b71-444a-4d55-ad2e-bdac5c587a98")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "4e67072f-6849-4bf7-a8b0-14302b3b7139")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/4ca4e7eb-6ed3-4c77-ab6c-dbf504c255ec")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d62e4f78-7291-4646-9e76-8cbaf2dd1c85")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c68b40d0-1b4a-4cde-bab3-15a1791b109f")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ef618b87-16b8-4928-a238-80ecf576a61a")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "f4e5911b-b04e-4bba-9861-99524b58b3ee")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "0f6c1376-b060-4572-94ad-4f4a4e14d1f8")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "4c32ee06-b68b-4452-af2a-c6cd214e5186")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "45444a91-720d-4a20-8aba-a863259846a2")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9ddd0034-f214-48c6-9033-700a3f7c995e")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "fef599a1-99e1-46d0-8115-1352ce663a58")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f7405c74-8379-4618-8ca4-3d930269572a")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "1bf5ab4f-e92e-471b-afc4-06e3fc1fc67a")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f9e9ef35-e456-4175-a2b8-c1d7cb3564b1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "2c4be4ee-c511-47cd-8137-3e109146648b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 26 "KEYPAD_ROW_3")
			(pinfunction "K")
			(pintype "passive")
			(uuid "933e2790-eeeb-4272-9c72-dd8df378a165")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 30 "Net-(D12-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "d77d263a-757d-4029-a89f-203cca25ae6a")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "f395dda1-401f-46b0-aa3a-973c4ce86d1e")
		(at 87.485 139.5975)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D20"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(uuid "e0f5fb6d-c649-481c-b9fa-65e761b808e1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "D"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(uuid "4d3367f7-6586-4693-80b7-4f3111c4f1cf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "64dab1f8-3122-49bf-bc22-c84311fab1d1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "0c89bdb1-9267-4d44-84b7-4a28ae7b8b67")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "79c3de42-3262-4c0d-9720-72a7d1658aab")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "6a0188ed-aafe-4e77-96be-06ef28381e3b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/f93e3a62-40f3-4b77-8177-ce68b720a118")
		(sheetname "/")
		(sheetfile "PID Toaster.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.86 -0.96)
			(end 1 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "587eaa05-4922-4820-aa18-598f68c66509")
		)
		(fp_line
			(start -1.86 0.96)
			(end -1.86 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "82fc59ab-045d-406e-9341-7e7f9465ffe5")
		)
		(fp_line
			(start 1 0.96)
			(end -1.86 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ee403925-6a79-4fda-90b6-228e0d1c6834")
		)
		(fp_line
			(start -1.85 -0.95)
			(end -1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "ccc75a63-0425-4c49-8cbf-90280c71a83c")
		)
		(fp_line
			(start -1.85 0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "a2815252-42eb-4211-ac73-6f9315308b9d")
		)
		(fp_line
			(start 1.85 -0.95)
			(end -1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "08a96d19-14e6-4c33-b4ab-d46469d216e8")
		)
		(fp_line
			(start 1.85 0.95)
			(end 1.85 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "d8c27d2b-bc6a-436c-804d-32dd13229155")
		)
		(fp_line
			(start -1 -0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9f173354-544c-4b43-b9e7-35666a462c2e")
		)
		(fp_line
			(start -1 0.3)
			(end -1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "227e5507-a562-46fa-9ea3-e4f44f518391")
		)
		(fp_line
			(start -0.7 0.6)
			(end -1 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c0000923-e006-4176-b21a-f834367c657d")
		)
		(fp_line
			(start 1 -0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "612702e5-33fd-413c-a466-ed5ffcd08bbe")
		)
		(fp_line
			(start 1 0.6)
			(end -0.7 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9a8d4b34-6167-4fe8-88d2-7bf7f12995be")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(uuid "ea06679d-12b7-4136-83fe-8291a6759abe")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 26 "KEYPAD_ROW_3")
			(pinfunction "K")
			(pintype "passive")
			(uuid "525cd856-6086-4cad-b069-ef772571ff19")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 38 "Net-(D20-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "3cc17521-0130-4b21-9881-df0e0b6cab6e")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(embedded_fonts no)
)
