(footprint "SATA_Power" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at -3.5 3 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4f3e038b-b65c-4219-ba20-fdf0c83c59e9)
  )
  (fp_text value "SATA_Power" (at 9.5 3.1 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e1657f30-ef1d-4843-9af0-dbfe4a4e8100)
  )
  (fp_text user "${REFERENCE}" (at 9.5 4.6 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6172b6d4-a6b1-4f83-a0a7-3073cb57e5ad)
  )
  (fp_rect (start -5.46 -2) (end 23.24 2)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp ae176cf2-9554-4ca4-bb53-b68da67a0d8f))
  (fp_rect (start -0.1 -2) (end 0.1 -1.4)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 6688b99d-9f03-48b7-8a0c-963c0489f4f8))
  (fp_rect (start -5.56 -2.1) (end 23.34 2.1)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp eb1a52d6-2527-4b48-88d0-0a3cf62d647a))
  (fp_line (start -0.61 -0.8) (end -0.61 0.8)
    (stroke (width 0.2) (type solid)) (layer "F.Fab") (tstamp b2ee8caf-e683-4905-8d76-b4bfcbd7dc0c))
  (fp_line (start -0.61 0.8) (end 18.49 0.8)
    (stroke (width 0.2) (type solid)) (layer "F.Fab") (tstamp 01623d7d-27e1-4513-8006-26ca868952e7))
  (fp_rect (start -5.46 -2) (end 23.24 2)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 3b880b9d-c64c-4ba7-aab7-a991dca28c2d))
  (pad "" np_thru_hole circle (at -3.6 0) (size 2.2 2.2) (drill 1.6) (layers "F&B.Cu" "*.Mask") (tstamp 2c5818a8-5937-4862-9836-7f988475ee3e))
  (pad "" np_thru_hole circle (at 20.9 0) (size 2.2 2.2) (drill 1.6) (layers "F&B.Cu" "*.Mask") (tstamp ab6d9eb6-51d6-44ba-a86d-04cf011ba480))
  (pad "1" thru_hole oval (at 0 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp 0e2c9129-01a1-4013-95bb-52b0e6234227))
  (pad "2" thru_hole oval (at 1.27 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp f7f1ef48-ab19-4f33-b871-177f134bff5b))
  (pad "3" thru_hole oval (at 2.54 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp e192bde7-60d6-40ea-9f73-2181278d485f))
  (pad "4" thru_hole oval (at 3.81 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp 90af4af2-11d0-4fbe-a400-70b520ec9d28))
  (pad "5" thru_hole oval (at 5.08 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp ccfff14a-3e37-403f-b7ab-e1b764678508))
  (pad "6" thru_hole oval (at 6.35 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp a053bde9-3627-491c-8967-ae94c384a825))
  (pad "7" thru_hole oval (at 7.62 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp f13b3149-fb69-458d-80fb-15495c9be203))
  (pad "8" thru_hole oval (at 8.89 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp fd45c4c8-772a-4a4e-baf3-54d7fd5486b4))
  (pad "9" thru_hole oval (at 10.16 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp 27dd786d-7d94-49b6-8381-a603336461f7))
  (pad "10" thru_hole oval (at 11.43 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp 6f6ea440-92b8-4134-ba11-8cd8b87635a3))
  (pad "11" thru_hole oval (at 12.7 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp 61f97655-b83f-4c33-a2f9-32936d0fa5d6))
  (pad "12" thru_hole oval (at 13.97 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp df94f556-17b4-4042-81a9-01e1e4716afe))
  (pad "13" thru_hole oval (at 15.24 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp 8a44e3dc-417b-476b-8826-45d41c65ac57))
  (pad "14" thru_hole oval (at 16.51 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp bcd9935f-6f07-47c4-b7b3-a352f78d7fa4))
  (pad "15" thru_hole oval (at 17.78 0) (size 1 1.4) (drill 0.74) (layers "*.Cu" "*.Mask") (tstamp f1871de3-773e-4cf2-9c07-d624af5959fc))
  (model "${KIPRJMOD}/libs/3d/SATA-15PA.STEP"
    (offset (xyz 9 -2.5 2))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
