EESchema-DOCLIB  Version 2.0
#
$CMP TPS2121RUXT
D Power Switch ICs - Power Distribution 2.7-22V, 56mG , 4.5A, Priority Power MUX with Seamless Switchover 12-VQFN-HR -40 to 125
K
F https://www.arrow.com/en/products/tps2121ruxt/texas-instruments
$ENDCMP
#
#End Doc Library
