(module MX_Switch_Cutout (layer F.Cu) (tedit 59612069)
  (fp_text reference REF** (at 0.25 10.05) (layer Eco2.User) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value MX_Switch_Cutout (at 0 -15.24) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -9.5 -9.5) (end 9.5 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.5 9.5) (end -9.5 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.5 9.5) (end -9.5 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.5 -9.5) (end 9.5 9.5) (layer Dwgs.User) (width 0.15))
  (pad "" np_thru_hole oval (at 0 -6.731) (size 15.5956 0.508) (drill oval 15.5956 0.508) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 0 6.731) (size 15.5956 0.508) (drill oval 15.5956 0.508) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -7.5565 -4.699) (size 0.508 4.572) (drill oval 0.508 4.572) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 7.5565 -4.699) (size 0.508 4.572) (drill oval 0.508 4.572) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 7.5565 4.699) (size 0.508 4.572) (drill oval 0.508 4.572) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -7.5565 4.699) (size 0.508 4.572) (drill oval 0.508 4.572) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 6.731 0) (size 0.508 5.842) (drill oval 0.508 5.842) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -6.731 0) (size 0.508 5.842) (drill oval 0.508 5.842) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 0 -6.985) (size 5.08 1.27) (drill oval 5.08 1.27) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 0 6.985) (size 5.08 1.27) (drill oval 5.08 1.27) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -7.14375 -2.667) (size 1.3335 0.508) (drill oval 1.3335 0.508) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 7.14375 -2.667) (size 1.3335 0.508) (drill oval 1.3335 0.508) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -7.14375 2.667) (size 1.3335 0.508) (drill oval 1.3335 0.508) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 7.14375 2.667) (size 1.3335 0.508) (drill oval 1.3335 0.508) (layers *.Cu *.Mask))
)
