(module Reset_Pretty-Mask (layer F.Cu) (tedit 5C42C5CE)
  (attr virtual)
  (fp_text reference REF** (at 0 6) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Reset_Pretty-Mask (at 0 -6) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.5 3.75) (end -2.5 1.25) (layer F.SilkS) (width 0.25))
  (fp_line (start 2.5 3.75) (end -2.5 3.75) (layer F.SilkS) (width 0.25))
  (fp_line (start 2.5 1.25) (end 2.5 3.75) (layer F.SilkS) (width 0.25))
  (fp_line (start -2.5 1.25) (end 2.5 1.25) (layer F.SilkS) (width 0.25))
  (fp_text user GND (at 4.25 2.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user RST (at -4.25 2.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user MOSI (at 4.25 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user SCK (at -4 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VCC (at 4 -2.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user MISO (at -4.25 -2.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole circle (at -1.27 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu F.Mask))
  (pad 2 thru_hole circle (at 1.27 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu F.Mask))
  (pad 3 thru_hole circle (at -1.27 0) (size 1.7 1.7) (drill 1) (layers *.Cu F.Mask))
  (pad 4 thru_hole circle (at 1.27 0) (size 1.7 1.7) (drill 1) (layers *.Cu F.Mask))
  (pad 5 thru_hole circle (at -1.27 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu F.Mask))
  (pad 6 thru_hole rect (at 1.27 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu F.Mask))
)
