(footprint "vik-module-throughole" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 1.62 -0.5 unlocked) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp eb26614f-425b-4449-963b-5ed24e5e61a8)
  )
  (fp_text value "vik-module-throughole" (at 2.7 1 unlocked) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 36098acb-a4d3-48cf-9968-60aad765d2f9)
  )
  (fp_text user "SDA" (at -1.99 -2.82 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp 21efb994-0217-46ac-bfe0-0999afc9cf76)
  )
  (fp_text user "MISO" (at 8.33 -2.79 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp 275bf651-2d8f-4070-8109-86d17f385192)
  )
  (fp_text user "3.3V" (at -4.46 -2.78 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp 2f90b66a-007d-4f47-a3f2-d8b30d4c288d)
  )
  (fp_text user "MOSI" (at 3.27 6.05 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp 70f7aedb-93de-4fa6-bf4f-04437f5a0f54)
  )
  (fp_text user "SCLK" (at 8.37 6.21 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp 744b139f-0d05-4839-aa34-c34f851b8c63)
  )
  (fp_text user "SPI CS" (at 5.82 7.64 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp 9e97d068-77ee-4d3a-9b9c-8d886d830744)
  )
  (fp_text user "RGB" (at 0.68 -2.76 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp a51a2213-6f61-401d-8cd8-1218b3b2e263)
  )
  (fp_text user "GP AD2" (at 5.72 -2.48 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp aa396028-b86e-40e1-be35-000ada6b6c8e)
  )
  (fp_text user "5V" (at 0.7 4.48 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp bf9baf8e-5fc6-4b96-9f7f-9f49d0b2dc27)
  )
  (fp_text user "SCL" (at -1.91 5.31 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp c5f68e0b-f0de-4158-8a10-fc73c9d31a15)
  )
  (fp_text user "VIK IN" (at -6.75 2.46 90 unlocked) (layer "F.SilkS" knockout)
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp d24b72f2-346a-4e2d-a7fa-1385205157f0)
  )
  (fp_text user "GND" (at -4.38 5.59 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp d44eca05-6b62-4d42-817d-81bf87e6a833)
  )
  (fp_text user "GP AD1" (at 3.23 -2.46 90 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
    (tstamp df40c44f-6991-4248-9d0f-fd6df1f41818)
  )
  (pad "1" thru_hole circle (at 7.7 1.27) (size 1.5 1.5) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 6dc998f0-8589-4185-b1b0-af864daa711b))
  (pad "2" thru_hole circle (at 7.7 -1.27) (size 1.5 1.5) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 8792fca8-804c-4ec9-8760-ce99048e45cd))
  (pad "3" thru_hole circle (at 5.16 1.27) (size 1.5 1.5) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp fd546028-f98c-4af7-baff-0e26660c88b7))
  (pad "4" thru_hole circle (at 5.16 -1.27) (size 1.5 1.5) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp aa9e3d24-644d-4a77-938f-442e8b9077d6))
  (pad "5" thru_hole circle (at 2.62 1.27) (size 1.5 1.5) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 88257fb9-cb1a-4f02-84b3-bb9052210889))
  (pad "6" thru_hole circle (at 2.62 -1.27) (size 1.5 1.5) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 122cdd8b-f10a-4ee6-a80f-88347822c37e))
  (pad "7" thru_hole circle (at 0.08 1.27) (size 1.5 1.5) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 2e753262-ae42-4e4d-865e-1f715cc786db))
  (pad "8" thru_hole circle (at 0.08 -1.27) (size 1.5 1.5) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 1ff5b634-79ad-4af8-90e8-1feac5150784))
  (pad "9" thru_hole circle (at -2.46 1.27) (size 1.5 1.5) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp d88bd4a2-4ad2-4780-8252-6d128d2b258c))
  (pad "10" thru_hole circle (at -2.46 -1.27) (size 1.5 1.5) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp ea1c4ac6-520b-4ee9-a4f6-c30ed89b4a12))
  (pad "11" thru_hole circle (at -5 1.27) (size 1.5 1.5) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 74e9ff98-0ce3-4a3c-b76a-35f1696ed318))
  (pad "12" thru_hole circle (at -5 -1.27) (size 1.5 1.5) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 8d7ea8c9-e9ff-4abc-8c6b-611df631a621))
)
