(module ArduinoProMicro-Mini-USB-ZigZag (layer F.Cu) (tedit 5CEEEAD7)
  (fp_text reference U1 (at 0 1.125) (layer F.SilkS) hide
    (effects (font (size 1.27 1.524) (thickness 0.2032)))
  )
  (fp_text value ProMicro (at 0 -1) (layer F.SilkS) hide
    (effects (font (size 1.27 1.524) (thickness 0.2032)))
  )
  (fp_line (start -12.7 8.85) (end -12.7 11.39) (layer B.SilkS) (width 0.381))
  (fp_line (start -15.24 8.85) (end -12.7 8.85) (layer B.SilkS) (width 0.381))
  (fp_text user D2 (at -11.43 7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user D0 (at -1.27 7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user D1 (at -3.81 7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user GND (at -6.35 7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user GND (at -8.89 7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user D4 (at 1.27 7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user C6 (at 3.81 7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user D7 (at 6.35 7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user E6 (at 8.89 7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user B4 (at 11.43 7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user B5 (at 13.97 7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user B6 (at 13.97 -7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user B2 (at 11.43 -7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user B3 (at 8.89 -7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user B1 (at 6.35 -7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user F7 (at 3.81 -7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user F6 (at 1.27 -7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user F5 (at -1.27 -7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user F4 (at -3.81 -7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user VCC (at -6.35 -7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user GND (at -11.43 -7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user RAW (at -13.97 -7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user RAW (at -13.97 -7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GND (at -11.43 -7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user ST (at -8.92 -8.23312 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user VCC (at -6.35 -7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user F4 (at -3.81 -7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user F5 (at -1.27 -7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user F6 (at 1.27 -7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user F7 (at 3.81 -7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user B1 (at 6.35 -7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user B3 (at 8.89 -7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user B2 (at 11.43 -7.961 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user B6 (at 13.97 -7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user B5 (at 13.97 7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user B4 (at 11.43 7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user E6 (at 8.89 7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user D7 (at 6.35 7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user C6 (at 3.81 7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user D4 (at 1.27 7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GND (at -8.89 7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GND (at -6.35 7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user D1 (at -3.81 7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user D0 (at -1.27 7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user D2 (at -11.43 7.961 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user TX0/D3 (at -13.97 6.071872 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_text user TX0/D3 (at -13.97 6.071872 90) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_line (start -24.04 -11.39) (end -24.04 11.39) (layer F.SilkS) (width 0.381))
  (fp_line (start -24.04 11.39) (end 15.24 11.39) (layer F.SilkS) (width 0.381))
  (fp_line (start 15.24 11.39) (end 15.24 -11.39) (layer F.SilkS) (width 0.381))
  (fp_line (start 15.24 -11.39) (end -24.04 -11.39) (layer F.SilkS) (width 0.381))
  (fp_line (start -15.24 8.85) (end -12.7 8.85) (layer F.SilkS) (width 0.381))
  (fp_line (start -12.7 8.85) (end -12.7 11.39) (layer F.SilkS) (width 0.381))
  (fp_poly (pts (xy -9.36064 -7.431568) (xy -9.06064 -7.431568) (xy -9.06064 -7.331568) (xy -9.36064 -7.331568)) (layer F.SilkS) (width 0.15))
  (fp_poly (pts (xy -8.96064 -7.231568) (xy -8.86064 -7.231568) (xy -8.86064 -7.131568) (xy -8.96064 -7.131568)) (layer F.SilkS) (width 0.15))
  (fp_poly (pts (xy -9.36064 -7.431568) (xy -9.26064 -7.431568) (xy -9.26064 -6.931568) (xy -9.36064 -6.931568)) (layer F.SilkS) (width 0.15))
  (fp_poly (pts (xy -9.36064 -7.031568) (xy -8.56064 -7.031568) (xy -8.56064 -6.931568) (xy -9.36064 -6.931568)) (layer F.SilkS) (width 0.15))
  (fp_poly (pts (xy -8.76064 -7.431568) (xy -8.56064 -7.431568) (xy -8.56064 -7.331568) (xy -8.76064 -7.331568)) (layer F.SilkS) (width 0.15))
  (fp_text user ST (at -8.91 -7.54 90) (layer B.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)) (justify mirror))
  )
  (fp_poly (pts (xy -8.95097 -8.544635) (xy -8.85097 -8.544635) (xy -8.85097 -8.644635) (xy -8.95097 -8.644635)) (layer B.SilkS) (width 0.15))
  (fp_poly (pts (xy -9.35097 -8.744635) (xy -8.55097 -8.744635) (xy -8.55097 -8.844635) (xy -9.35097 -8.844635)) (layer B.SilkS) (width 0.15))
  (fp_poly (pts (xy -8.75097 -8.344635) (xy -8.55097 -8.344635) (xy -8.55097 -8.444635) (xy -8.75097 -8.444635)) (layer B.SilkS) (width 0.15))
  (fp_poly (pts (xy -9.35097 -8.344635) (xy -9.05097 -8.344635) (xy -9.05097 -8.444635) (xy -9.35097 -8.444635)) (layer B.SilkS) (width 0.15))
  (fp_poly (pts (xy -9.35097 -8.344635) (xy -9.25097 -8.344635) (xy -9.25097 -8.844635) (xy -9.35097 -8.844635)) (layer B.SilkS) (width 0.15))
  (fp_line (start 15.24 -11.39) (end -24.04 -11.39) (layer B.SilkS) (width 0.381))
  (fp_line (start 15.24 11.39) (end 15.24 -11.39) (layer B.SilkS) (width 0.381))
  (fp_line (start -24.04 11.39) (end 15.24 11.39) (layer B.SilkS) (width 0.381))
  (fp_line (start -24.04 -11.39) (end -24.04 11.39) (layer B.SilkS) (width 0.381))
  (fp_line (start -15.24 8.85) (end -15.24 11.39) (layer F.SilkS) (width 0.381))
  (fp_line (start -15.24 8.85) (end -15.24 11.39) (layer B.SilkS) (width 0.381))
  (fp_line (start -16 4) (end -16 -4) (layer F.SilkS) (width 0.2))
  (fp_line (start -16 -4) (end -25.5 -4) (layer F.SilkS) (width 0.2))
  (fp_line (start -25.5 -4) (end -25.5 4) (layer F.SilkS) (width 0.2))
  (fp_line (start -25.5 4) (end -16 4) (layer F.SilkS) (width 0.2))
  (pad 1 thru_hole rect (at -13.97 10.3486) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 2 thru_hole circle (at -11.43 9.8914) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 3 thru_hole circle (at -8.89 10.3486) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 4 thru_hole circle (at -6.35 9.8914) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 5 thru_hole circle (at -3.81 10.3486) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 6 thru_hole circle (at -1.27 9.8914) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 7 thru_hole circle (at 1.27 10.3486) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 8 thru_hole circle (at 3.81 9.8914) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 9 thru_hole circle (at 6.35 10.3486) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 10 thru_hole circle (at 8.89 9.8914) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 11 thru_hole circle (at 11.43 10.3486) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 13 thru_hole circle (at 13.97 -9.8914) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 14 thru_hole circle (at 11.43 -10.3486) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 15 thru_hole circle (at 8.89 -9.8914) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 16 thru_hole circle (at 6.35 -10.3486) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 17 thru_hole circle (at 3.81 -9.8914) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 18 thru_hole circle (at 1.27 -10.3486) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 19 thru_hole circle (at -1.27 -9.8914) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 20 thru_hole circle (at -3.81 -10.3486) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 21 thru_hole circle (at -6.35 -9.8914) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 22 thru_hole circle (at -8.89 -10.3486) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 23 thru_hole circle (at -11.43 -9.8914) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 12 thru_hole circle (at 13.97 9.8914) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 24 thru_hole circle (at -13.97 -10.3486) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
)
