(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "SATA_COMBINED_22" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at 0 -31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SATA_COMBINED_22" (id 1) (at 0 31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 3.81 10.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 3.81 10.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "SATA 22-pin Female Data and Power Connector" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SATA_COMBINED_22_0_1"
      (rectangle (start 3.81 30.48) (end -3.81 -30.48)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "SATA_COMBINED_22_1_1"
      (pin power_out line (at -7.62 27.94 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 2.54 0) (length 3.81)
        (name "PWDIS" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 0 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -2.54 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -5.08 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -7.62 0) (length 3.81)
        (name "V5.0" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -10.16 0) (length 3.81)
        (name "V5.0" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -12.7 0) (length 3.81)
        (name "V5.0" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -15.24 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -7.62 -17.78 0) (length 3.81)
        (name "ACT" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -20.32 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -7.62 25.4 0) (length 3.81)
        (name "A+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -22.86 0) (length 3.81)
        (name "V12" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -25.4 0) (length 3.81)
        (name "V12" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -27.94 0) (length 3.81)
        (name "V12" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -7.62 22.86 0) (length 3.81)
        (name "A-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 20.32 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 17.78 0) (length 3.81)
        (name "B-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 15.24 0) (length 3.81)
        (name "B+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 12.7 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 7.62 0) (length 3.81)
        (name "V3.3" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 5.08 0) (length 3.81)
        (name "V3.3" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SATA_DATA_7" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at 0 -11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SATA_DATA_7" (id 1) (at 0 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 7.62 11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 7.62 11.43 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "SATA 7-pin Male Data Connector" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SATA_DATA_7_0_1"
      (rectangle (start 3.81 10.16) (end -3.81 -10.16)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "SATA_DATA_7_1_1"
      (pin power_out line (at -7.62 7.62 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -7.62 5.08 0) (length 3.81)
        (name "A+" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -7.62 2.54 0) (length 3.81)
        (name "A-" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 0 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -2.54 0) (length 3.81)
        (name "B-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -7.62 -5.08 0) (length 3.81)
        (name "B+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -7.62 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SATA_POWER_15" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at 0 -31.75 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SATA_POWER_15" (id 1) (at 0 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 -34.29 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 3.81 10.16 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "SATA 15-pin Male Power Connector" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SATA_POWER_15_0_1"
      (rectangle (start 3.81 10.16) (end -3.81 -30.48)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "SATA_POWER_15_1_1"
      (pin power_out line (at -7.62 7.62 0) (length 3.81)
        (name "V3.3" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -15.24 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -7.62 -17.78 0) (length 3.81)
        (name "ACT" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -20.32 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -22.86 0) (length 3.81)
        (name "V12" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -25.4 0) (length 3.81)
        (name "V12" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -27.94 0) (length 3.81)
        (name "V12" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 5.08 0) (length 3.81)
        (name "V3.3" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 2.54 0) (length 3.81)
        (name "PWDIS" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 0 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -2.54 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -5.08 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -7.62 0) (length 3.81)
        (name "V5.0" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -10.16 0) (length 3.81)
        (name "V5.0" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -7.62 -12.7 0) (length 3.81)
        (name "V5.0" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
