(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "LR1110IMLTRT" (in_bom yes) (on_board yes)
    (property "Reference" "IC" (at 36.83 22.86 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "LR1110IMLTRT" (at 36.83 20.32 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "QFN50P500X500X100-33N-D" (at 36.83 -79.68 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "" (at 36.83 -179.68 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "RF Transceiver LONG RANGE WI-FI LOC LORA TRANSCEIVER" (at 36.83 -279.68 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "1" (at 36.83 -379.68 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "SEMTECH" (at 36.83 -479.68 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "LR1110IMLTRT" (at 36.83 -579.68 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "947-LR1110IMLTRT" (at 36.83 -679.68 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Semtech/LR1110IMLTRT?qs=GedFDFLaBXFCcMA0cJwOqg%3D%3D" (at 36.83 -779.68 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Part Number" "LR1110IMLTRT" (at 36.83 -879.68 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/lr1110imltrt/semtech?region=nac" (at 36.83 -979.68 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 17.78)
      (end 35.56 -30.48)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin passive line (at 0 0 0) (length 5.08)
      (name "VR_PA" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "VBAT_RF" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "VTCXO" (effects (font (size 1.27 1.27))))
      (number "3" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -7.62 0) (length 5.08)
      (name "XTA" (effects (font (size 1.27 1.27))))
      (number "4" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -10.16 0) (length 5.08)
      (name "XTB" (effects (font (size 1.27 1.27))))
      (number "5" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -12.7 0) (length 5.08)
      (name "NRESET" (effects (font (size 1.27 1.27))))
      (number "6" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -15.24 0) (length 5.08)
      (name "32K_P/_DIO11" (effects (font (size 1.27 1.27))))
      (number "7" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -17.78 0) (length 5.08)
      (name "32K_N/_DIO10" (effects (font (size 1.27 1.27))))
      (number "8" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 10.16 -35.56 90) (length 5.08)
      (name "DIO9" (effects (font (size 1.27 1.27))))
      (number "9" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 12.7 -35.56 90) (length 5.08)
      (name "DIO8" (effects (font (size 1.27 1.27))))
      (number "10" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 15.24 -35.56 90) (length 5.08)
      (name "DIO7" (effects (font (size 1.27 1.27))))
      (number "11" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 17.78 -35.56 90) (length 5.08)
      (name "VREG" (effects (font (size 1.27 1.27))))
      (number "12" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 20.32 -35.56 90) (length 5.08)
      (name "GND_1" (effects (font (size 1.27 1.27))))
      (number "13" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 22.86 -35.56 90) (length 5.08)
      (name "DCC_SW" (effects (font (size 1.27 1.27))))
      (number "14" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 25.4 -35.56 90) (length 5.08)
      (name "VBAT" (effects (font (size 1.27 1.27))))
      (number "15" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 27.94 -35.56 90) (length 5.08)
      (name "DNC_1" (effects (font (size 1.27 1.27))))
      (number "16" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 40.64 0 180) (length 5.08)
      (name "DIO1" (effects (font (size 1.27 1.27))))
      (number "24" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 40.64 -2.54 180) (length 5.08)
      (name "DIO2" (effects (font (size 1.27 1.27))))
      (number "23" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 40.64 -5.08 180) (length 5.08)
      (name "DIO3" (effects (font (size 1.27 1.27))))
      (number "22" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 40.64 -7.62 180) (length 5.08)
      (name "DIO4" (effects (font (size 1.27 1.27))))
      (number "21" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 40.64 -10.16 180) (length 5.08)
      (name "DIO5" (effects (font (size 1.27 1.27))))
      (number "20" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 40.64 -12.7 180) (length 5.08)
      (name "DIO6" (effects (font (size 1.27 1.27))))
      (number "19" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 40.64 -15.24 180) (length 5.08)
      (name "DNC_3" (effects (font (size 1.27 1.27))))
      (number "18" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 40.64 -17.78 180) (length 5.08)
      (name "DNC_2" (effects (font (size 1.27 1.27))))
      (number "17" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 10.16 22.86 270) (length 5.08)
      (name "GND_2" (effects (font (size 1.27 1.27))))
      (number "33" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 12.7 22.86 270) (length 5.08)
      (name "RFO_HP_LF" (effects (font (size 1.27 1.27))))
      (number "32" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 15.24 22.86 270) (length 5.08)
      (name "RFO_LP_LF" (effects (font (size 1.27 1.27))))
      (number "31" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 17.78 22.86 270) (length 5.08)
      (name "RFI_P_LF0" (effects (font (size 1.27 1.27))))
      (number "30" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 20.32 22.86 270) (length 5.08)
      (name "RFI_N_LF0" (effects (font (size 1.27 1.27))))
      (number "29" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 22.86 22.86 270) (length 5.08)
      (name "RFI_P_LF1" (effects (font (size 1.27 1.27))))
      (number "28" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 25.4 22.86 270) (length 5.08)
      (name "RFI_N_LF1" (effects (font (size 1.27 1.27))))
      (number "27" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 27.94 22.86 270) (length 5.08)
      (name "RFIO_HF" (effects (font (size 1.27 1.27))))
      (number "26" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 30.48 22.86 270) (length 5.08)
      (name "DIO0/BUSY" (effects (font (size 1.27 1.27))))
      (number "25" (effects (font (size 1.27 1.27))))
    )
  )
)
