(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "MASWSS0136TR-3000" (in_bom yes) (on_board yes)
    (property "Reference" "S" (at 21.59 7.62 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "MASWSS0136TR-3000" (at 21.59 5.08 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "SOT65P210X110-6N" (at 21.59 -94.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "https://rs.componentsearchengine.com/Datasheets/1/MASWSS0136TR-3000.pdf" (at 21.59 -194.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "RF Switch ICs DC-3.0GHz ISO 27dB IL .4dB @2.4GHz" (at 21.59 -294.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "1.1" (at 21.59 -394.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "MACOM" (at 21.59 -494.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "MASWSS0136TR-3000" (at 21.59 -594.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "937-MASWSS0136-T" (at 21.59 -694.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/MACOM/MASWSS0136TR-3000?qs=3Wmz%2FrCSAaHZLGvANOUDKw%3D%3D" (at 21.59 -794.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Part Number" "" (at 21.59 -894.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Price/Stock" "" (at 21.59 -994.92 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 2.54)
      (end 20.32 -7.62)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin bidirectional line (at 0 0 0) (length 5.08)
      (name "RF1" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "GND" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "RF2" (effects (font (size 1.27 1.27))))
      (number "3" (effects (font (size 1.27 1.27))))
    )
    (pin input line (at 25.4 0 180) (length 5.08)
      (name "V1" (effects (font (size 1.27 1.27))))
      (number "6" (effects (font (size 1.27 1.27))))
    )
    (pin bidirectional line (at 25.4 -2.54 180) (length 5.08)
      (name "RFC" (effects (font (size 1.27 1.27))))
      (number "5" (effects (font (size 1.27 1.27))))
    )
    (pin input line (at 25.4 -5.08 180) (length 5.08)
      (name "V2" (effects (font (size 1.27 1.27))))
      (number "4" (effects (font (size 1.27 1.27))))
    )
  )
)
